diff --git a/drivers/gpu/drm/amd/amdgpu/amdgpu_cgs.c b/drivers/gpu/drm/amd/amdgpu/amdgpu_cgs.c
index c0a8062..65c1170 100644
--- a/drivers/gpu/drm/amd/amdgpu/amdgpu_cgs.c
+++ b/drivers/gpu/drm/amd/amdgpu/amdgpu_cgs.c
@@ -734,7 +734,7 @@ static int amdgpu_cgs_get_firmware_info(struct cgs_device *cgs_device,
 
 			err = amdgpu_ucode_validate(adev->pm.fw);
 			if (err) {
-				DRM_ERROR("Failed to load firmware \"%s\"", fw_name);
+				DRM_ERROR("Failed to load firmware", fw_name);
 				release_firmware(adev->pm.fw);
 				adev->pm.fw = NULL;
 				return err;
diff --git a/drivers/gpu/drm/amd/amdgpu/amdgpu_uvd.c b/drivers/gpu/drm/amd/amdgpu/amdgpu_uvd.c
index 2ca09f1..15caf24 100644
--- a/drivers/gpu/drm/amd/amdgpu/amdgpu_uvd.c
+++ b/drivers/gpu/drm/amd/amdgpu/amdgpu_uvd.c
@@ -173,7 +173,7 @@ int amdgpu_uvd_sw_init(struct amdgpu_device *adev)
 
 	r = request_firmware(&adev->uvd.fw, fw_name, adev->dev);
 	if (r) {
-		dev_err(adev->dev, "amdgpu_uvd: Can't load firmware \"%s\"\n",
+		dev_err(adev->dev, "amdgpu_uvd: Can't load firmware\n",
 			fw_name);
 		return r;
 	}
diff --git a/drivers/gpu/drm/amd/amdgpu/amdgpu_vce.c b/drivers/gpu/drm/amd/amdgpu/amdgpu_vce.c
index b692ad4..1ca7f9f 100644
--- a/drivers/gpu/drm/amd/amdgpu/amdgpu_vce.c
+++ b/drivers/gpu/drm/amd/amdgpu/amdgpu_vce.c
@@ -140,7 +140,7 @@ int amdgpu_vce_sw_init(struct amdgpu_device *adev, unsigned long size)
 
 	r = request_firmware(&adev->vce.fw, fw_name, adev->dev);
 	if (r) {
-		dev_err(adev->dev, "amdgpu_vce: Can't load firmware \"%s\"\n",
+		dev_err(adev->dev, "amdgpu_vce: Can't load firmware\n",
 			fw_name);
 		return r;
 	}
diff --git a/drivers/gpu/drm/amd/amdgpu/ci_dpm.c b/drivers/gpu/drm/amd/amdgpu/ci_dpm.c
index cb508a2..ca4453b 100644
--- a/drivers/gpu/drm/amd/amdgpu/ci_dpm.c
+++ b/drivers/gpu/drm/amd/amdgpu/ci_dpm.c
@@ -5848,7 +5848,7 @@ static int ci_dpm_init_microcode(struct amdgpu_device *adev)
 
 out:
 	if (err) {
-		pr_err("cik_smc: Failed to load firmware \"%s\"\n", fw_name);
+		pr_err("cik_smc: Failed to load firmware\n", fw_name);
 		release_firmware(adev->pm.fw);
 		adev->pm.fw = NULL;
 	}
diff --git a/drivers/gpu/drm/amd/amdgpu/cik_sdma.c b/drivers/gpu/drm/amd/amdgpu/cik_sdma.c
index c216e16..4a399cc 100644
--- a/drivers/gpu/drm/amd/amdgpu/cik_sdma.c
+++ b/drivers/gpu/drm/amd/amdgpu/cik_sdma.c
@@ -142,7 +142,7 @@ static int cik_sdma_init_microcode(struct amdgpu_device *adev)
 	}
 out:
 	if (err) {
-		pr_err("cik_sdma: Failed to load firmware \"%s\"\n", fw_name);
+		pr_err("cik_sdma: Failed to load firmware\n", fw_name);
 		for (i = 0; i < adev->sdma.num_instances; i++) {
 			release_firmware(adev->sdma.instance[i].fw);
 			adev->sdma.instance[i].fw = NULL;
diff --git a/drivers/gpu/drm/amd/amdgpu/gfx_v7_0.c b/drivers/gpu/drm/amd/amdgpu/gfx_v7_0.c
index 37b45e4..b7fa33c 100644
--- a/drivers/gpu/drm/amd/amdgpu/gfx_v7_0.c
+++ b/drivers/gpu/drm/amd/amdgpu/gfx_v7_0.c
@@ -973,7 +973,7 @@ static int gfx_v7_0_init_microcode(struct amdgpu_device *adev)
 
 out:
 	if (err) {
-		pr_err("gfx7: Failed to load firmware \"%s\"\n", fw_name);
+		pr_err("gfx7: Failed to load firmware\n", fw_name);
 		release_firmware(adev->gfx.pfp_fw);
 		adev->gfx.pfp_fw = NULL;
 		release_firmware(adev->gfx.me_fw);
diff --git a/drivers/gpu/drm/amd/amdgpu/gfx_v8_0.c b/drivers/gpu/drm/amd/amdgpu/gfx_v8_0.c
index aa5a50f..c7acffb 100644
--- a/drivers/gpu/drm/amd/amdgpu/gfx_v8_0.c
+++ b/drivers/gpu/drm/amd/amdgpu/gfx_v8_0.c
@@ -1106,7 +1106,7 @@ static int gfx_v8_0_init_microcode(struct amdgpu_device *adev)
 out:
 	if (err) {
 		dev_err(adev->dev,
-			"gfx8: Failed to load firmware \"%s\"\n",
+			"gfx8: Failed to load firmware\n",
 			fw_name);
 		release_firmware(adev->gfx.pfp_fw);
 		adev->gfx.pfp_fw = NULL;
diff --git a/drivers/gpu/drm/amd/amdgpu/gmc_v7_0.c b/drivers/gpu/drm/amd/amdgpu/gmc_v7_0.c
index 7e9ea53..6815fb5 100644
--- a/drivers/gpu/drm/amd/amdgpu/gmc_v7_0.c
+++ b/drivers/gpu/drm/amd/amdgpu/gmc_v7_0.c
@@ -163,7 +163,7 @@ static int gmc_v7_0_init_microcode(struct amdgpu_device *adev)
 
 out:
 	if (err) {
-		pr_err("cik_mc: Failed to load firmware \"%s\"\n", fw_name);
+		pr_err("cik_mc: Failed to load firmware\n", fw_name);
 		release_firmware(adev->mc.fw);
 		adev->mc.fw = NULL;
 	}
diff --git a/drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c b/drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c
index cc9f880..67359b3 100644
--- a/drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c
+++ b/drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c
@@ -247,7 +247,7 @@ static int gmc_v8_0_init_microcode(struct amdgpu_device *adev)
 
 out:
 	if (err) {
-		pr_err("mc: Failed to load firmware \"%s\"\n", fw_name);
+		pr_err("mc: Failed to load firmware\n", fw_name);
 		release_firmware(adev->mc.fw);
 		adev->mc.fw = NULL;
 	}
diff --git a/drivers/gpu/drm/amd/amdgpu/sdma_v2_4.c b/drivers/gpu/drm/amd/amdgpu/sdma_v2_4.c
index f2d0710..bf0edd5 100644
--- a/drivers/gpu/drm/amd/amdgpu/sdma_v2_4.c
+++ b/drivers/gpu/drm/amd/amdgpu/sdma_v2_4.c
@@ -170,7 +170,7 @@ static int sdma_v2_4_init_microcode(struct amdgpu_device *adev)
 
 out:
 	if (err) {
-		pr_err("sdma_v2_4: Failed to load firmware \"%s\"\n", fw_name);
+		pr_err("sdma_v2_4: Failed to load firmware\n", fw_name);
 		for (i = 0; i < adev->sdma.num_instances; i++) {
 			release_firmware(adev->sdma.instance[i].fw);
 			adev->sdma.instance[i].fw = NULL;
diff --git a/drivers/gpu/drm/amd/amdgpu/sdma_v3_0.c b/drivers/gpu/drm/amd/amdgpu/sdma_v3_0.c
index 1d766ae..1103992 100644
--- a/drivers/gpu/drm/amd/amdgpu/sdma_v3_0.c
+++ b/drivers/gpu/drm/amd/amdgpu/sdma_v3_0.c
@@ -321,7 +321,7 @@ static int sdma_v3_0_init_microcode(struct amdgpu_device *adev)
 	}
 out:
 	if (err) {
-		pr_err("sdma_v3_0: Failed to load firmware \"%s\"\n", fw_name);
+		pr_err("sdma_v3_0: Failed to load firmware\n", fw_name);
 		for (i = 0; i < adev->sdma.num_instances; i++) {
 			release_firmware(adev->sdma.instance[i].fw);
 			adev->sdma.instance[i].fw = NULL;
diff --git a/drivers/gpu/drm/drm_edid_load.c b/drivers/gpu/drm/drm_edid_load.c
index 1c0495a..0085e8e 100644
--- a/drivers/gpu/drm/drm_edid_load.c
+++ b/drivers/gpu/drm/drm_edid_load.c
@@ -188,8 +188,8 @@ static void *edid_load(struct drm_connector *connector, const char *name,
 		err = request_firmware(&fw, name, &pdev->dev);
 		platform_device_unregister(pdev);
 		if (err) {
-			DRM_ERROR("Requesting EDID firmware \"%s\" failed (err=%d)\n",
-				  name, err);
+			DRM_ERROR("Requesting EDID firmware failed (err=%d)\n",
+				  err);
 			return ERR_PTR(err);
 		}
 
diff --git a/drivers/gpu/drm/nouveau/nvkm/engine/xtensa.c b/drivers/gpu/drm/nouveau/nvkm/engine/xtensa.c
index 06bdb67..7eca739 100644
--- a/drivers/gpu/drm/nouveau/nvkm/engine/xtensa.c
+++ b/drivers/gpu/drm/nouveau/nvkm/engine/xtensa.c
@@ -109,7 +109,7 @@ nvkm_xtensa_init(struct nvkm_engine *engine)
 
 		ret = request_firmware(&fw, name, device->dev);
 		if (ret) {
-			nvkm_warn(subdev, "unable to load firmware %s\n", name);
+			nvkm_warn(subdev, "unable to load firmware\n", name);
 			return ret;
 		}
 
diff --git a/drivers/gpu/drm/r128/r128_cce.c b/drivers/gpu/drm/r128/r128_cce.c
index c9890af..cfe11ce 100644
--- a/drivers/gpu/drm/r128/r128_cce.c
+++ b/drivers/gpu/drm/r128/r128_cce.c
@@ -155,13 +155,13 @@ static int r128_cce_load_microcode(drm_r128_private_t *dev_priv)
 	rc = request_firmware(&fw, FIRMWARE_NAME, &pdev->dev);
 	platform_device_unregister(pdev);
 	if (rc) {
-		pr_err("r128_cce: Failed to load firmware \"%s\"\n",
+		pr_err("r128_cce: Failed to load firmware\n",
 		       FIRMWARE_NAME);
 		return rc;
 	}
 
 	if (fw->size != 256 * 8) {
-		pr_err("r128_cce: Bogus length %zu in firmware \"%s\"\n",
+		pr_err("r128_cce: Bogus length %zu in firmware\n",
 		       fw->size, FIRMWARE_NAME);
 		rc = -EINVAL;
 		goto out_release;
diff --git a/drivers/gpu/drm/radeon/cik.c b/drivers/gpu/drm/radeon/cik.c
index 3cb6c55..5bf3ff6 100644
--- a/drivers/gpu/drm/radeon/cik.c
+++ b/drivers/gpu/drm/radeon/cik.c
@@ -2072,7 +2072,7 @@ static int cik_init_microcode(struct radeon_device *rdev)
 		if (err)
 			goto out;
 		if (rdev->pfp_fw->size != pfp_req_size) {
-			pr_err("cik_cp: Bogus length %zu in firmware \"%s\"\n",
+			pr_err("cik_cp: Bogus length %zu in firmware\n",
 			       rdev->pfp_fw->size, fw_name);
 			err = -EINVAL;
 			goto out;
@@ -2080,7 +2080,7 @@ static int cik_init_microcode(struct radeon_device *rdev)
 	} else {
 		err = radeon_ucode_validate(rdev->pfp_fw);
 		if (err) {
-			pr_err("cik_fw: validation failed for firmware \"%s\"\n",
+			pr_err("cik_fw: validation failed for firmware\n",
 			       fw_name);
 			goto out;
 		} else {
@@ -2096,14 +2096,14 @@ static int cik_init_microcode(struct radeon_device *rdev)
 		if (err)
 			goto out;
 		if (rdev->me_fw->size != me_req_size) {
-			pr_err("cik_cp: Bogus length %zu in firmware \"%s\"\n",
+			pr_err("cik_cp: Bogus length %zu in firmware\n",
 			       rdev->me_fw->size, fw_name);
 			err = -EINVAL;
 		}
 	} else {
 		err = radeon_ucode_validate(rdev->me_fw);
 		if (err) {
-			pr_err("cik_fw: validation failed for firmware \"%s\"\n",
+			pr_err("cik_fw: validation failed for firmware\n",
 			       fw_name);
 			goto out;
 		} else {
@@ -2119,14 +2119,14 @@ static int cik_init_microcode(struct radeon_device *rdev)
 		if (err)
 			goto out;
 		if (rdev->ce_fw->size != ce_req_size) {
-			pr_err("cik_cp: Bogus length %zu in firmware \"%s\"\n",
+			pr_err("cik_cp: Bogus length %zu in firmware\n",
 			       rdev->ce_fw->size, fw_name);
 			err = -EINVAL;
 		}
 	} else {
 		err = radeon_ucode_validate(rdev->ce_fw);
 		if (err) {
-			pr_err("cik_fw: validation failed for firmware \"%s\"\n",
+			pr_err("cik_fw: validation failed for firmware\n",
 			       fw_name);
 			goto out;
 		} else {
@@ -2142,14 +2142,14 @@ static int cik_init_microcode(struct radeon_device *rdev)
 		if (err)
 			goto out;
 		if (rdev->mec_fw->size != mec_req_size) {
-			pr_err("cik_cp: Bogus length %zu in firmware \"%s\"\n",
+			pr_err("cik_cp: Bogus length %zu in firmware\n",
 			       rdev->mec_fw->size, fw_name);
 			err = -EINVAL;
 		}
 	} else {
 		err = radeon_ucode_validate(rdev->mec_fw);
 		if (err) {
-			pr_err("cik_fw: validation failed for firmware \"%s\"\n",
+			pr_err("cik_fw: validation failed for firmware\n",
 			       fw_name);
 			goto out;
 		} else {
@@ -2180,14 +2180,14 @@ static int cik_init_microcode(struct radeon_device *rdev)
 		if (err)
 			goto out;
 		if (rdev->rlc_fw->size != rlc_req_size) {
-			pr_err("cik_rlc: Bogus length %zu in firmware \"%s\"\n",
+			pr_err("cik_rlc: Bogus length %zu in firmware\n",
 			       rdev->rlc_fw->size, fw_name);
 			err = -EINVAL;
 		}
 	} else {
 		err = radeon_ucode_validate(rdev->rlc_fw);
 		if (err) {
-			pr_err("cik_fw: validation failed for firmware \"%s\"\n",
+			pr_err("cik_fw: validation failed for firmware\n",
 			       fw_name);
 			goto out;
 		} else {
@@ -2203,14 +2203,14 @@ static int cik_init_microcode(struct radeon_device *rdev)
 		if (err)
 			goto out;
 		if (rdev->sdma_fw->size != sdma_req_size) {
-			pr_err("cik_sdma: Bogus length %zu in firmware \"%s\"\n",
+			pr_err("cik_sdma: Bogus length %zu in firmware\n",
 			       rdev->sdma_fw->size, fw_name);
 			err = -EINVAL;
 		}
 	} else {
 		err = radeon_ucode_validate(rdev->sdma_fw);
 		if (err) {
-			pr_err("cik_fw: validation failed for firmware \"%s\"\n",
+			pr_err("cik_fw: validation failed for firmware\n",
 			       fw_name);
 			goto out;
 		} else {
@@ -2233,7 +2233,7 @@ static int cik_init_microcode(struct radeon_device *rdev)
 			}
 			if ((rdev->mc_fw->size != mc_req_size) &&
 			    (rdev->mc_fw->size != mc2_req_size)){
-				pr_err("cik_mc: Bogus length %zu in firmware \"%s\"\n",
+				pr_err("cik_mc: Bogus length %zu in firmware\n",
 				       rdev->mc_fw->size, fw_name);
 				err = -EINVAL;
 			}
@@ -2241,7 +2241,7 @@ static int cik_init_microcode(struct radeon_device *rdev)
 		} else {
 			err = radeon_ucode_validate(rdev->mc_fw);
 			if (err) {
-				pr_err("cik_fw: validation failed for firmware \"%s\"\n",
+				pr_err("cik_fw: validation failed for firmware\n",
 				       fw_name);
 				goto out;
 			} else {
@@ -2258,20 +2258,20 @@ static int cik_init_microcode(struct radeon_device *rdev)
 			snprintf(fw_name, sizeof(fw_name), "radeon/%s_smc.bin", chip_name);
 			err = request_firmware(&rdev->smc_fw, fw_name, rdev->dev);
 			if (err) {
-				pr_err("smc: error loading firmware \"%s\"\n",
+				pr_err("smc: error loading firmware\n",
 				       fw_name);
 				release_firmware(rdev->smc_fw);
 				rdev->smc_fw = NULL;
 				err = 0;
 			} else if (rdev->smc_fw->size != smc_req_size) {
-				pr_err("cik_smc: Bogus length %zu in firmware \"%s\"\n",
+				pr_err("cik_smc: Bogus length %zu in firmware\n",
 				       rdev->smc_fw->size, fw_name);
 				err = -EINVAL;
 			}
 		} else {
 			err = radeon_ucode_validate(rdev->smc_fw);
 			if (err) {
-				pr_err("cik_fw: validation failed for firmware \"%s\"\n",
+				pr_err("cik_fw: validation failed for firmware\n",
 				       fw_name);
 				goto out;
 			} else {
@@ -2292,7 +2292,7 @@ static int cik_init_microcode(struct radeon_device *rdev)
 out:
 	if (err) {
 		if (err != -EINVAL)
-			pr_err("cik_cp: Failed to load firmware \"%s\"\n",
+			pr_err("cik_cp: Failed to load firmware\n",
 			       fw_name);
 		release_firmware(rdev->pfp_fw);
 		rdev->pfp_fw = NULL;
diff --git a/drivers/gpu/drm/radeon/ni.c b/drivers/gpu/drm/radeon/ni.c
index 9eccd0c..3b9b7d6 100644
--- a/drivers/gpu/drm/radeon/ni.c
+++ b/drivers/gpu/drm/radeon/ni.c
@@ -774,7 +774,7 @@ int ni_init_microcode(struct radeon_device *rdev)
 	if (err)
 		goto out;
 	if (rdev->pfp_fw->size != pfp_req_size) {
-		pr_err("ni_cp: Bogus length %zu in firmware \"%s\"\n",
+		pr_err("ni_cp: Bogus length %zu in firmware\n",
 		       rdev->pfp_fw->size, fw_name);
 		err = -EINVAL;
 		goto out;
@@ -785,7 +785,7 @@ int ni_init_microcode(struct radeon_device *rdev)
 	if (err)
 		goto out;
 	if (rdev->me_fw->size != me_req_size) {
-		pr_err("ni_cp: Bogus length %zu in firmware \"%s\"\n",
+		pr_err("ni_cp: Bogus length %zu in firmware\n",
 		       rdev->me_fw->size, fw_name);
 		err = -EINVAL;
 	}
@@ -795,7 +795,7 @@ int ni_init_microcode(struct radeon_device *rdev)
 	if (err)
 		goto out;
 	if (rdev->rlc_fw->size != rlc_req_size) {
-		pr_err("ni_rlc: Bogus length %zu in firmware \"%s\"\n",
+		pr_err("ni_rlc: Bogus length %zu in firmware\n",
 		       rdev->rlc_fw->size, fw_name);
 		err = -EINVAL;
 	}
@@ -807,7 +807,7 @@ int ni_init_microcode(struct radeon_device *rdev)
 		if (err)
 			goto out;
 		if (rdev->mc_fw->size != mc_req_size) {
-			pr_err("ni_mc: Bogus length %zu in firmware \"%s\"\n",
+			pr_err("ni_mc: Bogus length %zu in firmware\n",
 			       rdev->mc_fw->size, fw_name);
 			err = -EINVAL;
 		}
@@ -817,12 +817,12 @@ int ni_init_microcode(struct radeon_device *rdev)
 		snprintf(fw_name, sizeof(fw_name), "radeon/%s_smc.bin", chip_name);
 		err = request_firmware(&rdev->smc_fw, fw_name, rdev->dev);
 		if (err) {
-			pr_err("smc: error loading firmware \"%s\"\n", fw_name);
+			pr_err("smc: error loading firmware\n", fw_name);
 			release_firmware(rdev->smc_fw);
 			rdev->smc_fw = NULL;
 			err = 0;
 		} else if (rdev->smc_fw->size != smc_req_size) {
-			pr_err("ni_mc: Bogus length %zu in firmware \"%s\"\n",
+			pr_err("ni_mc: Bogus length %zu in firmware\n",
 			       rdev->mc_fw->size, fw_name);
 			err = -EINVAL;
 		}
@@ -831,7 +831,7 @@ int ni_init_microcode(struct radeon_device *rdev)
 out:
 	if (err) {
 		if (err != -EINVAL)
-			pr_err("ni_cp: Failed to load firmware \"%s\"\n",
+			pr_err("ni_cp: Failed to load firmware\n",
 			       fw_name);
 		release_firmware(rdev->pfp_fw);
 		rdev->pfp_fw = NULL;
diff --git a/drivers/gpu/drm/radeon/r100.c b/drivers/gpu/drm/radeon/r100.c
index c31e660..658eaf8 100644
--- a/drivers/gpu/drm/radeon/r100.c
+++ b/drivers/gpu/drm/radeon/r100.c
@@ -1042,9 +1042,9 @@ static int r100_cp_init_microcode(struct radeon_device *rdev)
 
 	err = request_firmware(&rdev->me_fw, fw_name, rdev->dev);
 	if (err) {
-		pr_err("radeon_cp: Failed to load firmware \"%s\"\n", fw_name);
+		pr_err("radeon_cp: Failed to load firmware\n", fw_name);
 	} else if (rdev->me_fw->size % 8) {
-		pr_err("radeon_cp: Bogus length %zu in firmware \"%s\"\n",
+		pr_err("radeon_cp: Bogus length %zu in firmware\n",
 		       rdev->me_fw->size, fw_name);
 		err = -EINVAL;
 		release_firmware(rdev->me_fw);
diff --git a/drivers/gpu/drm/radeon/r600.c b/drivers/gpu/drm/radeon/r600.c
index e06e2d8..9004945 100644
--- a/drivers/gpu/drm/radeon/r600.c
+++ b/drivers/gpu/drm/radeon/r600.c
@@ -2550,7 +2550,7 @@ int r600_init_microcode(struct radeon_device *rdev)
 	if (err)
 		goto out;
 	if (rdev->pfp_fw->size != pfp_req_size) {
-		pr_err("r600_cp: Bogus length %zu in firmware \"%s\"\n",
+		pr_err("r600_cp: Bogus length %zu in firmware\n",
 		       rdev->pfp_fw->size, fw_name);
 		err = -EINVAL;
 		goto out;
@@ -2561,7 +2561,7 @@ int r600_init_microcode(struct radeon_device *rdev)
 	if (err)
 		goto out;
 	if (rdev->me_fw->size != me_req_size) {
-		pr_err("r600_cp: Bogus length %zu in firmware \"%s\"\n",
+		pr_err("r600_cp: Bogus length %zu in firmware\n",
 		       rdev->me_fw->size, fw_name);
 		err = -EINVAL;
 	}
@@ -2571,7 +2571,7 @@ int r600_init_microcode(struct radeon_device *rdev)
 	if (err)
 		goto out;
 	if (rdev->rlc_fw->size != rlc_req_size) {
-		pr_err("r600_rlc: Bogus length %zu in firmware \"%s\"\n",
+		pr_err("r600_rlc: Bogus length %zu in firmware\n",
 		       rdev->rlc_fw->size, fw_name);
 		err = -EINVAL;
 	}
@@ -2580,12 +2580,12 @@ int r600_init_microcode(struct radeon_device *rdev)
 		snprintf(fw_name, sizeof(fw_name), "radeon/%s_smc.bin", smc_chip_name);
 		err = request_firmware(&rdev->smc_fw, fw_name, rdev->dev);
 		if (err) {
-			pr_err("smc: error loading firmware \"%s\"\n", fw_name);
+			pr_err("smc: error loading firmware\n", fw_name);
 			release_firmware(rdev->smc_fw);
 			rdev->smc_fw = NULL;
 			err = 0;
 		} else if (rdev->smc_fw->size != smc_req_size) {
-			pr_err("smc: Bogus length %zu in firmware \"%s\"\n",
+			pr_err("smc: Bogus length %zu in firmware\n",
 			       rdev->smc_fw->size, fw_name);
 			err = -EINVAL;
 		}
@@ -2594,7 +2594,7 @@ int r600_init_microcode(struct radeon_device *rdev)
 out:
 	if (err) {
 		if (err != -EINVAL)
-			pr_err("r600_cp: Failed to load firmware \"%s\"\n",
+			pr_err("r600_cp: Failed to load firmware\n",
 			       fw_name);
 		release_firmware(rdev->pfp_fw);
 		rdev->pfp_fw = NULL;
diff --git a/drivers/gpu/drm/radeon/radeon_uvd.c b/drivers/gpu/drm/radeon/radeon_uvd.c
index d34d1cf..10e859c 100644
--- a/drivers/gpu/drm/radeon/radeon_uvd.c
+++ b/drivers/gpu/drm/radeon/radeon_uvd.c
@@ -140,7 +140,7 @@ int radeon_uvd_init(struct radeon_device *rdev)
 		/* Let's try to load the newer firmware first */
 		r = request_firmware(&rdev->uvd_fw, fw_name, rdev->dev);
 		if (r) {
-			dev_err(rdev->dev, "radeon_uvd: Can't load firmware \"%s\"\n",
+			dev_err(rdev->dev, "radeon_uvd: Can't load firmware\n",
 				fw_name);
 		} else {
 			struct common_firmware_header *hdr = (void *)rdev->uvd_fw->data;
@@ -175,7 +175,7 @@ int radeon_uvd_init(struct radeon_device *rdev)
 	if (!fw_name || r) {
 		r = request_firmware(&rdev->uvd_fw, legacy_fw_name, rdev->dev);
 		if (r) {
-			dev_err(rdev->dev, "radeon_uvd: Can't load firmware \"%s\"\n",
+			dev_err(rdev->dev, "radeon_uvd: Can't load firmware\n",
 				legacy_fw_name);
 			return r;
 		}
diff --git a/drivers/gpu/drm/radeon/radeon_vce.c b/drivers/gpu/drm/radeon/radeon_vce.c
index c1c619f..744612d 100644
--- a/drivers/gpu/drm/radeon/radeon_vce.c
+++ b/drivers/gpu/drm/radeon/radeon_vce.c
@@ -87,7 +87,7 @@ int radeon_vce_init(struct radeon_device *rdev)
 
 	r = request_firmware(&rdev->vce_fw, fw_name, rdev->dev);
 	if (r) {
-		dev_err(rdev->dev, "radeon_vce: Can't load firmware \"%s\"\n",
+		dev_err(rdev->dev, "radeon_vce: Can't load firmware\n",
 			fw_name);
 		return r;
 	}
diff --git a/drivers/gpu/drm/radeon/si.c b/drivers/gpu/drm/radeon/si.c
index 1907c95..7ff65cc 100644
--- a/drivers/gpu/drm/radeon/si.c
+++ b/drivers/gpu/drm/radeon/si.c
@@ -1786,7 +1786,7 @@ static int si_init_microcode(struct radeon_device *rdev)
 		if (err)
 			goto out;
 		if (rdev->pfp_fw->size != pfp_req_size) {
-			pr_err("si_cp: Bogus length %zu in firmware \"%s\"\n",
+			pr_err("si_cp: Bogus length %zu in firmware\n",
 			       rdev->pfp_fw->size, fw_name);
 			err = -EINVAL;
 			goto out;
@@ -1794,7 +1794,7 @@ static int si_init_microcode(struct radeon_device *rdev)
 	} else {
 		err = radeon_ucode_validate(rdev->pfp_fw);
 		if (err) {
-			pr_err("si_cp: validation failed for firmware \"%s\"\n",
+			pr_err("si_cp: validation failed for firmware\n",
 			       fw_name);
 			goto out;
 		} else {
@@ -1810,14 +1810,14 @@ static int si_init_microcode(struct radeon_device *rdev)
 		if (err)
 			goto out;
 		if (rdev->me_fw->size != me_req_size) {
-			pr_err("si_cp: Bogus length %zu in firmware \"%s\"\n",
+			pr_err("si_cp: Bogus length %zu in firmware\n",
 			       rdev->me_fw->size, fw_name);
 			err = -EINVAL;
 		}
 	} else {
 		err = radeon_ucode_validate(rdev->me_fw);
 		if (err) {
-			pr_err("si_cp: validation failed for firmware \"%s\"\n",
+			pr_err("si_cp: validation failed for firmware\n",
 			       fw_name);
 			goto out;
 		} else {
@@ -1833,14 +1833,14 @@ static int si_init_microcode(struct radeon_device *rdev)
 		if (err)
 			goto out;
 		if (rdev->ce_fw->size != ce_req_size) {
-			pr_err("si_cp: Bogus length %zu in firmware \"%s\"\n",
+			pr_err("si_cp: Bogus length %zu in firmware\n",
 			       rdev->ce_fw->size, fw_name);
 			err = -EINVAL;
 		}
 	} else {
 		err = radeon_ucode_validate(rdev->ce_fw);
 		if (err) {
-			pr_err("si_cp: validation failed for firmware \"%s\"\n",
+			pr_err("si_cp: validation failed for firmware\n",
 			       fw_name);
 			goto out;
 		} else {
@@ -1856,14 +1856,14 @@ static int si_init_microcode(struct radeon_device *rdev)
 		if (err)
 			goto out;
 		if (rdev->rlc_fw->size != rlc_req_size) {
-			pr_err("si_rlc: Bogus length %zu in firmware \"%s\"\n",
+			pr_err("si_rlc: Bogus length %zu in firmware\n",
 			       rdev->rlc_fw->size, fw_name);
 			err = -EINVAL;
 		}
 	} else {
 		err = radeon_ucode_validate(rdev->rlc_fw);
 		if (err) {
-			pr_err("si_cp: validation failed for firmware \"%s\"\n",
+			pr_err("si_cp: validation failed for firmware\n",
 			       fw_name);
 			goto out;
 		} else {
@@ -1887,7 +1887,7 @@ static int si_init_microcode(struct radeon_device *rdev)
 		}
 		if ((rdev->mc_fw->size != mc_req_size) &&
 		    (rdev->mc_fw->size != mc2_req_size)) {
-			pr_err("si_mc: Bogus length %zu in firmware \"%s\"\n",
+			pr_err("si_mc: Bogus length %zu in firmware\n",
 			       rdev->mc_fw->size, fw_name);
 			err = -EINVAL;
 		}
@@ -1895,7 +1895,7 @@ static int si_init_microcode(struct radeon_device *rdev)
 	} else {
 		err = radeon_ucode_validate(rdev->mc_fw);
 		if (err) {
-			pr_err("si_cp: validation failed for firmware \"%s\"\n",
+			pr_err("si_cp: validation failed for firmware\n",
 			       fw_name);
 			goto out;
 		} else {
@@ -1914,19 +1914,19 @@ static int si_init_microcode(struct radeon_device *rdev)
 		snprintf(fw_name, sizeof(fw_name), "radeon/%s_smc.bin", chip_name);
 		err = request_firmware(&rdev->smc_fw, fw_name, rdev->dev);
 		if (err) {
-			pr_err("smc: error loading firmware \"%s\"\n", fw_name);
+			pr_err("smc: error loading firmware\n", fw_name);
 			release_firmware(rdev->smc_fw);
 			rdev->smc_fw = NULL;
 			err = 0;
 		} else if (rdev->smc_fw->size != smc_req_size) {
-			pr_err("si_smc: Bogus length %zu in firmware \"%s\"\n",
+			pr_err("si_smc: Bogus length %zu in firmware\n",
 			       rdev->smc_fw->size, fw_name);
 			err = -EINVAL;
 		}
 	} else {
 		err = radeon_ucode_validate(rdev->smc_fw);
 		if (err) {
-			pr_err("si_cp: validation failed for firmware \"%s\"\n",
+			pr_err("si_cp: validation failed for firmware\n",
 			       fw_name);
 			goto out;
 		} else {
@@ -1945,7 +1945,7 @@ static int si_init_microcode(struct radeon_device *rdev)
 out:
 	if (err) {
 		if (err != -EINVAL)
-			pr_err("si_cp: Failed to load firmware \"%s\"\n",
+			pr_err("si_cp: Failed to load firmware\n",
 			       fw_name);
 		release_firmware(rdev->pfp_fw);
 		rdev->pfp_fw = NULL;
diff --git a/drivers/net/wireless/intel/ipw2x00/ipw2200.c b/drivers/net/wireless/intel/ipw2x00/ipw2200.c
index 9368abd..fa4de6a 100644
--- a/drivers/net/wireless/intel/ipw2x00/ipw2200.c
+++ b/drivers/net/wireless/intel/ipw2x00/ipw2200.c
@@ -3417,12 +3417,12 @@ static int ipw_get_fw(struct ipw_priv *priv,
 	/* ask firmware_class module to get the boot firmware off disk */
 	rc = request_firmware(raw, name, &priv->pci_dev->dev);
 	if (rc < 0) {
-		IPW_ERROR("%s request_firmware failed: Reason %d\n", name, rc);
+		IPW_ERROR("request_firmware failed: Reason %d\n", rc);
 		return rc;
 	}
 
 	if ((*raw)->size < sizeof(*fw)) {
-		IPW_ERROR("%s is too small (%zd)\n", name, (*raw)->size);
+		IPW_ERROR("Firmware file is too small (%zd)\n", (*raw)->size);
 		return -EINVAL;
 	}
 
@@ -3430,13 +3430,12 @@ static int ipw_get_fw(struct ipw_priv *priv,
 
 	if ((*raw)->size < sizeof(*fw) + le32_to_cpu(fw->boot_size) +
 	    le32_to_cpu(fw->ucode_size) + le32_to_cpu(fw->fw_size)) {
-		IPW_ERROR("%s is too small or corrupt (%zd)\n",
-			  name, (*raw)->size);
+		IPW_ERROR("Firmware file is too small or corrupt (%zd)\n",
+			  (*raw)->size);
 		return -EINVAL;
 	}
 
-	IPW_DEBUG_INFO("Read firmware '%s' image v%d.%d (%zd bytes)\n",
-		       name,
+	IPW_DEBUG_INFO("Read firmware image v%d.%d (%zd bytes)\n",
 		       le32_to_cpu(fw->ver) >> 16,
 		       le32_to_cpu(fw->ver) & 0xff,
 		       (*raw)->size - sizeof(*fw));
@@ -3569,7 +3568,7 @@ static int ipw_load(struct ipw_priv *priv)
 	/* DMA the initial boot firmware into the device */
 	rc = ipw_load_firmware(priv, boot_img, le32_to_cpu(fw->boot_size));
 	if (rc < 0) {
-		IPW_ERROR("Unable to load boot firmware: %d\n", rc);
+		IPW_ERROR("Unable to load boot firmware\n", rc);
 		goto error;
 	}
 
@@ -3601,7 +3600,7 @@ static int ipw_load(struct ipw_priv *priv)
 	/* DMA bss firmware into the device */
 	rc = ipw_load_firmware(priv, fw_img, le32_to_cpu(fw->fw_size));
 	if (rc < 0) {
-		IPW_ERROR("Unable to load firmware: %d\n", rc);
+		IPW_ERROR("Unable to load firmware\n", rc);
 		goto error;
 	}
 #ifdef CONFIG_PM
@@ -11213,7 +11212,7 @@ static int ipw_up(struct ipw_priv *priv)
 		 * Also start the clocks. */
 		rc = ipw_load(priv);
 		if (rc) {
-			IPW_ERROR("Unable to load firmware: %d\n", rc);
+			IPW_ERROR("Unable to load firmware\n", rc);
 			return rc;
 		}
 
diff --git a/drivers/net/wireless/intel/iwlegacy/3945-mac.c b/drivers/net/wireless/intel/iwlegacy/3945-mac.c
index 38bf403..a7934a6 100644
--- a/drivers/net/wireless/intel/iwlegacy/3945-mac.c
+++ b/drivers/net/wireless/intel/iwlegacy/3945-mac.c
@@ -1861,7 +1861,7 @@ il3945_read_ucode(struct il_priv *il)
 		sprintf(buf, "%s%u%s", name_pre, idx, ".ucode");
 		ret = request_firmware(&ucode_raw, buf, &il->pci_dev->dev);
 		if (ret < 0) {
-			IL_ERR("%s firmware file req failed: %d\n", buf, ret);
+			IL_ERR("Firmware file req failed\n", buf, ret);
 			if (ret == -ENOENT)
 				continue;
 			else
@@ -1870,7 +1870,7 @@ il3945_read_ucode(struct il_priv *il)
 			if (idx < api_max)
 				IL_ERR("Loaded firmware %s, "
 				       "which is deprecated. "
-				       " Please use API v%u instead.\n", buf,
+				       "\n", buf,
 				       api_max);
 			D_INFO("Got firmware '%s' file "
 			       "(%zd bytes) from disk\n", buf, ucode_raw->size);
@@ -1906,16 +1906,14 @@ il3945_read_ucode(struct il_priv *il)
 
 	if (api_ver < api_min || api_ver > api_max) {
 		IL_ERR("Driver unable to support your firmware API. "
-		       "Driver supports v%u, firmware is v%u.\n", api_max,
+		       "\n", api_max,
 		       api_ver);
 		il->ucode_ver = 0;
 		ret = -EINVAL;
 		goto err_release;
 	}
 	if (api_ver != api_max)
-		IL_ERR("Firmware has old API version. Expected %u, "
-		       "got %u. New firmware can be obtained "
-		       "from http://www.intellinuxwireless.org.\n", api_max,
+		IL_ERR("Firmware has old API version\n", api_max,
 		       api_ver);
 
 	IL_INFO("loaded firmware version %u.%u.%u.%u\n",
diff --git a/drivers/net/wireless/intel/iwlegacy/4965-mac.c b/drivers/net/wireless/intel/iwlegacy/4965-mac.c
index 5b51fba..b16ab69 100644
--- a/drivers/net/wireless/intel/iwlegacy/4965-mac.c
+++ b/drivers/net/wireless/intel/iwlegacy/4965-mac.c
@@ -4708,7 +4708,7 @@ il4965_request_firmware(struct il_priv *il, bool first)
 
 	sprintf(il->firmware_name, "%s%s%s", name_pre, tag, ".ucode");
 
-	D_INFO("attempting to load firmware '%s'\n", il->firmware_name);
+	D_INFO("attempting to load firmware\n", il->firmware_name);
 
 	return request_firmware_nowait(THIS_MODULE, 1, il->firmware_name,
 				       &il->pci_dev->dev, GFP_KERNEL, il,
@@ -4799,7 +4799,7 @@ il4965_ucode_callback(const struct firmware *ucode_raw, void *context)
 
 	if (!ucode_raw) {
 		if (il->fw_idx <= il->cfg->ucode_api_max)
-			IL_ERR("request for firmware file '%s' failed.\n",
+			IL_ERR("request for firmware failed.\n",
 			       il->firmware_name);
 		goto try_again;
 	}
@@ -4829,16 +4829,13 @@ il4965_ucode_callback(const struct firmware *ucode_raw, void *context)
 	 * on the API version read from firmware header from here on forward
 	 */
 	if (api_ver < api_min || api_ver > api_max) {
-		IL_ERR("Driver unable to support your firmware API. "
-		       "Driver supports v%u, firmware is v%u.\n", api_max,
+		IL_ERR("Driver unable to support your firmware API.\n", api_max,
 		       api_ver);
 		goto try_again;
 	}
 
 	if (api_ver != api_max)
-		IL_ERR("Firmware has old API version. Expected v%u, "
-		       "got v%u. New firmware can be obtained "
-		       "from http://www.intellinuxwireless.org.\n", api_max,
+		IL_ERR("Firmware has old API version.\n", api_max,
 		       api_ver);
 
 	IL_INFO("loaded firmware version %u.%u.%u.%u\n",
diff --git a/drivers/net/wireless/intel/iwlwifi/iwl-drv.c b/drivers/net/wireless/intel/iwlwifi/iwl-drv.c
index 4e0f86f..05ac835 100644
--- a/drivers/net/wireless/intel/iwlwifi/iwl-drv.c
+++ b/drivers/net/wireless/intel/iwlwifi/iwl-drv.c
@@ -257,7 +257,7 @@ static int iwl_request_firmware(struct iwl_drv *drv, bool first)
 	snprintf(drv->firmware_name, sizeof(drv->firmware_name), "%s%s.ucode",
 		 fw_pre_name, tag);
 
-	IWL_DEBUG_INFO(drv, "attempting to load firmware '%s'\n",
+	IWL_DEBUG_INFO(drv, "attempting to load firmware\n",
 		       drv->firmware_name);
 
 	return request_firmware_nowait(THIS_MODULE, 1, drv->firmware_name,
diff --git a/drivers/net/wireless/intel/iwlwifi/mvm/fw.c b/drivers/net/wireless/intel/iwlwifi/mvm/fw.c
index 82863e9..1f2f235 100644
--- a/drivers/net/wireless/intel/iwlwifi/mvm/fw.c
+++ b/drivers/net/wireless/intel/iwlwifi/mvm/fw.c
@@ -1677,7 +1677,7 @@ int iwl_mvm_load_d3_fw(struct iwl_mvm *mvm)
 
 	ret = iwl_mvm_load_ucode_wait_alive(mvm, IWL_UCODE_WOWLAN);
 	if (ret) {
-		IWL_ERR(mvm, "Failed to start WoWLAN firmware: %d\n", ret);
+		IWL_ERR(mvm, "Failed to start WoWLAN firmware\n", ret);
 		goto error;
 	}
 
diff --git a/drivers/net/wireless/intel/iwlwifi/mvm/nvm.c b/drivers/net/wireless/intel/iwlwifi/mvm/nvm.c
index dac7e54..d2aefe6 100644
--- a/drivers/net/wireless/intel/iwlwifi/mvm/nvm.c
+++ b/drivers/net/wireless/intel/iwlwifi/mvm/nvm.c
@@ -410,7 +410,7 @@ int iwl_mvm_read_external_nvm(struct iwl_mvm *mvm)
 	ret = request_firmware(&fw_entry, mvm->nvm_file_name,
 			       mvm->trans->dev);
 	if (ret) {
-		IWL_ERR(mvm, "ERROR: %s isn't available %d\n",
+		IWL_ERR(mvm, "ERROR: firmware isn't available \n",
 			mvm->nvm_file_name, ret);
 		return ret;
 	}
diff --git a/drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_core.c b/drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_core.c
index 21e5ef0..520e63b 100644
--- a/drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_core.c
+++ b/drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_core.c
@@ -2074,9 +2074,9 @@ int rtl8xxxu_load_firmware(struct rtl8xxxu_priv *priv, char *fw_name)
 	int ret = 0;
 	u16 signature;
 
-	dev_info(dev, "%s: Loading firmware %s\n", DRIVER_NAME, fw_name);
+	dev_info(dev, "%s: Loading firmware\n", DRIVER_NAME, fw_name);
 	if (request_firmware(&fw, fw_name, &priv->udev->dev)) {
-		dev_warn(dev, "request_firmware(%s) failed\n", fw_name);
+		dev_warn(dev, "request_firmware failed\n", fw_name);
 		ret = -EAGAIN;
 		goto exit;
 	}
diff --git a/drivers/net/wireless/realtek/rtlwifi/core.c b/drivers/net/wireless/realtek/rtlwifi/core.c
index b0ad061..dab2248 100644
--- a/drivers/net/wireless/realtek/rtlwifi/core.c
+++ b/drivers/net/wireless/realtek/rtlwifi/core.c
@@ -106,7 +106,7 @@ static void rtl_fw_do_work(const struct firmware *firmware, void *context,
 			err = request_firmware(&firmware,
 					       rtlpriv->cfg->alt_fw_name,
 					       rtlpriv->io.dev);
-			pr_info("Loading alternative firmware %s\n",
+			pr_info("Loading alternative firmware \n",
 				rtlpriv->cfg->alt_fw_name);
 			if (!err)
 				goto found_alt;
diff --git a/drivers/net/wireless/realtek/rtlwifi/rtl8188ee/sw.c b/drivers/net/wireless/realtek/rtlwifi/rtl8188ee/sw.c
index 774e720..a364c1b 100644
--- a/drivers/net/wireless/realtek/rtlwifi/rtl8188ee/sw.c
+++ b/drivers/net/wireless/realtek/rtlwifi/rtl8188ee/sw.c
@@ -169,7 +169,7 @@ int rtl88e_init_sw_vars(struct ieee80211_hw *hw)
 
 	fw_name = "rtlwifi/rtl8188efw.bin";
 	rtlpriv->max_fw_size = 0x8000;
-	pr_info("Using firmware %s\n", fw_name);
+	pr_info("Using firmware \n", fw_name);
 	err = request_firmware_nowait(THIS_MODULE, 1, fw_name,
 				      rtlpriv->io.dev, GFP_KERNEL, hw,
 				      rtl_fw_cb);
diff --git a/drivers/net/wireless/realtek/rtlwifi/rtl8192ce/sw.c b/drivers/net/wireless/realtek/rtlwifi/rtl8192ce/sw.c
index bcbb0c6..a1a9734 100644
--- a/drivers/net/wireless/realtek/rtlwifi/rtl8192ce/sw.c
+++ b/drivers/net/wireless/realtek/rtlwifi/rtl8192ce/sw.c
@@ -170,7 +170,7 @@ int rtl92c_init_sw_vars(struct ieee80211_hw *hw)
 		fw_name = "rtlwifi/rtl8192cfw.bin";
 
 	rtlpriv->max_fw_size = 0x4000;
-	pr_info("Using firmware %s\n", fw_name);
+	pr_info("Using firmware \n", fw_name);
 	err = request_firmware_nowait(THIS_MODULE, 1, fw_name,
 				      rtlpriv->io.dev, GFP_KERNEL, hw,
 				      rtl_fw_cb);
diff --git a/drivers/net/wireless/realtek/rtlwifi/rtl8192cu/sw.c b/drivers/net/wireless/realtek/rtlwifi/rtl8192cu/sw.c
index 96c923b..26eece2 100644
--- a/drivers/net/wireless/realtek/rtlwifi/rtl8192cu/sw.c
+++ b/drivers/net/wireless/realtek/rtlwifi/rtl8192cu/sw.c
@@ -80,7 +80,7 @@ static int rtl92cu_init_sw_vars(struct ieee80211_hw *hw)
 	}
 	/* provide name of alternative file */
 	rtlpriv->cfg->alt_fw_name = "rtlwifi/rtl8192cufw.bin";
-	pr_info("Loading firmware %s\n", fw_name);
+	pr_info("Loading firmware \n", fw_name);
 	rtlpriv->max_fw_size = 0x4000;
 	err = request_firmware_nowait(THIS_MODULE, 1,
 				      fw_name, rtlpriv->io.dev,
diff --git a/drivers/net/wireless/realtek/rtlwifi/rtl8192de/sw.c b/drivers/net/wireless/realtek/rtlwifi/rtl8192de/sw.c
index 16132c6..dc9db6d 100644
--- a/drivers/net/wireless/realtek/rtlwifi/rtl8192de/sw.c
+++ b/drivers/net/wireless/realtek/rtlwifi/rtl8192de/sw.c
@@ -175,7 +175,7 @@ static int rtl92d_init_sw_vars(struct ieee80211_hw *hw)
 
 	rtlpriv->max_fw_size = 0x8000;
 	pr_info("Driver for Realtek RTL8192DE WLAN interface\n");
-	pr_info("Loading firmware file %s\n", fw_name);
+	pr_info("Loading firmware file\n", fw_name);
 
 	/* request fw */
 	err = request_firmware_nowait(THIS_MODULE, 1, fw_name,
diff --git a/drivers/net/wireless/realtek/rtlwifi/rtl8192ee/sw.c b/drivers/net/wireless/realtek/rtlwifi/rtl8192ee/sw.c
index eaa503b..343f691 100644
--- a/drivers/net/wireless/realtek/rtlwifi/rtl8192ee/sw.c
+++ b/drivers/net/wireless/realtek/rtlwifi/rtl8192ee/sw.c
@@ -171,7 +171,7 @@ int rtl92ee_init_sw_vars(struct ieee80211_hw *hw)
 	fw_name = "rtlwifi/rtl8192eefw.bin";
 
 	rtlpriv->max_fw_size = 0x8000;
-	pr_info("Using firmware %s\n", fw_name);
+	pr_info("Using firmware \n", fw_name);
 	err = request_firmware_nowait(THIS_MODULE, 1, fw_name,
 				      rtlpriv->io.dev, GFP_KERNEL, hw,
 				      rtl_fw_cb);
diff --git a/drivers/net/wireless/realtek/rtlwifi/rtl8192se/sw.c b/drivers/net/wireless/realtek/rtlwifi/rtl8192se/sw.c
index 2006b09..475940e 100644
--- a/drivers/net/wireless/realtek/rtlwifi/rtl8192se/sw.c
+++ b/drivers/net/wireless/realtek/rtlwifi/rtl8192se/sw.c
@@ -91,7 +91,7 @@ static void rtl92se_fw_cb(const struct firmware *firmware, void *context)
 			 "Firmware callback routine entered!\n");
 	complete(&rtlpriv->firmware_loading_complete);
 	if (!firmware) {
-		pr_err("Firmware %s not available\n", fw_name);
+		pr_err("Firmware not available\n", fw_name);
 		rtlpriv->max_fw_size = 0;
 		return;
 	}
@@ -209,7 +209,7 @@ static int rtl92s_init_sw_vars(struct ieee80211_hw *hw)
 	rtlpriv->max_fw_size = RTL8190_MAX_FIRMWARE_CODE_SIZE*2 +
 			       sizeof(struct fw_hdr);
 	pr_info("Driver for Realtek RTL8192SE/RTL8191SE\n"
-		"Loading firmware %s\n", fw_name);
+		"Loading firmware \n", fw_name);
 	/* request fw */
 	err = request_firmware_nowait(THIS_MODULE, 1, fw_name,
 				      rtlpriv->io.dev, GFP_KERNEL, hw,
diff --git a/drivers/net/wireless/realtek/rtlwifi/rtl8723ae/sw.c b/drivers/net/wireless/realtek/rtlwifi/rtl8723ae/sw.c
index 7bf9f25..a2acfac 100644
--- a/drivers/net/wireless/realtek/rtlwifi/rtl8723ae/sw.c
+++ b/drivers/net/wireless/realtek/rtlwifi/rtl8723ae/sw.c
@@ -178,7 +178,7 @@ int rtl8723e_init_sw_vars(struct ieee80211_hw *hw)
 		fw_name = "rtlwifi/rtl8723fw_B.bin";
 
 	rtlpriv->max_fw_size = 0x6000;
-	pr_info("Using firmware %s\n", fw_name);
+	pr_info("Using firmware \n", fw_name);
 	err = request_firmware_nowait(THIS_MODULE, 1, fw_name,
 				      rtlpriv->io.dev, GFP_KERNEL, hw,
 				      rtl_fw_cb);
diff --git a/drivers/net/wireless/realtek/rtlwifi/rtl8723be/sw.c b/drivers/net/wireless/realtek/rtlwifi/rtl8723be/sw.c
index f9d10f1..9048c51 100644
--- a/drivers/net/wireless/realtek/rtlwifi/rtl8723be/sw.c
+++ b/drivers/net/wireless/realtek/rtlwifi/rtl8723be/sw.c
@@ -182,7 +182,7 @@ int rtl8723be_init_sw_vars(struct ieee80211_hw *hw)
 	}
 
 	rtlpriv->max_fw_size = 0x8000;
-	pr_info("Using firmware %s\n", fw_name);
+	pr_info("Using firmware \n", fw_name);
 	err = request_firmware_nowait(THIS_MODULE, 1, fw_name,
 				      rtlpriv->io.dev, GFP_KERNEL, hw,
 				      rtl_fw_cb);
diff --git a/drivers/net/wireless/realtek/rtlwifi/rtl8821ae/sw.c b/drivers/net/wireless/realtek/rtlwifi/rtl8821ae/sw.c
index d71d277..f2c70e1 100644
--- a/drivers/net/wireless/realtek/rtlwifi/rtl8821ae/sw.c
+++ b/drivers/net/wireless/realtek/rtlwifi/rtl8821ae/sw.c
@@ -209,7 +209,7 @@ int rtl8821ae_init_sw_vars(struct ieee80211_hw *hw)
 
 	rtlpriv->max_fw_size = 0x8000;
 	/*load normal firmware*/
-	pr_info("Using firmware %s\n", fw_name);
+	pr_info("Using firmware \n", fw_name);
 	err = request_firmware_nowait(THIS_MODULE, 1, fw_name,
 				      rtlpriv->io.dev, GFP_KERNEL, hw,
 				      rtl_fw_cb);
@@ -226,7 +226,7 @@ int rtl8821ae_init_sw_vars(struct ieee80211_hw *hw)
 		}
 	}
 	/*load wowlan firmware*/
-	pr_info("Using firmware %s\n", wowlan_fw_name);
+	pr_info("Using firmware \n", wowlan_fw_name);
 	err = request_firmware_nowait(THIS_MODULE, 1,
 				      wowlan_fw_name,
 				      rtlpriv->io.dev, GFP_KERNEL, hw,
