#! /bin/sh

# deblob-check version 2022-07-10 r18820
#        modified with 2022-08-25 r18881
#        modified with 2022-09-11 r18905
# Inspired in gNewSense's find-firmware script.
# Written by Alexandre Oliva <lxoliva@fsfla.org>

# Check http://www.fsfla.org/svn/fsfla/software/linux-libre for newer
# versions.

# Copyright 2008-2022 Alexandre Oliva <lxoliva@fsfla.org>
#
# This program is part of GNU Linux-libre, a GNU project that
# publishes scripts to clean up Linux so as to make it suitable for
# use in the GNU Project and in Free System Distributions.
#
# This program is free software; you can redistribute it and/or modify
# it under the terms of the GNU General Public License as published by
# the Free Software Foundation; either version 2 of the License, or
# (at your option) any later version.
#
# This program is distributed in the hope that it will be useful, but
# WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
# General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write to the Free Software
# Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA 02110-1301
# USA


# usage: deblob-check [-S] [-v] [-v] [-s S] [--reverse-patch] \
#        [--use-...|--gen-flex] [-lDdBbCcXxPpFftVh?H] \
#        *.tar* patch-* [-i prefix/] *.patch *.diff...

# Look for and report too-long undocumented sequences of numbers
# (generally blobs in disguise) in source files, as well as requests
# for loading non-Free firmware.

# The order of command line flags is significant.  Flags given out of
# the order above won't be handled correctly, sorry.

# -s --sensitivity: Specifies the number of consecutive integral or
#		character constants that trigger the blob detector.
#	        Must be followed by a blank and a number.

#    --reverse-patch: Test the removed parts of a patch, rather than
#		the added ones.

#    --use-python: Choose the internal python script for the bulk of
#		the work.  This is the fastest for cleaning up,
#		because of the fast startup time of the regular
#		expression engine.  This option is the default if
#		python is found.  Set PYTHON to override the python
#		interpreter.  The internal script works in both Python
#		2 and 3.

#    --use-awk: Choose the internal GNU awk script for the bulk of the
#		work.  This is the recommended option to check entire
#		tarballs, because its regular expression engine offers
#		the best speed/memory use.  This is the default option
#		if python is not found.  Set AWK to specify GNU awk's
#		name.

#    --use-perl: Choose the internal perl script.  This is not
#		recommended, because our regular expressions exceed
#		some limits hard-coded into perl.  Set PERL to specify
#		which perl implementation to use.  This is the default
#		option if neither python nor GNU awk are found, AND if
#		PERL is set.

#    --use-sed: Choose the internal GNU sed script for the bulk of the
#		work.  This is the default option, if no other
#		alternative is found.  Use SED to specify which sed
#		program to use.

#    --save-script-input: Save the input that would have been fed to
#		any of the engines above.

#    --gen-flex: Generate a flex input file with all known blob and
#		false positive patterns.  It might have been a fast
#		regular expression processor if only the flex program
#		completed in reasonable time.


# For reference, as of 5.8-rc6-gnu, checking the full tarball (with
# -B, not -C) takes up:

# Engine            top mem   time
# GNU awk 5.0.1     2.2GB       1x
# Python 3.8.3         48MB    14x
# Perl 5.30.3          22MB    45x
# GNU sed 4.5      24GB         4x


# The default sensitivity is 32 constants.

# The sensitivity, if present, must be the first option.  The action
# selection, if present, must be the first argument, except for the
# sensitivity and verbosity.

# The default can be overridden with one of:

# -l --list-blobs: list files that contain sequences that match the
#		blob detector test and that are not known to be false
#		positives.  This is the default option.

# -d --deblob --mark-blobs: print the processed input, replacing
#		sequences that match the blob detector test and that
#		are NOT known to be false positives with
#		/*(DEBLOBBED)*/.

# -D --cat: print the processed input, as it would have been fed to
#		the blob detector script.  Use -S to save the sed
#		script used to process it, and search for `sedcat:' in
#		comments to locate the relevant adaptation points.

# -b --print-marked-blobs: like -d, but print only the matching
#		sequences.

# -B --print-blobs: like -b, but do not deblob the sequences.

# -c --print-marked-blobs-with-context: like -b, but try to maximize
#		the context around the blobs.  This maximization will
#		sometimes disregard known false positives, if they
#		happen to be contained within the extended match.
#		This is probably an indication that the false positive
#		matching rule could be improved.

# -C --print-blobs-with-context: like -B, but try to maximize the
#		context around the blobs.

# -X --print-all-matches: print all blobs, be they known false
#		positives or actual blobs.

# -x --list-all-matches: list files that contain sequences that appear
#		to be blobs, be they known false positives or not.

# -p --mark-false-positives: print the processed input, replacing
#		sequences that match the blob detector test, even those
#		known to be false positives, with /*(DEBLOBBED)*/.

# -P --list-false-positives: list files that contain false positives.

# -f --print-marked-false-positives: like -p, but print only the
#		matching sequences.

# -F --print-false-positives: like -f, but do not deblob the sequences.

# -t --test: run (very minimal) self-test.

# -V --version: print a version number

# -h -? -H --help: print short or long help message


# debugging options:

# -S --save-scripts: save scripts and temporary files.

# -v --verbose: increase verbosity level, for internal debugging.  May
#		be given at most twice.


# file options:

# --: Don't process command-line options any further.  All following
#		arguments are taken as filenames.

# -i --implied-prefix --prefix: prepend the given prefix to each filename
#		listed after this option, when configuring false positives
#		and negatives.

# *.tar*: iterate over all files in the named tar file.

# *.patch, patch-*, *.diff: Look for blobs in the [ +] parts of the
# 		*patch, unless --reverse-patch is given, in which case
# 		the [ -] parts will be used.

# Anything else is assumed to be a source file.

# *.gz | *.bz2 | *.xz | *.lz: Decompress automatically.


# The exit status is only significant for the --list options: it will
# be true if nothing was found, and false otherwise.

: # Mark the end of the help message.

# TODO:

# - Improve handling of command-line arguments, so as to not make the
# order relevant.

# - Add an option for the user to feed their own false positive
# patterns.

# - Add support to recognize known blobs (or other non-Free
# signatures, really), to speed up the scanning of files containing
# blobs, and to avoid attempts to disguise blobs.

# - Factor out the code in the various print_* and list_* parts of the
# sed script, at least in the shell sources.  Make sure they're all
# included and expanded in a saved --cat script though.

# - Add support for file name tagging in patterns, such that blobs or
# false positives are recognized only when handling the specific
# filename, be it stand-alone, as part of a patch or a tarball.  This
# should help avoid recognition of actual blobs as false positives
# just because there's a symbol with a different name elsewhere.

#   It is convenient that the patterns provided by the user to
# recognize file names can be empty (for backward compatibility), but
# this should ideally be phased out in favor of more precise matches.
# It's important that files can be recognized with leading tarball or
# patch names, that the filename used within the tarball contain
# leading garbage, and even that a partial pathname be recognizable
# (say recognize drivers/net/whatever.c when the input file is named
# ../net/whatever.c).

#   Rather than using regular expressions to recognize multiple files
# it's convenient (but not quite essential) that filename patterns be
# specifiable as regular expressions, rather than simple filenames,
# but there are other ways around this.

#   Maintaining begin/end markers in a stack-like fashion as part of
# the processed stream, and using the names in them as (optional) part
# of the recognition patterns, would enable us to do it.

#   Introducing annotations next to the false positives (and recognized
# blobs) as an early part of the process may speed things up and
# enable fast processing, but how to introduce the annotations quickly
# in the first place?  Given patterns such as

#   \(\(file1\)\(.*\)\(pat1\)\|\(file2\)\(.*\)\(pat2\)\|...\)

# how do we get sed to introduce a marker that contains file2 right
# before or right after pat2, without turning a big efficient regexp
# into a slowish sequence of s/// commands?

# - Re-check and narrow false-positive patterns to make sure they
# apply only to the relevant content.

# - Scripting abilities, so as to be able to automate the removal of
# source files or of blobs from source files in a tarball without
# having to extract the entire tarball (as in tar --update/--delete)
# would be nice.  Carrying over removed files automatically into
# patches would also be great, and this sort of script would be
# perfect to document what has been done to a tarball plus a set of
# patches.  Something like deblob.script:
#
#   tarball linux-2.6.24.tar.bz2
#   delete net/wireloss/freedom.c drivers/me/crazy.c
#   deblob include/linux/slab-blob-kfree.h
#   deconfig drivers/char/drm DRM_IS_BAD
#
#   patch patch-2.6.25-rc7.bz2
#   delete arch/power/over/you.c

# such that the deletes from an earlier file would carry over into the
# subsequent ones, and new tarballs and patch files would be generated
# with the libre- prefix in their basename, and the xdeltas between
# the original files and the modified files would be minimal, and
# redundant with this script and the input script while at that.

# - Improve documentation of the code.

# - Write a decent testsuite.

# - Insert your idea here. :-)

# Yeah, lots of stuff to do.  Want to help?

# This makes it much faster, and mostly immune to non-ASCII stuff, as
# long as a 8-bit-safe sed is used.  Probably a safe assumption these
# days.
LC_ALL=C; export LC_ALL
LANGUAGE=C; export LANGUAGE

rm="rm -f"

for echo in 'echo' 'printf %s\n'; do
  case `$echo '\nx'` in
  '\nx') break;;
  esac
done
case `$echo '\nx'` in
'\nx') ;; *) echo Cannot find out what echo to use >&2; exit 1;;
esac

for echo_n in "echo -n" "printf %s"; do
  case `$echo_n '\na'; $echo_n '\nb'` in
  '\na\nb') break;;
  esac
done
case `$echo_n a; $echo_n b` in
'ab') ;; *) echo Cannot find out an echo -n equivalent to use >&2; exit 1;;
esac

case $1 in
--save-scripts | -S)
  shift
  rm="echo preserving"
  ;;
esac

# Choose verbosity level for sed script debugging and performance
# analysis.
case $1 in
--verbose | -v)
  shift
  case $1 in
  --verbose | -v)
    shift
    v="i\\
:
p
i\\
"
    vp="2"
    ;;
  *)
    v="P;i\\
"
    vp="1"
    ;;
  esac
  ;;
*)
  v="# "
  vp="0"
  ;;
esac

sens=31 # 32 - 1
case $1 in
--sensitivity | -s)
  sens=$2;
  shift 2 || exit 1

  if test "$sens" -gt 0 2>/dev/null; then
    :
  else
    echo invalid sensitivity: $sens >&2
    exit 1
  fi

  sens=`expr $sens - 1`
  ;;
esac

reverse_patch=false
case $1 in
--reverse-patch)
  reverse_patch=:
  shift;
  ;;
esac

prefix=/
case $1 in
--implied-prefix | --prefix| -i)
  prefix=$2
  case $prefix in
  /*/) ;;
  */) prefix=/$prefix ;;
  /*) prefix=$prefix/ ;;
  *) prefix=/$prefix/ ;;
  esac
  shift 2 || exit 1
  ;;
esac

test_mode=false

name=deblob-check

set_eqscript_main () {
  $set_main_cmd "$@"
}

set_eqscript_cmd () {
  set_eqscript_main "list_blob"
}

set_sed_cmd () {
  set_sed_main "
i\\
$file\\
/*(DEBLOB-\\
ERROR)*/
q 1"
}

set_flex_cmd () {
  set_flex_main
}

set_save_script_input_cmd () {
  set_save_script_input_main
}

set_cmd=set_eqscript_cmd
if (${PYTHON-python} --version) > /dev/null 2>&1; then
  # Python will exhibit exponential behavior processing some regular
  # expressions, but we may have already fixed them all.  (see
  # http://swtch.com/~rsc/regexp/regexp1.html for details)
  set_main_cmd=set_python_main
elif (${AWK-gawk} --re-interval --version) > /dev/null 2>&1; then
  # GNU awk works fine, but it requires --re-interval to accept regexp
  # ranges, which we rely on to match blobs.  We could expand the blob
  # on our own, but, yuck.
  set_main_cmd=set_awk_main
elif (${PERL-false} --version) > /dev/null 2>&1; then
  # Don't choose perl by default.  Besides the potential for
  # exponential behavior, we exceed some internal recursion limits.
  set_main_cmd=set_perl_main
else
  # Sed takes GBs of RAM to compile all the huge regexps in the sed
  # script we generate with all known false positives and blobs in
  # Linux.  However, it is somewhat faster than GNU awk and even
  # python for long runs.
  # Try it: deblob-check --use-sed linux-2.6.32.tar.bz2
  set_cmd=set_sed_cmd
fi

case $1 in
--use-python)
  shift;
  set_cmd=set_eqscript_cmd;
  set_main_cmd=set_python_main;
  ;;

--use-perl)
  shift;
  set_cmd=set_eqscript_cmd;
  set_main_cmd=set_perl_main;
  ;;

--use-awk)
  shift;
  set_cmd=set_eqscript_cmd;
  set_main_cmd=set_awk_main;
  ;;

--use-sed)
  shift;
  set_cmd=set_sed_cmd;
  ;;

--gen-flex)
  shift;
  set_cmd=set_flex_cmd;
  ;;

--save-script-input)
  shift;
  set_cmd=set_save_script_input_cmd;
  ;;
esac

case $1 in
--version | -V)
  ${SED-sed} -e '/^# '$name' version /,/^# Written by/ { s/^# //; p; }; d' < $0
  exit 0
  ;;

-\? | -h)
  ${SED-sed} -n -e '/^# usage:/,/# -h/ { /^# -/,/^$/{s/^# \(-.*\):.*/\1/p; d; }; s/^\(# \?\)\?//p; }' < $0 &&
  echo
  echo "run \`$name --help | more' for full usage"
  exit 0
  ;;

--help | -H)
  ${SED-sed} -n -e '/^# '$name' version /,/^[^#]/ s/^\(# \?\)\?//p' < $0
  exit 0
  ;;

--test | -t)
  test_mode=:
  ;;

--mark-false-positives | -p)
  shift;
  set_sed_cmd () {
    set_sed_main "b list_both" "p" "b list_matches"
  }
  set_eqscript_cmd () {
    set_eqscript_main "replace_blob = print_blob = without_falsepos"
  }
  ;;

--print-marked-false-positives | -f)
  shift;
  set_sed_cmd () {
    set_sed_main "b print_marked_matches" "" "b print_marked_matches"
  }
  set_eqscript_cmd () {
    set_eqscript_main "replace_falsepos = print_falsepos"
  }
  ;;

--print-false-positives | -F)
  shift;
  set_sed_cmd () {
    set_sed_main "b print_matches" "" "b print_matches"
  }
  set_eqscript_cmd () {
    set_eqscript_main "print_falsepos"
  }
  ;;

--deblob | --mark-blobs | -d)
  shift;
  set_sed_cmd () {
    set_sed_main "b list_blobs" "p" "p"
  }
  set_eqscript_cmd () {
    set_eqscript_main "replace_blob = print_blob = print_falsepos = print_nomatch"
  }
  ;;

--cat | -D)
  shift;
  set_sed_cmd () {
    set_sed_main \
      "# sedcat: Actual blob detected, but there may be false positives." \
      "# sedcat: No blob whatsoever found." \
      "# sedcat: False positives found." \
      "p
d
# sedcat: Just print stuff, remove this line to run the actual script."
  }
  set_eqscript_cmd () {
    set_eqscript_main "print_blob = print_falsepos = print_nomatch"
  }
  ;;

--print-marked-blobs | -b)
  shift;
  set_sed_cmd () {
    set_sed_main "b print_marked_blobs"
  }
  set_eqscript_cmd () {
    set_eqscript_main "replace_blob = print_blob"
  }
  ;;

--print-blobs | -B)
  shift;
  set_sed_cmd () {
    set_sed_main "b print_blobs"
  }
  set_eqscript_cmd () {
    set_eqscript_main "print_blob"
  }
  ;;

--print-marked-blobs-with-context | -c)
  shift;
  set_sed_cmd () {
    set_sed_main "b print_marked_cblobs"
  }
  set_eqscript_cmd () {
    set_eqscript_main "with_context = replace_blob = print_blob"
  }
  ;;

--print-blobs-with-context | -C)
  shift;
  set_sed_cmd () {
    set_sed_main "b print_cblobs"
  }
  set_eqscript_cmd () {
    set_eqscript_main "with_context = print_blob"
  }
  ;;

--list-false-positives | -P)
  shift;
  set_sed_cmd () {
    set_sed_main "" "" "
i\\
$file\\
/*(DEBLOB-\\
ERROR)*/
q 1"
  }
  set_eqscript_cmd () {
    set_eqscript_main "list_falsepos"
  }
  ;;

--list-all-matches | -x)
  shift;
  set_sed_cmd () {
    set_sed_main "
i\\
$file\\
/*(DEBLOB-\\
ERROR)*/
q 1" "" "
i\\
$file\\
/*(DEBLOB-\\
ERROR)*/
q 1"
  }
  set_eqscript_cmd () {
    set_eqscript_main "list_blob = list_falsepos"
  }
  ;;

--print-all-matches | -X)
  shift;
  set_sed_cmd () {
    set_sed_main "b print_both" "" "b print_matches"
  }
  set_eqscript_cmd () {
    set_eqscript_main "print_blob = print_falsepos"
  }
  ;;

*)
  case $1 in
  --list-blobs | -l) shift;;
  esac
  case $1 in
  -- | --implied-prefix | --prefix | -i) ;;
  -*)
    if test ! -f "$1"; then
      echo "$name: \`$1' given too late or out of the proper sequence." >&2
      echo "$name: The order of arguments is significant, see the usage." >&2
      exit 1
    fi
    ;;
  esac
  ;;

esac

case $1 in
--)
  sawdashdash=t
  shift;;
esac

if $test_mode; then
 allpass=:
 for tool in awk perl python sed; do
  echo testing $tool...

  targs="-s 4 -i /deblob-check-testsuite/ --use-$tool"

  pass=:


  # Exercise some nasty inputs to see that we
  # recognize them as blobs with full context.
  test="positive context"
  for string in \
    "1,2,3,4" \
    "= {
1, 0x2, 03, L'\x4'
}" \
    "=
{
  '\\x1', '\\002'
  ,
  {
    { \"\\x3\", },
    \"\\004\"
  },
};" \
    ".long 1,2
     .long \$3,\$4" \
    "#define X { 1, 2, \\
		 3, 4, /* comment */ \\
	       }" \
    "= {
/*
 * multi-line
 * comment
 */
 {
   0x4c00c000, 0x00000000, 0x00060000, 0x00000000,
 },
}" \
    "= {
blob(
)
accept(
)
1, 2, 3, 4
}" \
  ; do
    case `$echo "$string" | $0 $targs -C` in
    "::: - :::
$string") ;;
    *) $echo "failed $test test for:
$string" >&2
       pass=false;;
    esac
  done

  # Make sure we do not recognize these as blobs.
  test=negative
  for string in \
    "#define X { 1, 2 }
#define Y { 3, 4 }" \
    " 0x00, 0x00, 0x00 " \
    "accept(1, 2, 3,
4, 5, 6)" \
  ; do
    case `$echo "$string" | $0 $targs` in
    "") ;;
    *) echo "failed $test test for:
$string" >&2
       pass=false;;
    esac
  done

  # Make sure we print only the lines with blobs.
  test="only blob"
  odd=:
  for string in \
    "= {
1, 0x2, 03, L'\x4'
}" \
	"1, 0x2, 03, L'\x4'" \
\
    "=
{
  '\\x1', '\\002'
  ,
  {
    { \"\\x3\", },
    \"\\004\"
  },
};" \
	"  '\\x1', '\\002'
  ,
  {
    { \"\\x3\", },
    \"\\004\"" \
\
    ".long 1,2
     .long \$3,\$4" \
	".long 1,2
     .long \$3,\$4" \
\
    "#define X { 1, 2, \\
		 3, 4, /* comment */ \\
	       }" \
	"#define X { 1, 2, \\
		 3, 4, /* comment */ \\" \
\
    "= {
/*
 * multi-line
 * comment
 */
 {
   0x4c00c000, 0x00000000, 0x00060000, 0x00000000,
 },
}" \
	"   0x4c00c000, 0x00000000, 0x00060000, 0x00000000," \
\
    "MODULE_FIRMWARE(x);
MODULE_FIRMWARE(y);
1, 2, 3, 4; 5, 6, 7, 8;
9, 10, 11" \
      "MODULE_FIRMWARE(x);
MODULE_FIRMWARE(y);
::: - :::
1, 2, 3, 4; 5, 6, 7, 8;" \
\
    "= {
blob()
accept()
1, 2, 3, 4
}" \
	"blob()
::: - :::
1, 2, 3, 4" \
\
    "a blobeol y
x" \
	"a blobeol y
x" \
\
  ; do
    if $odd; then
      input=$string odd=false
      continue
    fi
    case `$echo "$input" | $0 $targs -B` in
    "::: - :::
$string") ;;
    *)
      $echo "failed $test test for:
$input" >&2
      pass=false
      ;;
    esac
    odd=:
  done
  $odd || { echo "internal testsuite failure in $test" >&2; }

  # Make sure we deblob only the blobs.
  test="deblobs"
  odd=:
  for string in \
    "= { 1, 0x2, 03, L'\x4' }" \
	"= { /*(DEBLOBBED)*/' }" \
\
    "=
{
  '\\x1', '\\002'
  ,
  {
    { \"\\x3\", },
    \"\\004\"
  },
};" \
	"  '\\x/*(DEBLOBBED)*/\"" \
\
    ".long 1,2
     .long \$3,\$4" \
	".long /*(DEBLOBBED)*/" \
\
    "#define X { 1, 2, \\
		 3, 4, /* comment */ \\
	       }" \
	"#define X { /*(DEBLOBBED)*/, /* comment */ \\" \
\
    "= {
/*
 * multi-line
 * comment
 */
 {
   0x4c00c000, 0x00000000, 0x00060000, 0x00000000,
 },
}" \
	"   /*(DEBLOBBED)*/," \
\
    "MODULE_FIRMWARE(x);
MODULE_FIRMWARE(y);
1, 2, 3, 4; 5, 6; 7, 8, 9, 10;
9, 10, 11" \
      "/*(DEBLOBBED)*/
::: - :::
/*(DEBLOBBED)*/; 5, 6; /*(DEBLOBBED)*/;" \
\
    "= {
accept() blob() x blob(
) y
}" \
	"accept() /*(DEBLOBBED)*/ x /*(DEBLOBBED)*/ y" \
\
    "= {
accept() blob() x blob(
w) y
}" \
	"accept() /*(DEBLOBBED)*/ x /*(DEBLOBBED)*/ y" \
\
    "a blobeol y
x" \
	"a /*(DEBLOBBED)*/x" \
\
  ; do
    if $odd; then
      input=$string odd=false
      continue
    fi
    case `$echo "$input" | $0 $targs -b` in
    "::: - :::
$string") ;;
    *)
      $echo "failed $test test for:
$input" >&2
      pass=false
      ;;
    esac
    odd=:
  done
  $odd || { echo "internal testsuite failure in $test" >&2; }

  # How did we do?
  if $pass; then
    echo success for $tool
  else
    allpass=$pass
  fi
 done
 $allpass
 exit
fi

# Call addx as needed to set up more patterns to be recognized as
# false positives.  Takes the input filename in $1.

set_except () {
  case $prefix$1 in
  */*linux*.tar* | */*kernel*.tar* | */*linux-*.*/*)
    # false alarms, contain source
    # drivers/net/wan/wanxlfw.inc_shipped -> wanxlfw.S
    accept 'static[ ]u8[ ]firmware\[\]=[{][\n]0x60,\(0x00,\)*0x16,\(0x00,\)*\([\n]\(0x[0-9A-F][0-9A-F],\)*\)*[\n]0x23,0xFC,0x00,0x00,0x00,0x01,0xFF,0xF9,0x00,0xD4,0x61,0x00,0x06,0x74,0x33,0xFC,\([\n]\(0x[0-9A-F][0-9A-F],\)*\)*0x00[\n][}][;]'
    # drivers/usb/serial/xircom_pgs_fw.h -> xircom_pgs.S
    initnc 'static[ ]const[ ]struct[ ]ezusb_hex_record[ ]xircom_pgs_firmware\[\][ ]='
    # drivers/usb/serial/keyspan_pda_fw_h -> keyspan_pda.S
    initnc 'static[ ]const[ ]struct[ ]ezusb_hex_record[ ]keyspan_pda_firmware\[\][ ]='
    # arch/m68k/ifpsp060/*.sa -> src/*.s
    accept '[	]\.long[	]0x60ff0000,0x02360000,0x60ff0000,0x16260000[\n]'"$sepx$blobpat*"
    accept '[	]\.long[	]0x60ff0000,0x17400000,0x60ff0000,0x15f40000[\n]'"$sepx$blobpat*"
    # arch/powerpc/platforms/cell/spufs/spu_save_dump.h_shipped -> spu_save.c
    initnc 'static[ ]unsigned[ ]int[ ]spu_save_code\[\][ ][ ]__attribute__[(][(]__aligned__[(]128[)][)][)][ ]='
    # arch/powerpc/platforms/cell/spufs/spu_restore_dump.h_shipped -> spu_restore.c
    initnc 'static[ ]unsigned[ ]int[ ]spu_restore_code\[\][ ][ ]__attribute__[(][(]__aligned__[(]128[)][)][)][ ]='
    # drivers/net/ixp2000/ixp2400_tx.ucode -> ixp2400_tx.uc
    initnc '[	]\.initial_reg_values[	]=[ ][(]struct[ ]ixp2000_reg_value[ ]\[\][)][ ][{]' drivers/net/ixp2000/ixp2400_tx.ucode
    # drivers/net/ixp2000/ixp2400_rx.ucode -> ixp2400_rx.uc
    initnc '[	]\.initial_reg_values[	]=[ ][(]struct[ ]ixp2000_reg_value[ ]\[\][)][ ][{]' drivers/net/ixp2000/ixp2400_rx.ucode


    # checked:

    accept '[	][$]3[ ]=[ ][{][{]pge[ ]=[ ][{][{]ste[ ]=[ ][{]\(\([0-9][0-9a-fx{},\n 	]*\|\(pge\|ste\)[ ]=\|<repeats[ ][0-9]\+[ ]times>\)[{},\n 	]*\)*<repeats[ ]11[ ]times>[}]$'
    accept '__clz_tab:[\n][	]\.byte[	]0\(,[0-5]\)\+'"$sepx$blobpat*" arch/sparc/lib/divdi3.S
    accept 'PITBL:[\n][ ][ ]\.long[ ][ ]0xC0040000,0xC90FDAA2,'"$blobpat*" arch/sparc/lib/divdi3.S
    accept '\(0x[0F][0F],\)\+\\[\n]\(\(0x[0F][0F],\)\+\\[\n]\)*\(0x[0F][0F],\)\+0x00' arch/m68k/mac/mac_penguin.S
    accept '\.lowcase:[\n][	]\.byte[ ]0x00\(,0x0[1-7]\)\+'"$sepx$blobpat*"'$' arch/s390/kernel/head.S
    accept '_zb_findmap:[\n][ ][ ][ ][ ][ ][ ][ ][ ][ ]\.byte[ ][ ]0\(,[123],0\)\+,4'"$sepx$blobpat*"'$' arch/s390/kernel/bitmap.S
    accept '_sb_findmap:[\n][ ][ ][ ][ ][ ][ ][ ][ ][ ]\.byte[ ][ ]8\(,0,[123]\)\+,0'"$sepx$blobpat*"'$' arch/s390/kernel/bitmap.S
    accept '[	]\.section[ ]__ex_table,["]a["]'"$sepx$blobpat*" arch/powerpc/lib/copyuser_64.S
    accept '[	]memcpy[(]src,[ ]["]\\x01\\x00\\x00\\x01\\x00\\x00\\x00\\x00\\x00\\x00\\x00\\x00["].*PROGxxxx' arch/powerpc/platforms/iseries/mf.c
    initnc 'static[ ]const[ ]unsigned[ ]int[ ]cpu_745x\[2\]\[16\][ ]=' arch/ppc/platforms/ev64260.c
    initnc 'const[ ]unsigned[ ]char[ ]__flsm1_tab\[256\][ ]=' arch/alpha/lib/fls.c
    accept '#define[ ]_MAP_0_32_ASCII_SEG7_NON_PRINTABLE[	]\\[\n][	]\(0,\)\+$' 'drivers/input/misc/map_to_7segment\.h\|include/linux/map_to_7segment\.h'
    initc '[	]static[ ]int[ ][ ][ ][ ][ ][ ]init_values_b\[\][ ]=' sound/oss/ad1848.c
    initnc 'static[ ]unsigned[ ]char[ ]atkbd_set2_keycode\[512\][ ]=' drivers/input/keyboard/atkbd.c
    accept 'desc_config1:[\n][	]\.byte[ ]0x09,[ ]0x02'"$sepx$blobpat*" 'drivers/usb/serial/\(keyspan_pda\|xircom_pgs\).S'
    accept 'string_mfg:[\n]\?\([;]\?[	]\.byte[^\n]*[\n]\)\+string_mfg_end:' 'drivers/usb/serial/\(keyspan_pda\|xircom_pgs\).S'
    accept 'string_product:[\n]\?\([;]\?[	]\.byte[^\n]*[\n]\)\+string_product_end:' 'drivers/usb/serial/\(keyspan_pda\|xircom_pgs\).S'
    accept '[ ][ ][ ][/][*][ ]\(SQCIF\|QSIF\|QCIF\|SIF\|CIF\|VGA\)[ ][*][/][\n][ ][ ][ ][{][\n][ ][ ][ ][ ][ ][ ][{]'"$blobpat*" drivers/media/video/pwc/pwc-nala.h
    accept 'P[13]\([\n]#[^\n]*\)*[\n]*\([\n][0-9 ]*\)\+' drivers/video/logo/*.ppm
    accept 'for[ ]i[ ]in[ ][ 	0-9\\\n]*[\n]do' 'Documentation/specialix\.txt|Documentation/serial/specialix\.txt'
    accept '[ ][ ][ ][ ][ ][ ][ ][ ][ ]:[ ][ ][ ]3600000[ ][ ][ ]3400000[ ][ ][ ]3200000[ ][ ][ ]3000000[ ][ ][ ]2800000[ ]' Documentation/cpu-freq/cpufreq-stats.txt
    accept '00[ ]00[\n]64[ ]01[\n]8e[ ]0b[\n][\n][0-9a-f \n]*fe[ ]fe' 'Documentation/scsi/\(sym\|ncr\)53c8xx_2.txt'
    accept '0f[ ]00[ ]08[ ]08[ ]64[ ]00[ ]0a[ ]00[ ]-[ ]id[ ]0[\n]'"$blobpat*" 'Documentation/scsi/\(sym\|ncr\)53c8xx_2.txt'
    accept 'default[ ]nvram[ ]data:'"$sepx$blobpat*" 'Documentation/scsi/\(sym\|ncr\)53c8xx_2.txt'
    accept '0x0458[ ][ ][ ][ ][ ]0x7025[\n]'"$blobpat*" Documentation/video4linux/sn9c102.txt
    accept '0x102c[ ][ ][ ][ ][ ]0x6151[\n]'"$blobpat*" Documentation/video4linux/et61x251.txt
    accept '0x041e[ ][ ][ ][ ][ ]0x4017[\n]'"$blobpat*" Documentation/video4linux/zc0301.txt
    accept '[ ][ ][(]gdb[)][ ]x[/]100x[ ][$]25[\n][ ][ ]0x507d2434:[ ][ ][ ][ ][ ]0x507d2434[ ][ ][ ][ ][ ][ ]0x00000000[ ][ ][ ][ ][ ][ ]0x08048000[ ][ ][ ][ ][ ][ ]0x080a4f8c'"$sepx$blobpat*" Documentation/uml/UserModeLinux-HOWTO.txt
    accept '[ ][ ][ ][ ][ ][ ]1[ ][ ]0[ ][ ]0[ ][ ]0[ ][ ]0x308'"$sepx$blobpat*" Documentation/isdn/README.inc
    accept 'domain<N>[ ]<cpumask>[ ]1[ ]2[ ]3[ ]4[ ]5[ ]6[ ]7[ ]8[ ]9[ ]10[ ]11[ ]12[ ]13[ ]14[ ]15[ ]16[ ]17[ ]18[ ]19[ ]20[ ]21[ ]22[ ]23[ ]24[ ]25[ ]26[ ]27[ ]28[ ]29[ ]30[ ]31[ ]32[ ]33[ ]34[ ]35[ ]36$' Documentation/sched-stats.txt
    accept '[ *	]*0[ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ]1[ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ]2[ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ][ ]3[\n][ *	]*0[ ]1[ ]2[ ]3[ ]4[ ]5[ ]6[ ]7[ ]8[ ]9[ ]0[ ]1[ ]2[ ]3[ ]4[ ]5[ ]6[ ]7[ ]8[ ]9[ ]0[ ]1[ ]2[ ]3[ ]4[ ]5[ ]6[ ]7[ ]8[ ]9[ ]0[ ]1' 'net/\(netfilter\|ipv4\)/ipvs/ip_vs_sync.c|net/sctp/sm_make_chunk.c|include/linux/scpt.h'
    accept '[ ][*][ ][ ]1[ ]1[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]1[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0' arch/x86/lguest/boot.c
    ocomment '[	][/][*][ ]Configure[ ]the[ ]PCI[ ]bus[ ]bursts[ ]and[ ]FIFO[ ]thresholds.' drivers/net/fealnx.c
    ocomment '[/][*][ ]the[ ]original[ ]LUT[ ]values[ ]from[ ]Alex[ ]van[ ]Kaam[ ]<darkside@chello\.nl>' drivers/hwmon/via686a.c
    initc 'static[ ]const[ ]unsigned[ ]char[ ]init\[\][ ]=[ ][{][^;]*MODE=0[ ][;].*SAA_7114_NTSC_HSYNC_START' drivers/media/video/saa7114.c

    defsnc 'static[ ]struct[ ]cipher_testvec[ ]\(aes\|anubis\|bf\|camellia\|cts_mode\|des3_ede\|cast6\|salsa20_stream\|serpent\|tf\|tnepres\|xeta\|x\?tea\)\(_\(cbc\|ctr\(_rfc3686\)\?\|xts\)\)\?_\(enc\|dec\)_tv_template\[\][ ]=' 'crypto/\(tcrypt\|testmgr\).h'
    defsnc 'static[ ]struct[ ]comp_testvec[ ]\(deflate\|lzo\)_\(de\)\?comp_tv_template\[\][ ]=' 'crypto/\(tcrypt\|testmgr\).h'
    defsnc 'static[ ]struct[ ]hash_testvec[ ]\(aes_xcbc128\|crc32c\|hmac_sha2\(24\|56\)\|\(sha\|wp\)\(256\|384\|512\)\)_tv_template\[\][ ]=' 'crypto/\(tcrypt\|testmgr\).h'
    # initnc '[ 	]*\.\(digest\|entries\|input\|key\|output\|plaintext\|result\)[ \n	]*=[ ][{"]' 'crypto/\(tcrypt\|testmgr\).h'

    defsnc 'static[ ]\(const[ ]\)\?RegInitializer[ ]initData\[\][ ]__initdata[ ]=' 'drivers/ide/ali14xx\.c\|drivers/ide/legacy/ali14xx\.c'
    defsnc 'static[ ]const[ ]u8[ ]setup\[\][ ]=' 'drivers/ide/delkin_cb\.c\|drivers/ide/pci/delkin_cb\.c'
    defsnc 'static[ ]u8[ ]cvs_time_value\[\]\[XFER_UDMA_6[ ]-[ ]XFER_UDMA_0[ ][+][ ]1\][ ]=' 'drivers/ide/sis5513\.c\|drivers/ide/pci/sis5513\.c'
    defsnc 'static[ ]u8[ ]\(act\|ini\|rco\)_time_value\[\]\[8\][ ]=' 'drivers/ide/sis5513\.c\|drivers/ide/pci/sis5513\.c'
    defsnc 'static[ ]const[ ]u8[ ]speedtab[ ]\[3\]\[12\][ ]=' 'drivers/ide/umc8672\.c\|drivers/ide/legacy/umc8672\.c'
    defsnc 'static[ ]const[ ]s8[ ]\(b43\(legacy\)\?\|bcm43xx\)_tssi2dbm_[bg]_table\[\][ ]=' net/wireless/b43/phy.c
    defsnc 'static[ ]const[ ]char[ ]zr360[56]0_dht\[0x1a4\][ ]=' 'drivers/media/video/zr36060\.c\|drivers/media/video/zoran/zr36060\.c'
    defsnc 'static[ ]const[ ]char[ ]zr360[56]0_dqt\[0x86\][ ]=' 'drivers/media/video/zr36060\.c\|drivers/media/video/zoran/zr36060\.c'
    defsnc 'static[ ]u8[ ]tas3004_treble_table\[\][ ]=' sound/aoa/codecs/tas-basstreble.h

    # This file contains firmwares that we deblob with high
    # sensitivity, so make sure the sequences of numbers that are not
    # blobs are not deblobbed.  FIXME: we should have patterns to
    # recognize the blobs instead.
    defsnc '[	]static[ ]const[ ]u32[ ]test_pat\[4\]\[6\][ ]=' drivers/net/tg3.c
    accept "[	][}]\\(,\\?[ ]mem_tbl_5\\(70x\\|705\\|755\\|906\\)\\[\\][ ]=[ ][{]$sepx$blobpat*$sepx[}]\\)*[;]" drivers/net/tg3.c

    # end of generic checked expressions.
    # version-specific checked bits start here

    # removed in 2.6.28
    defsnc 'static[ ]unsigned[ ]char[ ]irq_xlate\[32\][ ]=' arch/sparc/kernel/sun4m_irq.c
    defsnc 'static[ ]int[ ]logitech_expanded_keymap\[LOGITECH_EXPANDED_KEYMAP_SIZE\][ ]=' drivers/hid/hid-input.c
    defsnc '[	]static[ ]const[ ]\(__\)\?u8[ ]\(read_indexs\|n\(set\)\?[0-9]*\(_other\)\?\|missing\)\[[0-9x]*\][ ]=' drivers/media/video/gspca/t613.c
    defsnc 'static[ ]const[ ]u_char[ ]nand_ecc_precalc_table\[\][ ]=' drivers/mtd/nand/nand_ecc.c
    oprepline '#define[ ]AR5K_RATES_\(11[ABG]\|TURBO\|XR\)[ ]' drivers/net/wireless/ath5k/ath5k.h
    defsnc 'static[ ]const[ ]struct[ ]ath_hal[ ]ar5416hal[ ]=' drivers/net/wireless/ath9k/hw.c
    defsnc 'const[ ]unsigned[ ]char[ ]INIT_2\[127\][ ]=' drivers/video/omap/lcd_sx1.c

    # removed in 2.6.24
    accept "[ ]Psize[ ][ ][ ][ ]Ipps[ ][ ][ ][ ][ ][ ][ ]Tput[ ][ ][ ][ ][ ]Rxint[ ][ ][ ][ ][ ]Txint[ ][ ][ ][ ]Done[ ][ ][ ][ ][ ]Ndone[\\n][ ]---------------------------------------------------------------\\([\\n][ 0-9]\\+\\)\\+"'$'
    initnc 'static[ ]u_short[ ]ataplain_map\[NR_KEYS\][ ]__initdata[ ]='
    initnc '[	]static[ ]const[ ]unsigned[ ]char[ ]invert5\[\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]alpa2target\[\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]target2alpa\[\][ ]='
    oprepline '#define[ ]INIT_THREAD[ ][{0},]\+[ 	]*\\[\n][ 	]*[{0},]\+'
    initnc 'static[ ]uint[ ]tas300\(1c\|4\)_\(master\|mixer\|treble\|bass\)_tab\[\]='
    initnc 'static[ ]short[ ]dmasound_[au]law2dma16\[\][ ]='
    initnc 'static[ ]const[ ]unsigned[ ]short[ ]DACVolTable\[101\][ ]='

    # removed in 2.6.23
    initnc 'static[ ]const[ ]UQItype[ ]__clz_tab\[\][ ]=' arch/arm26/lib/udivdi3.c
    initnc '[	]static[ ]unsigned[ ]char[ ]scale\[101\][ ]=' sound/oss/opl3sa2.c
    initnc '[}][ ]syncs\[\][ ]=' drivers/scsi/53c7xx.c
    initnc 'genoa_md:'"$sepx$blobpat*"'[\n][	]\.ascii[	]["]Genoa["]' arch/i386/boot/video.S

    # removed in 2.6.22
    initnc 'Vendor[ ]ID[ ][ ]Product[ ]ID[\n]-\+[ ][ ]-\+[\n]'"$blobpat*" Documentation/video4linux/sn9c102.txt
    defsnc 'static[ ]short[ ][au]law2dma16\[\]' arch/ppc/8xx_io/cs4218_tdm.c
    defsnc '[	]static[ ]const[ ]char[ ]minimal_ascii_table\[\]' drivers/ieee1394/csr1212.c
    defsnc 'static[ ]u16[ ]key_map[ ]\[256\][ ]=' drivers/media/dvb/ttpci/av7110_ir.c
    defsnc 'static[ ]unsigned[ ]char[ ]gf64_inv\[64\][ ]=' drivers/mtd/nand/cafe_ecc.c
    defsnc 'static[ ]unsigned[ ]short[ ]err_pos_lut\[4096\][ ]=' drivers/mtd/nand/cafe_ecc.c
    defsnc 'static[ ]unsigned[ ]char[ ]testdata\[TESTDATA_LEN\][ ]=' fs/jffs2/comprtest.c

    # added in 2.6.25
    accept "%canned_values[ ]=[ ][(][\\n][	]\\([0-9]\\+[ ]=>[ ]\\[[ 	\\n]\\+\\(\\([0-9]\\+\\|\\'0x[0-9a-f]\\+\\'\\),[ 	\\n]*\\)*\\]\\(,[ ]\\|[\\n]\\)\\)*[)][;]"

    # from 2.6.25-rc* patches
    initnc '[	]int[ ]bcomm_irq\[3[*]16\][ ]='
    initnc '[	]static[ ]const[ ]int8[ ]countLeadingZerosHigh\[\][ ]='
    initnc 'static[ ]struct[ ]nic_qp_map[ ]nic_qp_mapping_[01]\[\][ ]='
    initnc 'static[ ]struct[ ]regval[ ]ov_initvals\[\][ ]=' drivers/media/usb/stkwebcam/stk-sensor.c
    initnc 'static[ ]struct[ ]regval[ ]stk1125_initvals\[\][ ]=' drivers/media/usb/stkwebcam/stk-webcam.c
    initnc 'static[ ]u8[ ]bnx2x_stats_len_arr\[BNX2X_NUM_STATS\][ ]='
    defsnc 'static[ ]const[ ]struct[ ]arb_line[ ]read_arb_data\[NUM_RD_Q\]\[MAX_RD_ORD[ ][+][ ]1\][ ]=' drivers/net/bnx2x/bnx2x_init_opts.h
    defsnc 'static[ ]const[ ]struct[ ]arb_line[ ]write_arb_data\[NUM_WR_Q\]\[MAX_WR_ORD[ ][+][ ]1\][ ]=' drivers/net/bnx2x/bnx2x_init_opts.h
    initnc '[	][	][}][ ]blinkrates\[\][ ]='
    initnc 'static[ ]const[ ]struct[ ]ath5k_ini[ ]ar5212_ini\[\][ ]='
    defsnc 'static[ ]const[ ]struct[ ]ath5k_ini_mode[ ]rf5413_ini_mode_end\[\][ ]=' drivers/net/wireless/ath/ath5k/initvals.c
    defsnc 'static[ ]const[ ]struct[ ]ath5k_ini_rf[ ]rfregs_5111\[\][ ]=' drivers/net/wireless/ath/ath5k/rfbuffer.h
    defsnc 'static[ ]const[ ]struct[ ]ath5k_ini_rf[ ]rfregs_5112\[\][ ]=' drivers/net/wireless/ath/ath5k/rfbuffer.h
    defsnc 'static[ ]const[ ]struct[ ]ath5k_ini_rf[ ]rfregs_5112a\[\][ ]=' drivers/net/wireless/ath/ath5k/rfbuffer.h
    defsnc 'static[ ]const[ ]struct[ ]ath5k_ini_rf[ ]rfregs_5413\[\][ ]=' drivers/net/wireless/ath/ath5k/rfbuffer.h

    # new in 2.6.26
    initnc 'static[ ]u64[ ]vec2off\[68\][ ]=' arch/ia64/kvm/process.c
    accept "[	][	][	]interrupts[ ]=[ ]<\\(0x\\)\\?3[ ]\\(0x\\)\\?0[ ]\\(0x\\)\\?0[ ][ ]$blobpat*>[;]" 'arch/powerpc/boot/dts/\(cm5200\|lite5200b\?\|kuroboxHG\|pcm030\|tqm5200\).dts'
    initnc 'static[ ]const[ ]u32[ ]crctab32\[\][ ]=' arch/x86/boot/tools/build.c
    defsnc 'static[ ]struct[ ]mse2snr_tab[ ]\(vsb\|qam\(64\|256\)\)_mse2snr_tab\[\][ ]=' drivers/media/dvb/frontends/au8522.c
    defsnc '[}][ ]\(VSB\|QAM\(64\|256\)\?\)_mod_tab\[\][ ]=' 'drivers/media/dvb/frontends/au8522\(_dig\)\?\.c'
    initnc '[}][ ]itd1000_\(lpf_pga\|fre_values\)\[\][ ]=' drivers/media/dvb/frontends/itd1000.c
    initnc '[}][ ]\(vsb\|qam\(64\|256\)\)_snr_tab\[\][ ]=' drivers/media/dvb/frontends/s5h1411.c
    initnc '[}][ ]snr_tab\[\][ ]=' drivers/media/dvb/frontends/tda10048.c
    initnc 'static[ ]u32[ ]reg_init_initialize\[\][ ]=' drivers/media/video/saa717x.c
    initnc 'static[ ]const[ ]u32[ ]\(main\|gear\)_seedset\[BACKOFF_SEEDSET_ROWS\]\[BACKOFF_SEEDSET_LFSRS\][ ]=' drivers/net/forcedeth.c
    initnc 'static[ ]const[ ]struct[ ]ath5k_ini_mode[ ]rf24\(13\|25\)_ini_mode_end\[\][ ]=' drivers/net/wireless/ath5k/initvals.c
    initnc 'static[ ]const[ ]u16[ ]wm9713_reg\[\][ ]=' sound/soc/codecs/wm9713.c

    # new in 2.6.27
    accept '[	]\.section[ ]__ex_table,["]a["]'"$sepx$blobpat*" 'arch/x86/lib/copy_user_\(nocache_\)\?64.S'
    accept 'desc_config1:[\n][	]\.byte[ ]0x09,[ ]0x02'"$sepx$blobpat*" 'firmware/keyspan_pda/\(keyspan_pda\|xircom_pgs\).S'
    accept 'string_mfg:[\n]\?\([;]\?[	]\.byte[^\n]*[\n]\)\+string_mfg_end:' 'firmware/keyspan_pda/\(keyspan_pda\|xircom_pgs\).S'
    accept 'string_product:[\n]\?\([;]\?[	]\.byte[^\n]*[\n]\)\+string_product_end:' 'firmware/keyspan_pda/\(keyspan_pda\|xircom_pgs\).S'
    accept ':03000000020200F9[\n]:040023000205\(9B0037\|5F0073\)[\n]\(:050030000000000000CB[\n]\|:0400430002010000B6[\n]\)*'"$sepx$blobpat*"'[\n]:\(0E06E0006400670065007400060334003700F4\|0606A000060334003700E0\)[\n]:00000001FF' 'firmware/keyspan_pda/\(keyspan_pda\|xircom_pgs\).HEX'
    accept ':100000000C004000000000000000000000000000A4[\n]'"$sepx$blobpat*"'[\n][/][*][ ]DSP56001[ ]bootstrap[ ]code[ ][*][/]' firmware/dsp56k/bootstrap.bin.ihex
    initnc 'static[ ]const[ ]u16[ ]uda1380_reg\[UDA1380_CACHEREGNUM\][ ]=' sound/soc/codecs/uda1380.c
    defsnc 'static[ ]const[ ]u16[ ]wm8510_reg\[WM8510_CACHEREGNUM\][ ]=' sound/soc/codecs/wm8510.c
    initnc 'static[ ]const[ ]unsigned[ ]short[ ]atkbd_unxlate_table\[128\][ ]=' drivers/input/keyboard/atkbd.c
    initnc 'static[ ]const[ ]unsigned[ ]char[ ]usb_kbd_keycode\[256\][ ]=' drivers/hid/usbhid/usbkbd.c
    initnc '[	][	]u8[ ]buf,[ ]bufs\[\][ ]=' drivers/media/dvb/dvb-usb/cxusb.c
    initnc 'static[ ]struct[ ]dvb_pll_desc[ ][^\n]*[ ]=' drivers/media/dvb/frontends/dvb-pll.c
    initnc '[	]static[ ]int[ ]sysdiv_to_div_x_2\[\][ ]=' arch/powerpc/platforms/512x/clock.c
    defsnc 'static[ ]const[ ]__u8[ ]cx_inits_\(176\|320\|352\|640\)\[\][ ]=' drivers/media/video/gspca/conex.c
    defsnc 'static[ ]const[ ]__u8[ ]cx_jpeg_init\[\]\[8\][ ]=' drivers/media/video/gspca/conex.c
    defsnc 'static[ ]const[ ]__u8[ ]cxjpeg_\(640\|352\|320\|176\|qtable\)\[\]\[8\][ ]=' drivers/media/video/gspca/conex.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]quant\[\]\[0x88\][ ]=' drivers/media/video/gspca/jpeg.h
    defsnc 'static[ ]unsigned[ ]char[ ]huffman\[\][ ]=' drivers/media/video/gspca/jpeg.h
    initc '[	]\?static[ ]const[ ]struct[ ]ov_i2c_regvals[ ]norm_76[1247]0\[\][ ]=' drivers/media/video/gspca/ov519.c
    initnc 'static[ ]const[ ]__u8[ ]pac207_sensor_init\[\]\[8\][ ]=' drivers/media/video/gspca/pac207.c
    initnc 'static[ ]const[ ]__u8[ ]pac7311_jpeg_header\[\][ ]=' drivers/media/video/gspca/pac7311.c
    defsnc 'static[ ]const[ ]__u8[ ]\(start\|page[34]\)_73\(02\|11\)\[\][ ]=' 'drivers/media/video/gspca/pac73\(02\|11\)\.c'
    initnc 'static[ ]const[ ]__u8[ ]init\(Hv7131\|Ov\(6650\|7630\(_3\)\?\)\|Pas\(106\|202\)\|Tas51[13]0\)\[\][ ]=' drivers/media/video/gspca/sonixb.c
    initnc 'static[ ]const[ ]__u8[ ]\(hv7131\|ov\(6650\|7630\(_3\)\?\)\|pas\(106\|202\)\|tas51[13]0\)_sensor_init\(_com\)\?\[\]\[8\][ ]=' drivers/media/video/gspca/sonixb.c
    defsnc 'static[ ]\(const[ ]\)\?\(__\)\?u8[ ]\(mt9v111\|sp80708\|hv7131[rd]\|mi0360b\?\|mo4000\|ov76\([36]0\|48\)\|om6802\|po1030\)_sensor_\(init\|param1\)\[\]\[8\][ ]=' drivers/media/video/gspca/sonixj.c
    initnc 'static[ ]const[ ]__u8[ ]qtable4\[\][ ]=' drivers/media/video/gspca/sonixj.c
    initnc 'static[ ]const[ ]__u16[ ]\(spca500_visual\|Clicksmart510\)_defaults\[\]\[3\][ ]=' drivers/media/video/gspca/spca500.c
    initnc 'static[ ]const[ ]__u8[ ]qtable_\(creative_pccam\|kodak_ez200\|pocketdv\)\[2\]\[64\][ ]=' drivers/media/video/gspca/spca500.c
    initnc 'static[ ]const[ ]__u16[ ]spca501c\?_\(\(3com\|arowana\|mysterious\)_\)\?\(init\|open\)_data\[\]\[3\][ ]=' drivers/media/video/gspca/spca501.c
    defsnc 'static[ ]const[ ]\(__u16\|u8\)[ ]spca505b\?_\(init\|open\)_data\(_ccd\)\?\[\]\[3\][ ]=' drivers/media/video/gspca/spca505.c
    defsnc 'static[ ]const[ ]\(__\)\?u16[ ]spca508\(cs110\|_sightcam2\?\|_vista\)\?_init_data\[\]\[[23]\][ ]=' drivers/media/video/gspca/spca508.c
    initnc 'static[ ]const[ ]__u16[ ]\(spca561\|rev72a\)_init_data3\?\[\]\[2\][ ]=' drivers/media/video/gspca/spca561.c
    defsnc 'static[ ]const[ ]\(__u16\|struct[ ]cmd\)[ ]spca504\(_pccam600\|A_clicksmart420\)_\(init\|open\)_data\[\]\(\[3\]\)\?[ ]=' drivers/media/video/gspca/sunplus.c
    defsnc 'static[ ]const[ ]\(__\)\?u8[ ]qtable_\(creative_pccam\|spca504_default\)\[2\]\[64\][ ]=' drivers/media/video/gspca/sunplus.c
    initnc 'static[ ]const[ ]__u8[ ]\(effects\|gamma\)_table\[\(MAX_[A-Z]*\|[A-Z]*_MAX\)\]\[[0-9]*\][ ]=' drivers/media/video/gspca/t631.c
    initnc 'static[ ]const[ ]\(__\)\?u8[ ]tas5130a_sensor_init\[\]\[8\][ ]=' drivers/media/video/gspca/t613.c
    defsnc 'static[ ]const[ ]struct[ ]usb_action[ ]\(cs2102\|hdcs2020xx\|icm105a\(xx\)\?\|ov7630c\|mt9v111_[13]\|pb0330\([3x]x\)\?\|mi0360soc\)_Initial\(Scale\)\?\[\][ ]=' drivers/media/video/gspca/zc3xx.c
    initnc 'static[ ]const[ ]u8[ ]rtl8225z2_\(agc\|ofdm\|power_cck\(_ch14\)\?\)\[\][ ]=' drivers/net/wireless/rtl8187_rtl8225.c
    initnc 'static[ ]const[ ]__u16[ ]t10_dif_crc_table\[256\][ ]=' lib/crc-t10dif.c
    initnc 'static[ ]crb_128M_2M_block_map_t[ ]crb_128M_2M_map\[64\][ ]=' drivers/net/netxen/netxen_hw.c
    initnc 'static[ ]const[ ]__u16[ ]crc10_table\[256\][ ]=' drivers/usb/serial/safe_serial.c
    accept '[ 	]*\([ ]*0\)*\([ ]*1\)*[\n][ 	]*0[ ]1[ ]2[ ]3[ ]4[ ]5[ ]6[ ]7[ ]8[ ]9[ ]0[ ]1[ ]*2[ ]3[ ]4[ ]5[ ]6[ ]7' Documentation/bt8xxgpio.txt
    defsnc '[	]static[ ]int[ ]exp_lut\[256\][ ]=' drivers/isdn/mISDN/dsp_audio.c
    initnc 'static[ ]const[ ]u32[ ]bf_pbox\[16[ ][+][ ]2\][ ]=' drivers/isdn/mISDN/dsp_blowfish.c
    initnc 'static[ ]const[ ]u32[ ]bf_sbox\[256[ ][*][ ]4\][ ]=' drivers/isdn/mISDN/dsp_blowfish.c
    initnc 'static[ ]u8[ ]sample_\(german_\(all\|old\)\|american_\(dialtone\|ringing\|busy\)\|special[123]\|silence\)\[\][ ]=' drivers/isdn/mISDN/dsp_tones.c
    initnc 'struct[ ]pattern[ ][{][^}]*int[ ]tone[;][^}]*[}][ ]pattern\[\][ ]=' drivers/isdn/mISDN/dsp_tones.c
    initnc 'static[ ]u8[ ]\([au]\|_4\)law_to_\([ua]law\|4bit\)\[256\][ ]=' drivers/isdn/mISDN/l1oip_codec.c
    initnc 'static[ ]unsigned[ ]char[ ]banner_table\[\][ ]=' arch/sh/boards/mach-microdev/led.c
    defsnc '[	]static[ ]const[ ]int[ ]desc_idx_table\[\][ ]=' arch/arm/include/asm/hardware/iop3xx-adma.h
    defsnc 'static[ ]\(const[ ]\)\?u32[ ]ar\(5416\|9280\)\(Modes\(_fast_clock\)\?\|Common\|BB_RfGain\|Bank6\(TPC\)\?\|Addac\)\(_91[06]0\(_\?1_1\)\?\|_9280\(_2\)\?\)\?\[\]\[[236]\][ ]=' 'drivers/net/wireless/ath9k/\(ar\(5008\|9001\)_\)\?initvals\.h'

    # new in 2.6.28
    accept '\(static[ ]\)\?const[ ]char[ ]\(inv\)\?parity\[256\][ ]=[ ][{][	 \n01,]*[}][;]' 'Documentation/mtd/nand_ecc\.txt\|drivers/mtd/nand/nand_ecc\.c'
    defsnc 'static[ ]const[ ]char[ ]\(bitsperbyte\|addressbits\)\[256\][ ]=' drivers/mtd/nand/nand_ecc.c
    defsnc 'static[ ]struct[ ]pinmux_cfg_reg[ ]pinmux_config_regs\[\][ ]=' 'arch/sh/kernel/cpu/sh2a/pinmux-sh7203\.c\|arch/arm/mach-shmobile/pfc-sh73[67]7\.c'
    defsnc '[	]static[ ]const[ ]u8[ ]e_keymap\[\][ ]=' drivers/hid/hid-lg.c
    defsnc 'DEFINE_DEFAULT_PDR[(]0x0161,[ ]256,' drivers/net/wireless/hermes_dld.c
    defsnc 'static[ ]const[ ]int[ ]isink_cur\[\][ ]=' drivers/regulator/wm8350-regulator.c
    defsnc 'static[ ]const[ ]s16[ ]\(converge_speed_ipb\?\|LAMBDA_table\[4\]\)\[101\][ ]=' drivers/staging/go7007/go7007-fw.c
    defsnc 'static[ ]const[ ]u32[ ]addrinctab\[33\]\[2\][ ]=' drivers/staging/go7007/go7007-fw.c
    defsnc 'static[ ]const[ ]u8[ ]\(default_intra_quant_table\|\(val\|bits\)_[ad]c_\(lu\|chro\)minance\)\[\][ ]=' drivers/staging/go7007/go7007-fw.c
    defsnc 'static[ ]const[ ]int[ ]zz\[64\][ ]=' drivers/staging/go7007/go7007-fw.c
    defsnc '[	]u16[ ]pack\[\][ ]=' drivers/staging/go7007/go7007-fw.c
    defsnc 'static[ ]u8[ ]\(initial\|channel\)_registers\[\][ ]=' 'drivers/staging/go7007/wis-\(ov7640\|saa7113\|tw2804\).c'
    defsnc 'u16[ ]MTO_One_Exchange_Time_Tbl_[ls]\[MTO_MAX_FRAG_TH_LEVELS\]\[MTO_MAX_DATA_RATE_LEVELS\][ ]=' drivers/staging/winbond/mto.c
    defsnc 'u32[ ]\(al2230_txvga_data\|w89rf242_txvga_old_mapping\)\[\]\[2\][ ]=' drivers/staging/winbond/reg.c
    defsnc 'static[ ]const[ ]UINT16[ ]crc16tab\[256\][ ]=' drivers/staging/wlan-ng/hfa384x.c
    defsnc 'static[ ]const[ ]\(UINT32\|u32\)[ ]wep_crc32_table\[256\][ ]=' drivers/staging/wlan-ng/p80211wep.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]wm_vol\[256\][ ]=' 'sound/pci/ice1712/\(phase\|aureon\)\.c'
    defsnc 'static[ ]const[ ]u16[ ]wm8900_reg_defaults\[WM8900_MAXREG\][ ]=' sound/soc/wm8900.c
    defsnc '[}][ ]\(clk_sys_ratios\|bclk_divs\)\[\][ ]=' 'sound/soc/wm890[34]\.c'
    defsnc 'static[ ]u8[ ]af9015_ir_table_\(leadtek\|twinhan\|a_link\|msi\|mygictv\|kworld\)\[\][ ]=' drivers/media/dvb/dvb-usb/af9015.h
    defsnc 'static[ ]\(const[ ]\)\?struct[ ]\(snr_table\|af9013_snr\)[ ]\(qpsk\|qam\(16\|64\)\)_snr_\(table\|lut\)\[\][ ]=' drivers/media/dvb/frontends/af9013_priv.h
    defsnc 'static[ ]\(const[ ]\)\?struct[ ]\(regdesc\|af9013_reg_bit\)[ ]\(ofsm_init\|tuner_init_\(env77h11d5\|mt2060\(_2\)\?\|mxl500\(3d\|5\)\|qt1010\|mc44s803\|unknown\|tda18271\)\)\[\][ ]=' drivers/media/dvb/frontends/af9013_priv.h
    defsnc 'static[ ]u8[ ]stv0288_earda_inittab\[\][ ]=' drivers/media/dvb/frontends/eds1547.h
    defsnc 'static[ ]u8[ ]serit_sp1511lhb_inittab\[\][ ]=' drivers/media/dvb/frontends/si21xx.c
    defsnc 'static[ ]u8[ ]stv0288_inittab\[\][ ]=' drivers/media/dvb/frontends/stv0288.c
    defsnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_b\[\][ ]=' drivers/net/wireless/rt2x00/rt2400pci.c

    # request_firmware matches for 2.6.28
    accept 'D:[ ]Firmware[ ]loader[ ][(]request_firmware[)]' CREDITS
    accept 'FIRMWARE[ ]LOADER[ ][(]request_firmware[)]' MAINTAINERS
    accept '[	]-[ ]request_firmware[(][)][ ]hotplug[ ]interface[ ]info.' Documentation/00-INDEX
    accept 'This[ ]driver[ ]requires[ ]a[ ]patch[ ]for[ ]firmware_class[^\n]*[\n]request_firmware_nowait[ ]function\.' Documentation/dell_rbu.txt
    accept '\([ ]request_firmware[(][)][ ]hotplug[ ]interface:[\n][ ]--*[\n].*[ ]\)\?-[ ]request_firmware_nowait[(][)][ ]is[ ]also[ ]provided[ ]for[ ]convenience' Documentation/firmware_class/README
    accept 'Still,[ ]there[ ]are[ ]kernel[ ]threads[ ]that[ ]may[ ]want.*For[ ]example,[ ]if[ ]request_.*_firmware[(][)][ ]will[ ]fail[ ]regardless' Documentation/power/freezing-of-tasks.txt
    accept 'Also,[ ]there[ ]may[ ]be[ ]some[ ]operations,.*calling[ ]request_firmware[(][)][ ]from[ ]their[ ].resume[(][)][ ]routines' Documentation/power/notifiers.txt
    accept 'There[ ]is[ ]an[ ]USB[ ]interface[ ]for[ ]downloading[/]uploading.*request_firmware[ ]interface\.' Documentation/video4linux/si470x.txt
    accept '[	]-[ ]move[ ]firmware[ ]loading[ ]to[ ]request_firmware[(][)]' drivers/staging/slicoss/README
    accept 'config[ ]FIRMWARE_IN_KERNEL.*let[ ]firmware[ ]be[ ]loaded[ ]from[ ]userspace\.' drivers/base/Kconfig
    accept '[	 ]*and[ ]request_firmware[(][)][ ]in[ ]the[ ]source' drivers/base/Kconfig
    accept '\(static[ ]\(int\|void\)[\n ]\)\?_request_firmware\(_prepare\|_cleanup\)\?[(]const[ ]struct[ ]firmware[ ][*][*]\?firmware\(_p\)\?[,)][^{]*[\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*[\n]\+[}][\n]' drivers/base/firmware_class.c
    accept 'static[ ]int[\n ]request_firmware_work_func[(]void[ ][*]arg[)][\n][{]\([\n]\+[^\n}][^\n]*\)*ret[ ]=[ ]_request_firmware[(][^\n]*\([\n]\+[^\n}][^\n]*\)*[\n]\+[}][\n]' drivers/base/firmware_class.c
    accept '[/][*][*][\n][ ][*][ ]request_firmware:[ ]-[ ]send[ ]firmware[ ][^{]*[\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*[\n]\+[}][\n]' drivers/base/firmware_class.c
    accept '[/][*][*][\n][ ][*][ ]request_firmware_nowait\(:\|[ ]-\)[ ]asynchronous[ ]version[^{]*[\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*[\n]\+[}][\n]' drivers/base/firmware_class.c
    accept 'EXPORT_SYMBOL[(]request_firmware\(_nowait\)\?[)][;]' drivers/base/firmware_class.c
    accept 'int[ ]request_firmware\(_nowait\)\?[(][^;]*[)][;]' include/linux/firmware.h
    accept 'static[ ]inline[ ]int[ ]request_firmware\(_nowait\)\?[(][^{]*[)][\n][{][\n][	]return[ ]-EINVAL[;][\n][}]' include/linux/firmware.h
    accept 'static[ ]inline[ ]int[\n]\(maybe_\)\?reject_firmware\(_nowait\)\?[(][^{;]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*[\n]\+[}]' include/linux/firmware.h

    accept 'static[ ]inline[ ]int[ ]request_ihex_firmware\?[(][^{]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*[\n]\+[}][\n]' include/linux/ihex.h
    ocomment '[/][*][ ]Optional[ ]firmware\([^\n]*[\n][ ][*]\)*[^\n]*[ ]MODULE_FIRMWARE[(][)]'
    oprepline '#define[ ]MODULE_FIRMWARE[(]_firmware[)]' include/linux/module.h
    accept '[ ][*][ ]Sample[ ]code[ ]on[ ]how[ ]to[ ]use[ ]request_firmware[(][)][ ]from[ ]drivers\.' samples/firmware_class/firmware_sample_driver.c
    accept '[	]\(retval\|error\)[ ]=[ ]request_firmware\(_nowait\)\?[(][^;]*["]sample_driver_fw["],[^;]*[)][;]' samples/firmware_class/firmware_sample_driver.c
    ocomment '[	][/][*][ ]request_firmware[ ]blocks[ ]until[ ]userspace[ ]finished' samples/firmware_class/firmware_sample_driver.c
    accept '[	][	][ 	]*["][ ]request_firmware_nowait[ ]failed' samples/firmware_class/firmware_sample_driver.c

    # We used to remove these in early versions of Linux-libre.
    # They're now believed to be mere initialization data, rather than
    # code disguised as such, and they're not long enough so as to
    # render the software non-Free.
    defsnc 'static[ ]u8[ ]tda10021_inittab\[0x40\]=' drivers/media/dvb/frontends/tda10021.c
    defsnc 'static[ ]u8[ ]tda8083_init_tab[ ]\[\][ ]=' drivers/media/dvb/frontends/tda8083.c
    defsnc 'static[ ]u8[ ]ves1820_inittab\[\][ ]=' drivers/media/dvb/frontends/ves1820.c
    defsnc 'static[ ]u8[ ]init_1[89]93_w\?tab[ ]\?\[\][ ]=' drivers/media/dvb/frontends/ves1x93.c
    defsnc 'static[ ]const[ ]u8[ ]saa7113_tab\[\][ ]=' drivers/media/dvb/ttpci/budget-av.c
    defsnc 'static[ ]u8[ ]philips_sd1878_inittab\[\][ ]=' drivers/media/dvb/ttpci/budget-av.c
    defsnc 'const[ ]struct[ ]Kiara_table_entry[ ]Kiara_table\[PSZ_MAX\]\[6\]\[4\][ ]=' drivers/media/video/pwc/pwc-kiara.c
    defsnc 'const[ ]unsigned[ ]int[ ]KiaraRomTable[ ]\[8\]\[2\]\[16\]\[8\][ ]=' drivers/media/video/pwc/pwc-kiara.c
    defsnc 'const[ ]struct[ ]Timon_table_entry[ ]Timon_table\[PSZ_MAX\]\[PWC_FPS_MAX_TIMON\]\[4\][ ]=' drivers/media/video/pwc/pwc-timon.c
    defsnc 'const[ ]unsigned[ ]int[ ]TimonRomTable[ ]\[16\]\[2\]\[16\]\[8\][ ]=' drivers/media/video/pwc/pwc-timon.c
    defsnc '[	]static[ ]const[ ]struct[ ]struct_initData[ ]initData\[\][ ]=' drivers/media/video/usbvideo/ibmcam.c
    defsnc 'static[ ]const[ ]u8[ ]rtl8187b_reg_table\[\]\[3\][ ]=' drivers/net/wireless/rtl8187_dev.c
    defsnc 'unsigned[ ]char[ ]\(IDX_ACTIVATE_\(READ\|WRITE\)\|\(CM\|ULP\)_\(ENABLE\|SETUP\)\|DM_ACT\|IPA_PDU_HEADER\|\(READ\|WRITE\)_CCW\)\[\][ ]\?=' drivers/net/qeth_core_mpc.c
    defsnc 'static[ ]unsigned[ ]char[ ]camera_ncm03j_magic\[\][ ]=' 'arch/sh/boards/\(board-ap325rxa\.c\|mach-ap325rxa/setup\.c\)'
    defsnc 'static[ ]const[ ]unsigned[ ]short[ ]\(sync\|magic[0-3]\)_data\[\][ ]=' arch/sh/boards/mach-migor/lcd_qvga.c
    defsnc 'static[ ]unsigned[ ]char[ ]camera_ov772x_magic\[\][ ]=' arch/sh/boards/mach-migor/setup.c
    defsnc 'static[ ]struct[ ]chips_init_reg[ ]chips_init_[sgacfx]r\[\][ ]=' 'drivers/video/\(asiliant\|chips\)fb.c'

    # This one is quite suspicious, but it's small enough (64 bytes
    # total) that it's believable that it could be actual source code.
    defsnc 'static[ ]const[ ]__u8[ ]cx11646_fw1\[\]\[3\][ ]=' drivers/media/video/gspca/conex.c

    # Hunting down non-Free firmware-loading code and instructions.
    # Firmware names are to be caught anywhere.

    # 2.6.26 but not later

    blobname 'atmsar1[12]\.\(x\|start\|regions\|data\|bin[12]\?\)' 'drivers/atm/\(Makefile\|ambassador\.c\)'
    blob '#\(define\|include\)[ ]UCODE2\?[(][^\n]*' drivers/atm/ambassador.c
    blob 'static[ ]\(u32\|region\)[ ]__devinitdata[ ]ucode_\(start\|\(regions\|data\)\[\]\)[ ]=[^;]*[;]' drivers/atm/ambassador.c
    blob '\(#\(ifdef[ ]AMB_NEW_MICROCODE\|else\|endif\)[\n]#\(define\|include\)[ ]UCODE2\?[(][^\n]*[\n]\)\+\([\n]*static[ ]\(u32\|region\)[ ]__devinitdata[ ]ucode_\(start\|\(regions\|data\)\[\]\)[ ]=[^;]*[;]\)*' drivers/atm/ambassador.c

    blobname '\(pca\|sba\)200e\(_ecd\)\?\.\(data\|bin[12]\?\)' 'drivers/atm/\(Makefile\|fore200e\(_mkfirm\)\?\.c\)'
    blobna '[/][*][^*]*\([*]\+[^/*][^*]*\)*[*]*PCA-200E[ ]firmware[ ][*][/]' drivers/atm/fore200e_mkfirm.c
    blobna '_fore200e_\(pca\|sba\)_fw_\(data\|size\)' drivers/atm/fore200e.c
    blob '#ifdef[ ]CONFIG_ATM_FORE200E_\(PCA\|SBA\)\([\n]extern[ ]const[ ]unsigned[ ]\(char\|int\)[ ]*_fore200e_\(pca\|sba\)_fw_\(data\[\]\|size\)[;]\)\+[\n]#endif\([\n]\+#ifdef[ ]CONFIG_ATM_FORE200E_\(PCA\|SBA\)\([\n]extern[ ]const[ ]unsigned[ ]\(char\|int\)[ ]*_fore200e_\(pca\|sba\)_fw_\(data\[\]\|size\)[;]\)\+[\n]#endif\)*' drivers/atm/fore200e.c

    # 2.6.27 but not later

    blob 'cas_saturn_patch_t[ ]cas_saturn_patch\[\][ ]=[ ][{][^;]*[}][;]' drivers/net/cassini.h
    accept '[	][ ][ ]firmware[ ]files[ ]--[ ]the[ ]same[ ]names[ ]which[ ]appear[ ]in[ ]MODULE_FIRMWARE[(][)]' drivers/base/Kconfig

    # 2.6.28 or earlier

    blobname 'atmsar11\.fw' drivers/atm/ambassador.c

    blob '\(#ifdef[ ]__\(LITTLE\|BIG\)_ENDIAN[\n]\)\?#define[ ]FW_EXT[ ]["]\(_ecd\)\?\.bin2\?["]\([\n]#else[\n]#define[ ]FW_EXT[ ]["]\(_ecd\)\?\.bin2\?["]\)*\([\n]#endif\)\?' drivers/atm/fore200e.c
    blobna 'sprintf[(][^;]*fore200[^;]*FW_EXT[^;]*[)][;]' drivers/atm/fore200e.c
    blobname '\(pc\|sb\)a200e\(_ecd\)\?\.bin[12]\?' drivers/atm/fore200e.c
    blobna 'The[ ]supplied[ ]firmware[ ]images.*https\?:[/][/][^\n]*\(fore\|FORE_Systems\).*Rebuild[ ]and[ ]re-install[^.]*\.' Documentation/networking/fore200e.txt

    blobname 'intelliport2\.bin' drivers/char/ip2/ip2main.c

    blob 'static[ ]unsigned[ ]char[ ]warp_g[24]00_t2\?gzs\?a\?f\?\[\][ ]=[ ][{][^{};]*[}][;]\([\n][\n]*static[ ]unsigned[ ]char[ ]warp_g[24]00_t2\?gzs\?a\?f\?\[\][ ]=[ ][{][^{};]*[}][;]\)*' drivers/gpu/drm/mga/mga_ucode.h
    blob '\(#define[ ]WARP_UCODE_\(SIZE\|INSTALL\)[(][ ]*which\([^\n]*\\[ 	]*[\n]\)*[^\n]*\|static[ ]const[ ]unsigned[ ]int[ ]mga_warp_g[24]00_microcode_size[ ]=[^;]*[;]\|static[ ]int[ ]mga_warp_install_g[24]00_microcode[(][^{]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*[\n]\+[}]\)\([\n][\n]*\(#define[ ]WARP_UCODE_\(SIZE\|INSTALL\)[(][ ]*which\([^\n]*\\[ 	]*[\n]\)*[^\n]*\|static[ ]const[ ]unsigned[ ]int[ ]mga_warp_g[24]00_microcode_size[ ]=[^;]*[;]\|static[ ]int[ ]mga_warp_install_g[24]00_microcode[(][^{]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*[\n]\+[}]\)\)*' drivers/gpu/drm/mga/mga_warp.c
    blobna '\(case[ ]MGA_CARD_TYPE_G[^:]*:[ 	\n]*\)\+return[ ][^;]*mga_warp[^;]*microcode[^;]*[;]\([ 	\n]*\(case[ ]MGA_CARD_TYPE_G[^:]*:[ 	\n]*\)\+return[ ][^;]*mga_warp[^;]*microcode[^;]*[;][ 	]*\)*' drivers/gpu/drm/mga/mga_warp.c

    blob 'static[ ]u32[ ]r128_cce_microcode\[\][ ]=[ ][{][^;]*[}][;]' drivers/gpu/drm/r128/r128_cce.c
    blob 'static[ ]void[ ]r128_cce_load_microcode[(][^{]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*[\n]\+[}]' drivers/gpu/drm/r128/r128_cce.c
    # blobna 'R128_WRITE[(]R128_PM4_MICROCODE_DATA[HL],[\n	 ]*r128_cce_microcode\[i[ ][*][ ]2\([ ][+][ ]1\)\?\][)]\([;][\n 	]*R128_WRITE[(]R128_PM4_MICROCODE_DATA[HL],[\n	 ]*r128_cce_microcode\[i[ ][*][ ]2\([ ][+][ ]1\)\?\][)]\)*' drivers/gpu/drm/r128/r128_cce.c

    blob 'static[ ]const[ ]u32[ ]R[SV0-9]*[05]_\(c\|pf\)p_microcode\[\]\(\[[23]\]\)\?[ ]=[ ][{][^;]*[}][;]\([\n][\n]*static[ ]const[ ]u32[ ]R[SV0-9]*[05]_\(c\|pf\)p_microcode\[\]\(\[[23]\]\)\?[ ]=[ ][{][^;]*[}][;]\)*' 'drivers/gpu/drm/radeon/\(radeon\|r600\)_microcode\.h'
    blob 'static[ ]void[ ]r\(adeon\|[167]00\)_cp_load_microcode[(][^{]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*cp_microcode[^\n]*\([\n]\+[^\n}][^\n]*\)*[\n]\+[}]' 'drivers/gpu/drm/radeon/r\(\(adeon\|600\)_cp\|100\)\.c'
    # blobna 'RADEON_WRITE[(]R\(ADEON\|600\)_CP_\(ME_RAM\|PFP_UCODE\)_DATA[HL]\?,[\n	 ]*R[SV0-9]*[05]_\(c\|pf\)p_microcode\[i\]\(\[[012]\]\)\?[)]\([;][\n 	]*RADEON_WRITE[(]R\(ADEON\|600\)_CP_\(ME_RAM\|PFP_UCODE\)_DATA[HL]\?,[\n	 ]*R[SV0-9]*[05]_\(c\|pf\)p_microcode\[i\]\(\[[012]\]\)\?[)]\)*' 'drivers/gpu/drm/radeon/\(radeon\|r600\)_cp\.c'

    blob 'sub[ ]\(sp887[0x]\|tda1004\(5\|6\(lifeview\)\?\)\|av7110\|dec\(2\(00\|54\)0t\|3000s\)\|opera1\|vp7041\|dibusb\|nxt200[24]\|cx\(23\(1xx\|885\)\|18\)\|pvrusb2\|or51\(211\|132_\(qam\|vsb\)\)\|bluebird\|mpc718\|af9015\|ngene\)[ ]*[{]\([\n]\+[^\n}][^\n]*\)*[\n]\+[}]\([\n]\+sub[ ]\(sp887[0x]\|tda1004\(5\|6\(lifeview\)\?\)\|av7110\|dec\(2\(00\|54\)0t\|3000s\)\|opera1\|vp7041\|dibusb\|nxt200[24]\|cx\(23\(1xx\|885\)\|18\)\|pvrusb2\|or51\(211\|132_\(qam\|vsb\)\)\|bluebird\|mpc718\|af9015\|ngene\)[ ]*[{]\([\n]\+[^\n}][^\n]*\)*[\n]\+[}]\)*' Documentation/dvb/get_dvb_firmware
    blobna 'Please[ ]use[^\n]*firmware[^\n]*sp887x[^\n]*\([\n][^\n]\+\)\+' Documentation/dvb/avermedia.txt
    blob 'To[ ]extract[ ]the[ ]firmware[^\n]*Opera[ ]DVB-S1[ ]USB-Box.*[/]lib[/]firmware[/][ ]\.' Documentation/dvb/opera-firmware.txt
    blobname '\(dvb-usb-opera[^\n]*\.fw\|2830S[^\n]*2\.sys\)' Documentation/dvb/opera-firmware.txt
    blob 'Getting[ ]the[ ]Firmware\([\n][^\n]\+\)*' Documentation/dvb/ttusb-dec.txt

    blob '[/][*][\n 	]*File[ ]automatically[ ]generated[ ]by[ ]createinit\.py[ ]using[ ]data[\n 	]*extracted[ ]from[ ]AF05BDA\.sys.*[}][;]' drivers/media/dvb/dvb-usb/af9005-script.h
    blob '#include[ ]["]af9005-script\.h["]' drivers/media/dvb/dvb-usb/af9005-fe.c
    blobna '[\n][	]scriptlen[ ]=[ ]sizeof[(]script[)][^;]*[;][\n][	]for[^{]*scriptlen[^{]*[{][^}]*[^\n	}]' drivers/media/dvb/dvb-usb/af9005-fe.c

    accept 'struct[ ]\(sp8870\|tda1004x\)_config[\n][{][^}]*[(][*]request_firmware[)][^}]*[\n][}][;]' 'drivers/media/dvb/frontends/\(sp8870\|tda1004x\)\.h'
    blob '[/][*][^*]*\([*]\+[^/*][^*]*\)*[*]*get_dvb_firmware[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]\([\n]\(#define[ ]\(\([^\n 	]*_DEFAULT\|NONFREE\)_FIRMWARE\|["][^"]*["]\)[ ]\([^\n]\|[\\][\n]\)*\|[/][*][(]DEBLOBBED[)][*][/]\)\)*' 'drivers/media/dvb/frontends/\(nxt200x\|or51211\|sp887[0x]\|tda1004[8x]\)\.c'
    blobname 'dvb-fe-sp8870\.fw' drivers/media/dvb/frontends/sp8870.c
    blobname 'dvb-fe-tda1004[56]\.fw' drivers/media/dvb/frontends/tda1004x.c

    # This bootcode is actually Free Software under GPLv2, but since it's
    # being distributed without source code, we're taking it out.
    blob 'static[ ]u8[ ]bootcode\[\][ ]=[ ][{][^}]*[}][;]' drivers/media/dvb/ttpci/av7110_hw.c
    blobname 'dvb-ttpci-01\.fw' drivers/media/dvb/ttpci/av7110.c
    defsnc 'static[ ]u8[ ]nexusca_stv0297_inittab\[\][ ]=' drivers/media/dvb/ttpci/av7110.c

    defsnc 'static[ ]u8[ ]philips_su1278_tt_inittab\[\][ ]=' drivers/media/dvb/ttpci/budget-ci.c
    defsnc 'static[ ]u8[ ]dvbc_philips_tdm1316l_inittab\[\][ ]=' drivers/media/dvb/ttpci/budget-ci.c

    blobname 'ttusb-budget[/]dspbootcode\.bin' drivers/media/dvb/ttusb-budget/dvb-ttusb-budget.c

    blobname 'cpia2[/]stv0672_vp4\.bin' drivers/media/video/cpia2/cpia2_core.c

    blobname 'dabusb[/]\(firmware\.fw\|bitstream\.bin\)' drivers/media/video/dabusb.c

    blob 'static[ ]u32[ ]tigon2\?Fw\(Text\|Rodata\|Data\)\[[(]MAX_\(TEXT\|RODATA\|DATA\)_LEN[/]4[)][ ][+][ ]1\][ ]__\(dev\)\?initdata[ ]=[ ][{][^}]*[}][;]\([\n]static[ ]u32[ ]tigon2\?Fw\(Text\|Rodata\|Data\)\[[(]MAX_\(TEXT\|RODATA\|DATA\)_LEN[/]4[)][ ][+][ ]1\][ ]__\(dev\)\?initdata[ ]=[ ][{][^}]*[}][;]\)*' drivers/net/acenic_firmware.h
    blob '#define[ ]tigon2\?Fw[^ ]*\(Addr\|Len\)[ ]0x[^\n]*\([\n]#define[ ]tigon2\?Fw[^ ]*\(Addr\|Len\)[ ]0x[^\n]*\)\+' drivers/net/acenic_firmware.h
    blob '\([/][*][^*]*\([*]\+[^/*][^*]*\)*[*]*Do[ ]not[ ]try[ ]to[ ]clear[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/][\n][	]\)\?ace_clear[^;]*[;][\n]\([^}]*[{][^}]*ace_copy[^}]*tigon2\?Fw[^}]*[}]\)*[\n]\+[	]return[ ]0[;][\n][}]' drivers/net/acenic.c
    blob 'if[ ][(]\(ACE_IS_TIGON_I[(]ap[)]\|ap->version[ ]==[ ]2\)[)][\n][	][	]writel[(]tigon2\?FwStartAddr,[ ][&]regs->Pc[)][;]\([\n][	]if[ ][(]\(ACE_IS_TIGON_I[(]ap[)]\|ap->version[ ]==[ ]2\)[)][\n][	][	]writel[(]tigon2\?FwStartAddr,[ ][&]regs->Pc[)][;]\)*' drivers/net/acenic.c

    blob '#include[ ]["]starfire_firmware\.h["]' drivers/net/starfire.c
    blob '[/][*][^*]*\([*]\+[^/*][^*]*\)*[*]*Load[ ]Rx[/]Tx[ ]firmware[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]\([\n][	]for[ ][(][^)]*FIRMWARE_[RT]X_SIZE[^)]*[)][\n][	][	]writel[^;]*firmware_[rt]x[^;]*[;]\)\+' drivers/net/starfire.c

    blob 'static[ ]\(u8\|const[ ]u32\|struct[ ]fw_info\)[ ]bnx2_\(\(COM\|CP\|[RT]XP\|TPAT\)_b0[69]Fw\(Text\|Data\|Rodata\)\|\(xi_\)\?rv2p_proc[12]\|\(com\|cp\|[rt]xp\|tpat\)_fw_0[69]\)\(\[[^]};]*\]\)*[ ]=[ ][{][^}]*[}][;]\([\n][\n]*static[ ]\(u8\|const[ ]u32\|struct[ ]fw_info\)[ ]bnx2_\(\(COM\|CP\|[RT]XP\|TPAT\)_b0[69]Fw\(Text\|Data\|Rodata\)\|\(xi_\)\?rv2p_proc[12]\|\(com\|cp\|[rt]xp\|tpat\)_fw_0[69]\)\(\[[^]};]*\]\)*[ ]=[ ][{][^}]*[}][;]\)*' 'drivers/net/bnx2_fw2\?.h'
    blob '#include[ ]["]bnx2_fw\.h["][\n][\n]*#include[ ]["]bnx2_fw2\.h["]' drivers/net/bnx2.c
    blob 'static[ ]void[\n]load_rv2p_fw[(][^{]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*[\n]\+[}]' drivers/net/bnx2.c
    blob 'static[ ]int[\n]bnx2_init_cpus[(][^{]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*[\n]\+[}]' drivers/net/bnx2.c

    # init_data_e1h? might actually be just data, but it doesn't
    # really matter.
    blob 'static[ ]const[ ]u32[ ]\(init\?\|[tucx]sem_\(int_table\|pram\)\)_data_e1h\?\[\][ ]=[ ][{][^}]*[}][;]\([\n][\n]*static[ ]const[ ]u32[ ]\(init\?\|[tucx]sem_\(int_table\|pram\)\)_data_e1h\?\[\][ ]=[ ][{][^}]*[}][;]\)*' drivers/net/bnx2x_init_values.h
    blob 'static[ ]\(void[ ]\|const[ ]u32[ ][*]\)bnx2x_\(sel_blob\|init_wr_wb\|init_block\)[(][^{]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*[\n]\+[}]\([\n][\n]*static[ ]\(void[ ]\|const[ ]u32[ ][*]\)bnx2x_\(sel_blob\|init_wr_wb\|init_block\)[(][^{]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*[\n]\+[}]\)*' 'drivers/net/bnx2x_init\(_ops\)\?\.h'

    blobname 'sun[/]cassini\.bin' drivers/net/cassini.c

    blobna 'static[ ]u16[ ]\(sr\|twinax\)_edc\[\][ ]=[ ][{][^;]*[}][;]' drivers/net/cxgb3/ael1002.c
    blobna 'for[ ][(][^\n]*ARRAY_SIZE[(]\(sr\|twinax\)_edc[)][^\n]*[)][\n][^;]*mdio_write[^;]*[;]' drivers/net/cxgb3/ael1002.c
    blobname '\(cxgb3[/]\)\?t3\(fw\|\(%c\|.\)_p\(rotocol_\)\?sram\)-\(%d\|[0-9]*\)\.\(%d\|[0-9]*\)\.\(%d\|[0-9]*\)\.bin' drivers/net/cxgb3/cxgb3_main.c

    blob '\([/][*][*]\+[/][\n]*\)*\([/][*][^*]*\([*]\+[^/*][^*]*\)*[*]*Micro[ ]code[^*]*\([*]\+[^/*][^*]*\)*[*]*8086:[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]\([\n]*[/][*][^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]\)*\|#define[ ][ ]*D10\(1M\(_B\)\?\|1S\|2_E\)_\(CPUSAVER_\(TIMER\|BUNDLE\|MIN_SIZE\)_DWORD\|RCVBUNDLE_UCODE\)[ 	][^\n]*\([\\][\n][^\n]*\)*\)\([\n]*[/][*][^*]*\([*]\+\([^/*]\|[/][\n]*[/][*]\+\)[^*]*\)*[*]*Micro[ ]code[^*]*\([*]\+[^/*][^*]*\)*[*]*8086:[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]\([\n]*[/][*][^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]\)*\|[\n][\n]*#define[ ][ ]*D10\(1M\(_B\)\?\|1S\|2_E\)_\(CPUSAVER_\(TIMER\|BUNDLE\|MIN_SIZE\)_DWORD\|RCVBUNDLE_UCODE\)[ 	]\(\\[\n]\|[^\n]\)*\)*' drivers/net/e100.c
    blobna '\([/][*][^*]*\([*]\+[^/*][^*]*\)*[*]\+[/][\n]*[	][	]\)\(ucode\[opts->\(timer\|bundle\|min_size\)_dword\][ ].=[ ][^;]*[;][\n][\n]*[	][	]\)*[^}]*UCODE_SIZE[^}]*cb_ucode[^}]*return[;][\n][	][}]' drivers/net/e100.c

    blob 'static[ ]unsigned[ ]char[ ]__devinitdata[ ]lanai4_\(code\|data\)\[[0-9]*\][ ]=[ ][{][^;]*[}][;]' drivers/net/myri_code.h
    blob '#include[ ]["]myri_code\.h["]' drivers/net/myri_sbus.c
    blobna '\([/][*][^*]*\([*]\+[^/*][^*]*\)*[*]\+[/][\n	 ]*\)\?for[ ][(][^\n]*sizeof[(]lanai4_\(code\|data\)[^\n]*[)][\n][^\n]*sbus_writeb[^;]*lanai4_\(code\|data\)[^;]*lanai4_code_off[^;]*[;]\([\n	 ]*\([/][*][^*]*\([*]\+[^/*][^*]*\)*[*]\+[/][\n	 ]*\)\?for[ ][(][^\n]*sizeof[(]lanai4_\(code\|data\)[^\n]*[)][\n][^\n]*sbus_writeb[^;]*lanai4_\(code\|data\)[^;]*lanai4_\(code\|data\)_off[^;]*[;]\)*' drivers/net/myri_sbus.c

    blob 'static[ ]u32[ ]s_firmLoad\[\][ ]=[ ][{][^;]*[}][;]' drivers/net/tehuti_fw.h
    blobna 'bdx_tx_push_desc_safe[^;]*s_firmLoad[^;]*[;]' drivers/net/tehuti.c
    blobna 'for[ ][(][^\n]*ARRAY_SIZE[(]s_firmLoad[)][^\n]*[)][\n	 ]*s_firmLoad[^;]*=[^;]*s_firmLoad[^;]*[;]' drivers/net/tehuti.c

    blob '[ ][*][ ]Firmware[ ]is:[\n][ ][*][	]Derived[ ]from[ ]proprietary[^/]*notice[ ]is[ ]accompanying[ ]it\.[\n][ ][*][/]' drivers/net/tg3.c
    blobna 'Derived[ ]from[ ]proprietary[ ]unpublished[ ]source[ ]code' drivers/net/tg3.c
    blob '\(static[ ]\)\?\(const[ ]\)\?u32[ ]tg3\(Tso5\?\)\?Fw\(Text\|Rodata\|Data\)\[[^{]*\][ ]=[ ][{][^}]*[}][;]\([\n][\n]*\(static[ ]const[ ]u32[ ]tg3\(Tso5\?\)\?Fw\(Text\|Rodata\|Data\)\[[^{]*\][ ]=[ ][{][^}]*[}][;]\|#if[ ]0\([ ][/][*][^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]\)\?[\n]\(static[ ]const[ ]\)\?u32[ ]tg3\(Tso5\?\)\?Fw\(Text\|Rodata\|Data\)\[[^{]*\][ ]=[ ][{][^}]*[}][;][\n]#endif\)\)*' drivers/net/tg3.c

    blob 'static[ ]const[ ]u8[ ]typhoon_firmware_image\[\][ ]=[ ][{][^}]*[}][;]' drivers/net/typhoon-firmware.h

    blobna 'licensed[^\n]*strictly[ ]for[ ]use[^\n]*[\n]*[^\n]*COPS[ ]LocalTalk' 'drivers/net/appletalk/cops_\(ff\|lt\)drv\.h'
    blob 'static[ ]const[ ]unsigned[ ]char[ ]ffdrv_code\[\][ ]=[ ][{][^}]*[}][;]' drivers/net/appletalk/cops_ffdrv.h
    blob 'static[ ]const[ ]unsgined[ ]char[ ]ltdrv_code\[\][ ]=[ ][{][^}]*[}][;]' drivers/net/appletalk/cops_ltdrv.h
    blob '#include[ ]["]cops_\(lt\|ff\)drv\.h["][ 	]*\([/][*][^*]*\([*]\+[^/*][^*]*\)*[*]*Firmware[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]\)\?\([\n][\n]*#include[ ]["]cops_\(lt\|ff\)drv\.h["][ 	]*\([/][*][^*]*\([*]\+[^/*][^*]*\)*[*]*Firmware[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]\)\?\)*' drivers/net/appletalk/cops.c

    blob 'static[ ]unsigned[ ]char[ ]bits_1200\[\][ ]*=[ ][{][^}]*[}][;]' drivers/net/hamradio/yam1200.h
    blob 'static[ ]unsigned[ ]char[ ]bits_9600\[\][ ]*=[ ][{][^}]*[}][;]' drivers/net/hamradio/yam9600.h
    blob '#include[ ]["]yam\(96\|12\)00\.h["]\([\n][\n]*#include[ ]["]yam\(96\|12\)00\.h["]\)*' drivers/net/hamradio/yam.c

    blobna 'static[ ]const[ ]u_char[ ]__Xilinx7OD\[\][ ]=[ ][{][^}]*[}][;]' drivers/net/pcmcia/ositech.h
    blob '#include[ ]["]ositech\.h["]' drivers/net/pcmcia/smc91c92_cs.c
    blobna '\([/][*][ ]Download[ ]the[ ]Seven[ ]of[ ]Diamonds[ ]firmware[^/]*[*][/][\n	 ]*\)\?for[ ]*[(][^\n]*__Xilinx7OD[^{}]*[{][\n][	 ]*outb[ ]*[(]__Xilinx7OD[^}]*[}]' drivers/net/pcmcia/smc91c92_cs.c

    blob 'static[ ]const[ ]u8[ ]microcode\[\][ ]=[ ][{][^}]*[}][ ]*[;]' drivers/net/tokenring/3c359_microcode.h
    blob '#include[ ]["]3c359_microcode\.h["]' drivers/net/tokenring/3c359.c
    blobna 'start[ ]=[ ][(]0xFFFF[ ]-[ ][(]mc_size[)][^;]*[;][\n 	]*[/][*][^*]*\([*]\+[^/*][^*]*\)*[*]\+[/][\n 	]*printk[(]KERN_INFO[ ]["]3C359:[ ]Uploading[ ]Microcode:[ ]["][)][;][\n 	]*for[ ][(][^{]*\(mc_size[^{]*[)][ ][{][^}]*writeb[(]microcode\[\|[)][ ][{][^}]*writeb[(]microcode\[mc_size\)[^}]*[}]\([\n][ 	]*printk[^\n]*[;][\n 	]*for[ ][(][^{]*\(mc_size[^{]*[)][ ][{][^}]*writeb[(]microcode\[\|[)][ ][{][^}]*writeb[(]microcode\[mc_size\)[^}]*[}]\)*' drivers/net/tokenring/3c359.c

    blobname 'tr_smctr\.bin' drivers/net/tokenring/smctr.c

    blobname 'kaweth[/]\(new\|trigger\)_code\(_fix\)\?\.bin' drivers/net/usb/kaweth.c


    blobname '\(agere\|prism\)_\(sta\|ap\)_fw\.bin' 'drivers/net/wireless/\(orinico/\)\?\(orinoco\|fw\)\.c'
    blobname 'symbol_sp24t_\(prim\|sec\)_fw' 'drivers/net/wireless/\(\(orinico/\)\?orinoco\.c\|spectrum_cs\.c\)'

    blob 'unsigned[ ]short[ ]sbus_risc_code01\[\][ ]__devinitdata[ ]=[ ][{][^}]*[}][;]' drivers/scsi/qlogicpti_asm.c
    blob '#include[ ]["]qlogicpti_asm\.c["]' drivers/scsi/qlogicpti.c

    blob '\([/][*][ ]Microcode[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/][\n]*\)\?static[ ]\(u\(nsigned[ ]\)\?char\|unsigned[ ]short\|ADV_DCNT\)[ ]_\(asc_mcode\|adv_asc3\(550\|8C\(08\|16\)00\)\)_\(buf\[\][ ]=[ ][{][^}]*[}]\|size[ ]=[ ]sizeof[^;]*\|chksum[ ]=[ ]0x[^;]*\)[;]\([ 	]*[/][*][^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]\)\?\([\n][\n]*\([/][*][ ]Microcode[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/][\n]*\)\?static[ ]\(u\(nsigned[ ]\)\?char\|unsigned[ ]short\|ADV_DCNT\)[ ]_\(asc_mcode\|adv_asc3\(550\|8C\(08\|16\)00\)\)_\(buf\[\][ ]=[ ][{][^}]*[}]\|size[ ]=[ ]sizeof[^;]*\|chksum[ ]=[ ]0x[^;]*\)[;]\([ 	]*[/][*][^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]\)\?\)*' drivers/scsi/advansys.c

    blob '\(#ifdef[ ]UNIQUE_FW_NAME[\n]\)\?static[ ]unsigned[ ]short[ ]\(risc\|fw12\(80e\|160\)i\)_code01\[\][ ]=[ ][{]\([\n]#else[\n]static[ ]unsigned[ ]short[ ]risc_code01\[\][ ]=[ ][{][\n]#endif[\n]\)\?[^}]*[}][;]\([\n][\n]*\(#ifdef[ ]UNIQUE_FW_NAME[\n]\)\?static[ ]unsigned[ ]short[ ]\(risc_code\|fw12\(80e\|160\)i\)_length01[ ]=[ ][^;]*[;]\([\n]#else[\n]static[ ]unsigned[ ]short[ ]risc_code_length01[ ]=[ ][^;]*[;][\n]#endif\)\?\)\?' 'drivers/scsi/ql1\(04\|2\(8\|16\)\)0_fw\.h'

    blobname 'emi26[/]\(bitstream\|firmware\|loader\)\.fw' drivers/usb/misc/emi26.c

    blobname 'emi62[/]\(bitstream\|midi\|spdif\|loader\)\.fw' drivers/usb/misc/emi62.c

    blobname 'keyspan[/]\(mpr\|usa\(18x\|19\(q[iw]\|w\)\?\|28\(x\(a\|b\)\?\)\?\|49w\(lc\)\?\)\)\.fw' drivers/usb/serial/keyspan.c

    accept '[	][	]fw_name[ ]=[ ]["]keyspan_pda[/]\(keyspan_pda\|xircom_pgs\)\.fw["][;]' drivers/usb/serial/keyspan_pda.c
    blobna 'fw_name[ ]=[ ][^\n]*\([\n]\+[^\n}][^\n]*\)*\([/][*]KEYSPAN_PDA[*][/]\)\?request_ihex_firmware' drivers/usb/serial/keyspan_pda.c
    accept '[	]if[ ][(][/][*]KEYSPAN_PDA[*][/]request_ihex_firmware' drivers/usb/serial/keyspan_pda.c

    blobname 'edgeport[/]\(boot\|down\)2\?\.fw' drivers/usb/serial/io_edgeport.c
    blobname 'edgeport[/]down3\.bin' drivers/usb/serial/io_ti.c

    blobname 'ti_\(usb-\)\?\(%d\|3410\|5052\)\.\(fw\|bin\)' drivers/usb/serial/ti_usb_3410_5052.c

    blobname 'whiteheat\(_loader\(_debug\)\?\)\?\.fw' drivers/usb/serial/whiteheat.c

    blob 'static[ ]struct[ ]BA1struct[ ]BA1Struct[ ]=[ ][{][^;]*[}][;]' sound/pci/cs46xx/cs46xx_image.h

    blob 'static[ ]u32[ ]cwc\(4630\|async\|snoop\)_\(code\|parameter\)\[\][ ]=[ ][{][^;]*[}][;]' 'sound/pci/cs46xx/imgs/cwc\(4630\|async\|snoop\)\.h'
    # cwcbinhack appears to have been created by hand.
    # cwcdma has sources (not verified) in cwcdma.asp.
    accept 'static[ ]u32[ ]cwc\(binhack\|dma\)_code\[\][ ]=[ ][{][^;]*[}][;]' 'sound/pci/cs46xx/imgs/cwc\(binhack\|dma\)\.h'
    blob '#include[ ]["]\(cs46xx_image\|imgs[/]cwc\(4630\|async\|snoop\)\)\.h["]\([\n][\n]*#include[ ]["]\(cs46xx_image\|imgs[/]cwc\(4630\|async\|snoop\)\)\.h["]\)*' sound/pci/cs46xx/cs46xx_lib.c

    blobname 'korg[/]k1212\.dsp' sound/pci/korg1212/korg1212.c

    blobname 'ess[/]maestro3_assp_\(kernel\|minisrc\)\.fw' sound/pci/maestro3.c

    blobname 'yamaha[/]ds1e\?_\(ctrl\|dsp\)\.fw' sound/pci/ymfpci/ymfpci_main.c

    blobname 'sb16[/]\(\(a\|mu\)law_main\|ima_adpcm_\(init\|capture\|playback\)\)\.csp' sound/isa/sb/sb16_dsp.c

    blob 'static[ ]const[ ]struct[ ][{][^}]*[}][ ]yss225_registers\[\][ ]__devinitdata[ ]=[ ][{][^;]*[}][;]' sound/isa/wavefront/yss225.c
    blobname 'yamaha[/]yss225_registers\.bin' sound/isa/wavefront/wavefront_fx.c
    blobna 'firmware[ ]=[ ][&]yss225_registers_firmware[;]' sound/isa/wavefront/wavefront_fx.c
    blob 'static[ ]const[ ]struct[ ]firmware[ ]yss225_registers_firmware[ ]=[ ][{][^;]*[}][;]' sound/isa/wavefront/wavefront_fx.c
    blobna '\(ospath[	 ]*-[ ]Pathname[^\n]*ICS2115[^-]*wavefront\.os\|Note:[ ]the[ ]firmware[ ]file[ ]["]wavefront\.os["]\)[^-]*[/]lib[/]firmware\.\([^.]*after[ ]upgrading[ ]the[ ]kernel\)\?' Documentation/sound/alsa/ALSA-Configuration.txt
    blobname 'wavefront\.os' sound/isa/wavefront/wavefront_synth.c

    blobna 'and[\n]require[ ]the[ ]use[ ]of[^\n]*propr\?ietary[^:]*' Documentation/arm/IXP4xx
    blob 'If[ ]you[ ]need[ ]to[ ]use[ ]any[ ]of[ ]the[ ]above[^\n]*download[^:]*:[\n 	]*http:[^\n]*ixp4[^\n]*' Documentation/arm/IXP4xx

    blobname 'xc\(%d\|[0-9]*\)\.bin' arch/arm/mach-netx/include/mach/xc.h
    accept 'int[ ]xc_request_firmware[(]struct[ ]xc[ ]*[*][ ]*x[)][;]' arch/arm/mach-netx/include/mach/xc.h
    accept 'int[ ]xc_request_firmware[(]struct[ ]xc[ ]*[*][ ]*x[)][\n][{]' arch/arm/mach-netx/xc.c
    accept '[	][	]dev_err[(]x->dev,[ ]["]request_firmware[ ]failed\\n["][)][;]' arch/arm/mach-netx/xc.c
    accept 'EXPORT_SYMBOL[(]xc_request_firmware[)][;]' arch/arm/mach-netx/xc.c
    accept '[	][	]if[ ][(]xc_request_firmware[(]priv->xc[)][)][ ][{]' drivers/net/netx-eth.c

    blobname 'iop_fw_load_[sm]pu' arch/cris/arch-v32/drivers/iop_fw_load.c
    accept 'int[ ]iop_fw_load_[sm]pu[(]' arch/cris/arch-v32/drivers/iop_fw_load.c
    accept '[	]retval[ ]=[ ]request_firmware[^;]*[&]iop_[sm]pu_device' arch/cris/arch-v32/drivers/iop_fw_load.c
    accept 'EXPORT_SYMBOL[(]iop_fw_load_[sm]pu[)][;]' arch/cris/arch-v32/drivers/iop_fw_load.c

    accept '[/][*][ ]fake[ ]device[ ]for[ ]request_firmware[ ][*][/]' arch/x86/kernel/microcode_core.c

    blobname 'amd-ucode[/]microcode_amd\.bin' arch/x86/kernel/microcode_amd.c

    blobname 'intel-ucode[/]\([0-9a-f][0-9a-f]\|%02x\)-\([0-9a-f][0-9a-f]\|%02x\)-\([0-9a-f][0-9a-f]\|%02x\)' 'arch/x86/kernel/microcode\(_intel\)\?\.c'

    blobname 'BCM2033-\(MD\.hex\|FW\.bin\)' drivers/bluetooth/bcm203x.c

    blobname 'bfubase\.frm' drivers/bluetooth/bfusb.c

    blobname 'BT3CPCC\.bin' drivers/bluetooth/bt3c_cs.c

    blobname 'cyzfirm\.bin' drivers/char/cyclades.c

    accept 'MODULE_FIRMWARE[(]["]dsp56k[/]bootstrap\.bin["][)][;]' drivers/char/dsp56k.c
    blobna 'const[ ]char[ ]fw_name\[\][ ]=[ ]["]dsp56k[/]bootstrap\.bin["][;][^\n]*\([\n]\+[^\n}][^\n]*\)*request_firmware[^\n]*\([\n]\+[^\n}][^\n]*\)*[\n]\+[	]err[ ]=[ ]request_firmware[(][&]fw,[ ]fw_name,[ ]' drivers/char/dsp56k.c
    accept '[	]const[ ]char[ ]fw_name\[\][ ]=[ ]["]dsp56k[/]bootstrap\.bin["][;][^\n]*\([\n]\+[^\n}][^\n]*\)*[\n]\+[	]err[ ]=[ ]request_firmware[(][&]fw,[ ]fw_name,[ ]' drivers/char/dsp56k.c

    blobname 'isi\(6\(08\|\(08\|16\)em\)\|46\(08\|16\)\)\.bin' drivers/char/isicom.c

    blobname 'c\(218t\|p204\|320t\)unx\.cod' drivers/char/moxa.c
    accept '[	][	]printk[(]KERN_ERR[ ]["]MOXA:[ ]request_firmware[ ]failed' drivers/char/moxa.c

    # This driver enables the user to update the non-Free BIOS, but it
    # only issues a firmware request if specifically told to.  It
    # doesn't require any non-Free firmware to function, and it
    # doesn't actually recommend users to perform updates, so I'm
    # leaving it in.
    accept '[	][	][	]req_firm_rc[ ]=[ ]request_firmware_nowait[(][^;]*,[ ]["]dell_rbu["],' drivers/firmware/dell_rbu.c
    accept '[	]*["]dell_rbu:%s[ ]request_firmware_nowait["]' drivers/firmware/dell_rbu.c

    blobname 'xc3028-v27\.fw' drivers/media/common/tuners/tuner-xc2028.h
    blobname 'xc3028L-v36\.fw' drivers/media/common/tuners/tuner-xc2028.h

    blobname 'dvb-fe-xc5000-1\.1\.fw' drivers/media/common/tuners/xc5000.c

    blobname '4210\(100[12]\|%4X\)\.sb' drivers/net/irda/irda-usb.c
    blobna '[/][*][ 	\n*]*[ ]Known[ ]firmware[^*]*\([*]\+[^/*][^*]*\)*[*]*\(STIR421x\|4210\(100[12]\|%4X\)\.sb\)[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]' drivers/net/irda/irda-usb.c

    blobname 'myri10ge_\(rss_\)\?ethp\?_z8e\.dat' drivers/net/myri10ge.c
    blobna 'If[ ]the[ ]driver[ ]can[ ]neither[ ]enable[ ]ECRC[^*]*\([*]\+[^/*][^*]*\)*[*]*myri10ge_\(rss_\)\?ethp\?_z8e\.dat[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]' drivers/net/myri10ge.c

    blobname 'spider_fw\.bin' drivers/net/spider_net.h

    blobname 'tms380tr\.bin' drivers/net/tokenring/tms380tr.c

    blobname 'atmel_at76c50\(2\([de]\|_3com\)\?\|4a\?\(_2958\)\?\|6\)\(\.bin\)\?' drivers/net/wireless/atmel.c
    accept '[	]*priv->firmware[ ]=[ ]\(NULL\|new_firmware\)[;]' drivers/net/wireless/atmel.c

    blobname 'b43\(legacy\)\?\(%s\)\?[/]\(%s\|ucode\([2459]\|1[1345]\)\|pcm5\|[abn]0g[01]initvals\(5\|1[13]\)\)\.fw' 'drivers/net/wireless/b43\(legacy\)\?/main.c'
    blobname 'pcm5\.fw' drivers/net/wireless/b43/main.c
    blobna 'b43legacyerr[(][^;]*must[ ]go[ ]to[ ]http[^;]*b43#devicefirmware[^;]*[)][;]' drivers/net/wireless/b43legacy/main.c
    blobna 'You[ ]must[ ]go[ ]to[^;]*b43#devicefirmware[^;]*[^";)]' drivers/net/wireless/b43/main.c
    blobna 'http:[/][/]wireless[^ ";)]*b43#devicefirmware' drivers/net/wireless/b43/main.c

    blob '#define[ ]IPW2100_FW_\(\(\(MAJOR\|MINOR\)_VERSION\|\(MAJOR\|MINOR\)[(]x[)]\)\|VERSION\)\([^\n]*\\[\n]\)*[^\n]*\([\n][\n]*#define[ ]IPW2100_FW_\(\(\(MAJOR\|MINOR\)_VERSION\|\(MAJOR\|MINOR\)[(]x[)]\)\|VERSION\)\([^\n]*\\[\n]\)*[^\n]*\)*' 'drivers/net/wireless/\(ipw2x00/\)\?ipw2100\.c'
    blobname 'ipw2100-\(["]\([^"\n]\|[\\][\n]\)*["]\([^"]\|[\\]["]\)*\)\+' 'drivers/net/wireless/\(ipw2x00/\)\?ipw2100\.c'
    blobname '__stringify[(]IPW2100_FW_MINOR_VERSION[)]' 'drivers/net/wireless/\(ipw2x00/\)\?ipw2100\.c'
    accept '[ ]*Portions[ ]of[ ]ipw2100_\(do_\)\?mod_firmware_load[, 	]*\(ipw2100_\(do_\)\?mod_firmware_load[, 	and\n]*\)*' 'drivers/net/wireless/\(ipw2x00/\)\?ipw2100\.c'
    accept '[	]ipw2100_mod_firmware_load[(]fw[)][;]' 'drivers/net/wireless/\(ipw2x00/\)\?ipw2100\.c'
    accept 'static[ ]int[ ]ipw2100_mod_firmware_load[(]' 'drivers/net/wireless/\(ipw2x00/\)\?ipw2100\.c'
    blobna 'if[ ][(]IPW2100_FW_MAJOR[^{]*[{][^}]*[	][}]' 'drivers/net/wireless/\(ipw2x00/\)\?ipw2100\.c'
    blobname '["]["][ ]x[ ]["]\.fw["]' 'drivers/net/wireless/\(ipw2x00/\)\?ipw2100\.c'

    accept '[/][*][ ]Call[ ]this[ ]function[ ]from[ ]process[ ]context[^*]*\([*]\+[^/*][^*]*\)*[*]*request_firmware' 'drivers/net/wireless/\(ipw2x00/\)\?ipw2200.c'
    blobname 'ipw2200-\(i\?bss\|sniffer\)\.fw' 'drivers/net/wireless/\(ipw2x00/\)\?ipw2200.c'
    accept '[	][	]IPW_ERROR[(]["]%s[ ]request_firmware[ ]failed' 'drivers/net/wireless/\(ipw2x00/\)\?ipw2200.c'

    blobname 'iwlwifi-\(3945\|4965\|[156]000\(G2[AB]\)\?\|1[03]0\|6050\)["][ ]IWL\(3945\|4965\|[156]000\(G2[AB]\)\?\|1[03]0\|6050\)_UCODE_API[ ]["]\.ucode' 'drivers/net/iwlwifi/iwl\(3945-base\|-\(3945\|4965\|[156]000\)\)\.[ch]'
    blobname 'iwlwifi-3945-' drivers/net/iwlwifi/iwl-3945.h
    blobname '#api[ ]["]\.ucode["]' 'drivers/net/iwlwifi/iwl-\(3945.h\|\(4965\|[156]000\)\.c\)'
    accept '#define\([ ]_\?IWL3945_MODULE_FIRMWARE[(]api[)]\)\+' drivers/net/iwlwifi/iwl-3945.h
    accept '[	][ ][*][ ]request_firmware[(][)][ ]is[ ]synchronous' 'drivers/net/iwlwifi/iwl\(3945-base\|-agn\)\.c'
    blobname 'iwlwifi-4965-' drivers/net/iwlwifi/iwl-4965.c
    blobname 'iwlwifi-5\(00\|15\)0-' drivers/net/iwlwifi/iwl-5000.c
    blobname '%s%[dus]%s["],[\n 	]*name_pre,[ ]\(\(priv->fw_\)\?index\|tag\|idx\),[ ]["]\.ucode' 'drivers/net/iwlwifi/iwl\(3945-base\|-agn\).c'

    blobname 'libertas_cs\(_helper\)\?\.fw' drivers/net/wireless/libertas/if_cs.c
    blobname 'sd\(8385\|868[68]\)\(_helper\)\?\.bin\(["],[\n][	]*\.firmware[ 	]=[ ]["]sd\(8385\|868[68]\)\.bin\)\?' 'drivers/\(net/wireless/libertas/if_sdio\.c\|bluetooth/btmrvl_sdio\.c\)'
    blobname 'sd\(8385\|868[68]\)\(_helper\)\?\.bin' 'drivers/\(net/wireless/libertas/if_sdio\.c\|bluetooth/btmrvl_sdio\.c\)'
    accept '[	]*card->firmware[ ]=[ ]\(if_sdio\|lbs_fw\|fw_name\)' drivers/net/wireless/libertas/if_sdio.c
    blobname 'usb8388\(-5\.126\.0\.p5\)\?\.bin' drivers/net/wireless/libertas/if_usb.c
    blob '[/][*][^*]*\([*]\+[^/*][^*]*\)*[*]*usb8388\(-5\.126\.0\.p5\)\?\.bin[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]' drivers/net/wireless/libertas/if_usb.c
    accept '[	][	]lbs_pr_err[(]["]request_firmware\([(][)]\)\?[ ]failed' 'drivers/net/wireless/if_\(spi\|usb\)\.c'
    blobna 'o\.[ ]Copy[ ]the[ ]firmware[ ]image[^\n]*usb8388\([^\n]\|[\n][ 	]*[^ 	\n]\)*' drivers/net/wireless/libertas/README
    blobna '\[fw_name=usb8388[^]]*\]' drivers/net/wireless/libertas/README

    blobname 'usb8388\.bin' drivers/base/Kconfig
    accept '[	][ ][ ]So,[ ]for[ ]example,[ ]you[ ]might[ ]set[ ]CONFIG_EXTRA_FIRMWARE=["]whatever\.bin["]' drivers/base/Kconfig
    accept '[	][ ][ ]kernel\.[ ]Then[ ]any[ ]request_firmware[(]\(["]whatever\.bin["]\)[)]' drivers/base/Kconfig

    blobname 'lbtf_usb\.bin' drivers/net/wireless/libertas_tf/if_usb.c

    blobname 'isl38\(86\|87\|90\)\(pci\|usb\(_bare\)\?\)\?' 'drivers/net/wireless/p54/p54\(pci\.c\|usb\.[ch]\)'
    blob '[/][*][ ]for[ ]isl3886[ ]register[ ]definitions[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]' drivers/net/wireless/p54/p54usb.h
    blobna 'If[ ]you[ ]enable[ ]this\([^\n]\|[\n][ 	]*[^ 	\n]\)*isl3890\([^\n]\|[\n][ 	]*[^ 	\n]\)*' drivers/net/wireless/Kconfig

    blobname 'isl38\(77\|86\|90\)' drivers/net/wireless/prism54/islpci_dev.c

    blobname 'rt2[56]61s\?\.bin' drivers/net/wireless/rt2x00/rt61pci.h
    blobname 'rt73\.bin' drivers/net/wireless/rt2x00/rt73usb.h

    blobname 'zd1201\(-ap\)\?\.fw' drivers/net/wireless/zd1201.c

    blobname 'zd1211[/]zd1211b\?_\(u\([rb]\|phr\)\?\)\?' drivers/net/wireless/zd1211/zd_usb.c

    # ??? gotta introduce some means to match false-positives
    # including post context containing blobs, so that the macro name
    # is not flagged or deblobbed, but the blob name is.
    # blobna 'PCMCIA_\([PM]FC_\)\?DEVICE_CIS_\(MANF_CARD\|PROD_ID[1-4]*\)'
    # accept '[	]    PCMCIA_\([PM]FC_\)\?DEVICE_CIS_\(MANF_CARD\|PROD_ID[1-4]*\)[(][^)]*, ["][/][*][(]DEBLOBBED[)][*][/]["][)]'
    # accept '#define PCMCIA_\([PM]FC_\)\?DEVICE_CIS_\(MANF_CARD\|PROD_ID[1-4]*\)[(]' include/pcmcia/device_id.h

    # These are not software; they're Free, but GPLed without in-tree sources.
    # blobname '\(cis[/]\)\?3CCFEM556\.cis' drivers/net/pcmcia/3c574_cs.c
    # blobname '\(cis[/]\)\?3CXEM556\.cis' drivers/net/pcmcia/3c589_cs.c
    # blobname '\(cis[/]\)\?\(PCMLM28\|DP83903\|LA-PCM\|PE520\|NE2K\|PE-200\|tamarack\)\.cis' drivers/net/pcmcia/pcnet_cs.c
    # blobname '\(cis[/]\)\?\(PCMLM28\|DP83903\|3C\(CF\|X\)EM556\|MT5634ZLX\|COMpad[24]\|RS-COM-2P\|GLOBETROTTER\)\.cis' drivers/serial/serial_cs.c
    # These are not software; they're Free, but GPLed without textual sources.
    # It is safe to assume that these binaries *are* sources, since they
    # can be trivially converted back to a textual form, without loss.
    # blobname '\(cis[/]\)\?SW_\([78]xx\|555\)_SER\.cis' drivers/serial/serial_cs.c

    accept '[	]\(ds_\)\?\(dev_\)\?dbg[(]\(1[,][ ]\)\?\([&]dev->dev,[ ]\)\?["]trying[ ]to[ ]load[ ]\(CIS[ ]file\|firmware\)[ ]%s[\\]n["],[ ]filename[)][;][\n]*[	]if[ ][(]\(strlen[(]filename[)][^\n]*\([{][^}]*[	][}]\|[)][\n][	]*return[^\n]*[;]\)[\n]*[	]snprintf[(]path,[ ]\(20\|sizeof[(]path[)]\),[^\n]*,[ ]filename[)][;][\n]*[	]if[ ][(]request_firmware[(][&]fw,[ ]path\|request_firmware[(][&]fw,[ ]filename\),[ ][&]dev->dev[)][^\n]*[)][ ][{][\n][	]*if[ ][(]fw->size[ ]>=[ ]CISTPL_MAX_CIS_SIZE[)]' drivers/pcmcia/ds.c
    accept 'MODULE_FIRMWARE[(]["]\(cis[/]\)\?\(PCMLM28\|DP83903\|3C\(CF\|X\)EM556\|MT5634ZLX\|COMpad[24]\|RS-COM-2P\|GLOBETROTTER\|SW_\([78]xx\|555\)_SER\)\.cis["][)][;]\([\n]MODULE_FIRMWARE[(]["]\(cis[/]\)\?\(PCMLM28\|DP83903\|3C\(CF\|X\)EM556\|MT5634ZLX\|COMpad[24]\|RS-COM-2P\|GLOBETROTTER\|SW_\([78]xx\|555\)_SER\)\.cis["][)][;]\)*' drivers/serial/serial_cs.c
    accept 'MODULE_FIRMWARE[(]["]\(cis[/]\)\?\(PCMLM28\|DP83903\|LA-PCM\|PE520\|NE2K\|PE-200\|tamarack\)\.cis["][)][;]\([\n]MODULE_FIRMWARE[(]["]\(cis[/]\)\?\(PCMLM28\|DP83903\|LA-PCM\|PE520\|NE2K\|PE-200\|tamarack\)\.cis["][)][;]\)*' drivers/net/pcnet_cs.c

    # This enables but does not encourage firmware updates.
    accept '[	]err[ ]=[ ]request_firmware[(][&]asd_ha->bios_image,[\n 	]*filename_ptr,[\n 	]*[&]asd_ha->pcidev->dev[)][;]' drivers/scsi/aic94xx/aic94xx_init.c
    blobname 'aic94xx-seq\.fw' drivers/scsi/aic94xx/aic94xx_seq.h

    # This enables but does not encourage firmware updates.
    accept '[	]if[(]request_firmware[(]&fw_entry,[ ]fname,[ ]&ioa_cfg->pdev->dev[)][)]' drivers/scsi/ipr.c

    accept '[	]res[ ]=[ ]request_firmware[(]&fw,[ ]["]sas_addr["],[ ]&shost->shost_gendev[)][;]' drivers/scsi/libsas/sas_scsi_host.c

    blobname 'ql\(2\([12345]00\|322\)\|8[12]00\)_fw\.bin' drivers/scsi/qla2xxx/qla_os.c
    blobna 'By[ ]default,[ ]firmware[ ]for[ ]the[ ]ISP[ ]parts\([^\n]\|[\n]*[	]\)*ql2[12345]00_fw\.bin\([^\n]\|[\n]*[	]\)*ftp:[/][/][^\n]*firmware[/]\(.*linux-firmware[ ]tree[ ]as[ ]well\.\)\?' drivers/scsi/qla2xxx/Kconfig

    blobname 'icom_\(asc\|res_dce\|call_setup\)\.bin' drivers/serial/icom.c

    blobname 'fsl_qe_ucode_uart_\(%u\|[0-9]*\)_\(%u\|[0-9]*\)\(%u\|[0-9]*\)\.bin' drivers/serial/ucc_uart.c

    blobname 'atmel_at76c50\(3-\(i386[13]\|rfmd\(-acc\)\?\)\|5\(a\(mx\)\?\)\?-rfmd\(2958\)\?\)\.bin' 'drivers/\(\(staging\|net/wireless\)/at76_usb/at76_usb\.c\|at76c50x-usb\.c\)'

    accept 'static[ ]struct[ ]go7007_usb_board[ ]board_\(matrix_\(ii\|reload\|revolution\)\|star_trek\|px_tv402u\|xmen\|lifeview_lr192\|endura\|adlink_mpg24\|sensoray_2250\)[ ]=[ ][{][\n]\([	]\.flags[ 	]*=[ ][^",]*,[\n]*\)*[	]\.main_info[ 	]*=[ ][{][\n][	][	]\.firmware[ 	]*=[ ]' drivers/staging/go7007/go7007-usb.c
    accept 'static[ ]struct[ ]go7007_board_info[ ]board_voyager[ ]=[ ][{][\n][	]\.firmware[	 ]*=[ ]' drivers/staging/go7007/saa7134-go7007.c
    blobname 'go7007\(fw\|tv\)\.bin' 'drivers/staging/go7007/\(go7007-\(driver\|usb\)\|saa7134-go7007\)\.c'

    blobname 'cxacru-\(%s\|fw\|bp\|cf\)\.bin' drivers/usb/atm/cxacru.c

    blobname 'speedtch-\(%d\|[0-9]*\)\.bin\(\.\(%x\|\(0x\)\?[0-9a-fA-F]*\)\(\.\(%02x\|[0-9a-fA-F][0-9a-fA-F]\)\)\?\)\?' drivers/usb/atm/speedtch.c

    blobname 'ueagle-atm[/]' drivers/usb/atm/ueagle-atm.c
    blobname '\(adi930\|eagle\(I*\|IV\)\)\.fw' drivers/usb/atm/ueagle-atm.c
    blobname 'DSP[49e][ip]\.bin' drivers/usb/atm/ueagle-atm.c
    blobname '930-fpga\.bin' drivers/usb/atm/ueagle-atm.c
    blobname 'CMV[x9ae][yip]\.bin\(\.v2\)\?' drivers/usb/atm/ueagle-atm.c

    blobname 'isight\.fw' drivers/usb/misc/isight_firmware.c

    blobname '\(i1480-\(pre-phy\|usb\|phy\)\|ptc\)-0\.0\.bin' drivers/uwb/i1480/dfu/usb.c

    accept '[	]retval[ ]=[ ]request_firmware[(][&]fw_entry,[ ]["]metronome\.wbf["],[ ][&]dev->dev[)][;]' drivers/video/metronomefb.c

    blobname '\(vx[/]\)\?\(bx_1_v\(xp\|p4\)\.b56\|x1_\(1_v\(x[2p]\|p4\)\|2_v22\)\.xlx\|bd56\(002\|3v2\|3s3\)\.boot\|l_1_v\(x[2p]\|p4\|22\)\.d56\)' sound/drivers/vx/vx_hwdep.c

    blobname '\(ea[/]\)\?darla20_dsp\.fw' sound/pci/echoaudio/darla20.c
    blobname '\(ea[/]\)\?darla24_dsp\.fw' sound/pci/echoaudio/darla24.c
    blobname '\(ea[/]\)\?\(\(loader\|echo3g\)_dsp\|3g_asic\)\.fw' sound/pci/echoaudio/echo3g.c
    blobname '\(ea[/]\)\?gina20_dsp\.fw' sound/pci/echoaudio/gina20.c
    blobname '\(ea[/]\)\?\(\(loader\|gina24_3[06]1\)_dsp\|gina24_3[06]1_asic\)\.fw' sound/pci/echoaudio/gina24.c
    blobname '\(ea[/]\)\?\(loader\|indigo\)_dsp\.fw' sound/pci/echoaudio/indigo.c
    blobname '\(ea[/]\)\?\(loader\|indigo_dj\)_dsp\.fw' sound/pci/echoaudio/indigodj.c
    blobname '\(ea[/]\)\?\(loader\|indigo_io\)_dsp\.fw' sound/pci/echoaudio/indigoio.c
    blobname '\(ea[/]\)\?layla20_\(dsp\|asic\)\.fw' sound/pci/echoaudio/layla20.c
    blobname '\(ea[/]\)\?\(\(loader\|layla24\)_dsp\|layla24_\(1\|2[AS]\)_asic\)\.fw' sound/pci/echoaudio/layla24.c
    blobname '\(ea[/]\)\?\(loader\|mia\)_dsp\.fw' sound/pci/echoaudio/mia.c
    blobname '\(ea[/]\)\?\(\(loader\|mona_3[06]1\)_dsp\|mona_3[06]1\(_1\)\?_asic_\(48\|96\)\|mona_2_asic\)\.fw' sound/pci/echoaudio/gina24.mona
    blobname 'ea[/]%s' sound/pci/echoaudio/echoaudio.c

    blobname 'emu[/]\(hana\|\(audio\|micro\)_dock\|emu\(0404\|1010\(b\|_notebook\)\)\)\.fw' sound/pci/emu10k1/emu10k1_main.c

    blobname '\(mixart[/]\)\?miXart8\(AES\)\?\.\(xlx\|elf\)' sound/pci/mixart/mixart_hwdep.c

    blobname '\(pcxhr[/]\)\?\(x[ic]_1_882\|[ebd]321_512\|xlxint\|\(xlxc\|dsp[ebd]\)\(882\|1\?222\|924\)\(e\|hr\)\?\)\(\.dat\|\.[ebd]56\)' sound/pci/pcxhr/pcxhr_hwdep.c

    blobna 'You[ ]need[ ]to[ ]install[\n]*riptide\.hex[\n]\.[\n]' Documentation/sound/alsa/ALSA-Configuration.txt
    blobname 'riptide\.hex' sound/pci/riptide/riptide.c
    defsnc 'static[ ]union[ ]firmware_version[ ]firmware_versions\[\][ ]=' sound/pci/riptide/riptide.c
    blobna 'chip->firmware[ ]=[ ]firmware[;]' sound/pci/riptide/riptide.c

    blobname '\(multi\|digi\)face_firmware\(_rev11\)\?\.bin' sound/pci/rme9652/hdsp.c

    accept '[ ][*][^*]*\([*]\+[^/*][^*]*\)*[*]*Caution:[ ]This[ ]API[^*]*\([*]\+[^/*][^*]*\)*[*]*request_firmware.' sound/sound_firmware.c
    accept 'static[ ]int[ ]do_mod_firmware_load[(]' sound/sound_firmware.c
    accept 'int[ ]mod_firmware_load[(]' sound/sound_firmware.c
    accept '[	]r[ ]=[ ]do_mod_firmware_load[(]' sound/sound_firmware.c
    accept 'EXPORT_SYMBOL[(]mod_firmware_load[)][;]' sound/sound_firmware.c
    accept 'extern[ ]int[ ]mod_firmware_load[(]' sound/oss/sound_firmware.h

    accept '[	]INITCODESIZE[ ]=[ ]mod_firmware_load[(]INITCODEFILE,[ ][&]INITCODE[)][;]' sound/oss/msnd_pinnacle.c
    accept '[	]PERMCODESIZE[ ]=[ ]mod_firmware_load[(]PERMCODEFILE,[ ][&]PERMCODE[)][;]' sound/oss/msnd_pinnacle.c
    blobname '\([/]etc[/]sound[/]\|turtlebeach[/]\)\?pndsp\(ini\|erm\)\.bin' '\(sound/oss/msnd_pinnacle.h\|Documentation/sound/alsa/ALSA-Configuration.txt\)'
    blobname '\([/]etc[/]sound[/]\|turtlebeach[/]\)\?msnd\(init\|perm\)\.bin' '\(sound/oss/msnd_classic.h\|Documentation/sound/alsa/ALSA-Configuration.txt\)'
    blobna '\(Important[ ]Notes[ ]-[ ]Read[ ]Before[ ]Using\|Obtaining[ ]and[ ]Creating[ ]Firmware[ ]Files\)[\n]#[ ][ ]~*\([^\n]\|[\n]#[ ]*\([\n]#[ ]*\([\n]#[ ]*For[ ]the[^\n]*[\n]#[ ]*~*[\n]\)\?\)\?[^\n ]\)*\.' Documentation/sound/oss/MultiSound

    accept '[	]len[ ]=[ ]mod_firmware_load[(]fn,[ ][&]data[)][;][\n][	]if[ ][^{]*[ ][{][\n][	][	 ]*printk[(]KERN_ERR[ ]["]sscape:' sound/oss/sscape.c
    blobname '[/]sndscape[/]\(scope\.cod\|sndscape\.co\([?dx01234]\|%d\)\)' sound/oss/sscape.c

    accept '[	][	]trix_boot_len[ ]=[ ]mod_firmware_load[(]' sound/oss/trix.c
    blobname '\([/]etc[/]sound[/]\)\?trxpro\.bin' sound/oss/trix.c

    accept '[	][	]smw_ucodeLen[ ]=[ ]mod_firmware_load[(]' sound/oss/sb_common.c
    blobname '\([/]etc[/]sound[/]\)\?midi0001\.bin' sound/oss/sb_common.c
    blobname '\([/]etc[/]sound[/]\|turtlebeach[/]\)\?msnd\(init\|perm\)\.bin' sound/oss/Kconfig

    blob 'When[ ]the[ ]module[ ]is[ ]loaded[^\n]*\([\n][^\n]*\)*[/]pss_synth[^\n]*\([\n][^\n]*\)*' Documentation/sound/oss/PSS
    blob 'pss_firmware[ \n	]*This[ ]parameter[^\n]*\([\n][^\n]*\)*[/]pss_synth[^\n]*\([\n][^\n]\+\)*' Documentation/sound/oss/PSS-updates
    accept '[	][	]pss_synthLen[ ]=[ ]mod_firmware_load[(]pss_firmware,[ ][(]void[ ][*][)][ ][&]pss_synth[)][;]' sound/oss/pss.c
    accept '[	]*if[ ]\?[(]\(!\|fw_load[ ][&][&][ ]\)\?pss_synth' sound/oss/pss.c
    accept '[	]*if[ ][(]!pss_download_boot[(]devc,[ ]pss_synth,[ ]pss_synthLen,' sound/oss/pss.c
    accept '[	]*vfree[(]pss_synth[)][;]' sound/oss/pss.c
    blobna 'to[ ]allow[ ]the[ ]user[ ][^/"]*fir[em]ware[ ]file[^/"]*["][^"*]*["]' sound/oss/pss.c
    blobname '\([/]etc[/]sound[/]\)\?pss_synth' sound/oss/pss.c
    accept '[	][$][(]obj[)][/]bin2hex[ ]pss_synth' sound/oss/Makefile
    accept '[	][ ]*echo[ ][\'"'"']static[ ]\(unsigned[ ]char[ ][*][ ]*\|int[ ]\)pss_synth\(Len\)\?[ ]=[ ]\(NULL\|0\)[;]' sound/oss/Makefile

    accept '[	]\.request_firmware[ ]=[ ]NULL,' drivers/media/dvb/dvb-usb/m920x.c

    accept '[	 ]*["]request_firmware[ ]\(fatal[ ]error\|unable[ ]to[ ]locate\|:[ ]Failed[ ]to[ ]find\)' drivers/media/video/pvrusb2/pvrusb2-hdw.c
    accept '[ ][*][ ]NOTE[ ]:[ ]the[ ]pointer[ ]to[ ]the[ ]firmware[ ]data[ ]given[ ]by[ ]request_firmware[(][)]' drivers/media/video/pvrusb2-hdw.c

    blobname 'dvb-usb-\(dw\(210[124]\|3101\)\|s630\)\.fw' drivers/media/dvb/dvb-usb/dw2102.c

    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]gp8psk_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/gp8psk.c
    blobname 'dvb-usb-gp8psk-0[12]\.fw' drivers/media/dvb/dvb-usb/gp8psk.c

    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]opera1_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/nova-t-usb2.c
    blobname 'dvb-usb-opera-\(fpga-\)\?-01\.fw' drivers/media/dvb/dvb-usb/opera1.c

    blobname 'dvb-fe-af9013\.fw' drivers/media/dvb/frontends/af9013_priv.h

    blobname 'dvb-fe-bcm3510-01\.fw' drivers/media/dvb/frontends/bcm3510.c

    blobname 'dvb-fe-cx24116\.fw' drivers/media/dvb/frontends/cx24116.c

    blobname 'dvb-fe-nxt2002\.fw' drivers/media/dvb/frontends/nxt200x.c

    blob '[/][*][\n][ ][*][ ]This[ ]driver[ ]needs[ ]two[ ]external[ ]firmware[ ]files[^*]*\([*]\+[^/*][^*]*\)*[*]*dvb-fe-or51132-\(vsb\|qam\)\.fw[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]' drivers/media/dvb/frontends/or51132.c
    blobname 'dvb-fe-or51132-\(vsb\|qam\)\.fw' drivers/media/dvb/frontends/or51132.c

    blobname 'dvb-fe-or51211\.fw' drivers/media/dvb/frontends/or51211.c

    blobname 'dvb-fe-sp887x\.fw' drivers/media/dvb/frontends/sp887x.c

    blobname 'dvb-fe-tda10048-1\.0\.fw' drivers/media/dvb/frontends/tda10048.c

    blobname '\(\(dvb\|tdmb\|isdbt\)_nova\|cmmb_vega\)_12mhz\(_b0\)\?\.inp' drivers/media/dvb/siano/smscoreapi.c

    blobname '\(dvb[th]\(_bda\)\?\|tdmb\)_stellar_usb\.inp' drivers/media/dvb/siano/smsusb.c

    blobname 'dvb-ttusb-dec-\(2000t\|2540t\|3000s\)\.fw' drivers/media/dvb/ttusb-dec/ttusb_dec.c

    blob 'For[ ]the[ ]WinTV[/]PVR[^:]*firmware[^:]*:[\n]hcwamc\.rbf[^\n]*\([\n][^\n][^\n]*\)*' Documentation/video4linux/bttv/README
    blobname 'hcwamc\.rbf' drivers/media/video/bt8xx/bttv-cards.c
    blobna 'The[ ]hcwamc\.rbf[ ]firmware[ ]file[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]' drivers/media/video/bt8xx/bttv-cards.c

    blobname 'v4l-cx23418-dig\.fw' drivers/media/video/cx18/cx18-av-firmware.c
    blobname 'v4l-cx23418-[ac]pu\.fw' drivers/media/video/cx18/cx18-firmware.c

    blobname 'v4l-cx23885-enc\.fw' 'drivers/media/video/cx23\(1xx\|885\)/cx23885-417.c'

    blobname 'v4l-\(cx23\(885\|1xx\)-avcore-01\|cx25840\)\.fw' drivers/media/video/cx25840/cx25840-firmware.c

    blobname 'v4l-cx2341x-\(enc\|dec\)\.fw' include/media/cr2341x.h

    blobname 'v4l-cx2341x-init\.mpg' drivers/media/video/ivtv/ivtv-firmware.c

    blobname 'v4l-pvrusb2-\(2[49]\|73\)xxx-01\.fw' drivers/media/video/pvrusb2/pvrusb2-devattr.c

    blobname 'f2255usb\.bin' drivers/media/video/s2255drv.c

    blobname 'drx397xD\.\(A2\|B1\)\.fw' drivers/media/dvb/frontends/drx397xD_fw.h

    accept '#define[ ]DIB0700_DEFAULT_DEVICE_PROPERTIES[ ]\\[\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^\n",]*,[ ]\\[\n]\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/dib0700_devices.c
    blobname 'dvb-usb-dib0700-1\.[12]0\.fw' 'drivers/media/dvb/dvb-usb/dib0700_\(devices\|core\)\.c'

    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]nova_t_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/nova-t-usb2.c
    blobname 'dvb-usb-nova-t-usb2-02\.fw' drivers/media/dvb/dvb-usb/nova-t-usb2.c

    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]umt_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/umt-010.c
    blobname 'dvb-usb-umt-010-02\.fw' drivers/media/dvb/dvb-usb/umt-010.c

    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]ttusb2_properties\(_s2400\)\?[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/ttusb2.c
    blobname 'dvb-usb-\(pctv-400e\|tt-s2400\)-01\.fw' drivers/media/dvb/dvb-usb/ttusb2.c

    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]cxusb_bluebird_\(lgh064f\|dee1601\|lgz201\|dtt7579\|nano2_needsfirmware\)_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/cxusb.c
    blobname 'dvb-usb-bluebird-0[12]\.fw' drivers/media/dvb/dvb-usb/cxusb.c

    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]\(dtt200u\|wt220u\(_\(fc\|zl0353\|miglia\)\)\?\)_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/dtt200u.c
    blobname 'dvb-usb-\(dtt200u-01\|wt220u-\(02\|fc03\|\(zl0353\|miglia\)-01\)\)\.fw' drivers/media/dvb/dvb-usb/dtt200u.c

    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]vp7045_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/vp7045.c
    blobname 'dvb-usb-vp7045-01\.fw' drivers/media/dvb/dvb-usb/vp7045.c

    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]\(dibusb\(1_1\(_an2235\)\?\|2_0b\)\|artec_t1_usb2\)_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/dibusb-mb.c
    blobname 'dvb-usb-\(dibusb-\(5\.0\.0\.11\|an2235-01\|6\.0\.0\.8\)\|adstech-usb2-02\)\.fw' drivers/media/dvb/dvb-usb/dibusb-mb.c

    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]a800_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]=[ ]' drivers/media/dvb/dvb-usb/a800.c
    blobname 'dvb-usb-avertv-a800-02\.fw' drivers/media/dvb/dvb-usb/a800.c

    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]af9005_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]=[ ]' drivers/media/dvb/dvb-usb/af9005.c
    blobname 'af9005\.fw' drivers/media/dvb/dvb-usb/af9005.c

    accept '[	][	]\.download_firmware[ ]=[ ]af9015_download_firmware,[\n][	][	]\.firmware[ ]=[ ]' drivers/media/dvb/dvb-usb/af9015.c
    blobname 'dvb-usb-af9015\.fw' drivers/media/dvb/dvb-usb/af9015.c

    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]dibusb_mc_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/dibusb-mc.c
    blobname 'dvb-usb-dibusb-6\.0\.0\.8\.fw' drivers/media/dvb/dvb-usb/dibusb-mc.c

    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]\(megasky\|digivox_mini_ii\|tvwalkertwin\|dposh\)_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/m920x.c
    blobname 'dvb-usb-\(\(megasky\|digivox\)-02\|tvwalkert\|dposh-01\)\.fw' drivers/media/dvb/dvb-usb/m920x.c

    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]vp702x_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/vp702x.c
    blobname 'dvb-usb-vp702x-02\.fw' drivers/media/dvb/dvb-usb/vp702x.c

    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]digitv_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/digitv.c
    blobname 'dvb-usb-digitv-02\.fw' drivers/media/dvb/dvb-usb/digitv.c

    blob 'Driver:[ ]\(acenic\|ADAPTEC_STARFIRE\|cxgb3\|e100\|tigon3\|korg1212\|maestro3\|ymfpci\|smctr\|kaweth\|ttusb-budget\|keyspan\|emi26\|emi62\|t[iu]_usb_3410_5052\|whiteheat\|ip2\|CPiA2\|DABUSB\|USB_VICAM\|USB_SERIAL_EDGEPORT\(_TI\)\?\|SND_SB16_CSP\|CASSINI\|ambassador\|SCSI_\(ADVANSYS\|QLOGIC\(_1280\|PTI\)\)\|TEHUTI\|TYPHOON\|YAM\|3C359\|PCMCIA_\(PCNET\|SMC91C92\|3C5\(89\|74\)\)\|MYRI_SBUS\|BNX2\|bnx2x\|wavefront\|SERIAL_8250_CS\|mga\|r128\|radeon\|ib_qib\)\([ ]--*\|:\)[ ]\([^\n]\|[\n]*[^\n\-]\)*\([\n][\n]--*[\n][\n]\?Driver:[ ]\(acenic\|ADAPTEC_STARFIRE\|cxgb3\|e100\|tigon3\|korg1212\|maestro3\|ymfpci\|smctr\|kaweth\|ttusb-budget\|keyspan\|emi26\|emi62\|t[iu]_usb_3410_5052\|whiteheat\|ip2\|CPiA2\|DABUSB\|USB_VICAM\|USB_SERIAL_EDGEPORT\(_TI\)\?\|SND_SB16_CSP\|CASSINI\|ambassador\|SCSI_\(ADVANSYS\|QLOGIC\(_1280\|PTI\)\)\|TEHUTI\|TYPHOON\|YAM\|3C359\|PCMCIA_\(PCNET\|SMC91C92\|3C5\(89\|74\)\)\|MYRI_SBUS\|BNX2\|bnx2x\|wavefront\|SERIAL_8250_CS\|mga\|r128\|radeon\|ib_qib\)\([ ]--*\|:\)[ ]\([^\n]\|[\n]*[^\n\-]\)*\)*' firmware/WHENCE

    blobname 'sms1xxx-\(stellar\|nova-[ab]\|hcw-55xxx\)-dvbt-0[12]\.fw' drivers/media/dvb/siano/sms-cards.c

    accept '[ ][ ][ ][ ]mv[ ]["][$]ofile["][ ]["][$]ofile\.elf["]' arch/powerpc/boot/wrapper
    accept '[ ][ ][ ][ ][$]objbin[/]mktree[ ]["][$]ofile\.elf["]' arch/powerpc/boot/wrapper
    accept '[	]rm[ ]-f[ ]["][$]ofile\.elf["]' arch/powerpc/boot/wrapper
    accept '[ ][ ][ ][ ][$][{]CROSS[}]objcopy[ ]-O[ ]binary[ ]["][$]ofile["][ ]["][$]ofile\.bin["]' arch/powerpc/boot/wrapper
    accept '[ ][ ][ ][ ]dd[ ]if=["][$]ofile\.bin["][ ]of=["][$]ofile\.bin["]' arch/powerpc/boot/wrapper
    accept '[ ][ ][ ][ ]odir=["][$][(]dirname[ ]["][$]ofile\.bin["][)]["]' arch/powerpc/boot/wrapper
    accept '[ ][ ][ ][ ]gzip[ ]--force[ ]-9[ ]--stdout[ ]["][$]ofile\.bin["][ ]>[ ]["][$]odir[/]otheros\.bld["]' arch/powerpc/boot/wrapper
    accept '[	]\.incbin[	]["]arch[/]x86[/]kernel[/]acpi[/]realmode[/]wakeup\.bin["]' arch/x86/kernel/acpi/wakeup_rm.S
    accept '[;]set[ ]executable[ ]["]2232\.bin["]' drivers/char/ser_a2232fw.ax

    blobname 'di\(\(dn\|pr\)load\|diva\(pp\)\?\|hscx\|v110\|modem\|fax\|_etsi\|_\(1tr6\|belg\|franc\|atel\|ni\|5ess\|japan\|swed\)\|dspdld\)\.\(bin\|s[xyqm]\|p\)' drivers/isdn/hardware/eicon/cardtype.h
    blobname 'dsp\(dload\|dqsig\|dvmdm\|dvfax\)\.bin' drivers/isdn/hardware/eicon/dsp_defs.h

    blobname 'vicam[/]firmware\.fw' drivers/media/video/usbvideo/vicam.c

    accept '#include[ ]["]ixp2400_[rt]x\.ucode["]' drivers/net/ixp2000/ixpdev.c

    # New in 2.6.29
    blobname 'acenic[/]tg[12]\.bin' drivers/net/acenic.c
    blobname 'adaptec[/]starfire_[rt]x\.bin' drivers/net/starfire.c
    blobname 'e100[/]d10\(1[ms]\|2e\)_ucode\.bin' drivers/net/e100.c
    blobname 'tigon[/]tg3\(_tso5\?\)\?\.bin' drivers/net/tg3.c
    blobname '\(ti_usb-v\(%04x\|[0-9a-f]*\)-p\(%04x\|[0-9a-f]*\)\|mts_\(cdma\|gsm\|edge\)\)\.\(bin\|fw\)' drivers/usb/serial/ti_usb_3410_5052.c
    blobname 'iw\?\(2400\|6050\)m\?-fw-\(sdio\|usb\)-\(\(["][ ]I2400M_FW_VERSION[ ]["]\|[0-9.]*\)\.sbcf\|[^". \n]*\)' 'drivers/net/wimax/i2400m/\(sdio\|usb\)\.c'
    blob '3\.[ ]Installing[ ]the[ ]firmware[^\n]*\([\n][\n]*[ ][ ][ ][^\n]*\)*[\n]*[$][^\n]*i2400m-fw[^\n]*\([\n][\n]*[ ][ ][ ][^\n]*\)*' Documentation/wimax/README.i2400m
    blob '6\.1\.[ ]Driver[ ]complains[^\n]*i2400m-fw[^\n]*\([\n][\n]*\([ ][ ][ ]\|i2400m_usb\)[^\n]*\)\+' Documentation/wimax/README.i2400m
    accept '[	][	]ranges[ ]=[ ]<'"$blobpat*"'>[;]' 'arch/powerpc/boot/dts/\(mpc8572ds\|p2020ds\|katmai\)\.dts'
    accept '\(div_table_\(clz\|inv\|ix\)\|zero_l\):\([\n][	]\.\(byte[	]-\?[0-9]*\|long[	]0x[0-9A-F]*\)\)*' arch/sh/lib/udivsi3_i4i.S
    defsnc 'const[ ]u32[ ]crypto_[fi][tl]_tab\[4\]\[256\][ ]=' crypto/aes_generic.c
    accept '[	][ ][ ]every[ ]driver[ ]which[ ]uses[ ]request_firmware[(][)][ ]and[ ]ships[ ]its' drivers/base/Kconfig
    defsnc 'static[ ]const[ ]u32[ ]filter_table\[\][ ]=' drivers/gpu/drm/i915/intel_tv.c
    defsnc 'static[ ]u8[ ]af9015_ir_table_\(avermedia\(_ks\)\?\|digittrade\|trekstor\)\[\][ ]=' drivers/media/dvb/dvb-usb/af9015.h
    defsnc '[	]static[ ]__u8[ ]lgdt3304_\(vsb8\|qam\(64\|256\)\)_data\[\][ ]=' drivers/media/dvb/frontends/lgdt3304.c
    defsnc 'static[ ]u8[ ]\(init\|c\)_table\[\]=' drivers/media/dvb/frontends/s921_core.c
    defsnc 'static[ ]\(const[ ]\)\?struct[ ]stb0899_tab[ ]stb0899_\(cn\|dvbs2\?rf\|quant\|est\)_tab\[\][ ]=' drivers/media/dvb/frontends/stb0899_drv.c
    defsnc 'static[ ]const[ ]struct[ ]stb6100_lkup[ ]lkup\[\][ ]=' drivers/media/dvb/frontends/stb6100.c
    initnc 'static[ ]const[ ]__u8[ ]ov\(534\|772x\)_reg_initdata\[\]\[2\][ ]=' drivers/media/video/gspca/ov534.c
    defsc 'static[ ]const[ ]\(__\)\?u8[ ]\(mi\(0360\|13[12]0\)\|po\(1200\|3130\)\|hv7131r\|ov76[67]0\)_\(\(soc\)\?_\?[iI]nit\(Q\?V\|SX\)GA\(_\(JPG\|data\)\)\?\|rundata\)\[\]\[4\][ ]=' drivers/media/video/gspca/vc032x.c
    defsnc 'static[ ]\(const[ ]\)\?u\(32\|_int32_t\)[ ]ar928[05]\(Common\|Modes\(_\(fast_clock\|backoff_[12]3db_rxgain\|\(original\|high_power\)_[tr]x_\?gain\)\)\?\)_928\(0_2\|5\(_1_2\)\?\)\[\]\[[236]\][ ]=' 'drivers/net/wireless/ath9k/\(ar9002_\)\?initvals\.h'
    defsnc 'static[ ]u32[ ]channel_tbl\[15\]\[9\][ ]=' drivers/staging/agnx/rf.c
    defsnc 'static[ ]const[ ]u32[\n]gain_table\[\][ ]=' drivers/staging/agnx/rf.c
    accept '<[frs]:[0-9]*x[0-9]*>[\n][01 \n]*' 'drivers/staging/asus_oled/\(linux\(_fr\?\)\?\|tux\(_r2\?\)\?\|zig\).txt'
    defsnc 'static[ ]unsigned[ ]char[ ]\(aud\|vid\)_regs\[\][ ]=' drivers/staging/go7007/s2250-board.c
    defsnc 'static[ ]u16[ ]vid_regs_fp\[\][ ]=' drivers/staging/go7007/s2250-board.c
    blobname 's2250\(_loader\)\?\.fw' drivers/staging/go7007/s2250-loader.c
    blobna 'me_xilinx_download' 'drivers/staging/meilhaus/.*'
    accept 'int[ ]me_xilinx_download[(]' 'drivers/staging/meilhaus/mefirmware\.[ch]'
    blobname 'me46[01]0\(_bosch\)\?\.bin' drivers/staging/meilhaus/me4600_device.c
    accept '\([	]if[ ][(]me4600_device->base\.info\.pci\.device_id[ ]==[ ]PCI_DEVICE_ID_MEILHAUS_ME4610[)][ ][{][	][/][/]Jekyll[ ]<=>[ ]me4610\|#ifdef[ ]BOSCH\|#else[ ][/][/]~BOSCH\)[\n][	][	]err[ ]=[\n][	][	][ ][ ][ ][ ]me_xilinx_download[(]me4600_device' drivers/staging/meilhaus/me4600_device.c
    blobname 'me6000\.bin' drivers/staging/meilhaus/me6000_device.c
    accept '[	][/][*][ ]Download[ ]the[ ]xilinx[ ]firmware[ ][*][/][\n][	]err[ ]=[ ]me_xilinx_download[(]me6000_device' drivers/staging/meilhaus/me6000_device.c
    defsnc '[	][}][ ]grtpkts\[\][ ]=' drivers/staging/mimio/mimio.c
    defsnc 'u16_t[ ]zgTkipSbox\(Lower\|Upper\)\[256\][ ]=' drivers/staging/otus/80211core/ctkip.c
    accept '[ 	]*[/][*][ ]*0\([ ]*[123]\)*[ ]*[*][/][\n][ 	]*[/][*][ ]0[ ]1[ ]2[ ]3[ ]4[ ]5[ ]6[ ]7[ ]8[ ]9\([ ][0-9]\)*[ ][*][/]' drivers/staging/otus/80211core/ctxrx.c
    defsnc 'u32_t[ ]crc32_tab\[\][ ]=' drivers/staging/otus/80211core/cwep.c
    blob 'const[ ]u32_t[ ]zc\(DK\|P2\)\?Fw\(Buf\)\?Image\(SPI\)\?\(\[\][ ]*=[ ]*[{][^;]*[}]\|Size[ ]*=[ ]*[0-9]*\)[;]\([\n][\n]*const[ ]u32_t[ ]zc\(DK\|P2\)\?Fw\(Buf\)\?Image\(SPI\)\?\(\[\][ ]*=[ ]*[{][^;]*[}]\|Size[ ]*=[ ]*[0-9]*\)[;]\)*' 'drivers/staging/otus/hal/hp.*fwu.*\.c'
    blob 'extern[ ]const[ ]u32_t[ ]zc\(DK\|P2\)\?Fw\(Buf\)\?Image\(SPI\)\?\(\[\]\|Size\)[;]\([\n]extern[ ]const[ ]u32_t[ ]zc\(DK\|P2\)\?Fw\(Buf\)\?Image\(SPI\)\?\(\[\]\|Size\)[;]\)*' drivers/staging/otus/hal/hpmain.c
    defsnc '[ ][ ][ ][ ]u32_t[ ]eepromBoardData\[15\]\[6\][ ]=' drivers/staging/otus/hal/hpmain.c
    defsnc 'static[ ]const[ ]u32_t[ ]channel_frequency_11A\[\][ ]=' drivers/staging/otus/ioctl.c
    defsnc 'static[ ]const[ ]u32_t[ ]\(ar5416Modes\|otusBank\)\[\]\[[36]\][ ]=' drivers/staging/otus/hal/otus.ini
    defsnc '[ ][ ][ ][ ]static[ ]UINT32[ ]MD5Table\[64\][ ]=' 'drivers/staging/rt28[67]0/common/md5\.c'
    defsnc 'static[ ]uint32[ ][FR]Sb\[256\][ ]=' 'drivers/staging/rt28[67]0/common/\(md5\|cmm_aes\)\.c'
    defsnc '\(UCHAR\|u8\)[ ]RateSwitchTable\(11B\?G\?\(N[123]S\(ForABand\)\?\)\?\)\?\[\][ ]=' 'drivers/staging/rt28[67]0/common/mlme\.c'
    defsnc '\(UCHAR\|u8\)[ 	]*ZeroSsid\[32\][ ]=' 'drivers/staging/rt28[67]0/common/mlme\.c'
    defsnc '\(RTMP_RF_REGS\|struct[ ]rt_rtmp_rf_regs\)[ ]RF2850RegTable\[\][ ]=' 'drivers/staging/rt28[67]0/common/\(mlme\.c\|cmm_asic\.c\)'
    defsnc '\(FREQUENCY_ITEM\|struct[ ]rt_frequency_item\)[ ]FreqItems3020\[\][ ]=' 'drivers/staging/rt28[67]0/common/\(mlme\.c\|cmm_asic\.c\)'
    blob '\(UCHAR\|u8\)[ ]FirmwareImage\(_\(2870\|30[79]0\)\)\?[ ]\[\][ ]=[ ][{][^;]*[}][ ][;]' 'drivers/staging/rt\(28[67]\|30[79]\)0/common/firmware\(_3070\)\?\.h'
    defsnc 'ULONG[ ][ ]*BIT32\[\][ ]=' 'drivers/staging/rt28[67]0/common/rtmp_init\.c'
    defsnc 'const[ ]unsigned[ ]short[ ]ccitt_16Table\[\][ ]=' 'drivers/staging/rt\(28[67]0\|3090\)/common/rtmp_init\.c'
    blobna '\(pFirmwareImage[ ]=\([ ]FirmwareImage\(_\(28[67]\|30[79]\)0\)\?\|[\n 	]*[(]\(PUCHAR\|u8[ ][*]\)[)][&][\n 	]*FirmwareImage\(_\(28\|30\)70\)\?\[FIRMWAREIMAGE\(V[12]\)\?_LENGTH\]\)\|File[lL]ength[ ]=[ ]\(sizeof[(]FirmwareImage[)]\|FIRMWAREIMAGE\(V[12]\|_MAX\)\?_LENGTH\)\)[;]\([\n	 ]*\(pFirmwareImage[ ]=\([ ]FirmwareImage\(_\(28[67]\|30[79]\)0\)\?\|[\n 	]*[(]\(PUCHAR\|u8[ ][*]\)[)][&][\n 	]*FirmwareImage\(_\(28\|30\)70\)\?\[FIRMWAREIMAGE\(V[12]\)\?_LENGTH\]\)\|File[lL]ength[ ]=[ ]\(sizeof[(]FirmwareImage[)]\|FIRMWAREIMAGE\(V[12]\|_MAX\)\?_LENGTH\)\)[;]\)*' 'drivers/staging/rt\(28[67]0\|30[79]0\)/common/rtmp_init\.c'
    blobname 'rate\.bin' drivers/staging/rt2870/rtmp_init.c
    defsnc '\(U\(INT\|CHAR\)\|u\(32\|8\)\)[ ]\(Tkip_Sbox_\(Lower\|Upper\)\|SboxTable\)\[256\][ ]=' 'drivers/staging/rt\(28[67]0\|3070\)/common/\(rtmp\|cmm\)_tkip\.c'
    defsnc '\(UINT\|u32\)[ ]FCSTAB_32\[256\][ ]=' 'drivers/staging/rt\(28[67]0\|3070\)/common/\(rtmp\|cmm\)_wep\.c'
    accept '[ ]*#[ ]*define[ ]\(STA_PROFILE\|CARD_INFO\)_PATH[	]*["][/]etc[/]Wireless[/]RT\(28[67]\|307\)0STA[/]RT\(28[67]\|307\)0STA\(Card\)\?\.dat["]' 'drivers/staging/rt\(28[67]0\|3070\)/rt_linux\.h'
    blobname '\([/]etc[/]Wireless[/]\)\?\(RT\(28[67]\|307\)0STA[/]\)\?\(RT\(28[67]\|307\)0STA\|rt28[67]0\)\.bin' 'drivers/staging/rt\(28[67]0\|3070\)/rt_linux\.h'
    blobname '\([/]etc[/]Wireless[/]\)\?\(RT28[67]0STA[/]\)\?e2p\.bin' 'drivers/staging/rt\(28[67]0\|3070\)/rt_ate\.[hc]'
    defsnc '\([ ][ ][ ][ ]\|[	]\)u_int32_t[ ]ralinkrate\[256\][ ]=' 'drivers/staging/rt\(28[67]0\|3070\)/rt_linux\.c'
    defsnc 'unsigned[ ]char[ ]\(QUALITY\|STRENGTH\)_MAP\[\][ ]=' drivers/staging/rtl8187se/r8180_core.c
    defsnc 'u\(8\|16\|32\)[ ]rtl8225\(\(a\|bcd\?\)_rxgain\|agc\|tx_\(gain_cck\|power\)_ofdm\|tx_power_cck\(_ch14\)\?\)\[\]=' drivers/staging/rtl8187se/r8180_rtl8225.c
    defsnc '\(static[ ]const[ ]\)\?u\(8\|16\|32\)[ ]\(rtl8225\(z2\)\?_\(threshold\|gain_\(a\|bg\)\|chan\|rxgain\|agc\|tx_\(gain_cck\|power\)_ofdm\|tx_power_cck\(_ch14\)\?\)\|ZEBRA2_CCK_OFDM_GAIN_SETTING\)\[\][ ]\?=' drivers/staging/rtl8187se/r8180_rtl8225z2.c
    defsnc 'static[ ]short[ ]rtl8255_agc\[\]=' drivers/staging/rtl8187se/r8180_rtl8255.c
    defsnc '[ ]\?static[ ]u\(8\|32\)[ ]\(MAC_REG_TABLE\[\]\[2\]\|[ ]*ZEBRA_\(AGC\|RF_RX_GAIN_TABLE\)\[\]\|OFDM_CONFIG\[\]\)=' drivers/staging/rtl8187se/r8185b_init.c
    accept '[	]-[ ]move[ ]firmware[ ]loading[ ]to[ ]request_firmware[(][)]' drivers/staging/slicoss/README
    blobname '\(\(oasis\|gb\)_rcv\|slic_\(oasis\|mojave\)\)\.bin' drivers/staging/slicoss/slicoss.c

    blob 'static[ ]unsigned[ ]char[ ]xilinx_firm\(_4610\)\?\[\][ ]=[ ][{]'"$sepx$blobpat*$sepx"'[}][;]' 'drivers/staging/me4000/me4\(00\|61\)0_firmware\.h'
    blob 'static[ ]struct[ ]PHY_UCODE[ ]PhyUcode\[\][ ]=[^;]*[;]' drivers/staging/sxg/sxgphycode.h
    blob 'static[ ]unsigned[ ]char[ ]SaharaUCode\[2\]\[57972\][ ]=[^;]*[;]' drivers/staging/sxg/saharadbgdownload.h
    blob '#include[ ]["]\(sxgphycode\(-1\.2\)\?\|saharadbgdownload\)\.h["]\([\n][\n]*#include[ ]["]\(sxgphycode\(-1\.2\)\?\|saharadbgdownload\)\.h["]\)*' drivers/staging/sxg/sxg.c
    blob 'static[ ]u8[ ]\(Mojave\|Oasis\)UCode\[2\]\[65536\][ ]=[^;]*[;]' 'drivers/staging/slicoss/\(gb\|oasis\(dbg\)\?\)download\.h'
    blob 'static[ ]u8[ ]\(GB\|Oasis\)RcvUCode\[2560\][ ]=[^;]*[;]' 'drivers/staging/slicoss/\(gb\|oasis\)rcvucode\.h'
    blob '#include[ ]["]\(gb\|oasis\)\(dbg\)\?\(download\|rcvucode\)\.h["]\([\n][\n]*#include[ ]["]\(gb\|oasis\)\(dbg\)\?\(download\|rcvucode\)\.h["]\)*' drivers/staging/slicoss/slicoss.c
    blobna 'instruction[ ]=[ ][^;]*\(Oasis\|GB\|Mojave\)\(Rcv\)\?UCode[^:}]*[;]' drivers/staging/slicoss/slicoss.c
    blobna 'seq_printf[(]seq[,][ ]["][^"]*%s[ ]%s[^"]*["][,][ 	\n]*\(GB_RCV\|MOJAVE_\)UCODE_VERS_STRING[,][ ]\(GB_RCV\|MOJAVE_\)UCODE_VERS_DATE[)][;]\([ 	\n]*seq_printf[(]seq[,][ ]["][^"]*%s[ ]%s[^"]*["][,][ 	\n]*\(GB_RCV\|MOJAVE_\)UCODE_VERS_STRING[,][ ]\(GB_RCV\|MOJAVE_\)UCODE_VERS_DATE[)][;]\)*' drivers/staging/slicoss/slicoss.c
    blobna 'numsects[ ]=[ ][OM]NumSections[;][\n][	]*for[ ][(][^;]*[;][^;]*[;][^;{]*[)][ ][{][\n][^}]*[\n][	][	][}]' drivers/staging/slicoss/slicoss.c

    # post 2.6.29 patches
    defsnc 'static[ ]int[ ]atom_dst_to_src\[8\]\[4\][ ]=' drivers/gpu/drm/radeon/atom.c
    defsnc 'const[ ]unsigned[ ]char[ ]map_table\[\][ ]=' drivers/input/lirc/lirc_ttusbir.c
    defsnc '\(static[ ]\)\?\(const[ ]\)\?struct[ ]au8522_register_config[ ]lpfilter_coef\[\][ ]=' drivers/media/dvb/frontends/au8522_decoder.c
    defsnc 'static[ ]const[ ]u8[ ]jpeg_head\[\][ ]=' drivers/media/video/gspca/jpeg.h
    defsnc 'static[ ]const[ ]u8[ ]\(bridge\|sensor\)_init_ov\(7[27]2x\|965x\(_2\)\?\)\[\]\[2\][ ]=' drivers/media/video/gspca/ov534.c
    defsnc '[	]static[ ]const[ ]u8[ ]probe_tb\[\]\[4\]\[8\][ ]=' drivers/media/video/gspca/sonixj.c
    defsnc 'static[ ]const[ ]u8[ ]eeprom_data\[\]\[3\][ ]=' drivers/media/gspca/tv8532.c
    defsnc '\(static[ ]uint32_t\|[}]\)[ ]nv04_graph_ctx_regs[ ]\?\[\][ ]=' drivers/char/drm/nv04_graph.c
    defsnc 'static[ ]int[ ]nv10_graph_ctx_regs[ ]\?\[\][ ]=' drivers/char/drm/nv10_graph.c

    # This looks suspicious, but it pretty much just sets stuff to zero.
    initnc 'static[ ]__u8[ ]mode8420\(pro\|con\)\[\][ ]=' drivers/media/video/cs8420.h

    # quite suspicious
    # arch/parisc/kernel/perf_images.h
    initc 'static[ ]uint32_t[ ]onyx_images\[\]\[PCXU_IMAGE_SIZE[/]sizeof[(]uint32_t[)]\][ ]__read_mostly[ ]='
    initc 'static[ ]uint32_t[ ]cuda_images\[\]\[PCXW_IMAGE_SIZE[/]sizeof[(]uint32_t[)]\][ ]__read_mostly[ ]='

    # These are regarded as ok
    initnc 'static[ ]const[ ]u8[ ]SN9C102_\(Y\|UV\)_QTABLE[01]\[64\][ ]=[ ][{]' drivers/media/usb/sn9c102/sn9c102_config.h
    initnc '[	]static[ ]\(const[ ]\)\?u8[ ]jpeg_header\[589\][ ]=[ ][{]' media/video/sn9c102/sn9c102_core.c
    accept '[	][	]\?err[ ]=[ ]sn9c102_write_const_regs[(]cam\(,[ 	\n]\+[{]0x[0-9a-fA-F][0-9a-fA-F],[ ]0x[0-9a-fA-F][0-9a-fA-F][}]\)*[)][;]'

    # too lax?
    defsnc 'static[ ]yyconst[ ]\(flex_int\(16\|32\)_t\|\(\(short[ ]\)\?int\)\)[ ]yy_[^[]*\[[][0-9]*\][ ]='
    defsnc 'static[ ]const[ ]\(yytype_u\?int\(8\|16\)\|\(unsigned[ ]\)\?\(short\([ ]int\)\?\|char\)\)[ ]yy[^[]*\[\][ ]='
    defsnc '\([	]\)\?static[ ]\(const[ ]\)\?\(unsigned[ ]\(short\|char\)\|struct[ ]SiS_[^ ]*\)[ ]SiS[^[]*\(\[[][ *0-9]*\]\)\+[ ]*='

    initnc 'static[ ]const[ ]a3d_Hrtf_t[ ]A3dHrirZeros[ ]=[ ][{]'
    initnc 'static[ ]const[ ]a3d_Hrtf_t[ ]A3dHrirImpulse[ ]=[ ][{]'
    initnc 'static[ ]const[ ]a3d_Hrtf_t[ ]A3dHrirOnes[ ]=[ ][{]'
    initnc 'static[ ]const[ ]a3d_Hrtf_t[ ]A3dHrirSatTest[ ]=[ ][{]'
    initnc 'static[ ]const[ ]a3d_Hrtf_t[ ]A3dHrirDImpulse[ ]=[ ][{]'
    initnc 'static[ ]const[ ]a3d_ItdDline_t[ ]A3dItdDlineZeros[ ]=[ ][{]'
    initnc 'static[ ]auxxEqCoeffSet_t[ ]asEqCoefsNormal[ ]=[ ][{]'
    defsnc 'static[ ]xtalk_dline_t[ ]const[ ]alXtalkDline\(Test\|Zeros\)[ ]=' sound/pci/au88x0/au88x0_xtalk.c
    initnc 'static[ ]struct[ ]nand_ecclayout[ ]rtc_from4_nand_oobinfo[ ]=[ ][{]'
    initnc 'static[ ]const[ ]s16[ ]tempLUT\[\][ ]='
    defsnc 'static[ ]const[ ]u8[ ]viaLUT\[\][ ]=' drivers/hwmon/via686a.c
    initnc 'static[ ]struct[ ][{][ ]int[ ]xres,[ ]yres,[ ]left,[ ]right,[ ]upper,[ ]lower,[ ]hslen,[ ]vslen,[ ]vfreq[;][ ][}][ ]timmings\[\][ ]__initdata[ ]=[ ][{]'
    initnc 'static[ ]struct[ ]platinum_regvals[ ]platinum_reg_init_[0-9]*[ ]=[ ][{]'
    defsnc '[}][ ]sisfb_ddc[sf]modes\[\][ ]\(__devinitdata[ ]\)\?=' drivers/video/sis/sis_main.h
    defsnc 'static[ ]struct[ ]dvb_pll_desc[ ][^\n]*[ ]=[ ][{]' drivers/media/dvb/frontends/dvb-pll.c
    initnc 'static[ ]u32[ ]LABELPATCHES\[\][ ]__attribute[(][(]unused[)][)][ ]='

    initnc 'static[ ]dbdev_tab_t[ ]dbdev_tab\[\][ ]='
    accept '\(EXP\|LOG\|ATAN\)TBL:'"$sepx$blobpat*"
    initnc 'static[ ]char[ ]fm_volume_table\[128\][ ]='
    initnc 'unsigned[ ]int[ ]snd_gf1_scale_table\[SNDRV_GF1_SCALE_TABLE_SIZE\][ ]='
    # remaining after original deblob_2_6_24, not fully checked

    oprepline '#define[ ]OV51[18]_\(Y\|UV\)QUANTABLE[ ][{]'
    initnc '[	][	]static[ ]unsigned[ ]char[ ]const[ ]data_bit\[64\][ ]='
    initnc '[	][	]static[ ]const[ ]u8[ ]data_sbit\[32\][ ]='
    initnc '[	]\.RightCoefs[ ]='
    defsnc '[	]#define[ ]WakeupSeq[ ][ ][ ][ ][{]' drivers/net/ethernet/i825xx/eepro.c
    initnc '[	]SetRate44100\[\][ ]='
    initnc '[	]const[ ]short[ ]period\[32\][ ]='
    defsnc '[	]\(const[ ]static\|static[ ]const\)[ ]int[ ]desc_idx_table\[\][ ]=' 'arch/arm/include/asm/hardware/iop3xx-adma.h|include/asm-arm/hardware/iop3xx-adma.h'
    initnc '[	]int[ ]prop_bcomm_irq\[3[*]16\][ ]='
    initnc '[	]static[ ]char[ ]logSlopeTable\[128\][ ]='
    initnc '[	]static[ ]const[ ]int[ ]uc_\(dup\|word\)_table\[\]\[2\][ ]='
    initnc '[	]static[ ]const[ ]struct[ ]mc7_timing_params[ ]mc7_timings\[\][ ]='
    initnc '[	]static[ ]const[ ]u8[ ]biphase_tbl\[\][ ]='
    initnc '[	]static[ ]const[ ]u8[ ]cs170\[7[ ][*][ ]8\][ ]='
    initnc '[	]static[ ]const[ ]u8[ ]cs3[13]a\[8[ ][*][ ]4\][ ]='
    initnc '[	]static[ ]const[ ]u8[ ]dramsr13\[12[ ][*][ ]5\][ ]='
    defsnc '[	]static[ ]const[ ]u8[ ]log10\[\][ ]=' drivers/net/wireless/zd1211rw/zd_chip.c
    initnc '[	]static[ ]const[ ]u8[ ]mpeg_hdr_data\[\][ ]='
    initnc '[	]static[ ]const[ ]u8[ ]sdramtype\[13\]\[5\][ ]='
    defsnc '[	]static[ ]const[ ]u8[ ]t\[\][ ]=' drivers/bcma/sprom.c
    initnc '[	]static[ ]const[ ]unsigned[ ]int[ ]avg_pkts\[NCCTRL_WIN\][ ]='
    initnc '[	]static[ ]const[ ]unsigned[ ]short[ ]ac97_defaults\[\][ ]='
    initnc '[	]static[ ]int[ ]exp_lut\[256\][ ]='
    defsnc '[	]static[ ]u16[ ]jpeg_tables\[\]\[70\][ ]=' drivers/media/pci/meye/meye.c
    defsnc '[	]static[ ]u16[ ]tables\[\][ ]=' drivers/media/pci/meye/meye.c
    initnc '[	]static[ ]u32[ ]logMagTable\[128\][ ]='
    defsnc '[	]static[ ]u8[ ]init_bufs\[13\]\[5\][ ]=' drivers/media/pci/cx88/cx88-cards.c
    defsnc '[	]static[ ]u_short[ ]geometry_table\[\]\[[45]\][ ]=' drivers/block/xd.c
    initnc '[	]static[ ]unsigned[ ]char[ ]CRCTable1\[\][ ]='
    initnc '[	]static[ ]unsigned[ ]char[ ]CRCTable2\[\][ ]='
    initnc '[	]static[ ]unsigned[ ]char[ ]default_colors\[\][ ]='
    defsnc '[	]static[ ]unsigned[ ]char[ ]iso_regs\[8\]\[4\][ ]=' drivers/media/usb/cpia2/cpia2_usb.c
    initnc '[	]static[ ]unsigned[ ]char[ ]log_scale\[101\][ ]=' sound/oss/pss.c
    initnc '[	]static[ ]unsigned[ ]char[ ]msg\[\][ ]='
    defsnc '[	]static[ ]unsigned[ ]char[ ]static_pad\[\][ ]=' drivers/s390/crypto/zcrypt_msgtype6.c
    defsnc '[	]static[ ]unsigned[ ]char[ ]table_alaw2ulaw\[\][ ]=' drivers/staging/telephony/ixj.c
    defsnc '[	]static[ ]unsigned[ ]char[ ]table_ulaw2alaw\[\][ ]=' drivers/staging/telephony/ixj.c
    defsnc '[	]\(static[ ]const[ ]\)\?u32[ ]reg_boundaries\[\][ ]=' drivers/net/bnx2.c
    defsnc '[	]u8[ ]b\[\][ ]=' drivers/media/usb/ttusb-dec/ttusbdecfe.c
    initnc '[	]uint8_t[ ]tx\[\][ ]='
    defsnc '[	]unsigned[ ]char[ ]saa7111_regs\[\][ ]=' drivers/media/parport/w9966.c
    initnc '[	]unsigned[ ]char[ ]sas_pcd_m_pg\[\][ ]='
    initnc '[	][}][ ]modedb\[5\][ ]='
    defsnc '[	][}][ ]reg_tbl\[\][ ]=' drivers/net/bnx2.c
    initnc '[	][}][ ]vals\[\][ ]='
    initnc '[	][}][ ]vm_devices\[\][ ]='
    initnc '[ ][ ][ ][ ]static[ ]const[ ]code[ ]distfix\[32\][ ]='
    initnc '[ ][ ][ ][ ]static[ ]const[ ]code[ ]lenfix\[512\][ ]='
    defsnc '[ ][ ]int[ ]poly\[\]=' drivers/net/pcmcia/nmclan_cs.c
    defsnc '[ ][ ]static[ ]const[ ]unsigned[ ]char[ ]asso_values\[\][ ]=' scripts/genksyms/keywords.c_shipped
    defsnc '[ ][ ]static[ ]unsigned[ ]char[ ]asso_values\[\][ ]=' scripts/kconfig/zconf.hash.c_shipped
    initnc '[ ][ ][}][ ]cards_ds\[\][ ]='
    initnc '[ ][ ][ ][ ]static[ ]const[ ]int8[ ]countLeadingZerosHigh\[\][ ]='
    initnc '[ ][ ][ ][ ]static[ ]const[ ]unsigned[ ]short[ ]d\(base\|ext\)\[32\][ ]='
    initnc '#define[ ]OV511_QUANTABLESIZE[	]64'
    initnc 'BYTE[ ]BtCard::SRAMTable_\(NTSC\|PAL\)\[\][ ]='
    initnc 'BYTE[ ]SRAMTable\[\]\[[ ]60[ ]\][ ]='
    accept 'irq_prio_\([hdl]\|l[cd]\):'"$sepx$blobpat*" 'arch/arm/inlcude/asm/hardware/entry-macro-iomd.S|include/asm-arm/hardware/entry-macro-iomd.S'
    initc '__u8[ ]_ascebc\[256\][ ]='
    initc '__u8[ ]_ebc_tolower\[256\][ ]='
    initc '__u8[ ]_ebc_toupper\[256\][ ]='
    initnc 'adapter_tag_info_t[ ]aic7[9x]xx_tag_info\[\][ ]='
    initnc 'char[ ]dmasound_alaw2dma8\[\][ ]='
    initnc 'char[ ]dmasound_ulaw2dma8\[\][ ]='
    initnc 'const[ ]struct[ ]aper_size_info_16[ ]agp3_generic_sizes\[AGP_GENERIC_SIZES_ENTRIES\][ ]='
    initnc 'const[ ]u16[ ]crc_itu_t_table\[256\][ ]='
    initnc 'const[ ]u8[ ]byte_rev_table\[256\][ ]='
    initnc 'const[ ]u8[ ]crc7_syndrome_table\[256\][ ]='
    initnc 'int[ ]snd_sf_vol_table\[128\][ ]='
    initnc 'static[	]u_char[	]irq_to_siubit\[\][ ]='
    initnc 'static[	]u_char[	]irq_to_siureg\[\][ ]='
    defsnc 'static[ ]Byte_t[ ]RData\[RDATASIZE\][ ]=' drivers/tty/rocket.c
    initnc 'static[ ]__const__[ ]__u16[ ]gx_coeff\[256\][ ]='
    defsnc 'static[ ]__u8[ ]init7121ntsc\[\][ ]=' drivers/media/video/saa7121.h
    defsnc 'static[ ]__u8[ ]init7121pal\[\][ ]=' drivers/media/video/saa7121.h
    defsnc 'static[ ]byte[ ]capidtmf_leading_zeroes_table\[0x100\][ ]=' drivers/isdn/hardware/eicon/capidtmf.c
    defsnc 'static[ ]char[ ]channel_map_madi_[sdq]s\[HDSPM_MAX_CHANNELS\][ ]=' sound/pci/rme9652/hdspm.c
    initnc 'static[ ]char[ ]coefficients\[NM_TOTAL_COEFF_COUNT[ ][*][ ]4\][ ]='
    initnc 'static[ ]char[ ]ecc_syndrome_table\[\][ ]='
    initnc 'static[ ]char[ ]isdn_audio_alaw_to_ulaw\[\][ ]='
    initnc 'static[ ]char[ ]isdn_audio_ulaw_to_alaw\[\][ ]='
    initnc 'static[ ]char[ ]mix_cvt\[101\][ ]='
    initnc 'static[ ]char[ ]opl3_volume_table\[128\][ ]='
    initnc 'static[ ]const[ ]__u16[ ]crc10_table\[256\][ ]='
    initnc 'static[ ]const[ ]__u32[ ]crc_c\[256\][ ]='
    defsnc 'static[ ]const[ ]fixp_t[ ]cos_table\[46\][ ]=' include/linux/fixp-arith.h
    initnc 'static[ ]const[ ]int[ ]init_seq\[\][ ]='
    initnc 'static[ ]const[ ]int[ ]mobile_vid_table\[32\][ ]='
    initnc 'static[ ]const[ ]s16[ ]snd_opl4_pitch_map\[0x600\][ ]='
    initnc 'static[ ]const[ ]s8[ ]budtab\[256\][ ]='
    initnc 'static[ ]const[ ]struct[ ]aper_size_info_8[ ]via_generic_sizes\[9\][ ]='
    initnc 'static[ ]const[ ]struct[ ]color[ ]clut_vga16\[16\][ ]='
    defsnc 'static[ ]const[ ]struct[ ]gain_entry[ ]gain_table\[2\]\[108\][ ]=' drivers/net/wireless/iwl-4965.c
    defsnc 'static[ ]const[ ]struct[ ]mV_pos[ ]__\(cpu\)\?initdata[ ]mobilevrm_mV\[32\][ ]=' arch/x86/kernel/cpu/cpufreq/longhaul.h
    defsnc 'static[ ]const[ ]struct[ ]mV_pos[ ]__\(cpu\)\?initdata[ ]vrm85_mV\[32\][ ]=' arch/x86/kernel/cpu/cpufreq/longhaul.h
    initnc 'static[ ]const[ ]struct[ ]menelaus_vtg_value[ ]vcore_values\[\][ ]='
    initnc 'static[ ]const[ ]struct[ ]opl4_region[ ]regions_[0-9a-frums]*\[\][ ]='
    initnc 'static[ ]const[ ]struct[ ]regval[ ]regval_table\[\][ ]='
    initnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_5222\[\][ ]='
    initnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_5225_2527\[\][ ]='
    initnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_5226\[\][ ]='
    initnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_bg\[\][ ]='
    initnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_bg_2522\[\][ ]='
    initnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_bg_2523\[\][ ]='
    initnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_bg_2524\[\][ ]='
    initnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_bg_2525\[\][ ]='
    initnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_bg_2525e\[\][ ]='
    initnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_bg_2528\[\][ ]='
    initnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_noseq\[\][ ]='
    initnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_seq\[\][ ]='
    defsnc 'static[ ]const[ ]u16[ ]Sbox\[256\][ ]=' # 'drivers/staging/rtl8192u/r819xU_firmware.c' and elsewhere
    initnc 'static[ ]const[ ]u16[ ]count_lut\[\][ ]=' drivers/misc/tsl2550.c
    defsnc 'static[ ]const[ ]u16[ ]e1000_igp_2_cable_length_table\[\][ ]=' drivers/net/e1000e/phy.c
    defsnc 'static[ ]const[ ]u16[ ]rtl8225\(bcd\|z2\)_rxgain\[\][ ]=' 'drivers/net/wireless/rtl818x/rtl818[07]/rtl8225\.c'
    defsnc 'static[ ]const[ ]u16[ ]stufftab\[5[ ][*][ ]256\][ ]=' drivers/isdn/gigaset/isocdata.c
    initnc 'static[ ]const[ ]u16[ ]tkip_sbox\[256\][ ]='
    defsnc 'static[ ]const[ ]u16[ ]wm8753_reg\[\][ ]=' sound/soc/codecs/wm8753.c
    initnc 'static[ ]const[ ]u32[ ]SS[0-3]\[256\][ ]='
    initnc 'static[ ]const[ ]u32[ ]S[1-8]\[64\][ ]='
    initnc 'static[ ]const[ ]u32[ ]T[0-5]\[256\][ ]='
    defsnc 'static[ ]const[ ]u32[ ]Tm\[24\]\[8\][ ]=' crypto/cast6_generic.c
    initnc 'static[ ]const[ ]u32[ ]bass_table\[41\]\[5\][ ]='
    initnc 'static[ ]const[ ]u32[ ]bf_sbox\[256[ ][*][ ]4\][ ]='
    defsnc 'static[ ]const[ ]u32[ ]camellia_sp0222\[256\][ ]=' crypto/camellia.c
    defsnc 'static[ ]const[ ]u32[ ]camellia_sp1110\[256\][ ]=' crypto/camellia.c
    defsnc 'static[ ]const[ ]u32[ ]camellia_sp3033\[256\][ ]=' crypto/camellia.c
    defsnc 'static[ ]const[ ]u32[ ]camellia_sp4404\[256\][ ]=' crypto/camellia.c
    defsnc 'static[ ]const[ ]u32[ ]crc32c_table\[256\][ ]=' crypto/crc32c.c
    initnc 'static[ ]const[ ]u32[ ]db_table\[101\][ ]='
    initnc 'static[ ]const[ ]u32[ ]m8xx_size_to_gray\[M8XX_SIZES_NO\][ ]='
    initnc 'static[ ]const[ ]u32[ ]mds\[4\]\[256\][ ]='
    initnc 'static[ ]const[ ]u32[ ]pc2\[1024\][ ]='
    defsnc 'static[ ]const[ ]u32[ ]s[1-7]\[256\][ ]=' crypto/cast5_generic.c
    defsnc 'static[ ]const[ ]u32[ ]sb8\[256\][ ]=' crypto/cast5_generic.c
    initnc 'static[ ]const[ ]u32[ ]tfrc_calc_x_lookup\[TFRC_CALC_X_ARRSIZE\]\[2\][ ]='
    initnc 'static[ ]const[ ]u32[ ]treble_table\[41\]\[5\][ ]='
    initnc 'static[ ]const[ ]u64[ ][CT][0-7]\[256\][ ]='
    initnc 'static[ ]const[ ]u64[ ]sbox[1-4]\[256\][ ]='
    initnc 'static[ ]const[ ]u64[ ]sha512_K\[80\][ ]=' 'crypto/sha512\(_generic\)\?.c'
    defsnc 'static[ ]const[ ]u8[ ]Tr\[4\]\[8\][ ]=' crpto/cast6_generic.c
    initnc 'static[ ]const[ ]u8[ ]aes_sbox\[256\][ ]='
    initnc 'static[ ]const[ ]u8[ ]calc_sb_tbl\[512\][ ]='
    initnc 'static[ ]const[ ]u8[ ]exp_to_poly\[492\][ ]='
    initnc 'static[ ]const[ ]u8[ ]legal_ansi_char_array\[0x40\][ ]='
    initnc 'static[ ]const[ ]u8[ ]parity\[\][ ]='
    initnc 'static[ ]const[ ]u8[ ]pc1\[256\][ ]='
    initnc 'static[ ]const[ ]u8[ ]poly_to_exp\[255\][ ]='
    initnc 'static[ ]const[ ]u8[ ]q[01]\[256\][ ]='
    defsnc 'static[ ]const[ ]u8[ ]ratio_lut\[\][ ]=' drivers/misc/tsl2550.c
    initnc 'static[ ]const[ ]u8[ ]rs\[256\][ ]='
    defsnc 'static[ ]const[ ]u8[ ]rtl8225_\(agc\|tx_\(power\|gain\)_cck\(_ch14\|_ofdm\)\?\)\[\][ ]=' 'drivers/net/wireless/rtl818x/rtl818[07]/rtl8225\.c'
    initnc 'static[ ]const[ ]u_char[ ]irq_to_siubit\[\][ ]='
    initnc 'static[ ]const[ ]u_char[ ]irq_to_siureg\[\][ ]='
    initnc 'static[ ]const[ ]uint8_t[ ]parity\[256\][ ]='
    initnc 'static[ ]const[ ]unsigned[ ]char[ ]\(UV\|Y\)_QUANTABLE\[64\][ ]='
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]__\(cpu\)\?initdata[ ]mV_mobilevrm\[32\][ ]=' arch/x86/kernel/cpu/cpufreq/longhaul.h
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]__\(cpu\)\?initdata[ ]mV_vrm85\[32\][ ]=' arch/x86/kernel/cpu/cpufreq/longhaul.h
    initnc 'static[ ]const[ ]unsigned[ ]char[ ]barco_p1\[2\]\[9\]\[7\]\[3\][ ]='
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]bitcounts\[256\][ ]=' drivers/isdn/gigaset/isocdata.c
    initnc 'static[ ]const[ ]unsigned[ ]char[ ]blue\[256\][ ]='
    initnc 'static[ ]const[ ]unsigned[ ]char[ ]chktab[hl]\[256\][ ]='
    initnc 'static[ ]const[ ]unsigned[ ]char[ ]comet_miireg2offset\[32\][ ]='
    initnc 'static[ ]\(const[ ]\)\?unsigned[ ]char[ ]euc2sjisibm_g3upper_map\[\]\[2\][ ]='
    initnc 'static[ ]const[ ]unsigned[ ]char[ ]green\[256\][ ]='
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]hash_table_ops\[64[*]4\][ ]=' drivers/media/usb/pwc/pwc-dec23.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]hid_keyboard\[256\][ ]=' drivers/hid/hid-input.c
    initnc 'static[ ]const[ ]unsigned[ ]char[ ]mts_direction\[256[/]8\][ ]='
    initnc 'static[ ]const[ ]unsigned[ ]char[ ]red\[256\][ ]='
    initnc 'static[ ]\(const[ ]\)\?unsigned[ ]char[ ]sjisibm2euc_map\[\]\[2\][ ]='
    initnc 'static[ ]const[ ]unsigned[ ]char[ ]vol_cvt_datt\[128\][ ]='
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]MulIdx\[16\]\[16\][ ]=' drivers/media/usb/pwc/pwc-dec23.c
    initnc 'static[ ]const[ ]unsigned[ ]int[ ]crctab32\[\][ ]='
    initnc 'static[ ]const[ ]unsigned[ ]short[ ]crc_flex_table\[\][ ]='
    defsnc 'static[ ]const[ ]unsigned[ ]short[ ]logtable\[256\][ ]=' drivers/media/dvb-core/dvb_math.c
    initnc 'static[ ]const[ ]unsigned[ ]short[ ]wd7000_iobase\[\][ ]='
    defsnc 'static[ ]const[ ]unsigned[ ]short[ ]x86_keycodes\[256\][ ]=' drivers/tty/vt/keyboard.c
    initnc 'static[ ]const[ ]unsigned[ ]table\[\][ ]='
    initnc 'static[ ]int[ ]MV300_reg_8bit\[256\][ ]\?=' drivers/video/atafb.c
    defsnc 'static[ ]int[ ]fifo_map\[\]\[MAX_TX_FIFOS\][ ]=' drivers/net/s2io.h
    initnc 'static[ ]int[ ]initial_lfsr\[\][ ]='
    initnc 'static[ ]int[ ]log_tbl\[129\][ ]='
    initnc 'static[ ]int[ ]miro_fmtuner\[\][ ][ ]=' drivers/media/video/bt8xx/bt-cards.c
    initnc 'static[ ]int[ ]miro_tunermap\[\][ ]=' drivers/media/video/bt8xx/bt-cards.c
    initnc 'static[ ]int[ ]register_size\[\][ ]='
    initnc 'static[ ]int[ ]reserve_list\[MAX_RES_ARGS\][ ]='
    initnc 'static[ ]int[ ]reverse6\[64\][ ]='
    initnc 'static[ ]short[ ]attack_time_tbl\[128\][ ]='
    defsnc 'static[ ]short[ ]beep_wform\[256\][ ]=' 'sound/ppc/beep.c|sound/oss/dmasound/dmasound_awacs.c|arch/ppc/8xx_io/cs4218_tdm.c'
    initnc 'static[ ]short[ ]decay_time_tbl\[128\][ ]='
    initnc 'static[ ]short[ ]isdn_audio_[ua]law_to_s16\[\][ ]='
    defsnc 'static[ ]struct[ ]iw\?l\(3945\)\?_tx_power[ ]power_gain_table\[2\]\[IW\?L_MAX_GAIN_ENTRIES\][ ]=' drivers/net/wireless/iwlegacy/iwl-3945.c
    initnc 'static[ ]struct[ ]ovcamchip_regvals[ ]regvals_init_\(76be\|7[16]20\|7x10\)\[\][ ]='
    initnc 'static[ ]struct[ ]regval_list[ ]ov7670_default_regs\[\][ ]=' drivers/media/i2c/ov7670.c
    initnc 'static[ ]struct[ ]s_c2[ ]SetRate48000\[\][ ]='
    initnc 'static[ ]struct[ ]tea6420_multiplex[ ]TEA6420_line\[MXB_AUDIOS[+]1\]\[2\][ ]='
    initnc 'static[ ]struct[ ]wm_info[ ]i810_wm_16_100\[\][ ]='
    initnc 'static[ ]struct[ ]wm_info[ ]i810_wm_16_133\[\][ ]='
    initnc 'static[ ]struct[ ]wm_info[ ]i810_wm_24_100\[\][ ]='
    initnc 'static[ ]struct[ ]wm_info[ ]i810_wm_24_133\[\][ ]='
    initnc 'static[ ]struct[ ]wm_info[ ]i810_wm_8_100\[\][ ]='
    initnc 'static[ ]struct[ ]wm_info[ ]i810_wm_8_133\[\][ ]='
    initnc 'static[ ]struct[ ][{][ ]struct[ ]fb_bitfield[ ]red,[ ]green,[ ]blue,[ ]transp[;][ ]int[ ]bits_per_pixel[;][ ][}][ ]colors\[\][ ]='
    initnc 'static[ ]u16[ ]asEqCoefsPipes\[64\][ ]='
    initnc 'static[ ]u16[ ]asEqCoefsZeros\[50\][ ]='
    initnc 'static[ ]u16[ ]asEqOutStateZeros\[48\][ ]='
    defsnc 'static[ ]u16[ ]default_key_map[ ]\[256\][ ]=' drivers/media/pci/ttpci/av7110_ir.c
    initnc 'static[ ]u16[ ]eq_levels\[64\][ ]='
    initnc 'static[ ]u32[ ][ ]crc32tab\[\][ ]__attribute__[ ][(][(]aligned[(]8[)][)][)][ ]='
    defsnc 'static[ ]u32[ ]ac3_frames\[3\]\[32\][ ]=' drivers/media/dvb-core/dvb_filter.c
    initnc 'static[ ]u32[ ]adwDecim8\[33\][ ]='
    initnc 'static[ ]u32[ ]h_prescale\[64\][ ]='
    initnc 'static[ ]u32[ ]v_gain\[64\][ ]='
    defsnc 'static[ ]u8[ ]SRAM_Table\[\]\[60\][ ]=' drivers/media/pci/bt8xx/bttv-driver.c
    defsnc 'static[ ]u8[ ]alps_tdee4_stv0297_inittab\[\][ ]=' drivers/media/common/b2c2/flexcop-fe-tuner.c
    defsnc 'static[ ]u8[ ]bnx2_570[68]_stats_len_arr\[BNX2_NUM_STATS\][ ]=' drivers/net/bnx2.c
    initnc 'static[ ]u8[ ]flit_desc_map\[\][ ]='
    defsnc 'static[ ]\(const[ ]\)\?u8[ ]init_tab[ ]\?\[\][ ]=' 'drivers/media/dvb/frontends/cx2270\(0\|2\)\.c'
    defsnc 'static[ ]u8[ ]mac_reader\[\][ ]=' drivers/net/wireless/atmel.c
    initnc 'static[ ]u8[ ]mt2131_config1\[\][ ]=' drivers/media/dvb/frontends/mt2131.c # <= 2.6.25
    initnc 'static[ ]u8[ ]mt2131_config1\[\][ ]=' drivers/media/common/tuners/mt2131.c # >= 2.6.26
    initnc 'static[ ]u8[ ]mt2266_init2\[\][ ]=' drivers/media/dvb/frontends/mt2266.c # <= 2.6.25
    initnc 'static[ ]u8[ ]mt2266_init2\[\][ ]=' drivers/media/common/tuners/mt2266.c # >= 2.6.26
    defsnc 'static[ ]u8[ ]opera1_inittab\[\][ ]=' drivers/media/usb/dvb-usb/opera1.c
    defsnc 'static[ ]u8[ ]saa7113_init_regs\[\][ ]=' drivers/media/pci/ttpci/av7110_v4l.c
    defsnc 'static[ ]u8[ ]samsung_tbmu24112_inittab\[\][ ]=' drivers/media/common/b2c2/flexcop-fe-tuner.c
    defsnc 'static[ ]u8[ ]w1_crc8_table\[\][ ]=' drivers/w1/w1_io.c
    initnc 'static[ ]u_char[ ]const[ ]data_sizes_32\[32\][ ]='
    initnc 'static[ ]u_long[ ]ident_map\[32\][ ]='
    initnc 'static[ ]u_short[ ]alt_map\[NR_KEYS\][ ]='
    initnc 'static[ ]u_short[ ]altgr_map\[NR_KEYS\][ ]='
    initnc 'static[ ]u_short[ ]ctrl_alt_map\[NR_KEYS\][ ]='
    initnc 'static[ ]u_short[ ]ctrl_map\[NR_KEYS\][ ]*='
    initnc 'static[ ]u_short[ ]shift_ctrl_map\[NR_KEYS\][ ]='
    initnc 'static[ ]u_short[ ]shift_map\[NR_KEYS\][ ]*='
    initnc 'static[ ]uchar[ ]perm1\[56\][ ]='
    initnc 'static[ ]uchar[ ]perm2\[48\][ ]='
    initnc 'static[ ]uchar[ ]perm3\[64\][ ]='
    initnc 'static[ ]uchar[ ]perm4\[48\][ ]='
    initnc 'static[ ]uchar[ ]perm5\[32\][ ]='
    initnc 'static[ ]uchar[ ]perm6\[64\][ ]='
    initnc 'static[ ]uchar[ ]sbox\[8\]\[4\]\[16\][ ]='
    initnc 'static[ ]uint16_t[ ]crc_table\[256\][ ]='
    initnc 'static[ ]uint8_t[ ]lpfcAlpaArray\[\][ ]='
    initnc 'static[ ]\(const[ ]\)\?uint8_t[ ]seqprog\[\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]V110_OffMatrix_9600\[\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]V110_OnMatrix_9600\[\][ ]='
    defsnc 'static[ ]unsigned[ ]char[ ]a2232_65EC02code\[\][ ]=' drivers/staging/generic_serial/ser_a2232fw.h
    initnc 'static[ ]unsigned[ ]char[ ]atkbd_set3_keycode\[512\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]atkbd_unxlate_table\[128\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]banner_table\[\][ ]=' arch/sh/boards/superh/microdev/led.c
    defsnc '\(static[ ]\)\?unsigned[ ]char[ ]\(__attribute__[ ][(][(]aligned[(]16[)][)][)][ ]\)\?bootlogo_bits\[\][ ]=' arch/m68k/platform/68328/bootlogo.h
    initnc 'static[ ]unsigned[ ]char[ ]bus2core_8260\[\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]bus2core_8280\[\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]caseorder\[256\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]crystal_key\[\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]dsp_ulaw\[\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]expressiontab\[128\][ ]='
    defsnc 'static[ ]unsigned[ ]char[ ]header2\[\][ ]=' drivers/media/usb/zr364xx/zr364xx.c
    initnc 'static[ ]unsigned[ ]char[ ]hidp_keycode\[256\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]nkbd_keycode\[128\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]pan_volumes\[256\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]parm_block\[32\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]raw3270_ebcgraf\[64\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]rfcomm_crc_table\[256\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]rwa_unlock\[\][ ]__initdata[ ]='
    initnc 'static[ ]unsigned[ ]char[ ]seqprog\[\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]snd_opl4_volume_table\[128\][ ]='
    defsnc 'static[ ]unsigned[ ]char[ ]splash_bits\[\][ ]=' arch/m68k/platform/68EZ328/bootlogo.h
    initnc 'static[ ]unsigned[ ]char[ ]sunkbd_keycode\[128\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]ufs_fragtable_8fpb\[\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]ufs_fragtable_other\[\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]ulaw_dsp\[\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]usb_kbd_keycode\[256\][ ]='
    defsnc 'static[ ]unsigned[ ]char[ ]vga_font\[cmapsz\][ ]\(BTDATA[ ]\)\?=' arch/sparc/kernel/btext.c
    initnc 'static[ ]unsigned[ ]char[ ]voltab[12]\[128\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]vpd89_data\[\][ ]='
    initnc 'static[ ]unsigned[ ]char[ ]xtkbd_keycode\[256\][ ]='
    defsnc 'static[ ]unsigned[ ]int[ ]ac3_bitrates\[32\][ ]=' drivers/media/dvb-core/dvb_filter.c
    initnc 'static[ ]unsigned[ ]int[ ]bass_volume_table\[\][ ]='
    defsnc 'static[ ]unsigned[ ]int[ ]bitrates\[3\]\[16\][ ]=' drivers/media/dvb-core/dvb_filter.c
    initnc 'static[ ]unsigned[ ]int[ ]isa_dma_port\[8\]\[7\][ ]='
    initnc 'static[ ]unsigned[ ]int[ ]master_volume_table\[\][ ]='
    initnc 'static[ ]unsigned[ ]int[ ]mixer_volume_table\[\][ ]='
    initnc 'static[ ]unsigned[ ]int[ ]pan_table\[63\][ ]='
    initnc 'static[ ]unsigned[ ]int[ ]snapper_bass_volume_table\[\][ ]='
    initnc 'static[ ]unsigned[ ]int[ ]snapper_treble_volume_table\[\][ ]='
    initnc 'static[ ]unsigned[ ]int[ ]treble_volume_table\[\][ ]='
    initnc 'static[ ]unsigned[ ]int[ ]valid_mem\[\][ ]='
    initnc 'static[ ]unsigned[ ]long[ ]arthur_to_linux_signals\[32\][ ]='
    defsnc 'static[ ]unsigned[ ]long[ ]shmedia_opcode_table\[64\][ ]=' arch/sh/kernel/traps_64.c
    initnc 'static[ ]unsigned[ ]nv\([34]\|10\)TableP\(FIFO\|GRAPH\|RAMIN\)\[\]\[2\][ ]='
    initnc 'static[ ]unsigned[ ]short[ ]fcstab\[256\][ ]='
    initnc 'static[ ]unsigned[ ]short[ ]init[1234]\[128\][ ][/][*]__devinitdata[*][/][ ]='
    initnc 'static[ ]unsigned[ ]short[ ]log_table\[LOG_TABLE_SIZE[*]2\][ ]='
    defsnc 'static[ ]unsigned[ ]short[ ]rc_ioport\[\][ ]=' drivers/staging/tty/riscom8.c
    defsnc 'static[ ]unsigned[ ]short[ ]translations\[\]\[256\][ ]=' drivers/tty/vt/consolemap.c
    initnc 'static[ ]unsigned[ ]short[ ]treble_parm\[12\]\[9\][ ]='
    initnc 'struct[ ]RGBColors[ ]TextCLUT\[256\][ ]='
    initnc 'struct[ ]VgaRegs[ ]GenVgaTextRegs\[NREGS[+]1\][ ]='
    defsnc 'struct[ ]battery_thresh[ ][ ]*\(spitz\|sharpsl\)_battery_levels_\(noac\|acin\)\[\][ ]=' arch/arm/mach-pxa/sharpsl_pm.c
    initnc 'struct[ ]fb_bitfield[ ]rgb_bitfields\[\]\[4\][ ]='
    initnc 'struct[ ]mode_registers[ ]std_modes\[\][ ]='
    initnc 'struct[ ]vmode_attr[ ]vmode_attrs\[VMODE_MAX\][ ]='
    initnc 'u16[ ]const[ ]crc16_table\[256\][ ]='
    initnc 'u16[ ]const[ ]crc_ccitt_table\[256\][ ]='
    initnc 'u16[ ]hfsplus_compose_table\[\][ ]='
    initnc 'u16[ ]hfsplus_decompose_table\[\][ ]='
    initnc 'u_char[ ]const[ ]data_sizes_16\[32\][ ]='
    defsnc 'u_short[ ]\(plain\|shift\(_ctrl\)\?\|alt\(gr\)\?\|ctrl\(_alt\)\?\)_map\[NR_KEYS\][ ]*=' drivers/tty/vt/defkeymap.c_shipped
    initnc '\(uint16_t\|u16\)[ ]e1000_igp_cable_length_table\[IGP01E1000_AGC_LENGTH_TABLE_SIZE\][ ]=' drivers/net/e1000/e1000_hw.c # u16 on 2.6.26
    initnc '\(uint16_t\|u16\)[ ]e1000_igp_2_cable_length_table\[IGP02E1000_AGC_LENGTH_TABLE_SIZE\][ ]=' drivers/net/e1000/e1000_hw.c # u16 on 2.6.26
    initnc '[}][ ]euc2sjisibm_jisx0212_map\[\][ ]='
    initnc '[}][ ]freq\[\][ ]='
    defsnc '[}][ ]hps_h_coeff_tab[ ]\[\][ ]=' drivers/media/common/saa7146/saa7146_hlp.c
    defsnc '[}][ ]hps_v_coeff_tab[ ]\[\][ ]=' drivers/media/common/saa7146/saa7146_hlp.c
    defsnc '[}][ ]init_tab\[\][ ]=' drivers/media/dvb-frontends/s5h1409.c
    initnc '[}][ ]maven_gamma\[\][ ]='
    defsnc '[}][ ]mem_table\[\][ ]=' drivers/net/ethernet/8390/smc-mca.c
    defsnc '[}][ ]mxb_saa7740_init\[\][ ]=' drivers/media/pci/saa7146/mxb.c
    initnc '[}][ ]pll_table\[\][ ]=' drivers/video/geode/lxfb_ops.c
    defsnc '[}][ ]qam256_snr_tab\[\][ ]=' drivers/media/dvb-frontends/s5h1409.c
    defsnc '[}][ ]qam64_snr_tab\[\][ ]=' drivers/media/dvb-frontends/s5h1409.c
    initnc '[}][ ]sil_port\[\][ ]='
    defsnc '[}][ ]vsb_snr_tab\[\][ ]=' drivers/media/dvb-frontends/s5h1409.c

    # new in 2.6.30
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]sync\[\][ ]=' Documentation/networking/timestamping/timestamping.c
    blob 'The[ ]driver[ ]requires[ ]firmware[ ]files[ ]["]turtlebeach\([^\n]*[^\n.][\n]\)*directory.' Documentation/sound/alsa/ALSA-Configuration.txt
    defsnc 'static[ ]int[ ]sdp3430_batt_table\[\][ ]=' arch/arm/mach-omap2/board-3430sdp.c
    defsnc 'const[ ]char[ ]_[zs]b_findmap\[\][ ]=' arch/s390/kernel/bitmap.c
    initnc '[	][{][ ]CnINT2MSKR0,[ ]CnINT2MSKCR0[ ],[ ]32,' arch/sh/kernel/cpu/sh4a/setup-sh7786.c
    blobname 'solos-\(\(db-\)\?FPGA\|Firmware\)\.bin' drivers/atm/solos-pci.c
    defsnc 'static[ ]u16[ ]__initdata[ ]i2c_clk_div\[50\]\[2\][ ]=' drivers/i2c/busses/i2c-imx.c
    defsnc 'static[ ]const[ ]struct[ ]mpc_i2c_divider[ ]mpc_i2c_dividers_\(52xx\|8xxx\)\[\][ ]\(__devinitconst[ ]\)\?=' drivers/i2c/busses/i2c-mpc.c
    accept '[	]const[ ]char[ ]\*fw_name[ ]=[ ]["]av7110[/]bootcode\.bin["][;]' drivers/media/dvb/ttpci/av7110_hw.c
    accept '[	]ret[ ]=[ ]request_firmware[(][^;]*[)][;][\n][	]if[ ][(]ret[)][ ][{][^}]*[}][\n][\n][	]mwdebi[(]av7110,[ ]DEBISWAB,[ ]DPRAM_BASE' drivers/media/dvb/ttpci/av7110_fw.c
    accept 'MODULE_FIRMWARE[(]["]av7110[/]bootcode\.bin["][)][;]' drivers/media/dvb/ttpci/av7110_fw.c
    defsnc 'static[ ]const[ ]u8[ ]jpeg_head\[\][ ]=' drivers/media/video/gspca/jpeg.h
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]nand_oob_128[ ]=' drivers/mtd/nand/nand_base.c
    blobname 'bnx2[/]bnx2-\(mips\|rv2p\)-[-0-9a-z.]*\.fw' drivers/net/bnx2.c
    accept 'static[ ]void[\n]load_rv2p_fw[(][^{)]*const[ ]struct[ ]bnx2_mips_fw_file_entry' drivers/net/bnx2.c
    accept 'static[ ]int[\n]bnx2_init_cpus[(][^{]*[)][\n][{][\n][	]const[ ]struct[ ]bnx2_mips_fw_file'
    blobname 'yam[/]\(12\|96\)00\.bin' drivers/net/hamradio/yam.c
    blobname 'myricom[/]lanai\.bin' drivers/net/myri_sbus.c
    blobname '3com[/]3C359\.bin' drivers/net/tokenring/3c359.c
    blobname '3com[/]typhoon\.bin' drivers/net/typhoon.c
    defsnc 'static[ ]struct[ ]ar9170_phy_init[ ]ar5416_phy_init\[\][ ]=' drivers/net/wireless/ar9170/phy.c
    defsnc 'static[ ]struct[ ]ar9170_rf_init[ ]ar9170_rf_init\[\][ ]=' drivers/net/wireless/ar9170/phy.c
    defsnc 'static[ ]const[ ]struct[ ]ar9170_phy_freq_entry[ ]ar9170_phy_freq_params\[\][ ]=' drivers/net/wireless/ar9170/phy.c
    accept 'static[ ]int[ ]ar9170_usb_request_firmware[(]' drivers/net/wireless/ar9170/usb.c
    accept '[	]\(err[ ]=\|return\)[ ]request_firmware\(_nowait\)\?[(][^\n]*["]ar9170\(-[12]\)\?\.fw["],' drivers/net/wireless/ar9170/usb.c
    accept '[	]err[ ]=[ ]ar9170_usb_request_firmware[(]' drivers/net/wireless/ar9170/usb.c
    accept 'MODULE_FIRMWARE[(]["]ar9170\(-[12]\)\?\.fw["][)][;]\([\n]MODULE_FIRMWARE[(]["]ar9170\(-[12]\)\?\.fw["][)][;]\)*' drivers/net/wireless/ar9170/usb.c
    blobname 'slicoss[/]\(oasis\|gb\)\(rcvucode\|download\)\.sys' drivers/staging/slicoss/slicoss.c
    blobname 'sxg[/]sahara\(dbg\)\?downloadB\.sys' drivers/staging/sxg/sxg.c
    blobname 'qlogic[/]isp1000\.bin' drivers/scsi/qlogicpti.c
    blobname 'advansys[/]\(3550\|38C\(08\|16\)00\|mcode\)\.bin' drivers/scsi/advansys.c
    blobname 'qlogic[/]\(1040\|1280\|12160\)\.bin' drivers/scsi/qla1280.c
    blobname 'yamaha[/]yss225_registers\.bin' sound/isa/wavefront/wavefront_fx.c
    defsnc 'static[ ]const[ ]struct[ ]ath5k_ini[ ]rf\([52]413\|2425\)_ini_common_end\[\][ ]=' drivers/net/wireless/ath5k/initvals.c
    defsnc 'static[ ]const[ ]struct[ ]ath5k_ini_rfbuffer[ ]rfb_\(511[12]a\?\|5413\|231[67]\|24\(1[37]\|25\)\)\[\][ ]=' drivers/net/wireless/ath5k/rfbuffer.h
    accept '#define\([ ]_\?IWL\(4965\|[156]000\(G2[AB]\)\?\|1[03]0\|5150\|6050\)_MODULE_FIRMWARE[(]api[)]\)\+' 'drivers/net/iwlwifi/iwl-\([156]000\|4965\)\.c'
    blobname 'iwlwifi-1000-' drivers/net/iwlwifi/iwl-1000.c
    blobname 'iwlwifi-60[05]0-' drivers/net/iwlwifi/iwl-6000.c
    blobname 'libertas[/]gspi\(%d\|[0-9]\+\)\(_hlp\)\?\.bin' drivers/net/wireless/libertas/if_spi.c
    blobname 'mwl8k[/]\(helper\|fmimage\)_\(%u\|[0-9]\+\)\.fw' drivers/net/wireless/mwl8k.c
    blobname '3826\.arm' 'drivers/\(net/wireless/p54/p54spi\|staging/stlc45xx/stlc45xx\)\.c'
    defsnc 'static[ ]unsigned[ ]char[ ]p54spi_eeprom\[\][ ]=' drivers/net/wireless/p54/p54spi_eeprom.h
    blobname '\([/ ][*][ ]The[ ]DSP[ ]on[ ]the[ ]board[^"]*["]\)\?\(comedi[/]\)\?jr3pci\.idm\(["]\.[\n][ ][*][/]\)\?' drivers/staging/comedi/drivers/jr3_pci.c
    accept '#define[ ]USBDUX_FIRMWARE[ \t]*["]usbdux_firmware\.bin["]' drivers/staging/comedi/drivers/usbdux.c
    accept 'MODULE_FIRMWARE[(]USBDUX_FIRMWARE[)][;]' drivers/staging/comedi/drivers/usbdux.c
    accept '#define[ ]FIRMWARE[ \t]*["]usbduxfast_firmware\.bin["]' drivers/staging/comedi/drivers/usbduxfast.c
    accept 'MODULE_DESCRIPTION[(]["]USB-DUXfast[^"]*["][)][;][\n]MODULE_LICENSE[(]["]GPL["][)][;][\n]MODULE_FIRMWARE[(]FIRMWARE[)][;]' drivers/staging/comedi/drivers/usbduxfast.c
    blobname 'RT30xxEEPROM\.bin' drivers/staging/rt3070/common/eeprom.c
    defsnc 'static[ ]const[ ]u8[ ]default_cal_\(channels\|rssi\)\[\][ ]=' drivers/staging/stlc45xx/stlc45xx.c
    accept '[	][	]stlc45xx_error[(]["]request_firmware[(][)][ ]failed' drivers/staging/stlc45xx/stlc45xx.c
    blob 'static[ ]struct[ ]phy_ucode[	]PhyUcode\[\][ ]=[^;]*[;]' drivers/staging/sxg/sxgphycode-1.2.h
    accept 'device[ ]drivers[ ]which[ ]predate[ ]the[ ]common[ ]use[ ]of[ ]request_firmware[(][)]' firmware/README.AddingFirmware
    accept 'As[ ]we[ ]update[ ]those[ ]drivers[ ]to[ ]use[ ]request_firmware[(][)]' firmware/README.AddingFirmware
    blob 'This[ ]directory[ ]is[ ]_NOT_[ ]for[ ]adding[ ]arbitrary[ ]new[ ]firmware[ ]images.*git[ ]pull[ ]request[ ]to:[\n][^\n]*\(infradead\.org\|decadent\.org\.uk\)>' firmware/README.AddingFirmware
    blobna 'linux-firmware\.git' firmware/README.AddingFirmware
    blobname '\(ea[/]\)\?\(loader\|indigo_djx\)_dsp\.fw' sound/pci/echoaudio/indigodjx.c
    blobname '\(ea[/]\)\?\(loader\|indigo_iox\)_dsp\.fw' sound/pci/echoaudio/indigoiox.c
    # blobname 'cis[/]LA-PCM\.cis' drivers/net/pcmcia/pcnet_cs.c
    blobname 'ositech[/]Xilinx7OD\.bin' drivers/net/pcmcia/smc91c92_cs.c
    blobname 'tehuti[/]\(firmware\|bdx\)\.bin' drivers/net/tehuti.c
    accept '[ 	]*["]b43-open%s[/]%s\.fw["]' drivers/net/wireless/b43/main.c
    blobname '\(nx\(romimg\|3fw\(ct\|mn\)\)\|phanfw\)\.bin' 'drivers/net/netxen/netxen_nic\(_\(hw\|init\)\.c\|\.h\)'

    # New in 2.6.31
    accept '[ ][*][ ]page[ ]tables[ ]as[ ]follows:[\n][ ][*][\n][ ][*][ ][ ][ ]3[ ]3[ ]2[ ]2[ ]2[ ]2[ ]2[ ]2[ ]2[ ]2[ ]2[ ]2[ ]1[ ]1[ ]1[ ]1[ ]1[ ]1[ ]1[ ]1[ ]1[ ]1[\n][ ][*][ ][ ][ ]1[ ]0[ ]9[ ]8[ ]7[ ]6[ ]5[ ]4[ ]3[ ]2[ ]1[ ]0[ ]9[ ]8[ ]7[ ]6[ ]5[ ]4[ ]3[ ]2[ ]1[ ]0[ ]9[ ]8[ ]7[ ]6[ ]5[ ]4[ ]3[ ]2[ ]1[ ]0' arch/arm/include/asm/pgtable.h
    defsnc '\([	]static[ ]const[ ]u8[ ]snum_init\[\][ ]=[ ][{]\|static[ ]void[ ]qe_snums_init[(]void[)]\)[\n][	][	]0x04,[ ]0x05,' arch/powerpc/sysdev/qe_lib/qe.c
    accept '[.]LgoS4:[\n][	][.]word[	][.]LmtoS4-\.LgoS4\([\n][	]\.\(long\|word\|byte\)[	][01]\(,0\)*\)*' arch/s390/kernel/sclp.S
    defsnc 'static[ ]int[ ]sh_clk_div6_divisors\[64\][ ]=' '\(arch/sh/kernel/cpu/clock-\|drivers/sh/clk/\)cpg\.c'
    accept '[ ][*][ ]*1[ ]1\([ ]0\)*[ ]1\([ ]0\)*' arch/x86/lguest/boot.c
    defsnc 'struct[ ]scrubrate[ ]scrubrates\[\][ ]=' drivers/edac/amd64_edac.c
    defsnc 'static[ ]const[ ]unsigned[ ]r\([35]\|s6\)00_reg_safe_bm\[[0-9]*\][ ]=' 'drivers/gpu/drm/radeon/r\(300\|v515\|s600\)\.c'
    defsnc 'static[ ]struct[ ]keyboard_layout_map_t[ ]keyboard_layout_maps\[\][ ]=' drivers/media/dvb/siano/smsir.c
    blobname 'dvb-cx18-mpc718-mt352\.fw' drivers/media/video/cx18/cx18-dvb.c
    defsnc '[	]const[ ]unsigned[ ]char[ ]\(y\|uv\)QuanTable51[18]\[\][ ]=' 'drivers/media/video/\(ov511\|gspca/ov519\)\.c'
    defsnc 'static[ ]const[ ]u8[ ]bridge_start_ov965x_\(\([qs]\?v\|x\)ga\|cif\)\[\]\[2\][ ]=' drivers/media/video/gspca/ov534.c
    defsnc 'static[ ]const[ ]\(int\|s16\)[ ]hsv_\(red\|green\|blue\)_[xy]\[\][ ]=' drivers/media/video/gspca/sn9c20x.c
    defsnc 'static[ ]\(u16\|struct[ ]i2c_reg_u16\)[ ]\(bridge\|mt9\(v\(11[12]\|011\)\|m001\)\)_init\[\]\(\[2\]\)\?[ ]=' drivers/media/video/gspca/sn9c20x.c
    defsnc 'static[ ]\(u8\|struct[ ]i2c_reg_u8\)[ ]\(soi968\|ov\(76[67]0\|965[05]\)\|hv7131r\)_init\[\]\(\[2\]\)\?[ ]=' drivers/media/video/gspca/sn9c20x.c
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]onenand_oob_128[ ]=' drivers/mtd/onenand/onenand_base.c
    # Moved down to avoid shorter earlier match.
    # blob '#define[ ]BCM_5710_FW_\(\(MAJOR\|MINOR\|REVISION\|ENGINEERING\)_VERSION\|COMPILE_FLAGS\)[ 	]*[0-9]\+\([\n]#define[ ]BCM_5710_FW_\(\(MAJOR\|MINOR\|REVISION\|ENGINEERING\)_VERSION\|COMPILE_FLAGS\)[ 	]*[0-9]\+\)*' 'drivers/net/\(bnx2x[/]\)\?bnx2x_hsi\.h'
    blob 'static[ ]int[ ]\(__devinit[ ]\)\?bnx2x_check_firmware[(]struct[ ]bnx2x[ ][*]bp[)][\n][{][^\n]*\([\n]\+[^\n}][^\n]*\)*[\n]\+[}]' 'drivers/net/\(bnx2x[/]\)\?bnx2x_main\.c'
    blobna 'if[ ][(][(]fw_ver\[[0-3]\][ ]!=[ ]BCM_5710_FW_\(MAJOR\|MINOR\|REVISION\|ENGINEERING\)_VERSION[)]\([ ][|][|][\n][ 	]*[(]fw_ver\[[0-3]\][ ]!=[ ]BCM_5710_FW_\(MAJOR\|MINOR\|REVISION\|ENGINEERING\)_VERSION[)]\)*[)][ ][{][^{}]*[}]' 'drivers/net/\(bnx2x[/]\)\?bnx2x_main\.c'
    blobna 'sprintf[(]fw_file_name[ ][+][ ]offset,[ ]["]%d[.]%d[.]%d[.]%d[.]fw["]\(,[\n][ 	]*BCM_5710_FW_\(MAJOR\|MINOR\|REVISION\|ENGINEERING\)_VERSION\)*[)][;]' 'drivers/net/\(bnx2x[/]\)\?bnx2x_main\.c'
    blobna 'rc[ ]=[ ]bnx2x_check_firmware[(]bp[)][;]' 'drivers/net/\(bnx2x[/]\)\?bnx2x_main\.c'
    defsnc 'crb_128M_2M_map\[64\][ ]__cacheline_aligned_in_smp[ ]=' 'drivers/net/\(netxen/netxen_nic_hw.c\|qlcnic/qlcnic_hw.c\)'
    defsnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals\(_3070\)\?\[\][ ]=' 'drivers/net/wireless/\(prism54/islpci_dev\.c\|rt2x00/rt2800usb\.c\)'
    blobname 'wl1251-\(fw\|nvs\)\.bin' 'drivers/net/wireless/wl12\(51\|xx\)/wl1251.h'
    blobname 'iwmc3200wifi-\([ul]mac\|calib\)-sdio\.bin' drivers/net/wireless/iwmc3200wifi/sdio.c
    defsnc 'u16[ ]MCS_DATA_RATE\[2\]\[2\]\[77\][ ]=' 'drivers/staging/\(rtl8192su/ieee80211/rtl819x_HTProc\.c\|rtl8192u/r819xU_firmware\.c\)'
    blob 'u8[ ]Rtl8192SUFw\(Img\|Main\|Data\)Array\[\(Img\|Main\|Data\)ArrayLength\][ ]=[ ][{]'"$sepx$blobpat*$sepx"'[}][;]\([\n][\n]*u8[ ]Rtl8192SUFw\(Img\|Main\|Data\)Array\[\(Img\|Main\|Data\)ArrayLength\][ ]=[ ][{]'"$sepx$blobpat*$sepx"'[}][;]\)*' drivers/staging/rtl8192su/r8192SU_HWImg.c
    blobname 'RTL8192SU[/]\(rtl8192sfw\.bin\|\(boot\|main\|data\)\.img\)' drivers/staging/rtl8192su/r8192S_firmware.c
    blobna 'case[ ]FW_SOURCE_HEADER_FILE:[\n]#if[ ]1[\n]#define[^#]*[\n]#endif[\n][	][	][	]break[;]' drivers/staging/rtl8192su/r8192S_firmware.c
    defsnc 'u32[ ]Rtl8192SU\(PHY_\(REG\|ChangeTo\)_\([12]T[12]R\)\?\|Radio[AB]_\(\(\(to\)\?[12]T\|GM\)_\)\?\|MAC\(PHY\|_[12]T\)_\|AGCTAB_\)Array\(_PG\)\?\[\(PHY_\(REG\|ChangeTo\)_\([12]T[12]R\)\?\|Radio[AB]_\(\(\(to\)\?[12]T\|GM\)_\)\?\|MAC\(PHY\|_[12]T\)_\|AGCTAB_\)Array\(_PG\)\?Length\][ ]=' drivers/staging/rtl8192su/rtl92SU_HWImg.c
    blob 'u8[ ]Rtl8192PciEFw\(Boot\|Main\|Data\)ArrayDTM\[\(Boot\|Main\|Data\)ArrayLengthDTM\][ ]=[ ][{][^}]*[}][;]' drivers/staging/rtl8192su/r8192S_FwImgDTM.h
    defsnc '\(static[ ]\)\?u32[ ]Rtl8192PciE\(PHY_REG\(_1T2R\)\?\|\(Radio[ABCD]\|MACPHY\|AGCTAB\)_\)Array\(_PG\)\?\(DTM\)\?\[\(\(PHY_REG\(_1T2R\)\?\|\(Radio[ABCD]\|MACPHY\|AGCTAB\)_\)Array\(_PG\)\?Length\(DTM\)\?\)\?\][ ]=' drivers/staging/rtl8192su/rtl8192S_FwImgDTM.h
    blobna '\([&]\|sizeof[(]\)rtl8190_fw\(boot\|main\|data\)_array\(\[0\]\|[)]\)\(,[ 	\n]*\([&]\|sizeof[(]\)rtl8190_fw\(boot\|main\|data\)_array\(\[0\]\|[)]\)\)*' 'drivers/staging/rtl8192su/r819\(2S\|xU\)_firmware\.c'
    blobname 'RTL8192U[/]\(boot\|main\|data\)\.img' 'drivers/staging/rtl8192s\?u/r819xU_firmware\.c'
    blob 'u8[ ]rtl8190_fw\(boot\|main\|data\)_array\[\][ ]=[ ]\?[{][^}]*[}][;]' 'drivers/staging/rtl8192s\?u/r8192xU_firmware_img\.c'
    defsnc 'u32[ ]Rtl8192Usb\(PHY_REG\(_1T2R\)\?\|\(Radio[ABCD]\|MACPHY\|AGCTAB\)_\)Array\(_PG\)\?\[\][ ]=' drivers/staging/rtl8192su/rtl819xU_firmware_img.c
    defsnc 'BYTE[ ]\(sbox\|dot[23]\)_table\[256\][ ]=' drivers/staging/vt6655/aes_ccmp.c
    defsnc '\(BYTE\|unsigned[ ]char\)[ ]byVT3253\(InitTab\|B0\(_AGC4\?\)\?\)_\(RFMD\(2959\)\?\|AIROHA2230\|UW2451\|AGC\)\[CB_VT3253\(B0\(_AGC4\?\)\?\)\?\(\(_INIT\)\?_FOR_\(RFMD\(2959\)\?\|AIROHA2230\|UW2451\|AGC\)\)\?\]\[2\][ ]=' drivers/staging/vt6655/baseband.c
    defsnc 'SCountryTable[ ]ChannelRuleTab\[CCODE_MAX[+]1\][ ]=' drivers/staging/vt6655/card.c
    defsnc 'static[ ]const[ ]long[ ]frequency_list\[\][ ]=' drivers/staging/vt6655/iwctl.c
    accept '#define[ ]CONFIG_PATH[ ]*["][/]etc[/]vntconfiguration[.]dat["]' drivers/staging/vt6655/device_cfg.h
    defsnc 'static[ ]const[ ]\(DWORD\|unsigned[ ]long\)[ ]s_adwCrc32Table\[256\][ ]=' drivers/staging/vt6655/tcrc.c
    defsnc 'const[ ]\(BYTE\|unsigned[ ]char\)[ ]TKIP_Sbox_\(Lower\|Upper\)\[256\][ ]=' drivers/staging/vt6655/tkip.c
    blobname 'prism2_ru\.\(hex\|fw\)' drivers/staging/wlan-ng/prism2fw.c
    defsnc 'static[ ]const[ ]u16[ ]wm8960_reg\[WM8960_CACHEREGNUM\][ ]=' sound/soc/codecs/wm8960.c
    blob '#include[ ]["]me4\(00\|61\)0_firmware\.h["]\([\n][\n]*#include[ ]["]me4\(00\|61\)0_firmware\.h["]\)*' drivers/staging/me4000/me4000.c
    blobna 'firm[ ]=[ ][^;]*xilinx_firm[^;]*[;]' drivers/staging/me4000/me4000.c
    # end of new in 2.6.31
    accept '[ 	]*ramdisk[ ]=[ ]["][/]boot[/][^ ]*initrd[^ ]*\.img["]' Documentation/ia64/xen.txt

    # in drm-*.patch, post-2.6.31
    blobname 'matrox[/]g[24]00_warp\.fw' drivers/gpu/drm/mga/mga_warp.c
    blobname 'r128[/]r128_cce\.bin' drivers/gpu/drm/r128/r128_cce.c
    blobname 'radeon[/]R\([123]0\|[45]2\|S6[09]\)0_cp\.bin' drivers/gpu/drm/radeon/r100.c
    blobname 'radeon[/]\(R\([67]0\|V6[1237]\|S7[1378]\)[05]\|CEDAR\|REDWOOD\|JUNIPER\|CYPRESS\|%s\)_\(pfp\|rlc\|me\)\.bin' drivers/gpu/drm/radeon/r600.c
    defsnc 'const[ ]u32[ ]r[67]xx_default_state\[\][ ]=' drivers/gpu/drm/radeon/r600_blit_shaders.c
    defsnc 'struct[ ]nv17_tv_norm_params[ ]nv17_tv_norms\[NUM_TV_NORMS\][ ]=' drivers/gpu/drm/nouveau/nv17_tv_modes.c

    # New in or modified for 2.6.32
    blobname '\(cxgb3[/]\)\?ael20\(05_\(opt\|twx\)\|20_twx\)_edc\.bin' drivers/net/cxgb3/cxgb3_main.c
    defsnc 'static[ ]const[ ]struct[ ]aper_size_info_32[ ]u3_sizes\[8\?\][ ]=' drivers/char/agp/uninorth-agp.c
    defsnc 'static[ ]const[ ]unsigned[ ]short[ ]atkbd_set[23]_keycode\[\(512\|ATKBD_KEYMAP_SIZE\)\][ ]=' drivers/input/keyboard/atkbd.c
    defsnc '[	][}][ ]common_modes\[17\][ ]=' drivers/gpu/drm/radeon/radeon_connectors.c
    defsnc '[	][	]*\(static[ ]\)\?\(const[ ]\)\?struct[ ]phy_reg[ ]phy_reg_init\(_0\)\?\[\][ ]=' drivers/net/r8169.c
    accept '[	][	]*struct[ ]phy_reg[ ]phy_reg_init_1\[\][ ]=[ ][{][^;]*0x8300[^;]*[}][;]' drivers/net/r8169.c
    blob 'static[ ]void[ ]rtl8168d_[12]_hw_phy_config[(]void[ ]__iomem[ ][*]ioaddr[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*[\n]\+[}]' drivers/net/r8169.c
    blobna 'rtl8168d_[12]_hw_phy_config[(]ioaddr[)][;]' drivers/net/r8169.c
    blobna 'static[ ]\(const[ ]\)\?struct[ ]phy_reg_init_[12]\[\][ ]=[ ][{][\n 	{}0-9a-fx]*0x06,[ ]0xf8f9[\n 	{}0-9a-fx]*[}][;]' drivers/net/r8169.c
    # This loads firmware to be flashed from filename provided through ethtool.
    accept 'int[ ]be_load_fw[(]struct[ ]be_adapter[ ][^\n;{]*[)][ \n][{]\([\n]\+[^\n}][^\n]*\)*request_firmware[^\n]*\([\n]\+[^\n}][^\n]*\)*[\n]\+[}]' drivers/net/benet/be_main.c
    defsnc '[	]u8[ ]init_hash_seed\[\][ ]=' drivers/net/qlge/qlge_main.c
    defsnc 'static[ ]const[ ]u_int32_t[ ]ar9287\(Common\|Modes\(_\([tr]x_gain\)\)\?\)_9287_1_[01]\[\]\[[236]\][ ]=' drivers/net/wireless/ath9k/initvals.h
    defsnc 'static[ ]const[ ]u_int32_t[ ]ar9271\(Common\|Modes\)_9271\(_1_0\)\?\[\]\[[26]\][ ]=' drivers/net/wireless/ath9k/initvals.h
    defsnc 'static[ ]const[ ]u8[ ]lpphy_min_sig_sq_table\[\][ ]=' drivers/net/wireless/b43/tables_lpphy.c
    defsnc 'static[ ]const[ ]u16[ ]lpphy_\(rev\(01\|2plus\)_noise_scale\|crs_gain_nft\|iqlo_cal\|rev[01]_ofdm_cck_gain\|\(a0_\)\?gain\|sw_control\)_table\[\][ ]=' drivers/net/wireless/b43/tables_lpphy.c
    defsnc 'static[ ]const[ ]u32[ ]lpphy_\(\(rev01_ps\|tx_power\)_control\|\(a0_\)\?gain_\(idx\|value\)\|papd_\(eps\|mult\)\)_table\[\][ ]=' drivers/net/wireless/b43/tables_lpphy.c
    blobname 'v4l-saa7164-1\.0\.[23]\.fw' drivers/media/video/saa7164/saa7164-fw.c
    defsnc 'static[ ]const[ ]u8[ ]n4_\(om6802\|other\|tas5130a\)\[\][ ]=' drivers/media/video/gspca/t613.c
    defsnc '[	][	]\(static[ ]\)\?const[ ]struct[ ]sensor_w_data[ ]\(cif\|vga\)_sensor[01]_init_data\[\][ ]=' drivers/media/video/gspca/mr97310a.c
    defsnc '[	]struct[ ]jlj_command[ ]start_commands\[\][ ]=' drivers/media/video/gspca/jeilinj.c
    defsnc 'static[ ]u8[ ]init_code\[\]\[2\][ ]=' drivers/media/dvb/dvb-usb/friio-fe.c
    defsnc 'static[ ]const[ ]u8[ ]va1j5jf8007[ts]_\(2[05]mhz_\)\?prepare_bufs\[\]\[2\][ ]=' 'drivers/media/dvb/pt1/va1j5jf8007[st]\.c'
    accept '[	 ]\+request_firmware[(][)][ ]will[ ]hit[ ]an[ ]OOPS' drivers/media/dvb/frontends/dib7000p.c
    defsnc 'static[ ]long[ ]limiter_times\[\][ ]=' drivers/media/radio/si4713-i2c.c
    blobname 'c[tb]fw\(_\(fc\|cna\)\)\?\.bin' drivers/scsi/bfa/bfad_fwimg.c
    defsnc 'static[ ]const[ ]u16[ ]\(VDCDC[1x]\|LDO[12]\)_VSEL_table\[\][ ]=' 'drivers/regulator/tps650\(23\|7x\)-regulator\.c'
    defsnc 'static[ ]\(const[ ]\)\?struct[ ]lms283gf05_seq[ ]disp_\(init\|pwdn\)seq\[\][ ]=' drivers/video/backlight/lms283gf05.c
    defsnc '[}][ ]csc_table\[\][ ]=' drivers/video/msm/mdp_csc_table.h
    defsnc '\(static[ ]\)\?struct[ ]mdp_table_entry[ ]mdp_\(\(upscale\|gaussian_blur\)_table\|downscale_[xy]_table_PT[2468]TO\(PT[468]\|1\)\)\[\][ ]=' drivers/video/msm/mdp_scale_tables.c
    accept '[	][	]card->firmware[ ]=[ ]data->firmware[;]'  drivers/bluetooth/btmrvl_sdio.c
    accept '[	]isar->firmware[ ]=[ ][&]load_firmware[;]' drivers/isdn/hardware/mISDN/mISDNisar.c
    blobname 'isdn[/]ISAR\.BIN' drivers/isdn/hardware/mISDN/speedfax.c
    blobname '\(sep[/]\)\?\(cache\|resident\)\.image\.bin' drivers/staging/sep/sep_driver.c
    blobname 'RTL8192E[/]\(boot\|main\|data\)\.img' drivers/staging/rtl8192e/r819xE_firmware.c
    defsnc '\(static[ ]\)\?u32[ ]Rtl8190PciE\?\(AGCTAB_\|PHY_REG\(_1T2R\)\?\|Radio[ABCD]_\)Array\[\(AGCTAB_\|PHY_REG\(_1T2R\)\?\|Radio[ABCD]_\)ArrayLength\][ ]=' 'drivers/staging/\(rtl8192e/r819xE_phy\.c\|rtl8192u/r819xU_firmware_img.c\)'
    accept '[ ][*][ ]File:[ ]main_usb\.c[\n][ ]\([*]\+[^/*][^*]*\)*[\n][ ][*][/]\([\n][\n]*#\(undef[ ][^\n]*\|include[ ]["][^\n]*["]\)\)*[\n][\n]*#include[ ]["]firmware\.h["]' drivers/staging/vt6656/main_usb.c
    blob 'const[ ]BYTE[ ]abyFirmware\[\][ ]=[ ][{][^;]*[}][;]' drivers/staging/vt6656/firmware.c
    defsnc '[}][ ]*ChannelRuleTab\[\][ ]=' drivers/staging/vt6656/channel.c
    defsnc '\(static[ ]\)\?struct[ ]register_address_value_pair[\n]\(preview_snapshot_mode\|noise_reduction\)_reg_settings_array\[\][ ]=' drivers/staging/dream/camera/mt9d112_reg.c
    blobname '\([/]tmp[/]\)\?RT30xxEEPROM\.bin' 'drivers/staging/rt3090/\(common/ee_efuse\.c\|rtmp_def\.h\)'
    defsnc 'static[ ]UINT8[ ]WPS_DH_\([PRX]\|RRModP\)_VALUE\[1\(9[23]\|84\)\][ ]=' drivers/staging/rt3090/common/crypt_biginteger.c
    defsnc '\(CH_FREQ_MAP\|struct[ ]rt_ch_freq_map\)[ ]CH_HZ_ID_MAP\[\][ ]\?=' 'drivers/staging/\(rt2860\|rt3090\)/common/rt_channel\.c'
    defsnc 'static[ ]const[ ]UINT32[ ]SHA256_K\[64\][ ]=' drivers/staging/rt3090/common/crpt_sha2.c
    defsnc '\(DOT11_REGULATORY_INFORMATION\|struct[ ]rt_dot11_regulatory_information\)[ ]\(USA\|Europe\|Japan\)RegulatoryInfo\[\][ ]=' 'drivers/staging/\(rt3090\|rt2860\)/common/spectrum\.c'
    defsnc 'static[ ]const[ ]USHORT[ ]Sbox\[256\][ ]=' drivers/staging/rt3090/sta/rtmp_ckipmic.c
    blob '#include[ 	]*["]\(\.\.[/]\(\.\.[/]rt\(28[67]\|30[79]\)0[/]\(common[/]\)\?\)\?\)\?firmware\(_\(28[67]\|30[79]\)0\)\?\.h["]\([\n][\n]*#include[ 	]*["]\(\.\.[/]\(\.\.[/]rt\(28[67]\|30[79]\)0[/]\(common[/]\)\?\)\?\)\?firmware\(_\(28[67]\|30[79]\)0\)\?\.h["]\)' 'drivers/staging/rt\(28[67]\|309\)0/common/rtmp_\(init\|mcu\)\.c'
    blobna 'FIRMWAREIMAGE_LENGTH[ ]==' drivers/staging/rt3090/common/rtmp_mcu.c
    defsnc 'int[ ]wm831x_isinkv_values\[WM831X_ISINK_MAX_ISEL[ ][+][ ][1]\][ ]=' drivers/mfd/wm831x-core.c
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]hwecc4_2048[ ]__initconst[ ]=' drivers/mtd/nand/davinci_nand.c
    defsnc 'static[ ]const[ ]u16[ ]wm8974_reg\[WM8974_CACHEREGNUM\][ ]=' sound/soc/codecs/wm8974.c
    defsnc 'static[ ]const[ ]u\(8\|16\)[ ]ak464[28]_reg\[\(AK4642_CACHEREGNUM\)\?\][ ]=' sound/soc/codecs/ak4642.c
    accept 'int[ ]snd_hda_load_patch[(][^\n;{]*[)][ \n][{][^\n]*\([\n]\+[^\n}][^\n]*\)*hda_codec[^\n]*\([\n]\+[^\n}][^\n]*\)*request_firmware[^\n]*\([\n]\+[^\n}][^\n]*\)*[\n]\+[}]' sound/pci/hda/hda_hwdep.c
    accept '[ ][ ][ ]Bit[ 0-7]*' Documentation/input/sentelic.txt
    accept 'The[ ]hd-audio[ ]driver[ ]reads[ ]the[ ]file[ ]via[ ]request_firmware[(][)]\.' Documentation/sound/alsa/HD-Audio.txt
    blob 'SD8688[ ]firmware:[\n]*\([/]lib[/]firmware[^\n]*[\n]*\)*The[ ]images[^:]*:[\n]*[^\n]*[/]linux-firmware[^\n]*' Documentation/btmrvl.txt
    defsnc 'static[ ]u8[ ]ibm405ex_fbdv_multi_bits\[\][ ]=' arch/powerpc/boot/4xx.c
    defsnc 'static[ ]int[ ]zoom2_batt_table\[\][ ]=' arch/arm/mach-omap2/board-zoom2.c
    defsnc 'static[ ]struct[ ]ad714x_platf\(or\|ro\)m_data[ ]ad714[27]_\(\(spi\|i2c\)_\)\?platf\(or\|ro\)m_data[ ]=' arch/blackfin/mach-bf537/boards/stamp.c
    blob 'static[ ]const[ ]u8[ ]lgs8g75_initdat\[\][ ]=[ ][{][^;]*[}][;]' drivers/media/dvb/frontends/lgs8gxx.c
    blob 'static[ ]int[ ]lgs8g75_init_data[(][^\n;{]*[)][ \n][{][^\n]*\([\n]\+[^\n}][^\n]*\)*lgs8g75_initdat[^\n]*\([\n]\+[^\n}][^\n]*\)*[\n]\+[}]' drivers/media/dvb/frontends/lgs8gxx.c
    defsc 'static[ ]struct[ ]idxdata[ ]tbl_common\(_[a-e]\|5\|_\?3B\?\)\[\][ ]=' 'drivers/media/video/gspca/gl860/gl860-\(mi2020\|mi1320\|ov9655\|ov2640\)\.c'
    defsnc 'static[ ]struct[ ]validx[ ]tbl_\(commm\?on\|init_\(at_startup\|post_alt\)\|sensor_settings_common\(_[ab]\|1\)\|big\(_[abc]\|[123]\)\|640\|800\)\[\][ ]=' 'drivers/media/video/gspca/gl860/gl860-\(mi2020\|mi1320\|ov9655\|ov2640\).c'
    defsnc 'static[ ]u8[ ][*]tbl_\(640\|800\|1280\)\[\][ ]=' 'drivers/media/video/gspca/gl860/gl860-\(mi1320\|ov9655\).c'
    accept '[<][<]\([/]Subtype[/]Type1\)\?[/]BaseFont[^ ]*[/]FontDescriptor[ ][0-9][0-9]*[ ]0[ ]R\([/]Type[/]Font\)\?[\n]\?[/]FirstChar[ ][0-9][0-9]*[/]LastChar[ ][0-9][0-9]*[/]Widths\[[\n][0-9 \n]*\]' 'Documentation/DocBook/v4l/.*\.pdf'

    # New in 2.6.33
    accept '[ ]*just[ ]run[ ]["]cat[ ][/]sys[/]firmware[/]acpi[/]tables[/]DSDT[ ]>[ ][/]tmp[/]dsdt[.]dat["]' Documentation/acpi/method-customizing.txt
    accept '[ ]*b[)][ ]disassemble[ ]the[ ]table[ ]by[ ]running[ ]["]iasl[ ]-d[ ]dsdt[.]dat["][.]' Documentation/acpi/method-customizing.txt
    accept '[ ]*x=["]7999\([ ][0-9]\+\)\+["]' Documentation/blockdev/drbd/DRBD-8.3-data-packets.svg
    defsnc 'static[ ]int[ ]zoom_batt_table\[\][ ]=' arch/arm/mach-omap2/board-zoom-peripherals.c
    defsnc 'static[ ]u16[ ]x[48]_vectors\[\][ ]=' drivers/edac/amd64_edac.c
    defsnc 'static[ ]const[ ]u16[ ]\(y\|uv\)_static_hcoeffs\[N_HORIZ_\(Y\|UV\)_TAPS[ ][*][ ]N_PHASES\][ ]=' drivers/gpu/drm/i915/intel_overlay.c
    accept '[	]\.download_firmware[ ]=[ ]ec168_download_firmware,[\n][	]\.firmware[ ]=[ ]' drivers/media/dvb/dvb-usb/ec168.c
    blobname 'dvb-usb-ec168\.fw' drivers/media/dvb/dvb-usb/ec168.c
    defsnc 'static[ ]const[ ]u16[ ]dib0090_defaults\[\][ ]=' drivers/media/dvb/frontends/dib0090.c
    blobname 'dvb-fe-ds3000\.fw' drivers/media/dvb/frontends/ds3000.c
    blob '[/][*][ ]\(as[ ]of[ ][^\n]*[ ]current[ ]DS3000[ ]firmware\|DS3000[ ]FW\)[^/]*[*][/]\([\n][/][*]\([ ]\(as[ ]of[ ][^\n]*[ ]current[ ]DS3000[ ]firmware\|DS3000[ ]FW\)[^/]*\|[(]DEBLOBBED[)]\)[*][/]\)*' drivers/media/dvb/frontends/ds3000.c
    defsnc 'static[ ]u8[ ]ds3000_dvbs2\?_init_tab\[\][ ]=' drivers/media/dvb/frontends/ds3000.c
    defsnc '[	]static[ ]const[ ]u16[ ]dvbs2_snr_tab\[\][ ]=' drivers/media/dvb/frontends/ds3000.c
    defsnc 'static[ ]const[ ]struct[ ]cnr[ ]cnr_tab\[\][ ]=' drivers/media/dvb/frontends/mb86a16.c
    defsnc 'u8[ ]lgtdqcs001f_inittab\[\][ ]=' drivers/media/dvb/mantis/mantis_vp1033.c
    defsnc 'static[ ]const[ ]struct[ ]ov9640_reg[ ]ov9640_regs_dflt\[\][ ]=' drivers/media/video/ov9640.c
    defsnc '\(const[ ]static\|static[ ]const\)[ ]struct[ ]rj54n1_reg_val[ ]bank_[4578]\[\][ ]=' drivers/media/video/rj54n1cb0c.c
    blob '#define[ ]_FW_NAME[(]api[)][ ]DRV_NAME[ ]["][.]["][ ]#api[ ]["]\.fw["]' drivers/media/video/iwmc3200top.h
    blob '#define[ ]FW_FILE_VERSION\([	]*[\\][\n][	]__stringify[(]BCM_5710_FW_\(MAJOR\|MINOR\|REVISION\|ENGINEERING\)_VERSION[)]\([ ]["][.]["]\)\?\)\+' 'drivers/net/\(bnx2x/\)\?bnx2x_main\.c'
    blobname '\(bnx2x[/]\)\?bnx2x-e[12]h\?-["][ ]FW_FILE_VERSION[ ]["]\.fw' 'drivers/net/\(bnx2x/\)\?bnx2x_main\.c'
    # Moved down to avoid shorter earlier match.
    # blobname '\(bnx2x[/]\)\?bnx2x-e[12]h\?-\([0-9.%d]*\.fw\)\?' 'drivers/net/\(bnx2x/\)\?bnx2x_main\.c'
    blob '#define[ ]FW_VERSION\([ 	]__stringify[(]FW_VERSION_\(MAJOR\|MINOR\|MICRO\)[)]\([ ]["][.]["]\)\?\([	]*[\\][\n]\)\?\)\+' drivers/net/cxgb3/cxgb3_main.c
    blobname 'cxgb3[/]t3fw-["][ ]FW_VERSION[ ]["]\.bin' drivers/net/cxgb3/cxgb3_main.c
    blob '#define[ ]TPSRAM_VERSION\([ 	]__stringify[(]TP_VERSION_\(MAJOR\|MINOR\|MICRO\)[)]\([ ]["][.]["]\)\?\([	]*[\\][\n]\)\?\)\+' drivers/net/cxgb3/cxgb3_main.c
    blobname 'cxgb3[/]t3\(%c\|[bc]\)_psram-["][ ]TPSRAM_VERSION[ ]["]\.bin' drivers/net/cxgb3/cxgb3_main.c
    defsnc '[	]static[ ]const[ ]u8[ ]rsshash\[40\][ ]=' drivers/net/igb/igb_main.c
    defsnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_3\(02\)\?x\[\][ ]=' drivers/net/wireless/rt2x00/rt2800lib.c
    defsnc 'static[ ]struct[ ]conf_drv_settings[ ]default_conf[ ]=' drivers/net/wireless/wl12xx/wl1271_main.c
    defsnc 'static[ ]\(const[ ]\)\?u16[ ]bios_to_linux_keycode\[256\][ ]\(__initconst[ ]\)\?=' drivers/platform/x86/dell-wmi.c
    accept '[	]err[ ]=[ ]request_firmware[(][&]pm8001_ha->fw_image,' drivers/scsi/pm8001/pm8001_ctl.c
    defsnc 'static[ ]unsigned[ ]char[ ]vpdb0_data\[\][ ]=' drivers/scsi/scsi_debug.c
    defsnc 'static[ ]struct[ ]vesa_mode_table[ ]vesa_mode\[\][ ]=' drivers/staging/sm7xx/smtcfb.c
    defsnc 'struct[ ]ModeInit[ ]VGAMode\[\][ ]=' drivers/staging/sm7xx/smtcfb.h
    blob 'static[ ]const[ ]hcf_8[ ]fw_image_[1234]_data\[\][ ]=[^;]*[;]\([ ]*[/][*][ ]fw_image_[1234]_data[ ][*][/]\)\?' 'drivers/staging/wlags49_h2/\(ap\|sta\)_h25\?\.c'
    blobname '[/]etc[/]agere[/]fw\.bin' drivers/staging/wlags49_h2/wl_profile.c
    defsnc 'static[ ]const[ ]long[ ]chan_freq_list\[\]\[MAX_CHAN_FREQ_MAP_ENTRIES\][ ]=' drivers/staging/wlags49_h2/wl_util.c
    blob 'The[ ]ssinit[ ]program.*nsoniq.*sndscape.*sound[ ]weird\.' Documentation/sound/oss/README.OSS
    blobname 'scope\.cod' 'sound/isa/\(Kconfig\|sscape\.c\)'
    blobname '\(sndscape\|soundscape\)\.co\([?dx01234]\|%d\)' 'sound/isa/\(Kconfig\|sscape\.c\)\|Documentation/sound/oss/README\.OSS'
    defsnc 'static[ ]const[ ]u8[ ]\(adcm1700\|om6802\|po1030\)_sensor_\(init\|param1\)\[\]\[8\][ ]=' drivers/media/video/gspca/sonixj.c
    blobname 'ath3k-1\.fw' drivers/bluetooth/ath3k.c
    blobname 'nouveau[/]nv\([0-9a-f][0-9a-f]\|%02x\)\.ctx\(prog\|vals\)' 'drivers/gpu/drm/nouveau/\(nv50_graph\|nouveau_grctx\)\.c'

    # New in 2.6.34
    blobname 'mts_mt9234\(mu\|zba\)\.fw' drivers/usb/serial/ti_usb_3410_5052.c
    blobname 'cxgb4[/]t4fw\.bin' 'drivers/\(net/cxgb4/cxgb4_main\.c\|scsi/csiostor/csio_hw\.h\)'
    defsnc '[	]static[ ]const[ ]unsigned[ ]int[ ]reg_ranges\[\][ ]=' drivers/net/cxgb4/cxgb4_main.c
    defsnc '[	]static[ ]const[ ]unsigned[ ]int[ ]avg_pkts\[NCCTRL_WIN\][ ]=' drivers/net/cxgb4/t4_hw.c
    # above in -rc5
    defsnc 'static[ ]u32[ ]epll_div\[\]\[5\][ ]=' arch/arm/mach-s5p6440/clock.c
    accept '[	]aru->firmware[ ]=[ ]fw[;]' drivers/net/wireless/ath/ar9170/usb.c
    accept '[	]err[ ]=[ ]request_firmware[(][&]fw_entry,[ ]["]broadsheet\.wbf["],[ ]dev[)][;]' drivers/video/broadsheetfb.c
    # above in -rc2, below in -rc1
    accept '\(#[ ]\)\?\(Usage:[ ]cxacru-cf\.py[ ][<]\|Warning:\|Note:[ ]support[ ]for\)[ ]cxacru-cf\.bin' 'Documentation/networking/cxacru\(-cf\.py\|\.txt\)'
    defsnc 'static[ ]struct[ ]cdce_reg[ ]cdce_y1_27000\[\][ ]=' arch/arm/mach-davinci/cdce949.c
    defsnc '[	]u16[ ]map\[\][ ]=' drivers/hwmon/asc7621.c
    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]az6027_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/az6027.c
    blobname 'dvb-usb-az6027-03\.fw' drivers/media/dvb/dvb-usb/az6027.c
    accept '[	]p7500->firmware[ ]=' drivers/media/dvb/dvb-usb/dw2102.c
    blobname 'dvb-usb-p7500\.fw' drivers/media/dvb/dvb-usb/dw2102.c
    defsnc 'static[ ]u8[ ]ITUDecoderSetup\[4\]\[16\][ ]=' drivers/media/dvb/ngene/ngene-core.c
    blobname 'ngene_1[5678]\.fw' drivers/media/dvb/ngene/ngene-core.c
    blobname 'sms1xxx-hcw-55xxx-i\?sdbt-02\.fw' drivers/media/dvb/siano/sms-cards.c
    defsnc 'static[ ]\(const[ ]\)\?u8[ ]samsung_smt_7020_inittab\[\][ ]=' drivers/media/video/cx88/cx88-dvb.c
    defsnc 'static[ ]const[ ]u8[ ]\(bridge\|sensor\)_init\(_2\)\?\[\]\[2\][ ]=' drivers/media/video/gspca/ov534_9.c
    defsnc 'static[ ]const[ ]u8[ ]bridge_start_\([qs]\?v\|x\)ga\[\]\[2\][ ]=' drivers/media/video/gspca/ov534_9.c
    defsnc '[	]struct[ ]init_command[ ]\(spy\|cif\|ms350\|genius\|vivitar\)_start_commands\[\][ ]=' drivers/media/video/gspca/sn9c2028.c
    defsnc 'static[ ]const[ ]u8[ ]n4_lt168g\[\][ ]=' drivers/media/video/gspca/t613.c
    initc 'static[ ]const[ ]\(__\)\?u8[ ]\(mi\(0360\|13[12]0\)\|po\(1200\|3130\)\|hv7131r\|ov76[67]0\)_\(\(soc\)\?_\?[iI]nit\(Q\?V\|SX\)GA\(_\(JPG\|data\)\)\?\|rundata\)\[\]\[4\][ ]=\([ ][{][*][/][;]\)\?' drivers/media/video/gspca/vc032x.c
    defsnc '[	]static[ ]const[ ]u8[ ]gamma_tb\[6\]\[16\][ ]=' drivers/media/video/gspca/zc3xx.c
    blobname 'tlg2300_firmware\.bin' drivers/media/video/tlg2300/pd-main.c
    defsnc '[	]u8[ ]pattern\[42\][ ]=' drivers/net/ksz884x.c
    defsnc '\(static[ ]\)\?const[ ]u8[ ]b43_ntab_framelookup\[\][ ]=' drivers/net/wireless/b43/tables_nphy.c
    defsnc 'const[ ]u32[ ]\(b43_ntab_tx_gain_rev\(0_1_2\|3plus_2ghz\|\([34]\|5plus\)_5ghz\)\|txpwrctrl_tx_gain_ipa\(_\(rev\)\?[56]g\?\)\?\)\[\][ ]=' drivers/net/wireless/b43/tables_nphy.c
    defsnc 'const[ ]u16[ ]tbl_iqcal_gainparams\[2\]\[9\]\[8\][ ]=' drivers/net/wireless/b43/tables_nphy.c
    defsnc 'const[ ]struct[ ]nphy_txiqcal_ladder[ ]ladder_\(lo\|iq\)\[\][ ]=' drivers/net/wireless/b43/tables_nphy.c
    defsnc 'const[ ]u16[ ]loscale\[\][ ]=' drivers/net/wireless/b43/tables_nphy.c
    blobname 'isl38\(86\|87\|90\)\(pci\|usb\(_bare\)\?\)\?' 'drivers/net/wireless/p54/p54\(pci\.c\|usb\.[ch]\)'
    defsnc 'static[ ]struct[ ]conf_drv_settings[ ]default_conf[ ]=[ ][{][*][/][;]' drivers/net/wireless/wl12xx/wl1271_main.c
    defsnc '[	][}][ ]grtpkts\[\][ ]=' drivers/staging/mimio/mimio.c
    blobname 'rt\(28[67]0\|30[79][01]\)\.bin' drivers/staging/rt2860/common/rtmp_mcu.c
    accept '[	]adapter->firmware[ ]=[ ]fw[;]' drivers/staging/rt2860/common/rtmp_mcu.c
    blobna '[/][*][^*]*\([*]\+[^/*][^*]*\)*[*]*RTL8192SU[/]rtl8192sfw\.bin[^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]' drivers/staging/rtl8192su/r8192S_firmware.c
    accept 'MODULE_FIRMWARE[(]["]keyspan_pda[/]\(keyspan_pda\|xircom_pgs\)\.fw["][)][;]' drivers/usb/serial/keyspan_pda.c
    # It's not clear that wm2000_anc.bin is pure data.
    # Check with developer, clean up for now.
    blobname 'wm2000_anc\.bin' sound/soc/codecs/wm2000.c
    blob '[ ][*][ ]The[ ]download[ ]image[ ]for[ ]the[ ]WM2000[^*]*\([*]\+[^/*][^*]*\)*[*]*[<][ ]file[^*\n]*[\n][ ][*][/]' sound/soc/codecs/wm2000.c
    # accept '[ ][*][ ].wm2000_anc\.bin.[ ]by[ ]default' sound/soc/codecs/wm2000.c
    # accept '[ ][*][ 	]*[<][ ]file[ ]\+[>]wm2000_anc\.bin' sound/soc/codecs/wm2000.c
    # accept '[	]filename[ ]=[ ]["]wm2000_anc\.bin["][;]' sound/soc/codecs/wm2000.c
    defsnc '[}][ ]\(clk_sys_ratios\|bclk_divs\)\[\][ ]=' 'sound/soc/wm890[34]\.c'
    defsnc '[}][ ]clock_cfgs\[\][ ]=' sound/soc/codecs/wm8955.c
    blobname 'siu_spb\.bin' sound/soc/sh/siu_dai.c
    defsnc 'static[ ]const[ ]u8[ ]poxxxx_\(init\(_common\|Q\?VGA\|_end_1\|_start_3\)\|gamma\)\[\]\[4\][ ]=' drivers/media/video/gspca/vc032x.c
    defsnc 'crb_128M_2M_map\[64\][ ]__cacheline_aligned_in_smp[ ]=' 'drivers/net/\(netxen/netxen_nic_hw.c\|qlcnic/qlcnic_hw.c\)'

    # New in 2.6.35
    defsnc 'static[ ]const[ ]u8[ ]gsm_fcs8\[256\][ ]=' drivers/char/n_gsm.c
    defsnc 'static[ ]u8[ ]\(reset_atetm\|atetm_[12]port\|portsel_\(port[12]\|2port\)\)\[BIT2BYTE[(]LEN_\(ETM\|PORT_SEL\)[)]\][ ]=' drivers/infiniband/hw/qib/qib_iba7322.c
    blobname 'qlogic[/]sd7220[.]fw' drivers/infiniband/hw/qib/qib_sd7220.c
    defsnc '[}][ ]est3_modes\[\][ ]=' drivers/gpu/drm/drm_edid.c
    defsnc 'static[ ]struct[ ]v_table[ ]v_table\[\][ ]=' drivers/gpu/drm/i915/i915_dma.c
    blobname 'orinoco_ezusb_fw' drivers/net/wireless/orinoco/orinoco_usb.c
    defsc 'static[ ]const[ ]struct[ ]ar9300_eeprom[ ]ar9300_default[ ]=' drivers/net/wireless/ath/ath9k/ar9003_eeprom.c
    accept '[	]hif_dev->firmware[ ]=[ ]NULL[;]' drivers/net/wireless/ath/ath9k/hif_usb.c
    defsnc 'static[ ]const[ ]u32[ ]ar9300_2p[02]_\(radio\|mac\|baseband\)_postamble\[\]\[5\][ ]=' 'drivers/net/wireless/ath/ath9k/ar9003_\(2p[02]_\)\?initvals\.h'
    defsnc 'static[ ]const[ ]u32[ ]ar9300Modes_\(\(low\(est\)\?\|high\)_ob_db\|high_power\)_tx_gain_table_2p[02]\[\]\[5\][ ]=' 'drivers/net/wireless/ath/ath9k/ar9003_\(2p[02]_\)\?initvals\.h'
    defsnc 'static[ ]const[ ]u32[ ]ar9\(300\|200_merlin\)_2p[02]_\(radio\|mac\|baseband\)_core\[\]\[2\][ ]=' 'drivers/net/wireless/ath/ath9k/ar9003_\(2p[02]_\)\?initvals\.h'
    defsnc 'static[ ]const[ ]u32[ ]ar9300Common_\(wo_xlna_\)\?rx_gain_table_\(merlin_\)\?2p[02]\[\]\[2\][ ]=' 'drivers/net/wireless/ath/ath9k/ar9003_\(2p[02]_\)\?initvals\.h'
    defsnc 'static[ ]const[ ]u32[ ]ar928\(5Modes_XE2\|7Modes_9287_1\)_0_\(normal\|high\)_power\[\]\[6\][ ]=' drivers/net/wireless/ath/ath9k/ar9002_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar92\(87Common_9287_1_[01]\|71Common_9271\)\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/ar9002_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar92\(87\|71\)Modes_\(\(normal\|high\)_power_\)\?\([tr]x_gain_\)\?92\(87_1_[01]\|71\(_ANI_reg\)\?\)\[\]\[6\][ ]=' drivers/net/wireless/ath/ath9k/ar9002_initvals.h
    defsnc 'static[ ]int[ ]ath_max_4ms_framelen\[4\]\[32\][ ]=' drivers/net/wireless/ath/ath9k/xmit.c
    defsnc 'static[ ]const[ ]u8[ ]\(gc0307\|po2030n\|soi768\)_sensor_\(init\|param1\)\[\]\[8\][ ]=' drivers/media/video/gspca/sonixj.c
    defsnc '\(static[ ]\)\?struct[ ]crb_128M_2M_block_map[ ]crb_128M_2M_map\[64\][ ]=' 'drivers/scsi/\(qla2xxx/qla_nx\.c\|qla4xxx/ql4_nx\.c\)'
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]BUCK[123]_\(suspend_\)\?table\[\][ ]=' drivers/regulator/88pm8607.c
    defsnc '[	]*static[ ]const[ ]char[ ]sha256_zero\[SHA256_DIGEST_SIZE\][ ]=' drivers/crypto/n2_core.c
    defsnc '[}][ ]XGI\(fb_vrate\|_TV_filter\)\[\][ ]=' drivers/staging/xgifb/XGI_main.h
    defsnc '\(static[ ]\)\?\(USHORT\|unsigned[ ]short\)[ ]XGINew_\(MD\|[CEV]G\)A_DAC\[\][ ]*=' drivers/staging/xgifb/vb_setmode.c
    defsnc '\(static[ ]\)\?\(const[ ]\)\?\(struct[ ]\)\?XGI_[ME]CLKData\(Struct\)\?[ ]XGI\(3[34]0\|27\)\(New\)\?_[ME]CLKData\[\][ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(const[ ]\)\?\(UCHAR\|unsigned[ ]char\)[ ]XGI340_CR6[BE]\[8\]\[4\][ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(const[ ]\)\?\(UCHAR\|unsigned[ ]char\)[ ]XGI340_CR6F\[8\]\[32\][ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(UCHAR\|unsigned[ ]char\)[ ]XGI330\(New\)\?_SR15\(_1\)\?\[8\]\[8\][ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(UCHAR\|unsigned[ ]char\)[ ]XGI330_cr40_1\[15\]\[8\][ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(const[ ]\)\?\(struct[ ]\)\?XGI_StStruct[ ]XGI330_SModeIDTable\[\][ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(const[ ]\)\?\(struct[ ]\)\?XGI_ExtStruct[ ][ ]\?XGI330_EModeIDTable\[\][ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(const[ ]\)\?\(struct[ ]\)\?\(XGI\|SiS\)_StandTable\(Struct\|_S\)[ ]XGI330_StandTable\(\[\]\)\?[ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\([/][*]\)\?\(static[ ]\)\?\(const[ ]\)\?\(struct[ ]\)\?\(XGI330\|SiS\)_LCDData\(Struct\)\?[ ][ ]\?XGI_\(\(St2\?\|Ext\)LCD\(1024x768\|1280x1024\)\|NoScaling\)Data\[\][ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(struct[ ]\)\?XGI330_TVDataStruct[ ][ ]XGI_\(St\|Ext\)\(PAL\|NTSC\|YPbPr\(525[ip]\|750p\)\)Data\[\][ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(UCHAR\|unsigned[ ]char\)[ ]XGI330_\(NTSC\|PAL\|HiTV\(Ext\|St[12]\|Text\)\|YPbPr\(750p\|525[ip]\)\)Timing\[\][ ][ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(UCHAR\|unsigned[ ]char\)[ ]XGI330_HiTVGroup3\(Data\|Simu\|Text\)\[\][ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(UCHAR\|unsigned[ ]char\)[ ]XGI330_Ren\(525\|750\)pGroup3\[\][ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(struct[ ]\)\?XGI_PanelDelayTblStruct[ ]XGI330_PanelDelayTbl\[\]' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(const[ ]\)\?\(struct[ ]\)\?\(XGI330\|SiS\)_LVDSData\(Struct\)\?[ ][ ]\?XGI\(330\)\?_LVDS\(320x480\|800x600\|1024x768\|1280x\(1024\|768[NS]\?\)\|1400x1050\|640x480\)Data_[12]\[\][ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(struct[ ]\)\?XGI_LVDSCRT1DataStruct[ ][ ]XGI_CHTVCRT1[UO]\(NTSC\|PAL\)\[\][ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(const[ ]\)\?\(struct[ ]\)\?XGI_ModeResInfo\(Struct\|_S\)[ ]XGI330_ModeResInfo\[\][ ]*=' drivers/staging/xgifb/vb_table.h
    defsnc '\(static[ ]\)\?\(USHORT\|unsigned[ ]short\)[ ]XGINew_DRAMType\[17\]\[5\][ ]*=' 'drivers/staging/xgifb/\(vb_table\.h\|vb_init\.c\)'
    defsnc '\(static[ ]\)\?\(USHORT\|unsigned[ ]short\)[ ]XGINew_SDRDRAM_TYPE\[13\]\[5\][ ]*=' 'drivers/staging/xgifb/\(vb_table\.h\|vb_init\.c\)'
    defsnc '\(static[ ]\)\?\(USHORT\|unsigned[ ]short\)[ ]XGINew_DDRDRAM_TYPE20\[12\]\[5\][ ]*=' 'drivers/staging/xgifb/\(vb_table\.h\|vb_init\.c\)'
    blobname 'TIInit_\(\(%d\|[0-9]\+\)[.]\)\+bts' drivers/staging/ti-st/st_kim.c
    defsnc 'static[ ]int16[ ]mdp_scale_\(pixel_repeat\|0p[2468]_to_[08]p[0468]\)_C[0123]\[MDP_SCALE_COEFF_NUM\][ ]=' drivers/staging/msm/mdp_ppp_v31.c
    # qseed_table2 is kind of suspicious, but there's some regularity
    # to it that makes me think it's just data.
    defsnc 'static[ ]uint32[ ]vg_qseed_table2\[\][ ]=' drivers/staging/msm/mdp4_util.c
    defsnc 'char[ ]gc_lut\[\][ ]=' drivers/staging/msm/mdp4_util.c
    defsnc 'uint32[ ]igc_\(video\|rgb\)_lut\[\][ ]=' drivers/staging/msm/mdp4_util.c
    defsnc 'static[ ]word[ ]convert_8_to_16_tbl\[256\][ ]=' drivers/staging/msm/ebi2_tmd20.c
    defsnc 'static[ ]struct[ ]sharp_spi_data[ ]init_sequence\[\][ ]=' drivers/staging/msm/lcdc_sharp_wvga_pt.c
    blobname 'xc3028L\?-v[0-9]\+\.fw' drivers/staging/tm6000/tm6000-cards.c
    defsnc 'static[ ]const[ ]struct[ ]chs_entry[ ]chs_table\[\][ ]=' drivers/mtd/sm_ftl.c
    blobname 'asihpi[/]dsp\(%04x\|[0-9a-f][0-9a-f][0-9a-f][0-9a-f]\)\.bin' sound/pci/asihpi/hpidspcd.c
    defsnc 'static[ ]unsigned[ ]long[ ]ident_map\[32\][ ]=' kernel/exec_domain.c
    defsnc 'static[ ]u32[ ]epll_div\[\]\[4\][ ]=' arch/arm/mach-s5pc100/clock.c
    blobname 'iwlwifi-6000g2[ab]-' drivers/net/iwlwifi/iwl-6000.c
    blobna '[/][*][^*]*\([*]\+[^/*][^*]*\)*[*]*[(]f2255usb\.bin[)][^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]' drivers/media/video/s2255drv.c

    # New in 2.6.36:
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]qi_lb60_ecclayout_[12]gb[ ]=' arch/mips/jz4740/board-qi_lb60.c
    blobname 'qt602240\.fw' drivers/input/touchscreen/qt602240_ts.c
    blobname 'lgs8g75\.fw' drivers/media/dvb/frontends/lgs8gxx.c
    defsnc 'static[ ]const[ ]struct[ ]ucbus_write_cmd[ ]\(icx098bq\|lz24bp\)_start_[012]\[\][ ]=' drivers/media/video/gspca/sq930x.c
    defsnc '[}][ ]capconfig\[4\]\[2\][ ]=' drivers/media/video/gspca/sq930x.c
    defsnc 'static[ ]u8[ ]sa2400_rf_rssi_map\[\][ ]=' drivers/net/wireless/rtl818x/rtl8180_sa2400.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]pwm_lookup_table\[256\][ ]=' drivers/platform/x86/compal-laptop.c
    defsnc 'static[ ]int[ ]tps6586x_\(ldo4\|sm2\|dvm\)_voltages\[\][ ]=' drivers/regulator/tps6586x-regulator.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]muxonechan\[\][ ]=' drivers/staging/comedi/drivers/adv_pci1710.c
    defsnc 'int[ ]tones\[2048\][ ]=' drivers/staging/easycap/easycap_testcard.c
    defsnc 'const[ ]unsigned[ ]char[ ]map_table\[\][ ]=' drivers/staging/lirc/lirc_ttusbir.c
    defsnc 'static[ ]unsigned[ ]char[ ]jpeg_header\[\][ ]=' drivers/staging/solo6x10/solo6010-jpeg.h
    defsc 'static[ ]const[ ]unsigned[ ]int[ ]solo_osd_font\[\][ ]=' drivers/staging/solo6x10/solo6010-osd-font.h
    defsnc '[	]unsigned[ ]char[ ]regs\[128\][ ]=' drivers/staging/solo6x10/solo6010-tw28.c
    defsnc 'static[ ]unsigned[ ]char[ ]vid_vop_header\[\][ ]=' drivers/staging/solo6x10/solo6010-v4l2-enc.c
    defsnc 'static[ ]const[ ]u16[ ]rop_\(map1\|action\|info\)\[\][ ]=' drivers/staging/tidspbridge/dynload/reloc_table_c6000.c
    defsnc 'static[ ]const[ ]u16[ ]tramp_\(map\|action\|info\)\[\][ ]=' drivers/staging/tidspbridge/dynload/tramp_table_c6000.c
    defsnc 'unsigned[ ]char[ ]\(sbox\|dot[23]\)_table\[256\][ ]=' drivers/staging/vt6655/aes_ccmp.c
    defsnc 'static[ ]struct[ ]pll_map[ ]pll_value\[\][ ]=' drivers/video/via/hw.c
    defsnc '[	][	]degrade_factor\[CPU_LOAD_IDX_MAX\]\[DEGRADE_SHIFT[ ][+][ ]1\][ ]=' kernel/sched.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]expected_result\[FIFO_SIZE\][ ]=' samples/kfifo/bytestream-example.c
    defsnc 'static[ ]const[ ]int[ ]expected_result\[FIFO_SIZE\][ ]=' samples/kfifo/inttype-example.c
    blobname 'haup-ir-blaster\.bin' drivers/input/lirc/lirc_zilog.c

    # New in 2.6.37, up to -rc5.
    defsnc 'static[ ]u32[ ]epll_div\[\]\[6\][ ]=' arch/arm/mach-s5pv210/clock.c
    defsnc 'static[ ]\(const[ ]\)\?struct[ ]titan_gpio_cfg[ ]titan_gpio_table\[\][ ]=' arch/mips/ar7/gpio.c
    # GNUtoo found potential sources for these on 2019-12-05, checking.
    blobname 'sdma-%s-to%d\.bin' drivers/dma/imx-sdma.c
    defsnc '[	]static[ ]u8[ ]def_regs\[\][ ]=' drivers/media/common/tuners/tda18218.c
    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]lme2510c\?_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*\([	]\.download_firmware[ ]=[ ]lme2510_download_firmware,[\n]\)\?[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/lmedm04.c
    blobname 'dvb-usb-lme2510c\?-\(lg\|s7395\)\.fw' drivers/media/dvb/dvb-usb/lmedm04.c
    defsnc 'static[ ]u8[ ]s7395_inittab\[\][ ]=' drivers/media/dvb/dvb-usb/lmedm04.h
    defsnc 'static[ ]const[ ]u16[ ]rca_initdata\[\]\[3\][ ]=' drivers/media/video/gspca/xirlink_cit.c
    blobname 'NXP7164-2010-03-10\.1\.fw' drivers/media/video/saa7164/saa7164-fw.c
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]fsmc_ecc4_lp_layout[ ]=' drivers/mtd/nand/fsmc_nand.c
    defsnc 'static[ ]struct[ ]pxa3xx_nand_timing[ ]timing\[\][ ]=' drivers/mtd/nand/pxa3xx_nand.c
    blobname 'ctfw_cna\.bin' drivers/net/bna/cna.h
    accept '[#]define[ ]CARL9170FW_NAME[ 	]\+["]carl9170-1\.fw["]' drivers/net/wireless/ath/carl9170/carl9170.h
    defsnc 'static[ ]struct[ ]carl9170_phy_init[ ]ar5416_phy_init\[\][ ]=' drivers/net/wireless/carl9170/phy.c
    defsnc 'static[ ]struct[ ]carl9170_rf_initvals[ ]carl9170_rf_initval\[\][ ]=' drivers/net/wireless/carl9170/phy.c
    defsnc 'static[ ]const[ ]struct[ ]carl9170_phy_freq_entry[ ]carl9170_phy_freq_params\[\][ ]=' drivers/net/wireless/carl9170/phy.c
    accept 'MODULE_FIRMWARE[(]CARL9170FW_NAME[)][;]' drivers/net/wireless/carl9170/usb.c
    accept '[	]return[ ]request_firmware_nowait[(][^\n]*,[ ]CARL9170FW_NAME,' drivers/net/wireless/carl9170/usb.c
    blobname 'iwlwifi-100-' drivers/net/iwlwifi/iwl-1000.c
    blobname 'iwlwifi-130-' drivers/net/iwlwifi/iwl-6000.c
    blobname 'libertas[/]cf83\(05\|8[15]\)\(_helper\)\?\.bin' drivers/net/wireless/libertas/if_cs.c
    blobname 'libertas[/]sd\(8385\|8686\(_v[89]\)\|8688\)\(_helper\)\?\.bin' drivers/net/wireless/libertas/if_sdio.c
    blobname 'libertas[/]gspi\(8385\|8686\(_v9\)\?\|8688\)\(_helper\|_hlp\)\?\.bin' drivers/net/wireless/libertas/if_spi.c
    blobname 'libertas[/]usb\(8388\(_v[59]\)\?\|8682\)\.bin' drivers/net/wireless/libertas/if_usb.c
    accept '[	][/][*][ ]Try[ ]user-specified[ ]firmware[ ]first[ ][*][/][\n][	]if[ ][(]fwname[)][\n][	][	]return[ ]request_firmware' drivers/net/wireless/libertas/if_usb.c
    accept '[	][	]ret[ ]=[ ]request_firmware[(]\(helper,[ ]user_helper\|mainfw,[ ]user_mainfw\)' drivers/net/wireless/libertas/main.c
    defsnc 'static[ ]const[ ]int[ ]\(ldo5\|buck1\)_voltage_map\[\][ ]=' drivers/regulator/lp3972.c
    accept '\([ ][*][ ]\(format\|information\)[^\n]*\|[#]define[ ]REG_DATA_FILE_A\?G[ ]*\)["]\([.][/]\)\?regulatoryData_A\?G\.bin["]' drivers/staging/ath6kl/include/common/regulatory/reg_dbschema.h
    blobname 'ath6k[/]AR6003[/]hw[12]\.0[/]\(otp\|athwlan\)\.bin\.z77' drivers/staging/ath6kl/os/linux/include/ar6000_drv.h
    blobname 'ath6k[/]AR6003[/]hw[12]\.0[/]\(athtcmd_ram\|device\|data\.patch\|endpointping\|bdata\.\(SD3[12]\|WB31\|CUSTOM\)\)\.bin' drivers/staging/ath6kl/os/linux/include/ar6000_drv.h
    defsnc 'static[ ]DDR_SET_NODE[ ]asT3\(LP\)\?B\?_DDRSetting\(80\|100\|133\|160\)MHz\[\][ ]\?=' drivers/staging/bcm/DDRInit.c
    blobname '\([/]lib[/]firmware[/]\)\?macxvi200\.bin' drivers/staging/bcm/Macros.h
    accept '-[ ]On-chip[ ]firmware[ ]loaded[ ]using[ ]standard[ ]request_firmware[(][)]' 'drivers/staging/brcm80211\(/brcmfmac\)\?/README'
    blobname 'brcm[/]bcm43xx\(_hdr\)\?-0[-0-9]*\.fw' 'drivers/\(staging\|net/wireless\)/brcm80211/README'
    blobname 'brcm[/]bcm4329-fullmac-4[-0-9]*\.\(bin\|txt\)' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmfmac/README'
    blob 'Firmware[ ]installation[\n]=\+\([\n]\+[^\n=][^\n]*\)\+\([/]lib[/]firmware[/]brcm\|\.fw\)[^\n]*\([\n][^\n=][^\n]*\)*\([\n][\n][^=\n][^\n]*[\n][^=\n][^\n]*\([\n][^\n=][^\n]*\)*\)*' 'drivers/staging/brcm80211\(/brcmfmac\)\?/README'
    defsnc '[	]u16[ ]nrate_list\[4\]\[8\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmfmac/wl_iw\.c'
    defsnc 'static[ ]chan_info_basic_t[ ]chan_info_all\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/phy/wlc_phy_cmn\.c'
    defsnc 'u16[ ]ltrn_list\[PHY_LTRN_LIST_LEN\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_cmn\.c\|brcmsmac/phy/phy_cmn\.c\)'
    defsnc 's8[ ]lcnphy_gain_index_offset_for_pkt_rssi\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_cmn\.c\|brcmsmac/phy/phy_cmn\.c\)'
    defsnc 'lcnphy_rx_iqcomp_t[ ]lcnphy_rx_iqcomp_table_rev0\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phy_lcn\.c\)'
    defsnc 'static[ ]const[ ]u32[ ]lcnphy_23bitgaincode_table\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phy_lcn\.c\)'
    defsnc 'static[ ]const[ ]s8[ ]lcnphy_gain_table\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phy_lcn\.c\)'
    defsnc 'static[ ]const[ ]s8[ ]lcnphy_gain_index_offset_for_rssi\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phy_lcn\.c\)'
    defsnc 'static[ ]chan_info_2064_lcnphy_t[ ]chan_info_2064_lcnphy\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phy_lcn\.c\)'
    defsnc 'lcnphy_radio_regs_t[ ]lcnphy_radio_regs_2064\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phy_lcn\.c\)'
    defsnc '\(static[ ]const[ ]\)\?s8[ ]lcnphy_gain_index_offset_for_pkt_rssi\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phy_lcn\.c\)'
    defsnc '\(static[ ]const[ ]\)\?u16[ \n]*LCNPHY_txdigfiltcoeffs_\(cck\|ofdm\)\[LCNPHY_NUM_TX_DIG_FILTERS_\(CCK\|OFDM\)\][\n 	]*\[LCNPHY_NUM_DIG_FILT_COEFFS[ ][+][ ]1\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmsmac/phy/phy_lcn\.c'
    defsnc '\(static[ ]const[ ]\)\?nphy_ipa_txrxgain_t[ ]nphy_ipa_rxcal_gaintbl_2GHz\(_rev7\)\?\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phy_n\.c\)'
    defsnc 'static[ ]\(const[ ]\)\?chan_info_nphy_\(radio\)\?205[5x7]\(_rev5\)\?_t[ ]chan_info_nphy\(rev[3-9]\(n6\)\?\)\?_205[5-7]\(_A1\|v\([5-8]\|11\)\|_rev[4-8]\(v1\)\?\)\?\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phy_n\.c\)'
    defsnc '\(static[ ]\)\?radio_\(20xx_\)\?regs_t[ ]regs_\(SYN_\|[RT]X_\)\?205[5-7]\(_A1\|_rev\([4-8]\|11\)\(v1\)\?\)\?\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phy_n\.c\)'
    defsnc 'static[ ]const[ ]u16[ ]tbl_iqcal_gainparams_nphy\[2\]\[NPHY_IQCAL_NUMGAINS\]\[8\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phy_n\.c\)'
    defsnc 'static[ ]\(const[ ]\)\?u32[ ]nphy_tpc_\(5GHz_\)\?txgain\(_[ei]pa\)\?\(\(_[25]g\)\?\(_\(2057\)\?\(rev\([3-7]\|4n6\)\?\)\?\)\?\|_HiPwrEPA\)\?\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phy_n\.c\)'
    defsnc 'static[ ]const[ ]u16[ ]nphy_tpc_loscale\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phy_n\.c\)'
    defsnc 'static[ ]\(const[ ]\)\?u8[ ]pad_all_gain_codes_2057\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phy_n\.c\)'
    defsnc 'static[ ]\(const[ ]\)\?u32[ ]nphy_papd_scaltbl\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phy_n\.c\)'
    defsnc '[	]s32[ ]poll_results\[8\]\[4\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phy_n\.c\)'
    defsnc '[	]nphy_txiqcal_ladder_t[ ]ladder_\(lo\|iq\)\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phy_n\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u32[ ]dot11lcn_gain_\(idx_\|val_\)\?tbl_\(rev[01]\|\(extlna_\)\?2G\|5G\)\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phytbl_lcn\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u16[ ]dot11lcn_aux_gain_idx_tbl_\(rev0\|\(extlna_\)\?2G\)\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phytbl_lcn\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u32[ ]dot11lcn_aux_gain_idx_tbl_5G\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phytbl_lcn\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u8[ ]dot11lcn_gain_val_tbl_\(rev0\|\(extlna_\)\?2G\)\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phytbl_lcn\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u16[ ]dot11lcn_\(min_sig_sq\|noise_scale\)_tbl_rev0\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phytbl_lcn\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u16[ ]dot11lcn_sw_ctrl_tbl_\(4313_\)\?\(bt_\)\?\(epa_\)\?\(p250_\)\?rev0\(_combo\)\?\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phytbl_lcn\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u8[ ]dot11lcn_spur_tbl_rev0\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phytbl_lcn\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u16[ ]dot11lcn_\(unsup_mcs\|iq_local\)_tbl_rev0\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phytbl_lcn\.c\)'
    defsnc '\(static[ ]\)\?const[ ]lcnphy_tx_gain_tbl_entry[ ]dot11lcnphy_[25]GHz_\(extPA_\)\?gaintable_rev0\[128\][ ]='  'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phytbl_lcn\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u32[ ]dot11lcn_papd_compdelta_tbl_rev0\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_lcn\.c\|brcmsmac/phy/phytbl_lcn\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u32[ ]frame_struct_rev[03]\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phytbl_n\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u8[ ]frame_lut_rev[03]\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phytbl_n\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u32[ ]\(tmap\|tdtrn\)_tbl_rev[037]\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phytbl_n\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u16[ ]pilot_tbl_rev[03]\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phytbl_n\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u32[ ]tdi_tbl[24]0_ant[01]_rev[03]\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phytbl_n\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u32[ ]chanest_tbl_rev[03]\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phytbl_n\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u8[ ]mcs_tbl_rev0\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phytbl_n\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u32[ ]noise_var_tbl[01]\?_rev[037]\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phytbl_n\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u8[ ]\(est\|adj\)_pwr_lut_core[01]_rev[03]\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phytbl_n\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u32[ ]\(gainctrl\|iq\)_lut_core[01]_rev[03]\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phytbl_n\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u16[ ]loft_lut_core[01]_rev[03]\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phytbl_n\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u16[ ]ant_swctrl_tbl_rev3\(_[1-3]\)\?\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phytbl_n\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u16[ ]mcs_tbl_rev3\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phytbl_n\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u16[ ]papd_comp_rfpwr_tbl_core[01]_rev3\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phytbl_n\.c\)'
    defsnc '\(static[ ]\)\?const[ ]u32[ ]papd_\(comp_epsilon\|cal_scalars\)_tbl_core[01]_rev[37]\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(phy/wlc_phy_n\.c\|brcmsmac/phy/phytbl_n\.c\)'
    blobname 'brcm[/]bcm43xx' 'drivers/\(staging\|net/wireless\)/brcm80211/sys/wl_mac80211\.c'
    blobname '%s\(_hdr\)\?-%d\.fw' 'drivers/\(staging\|net/wireless\)/brcm80211/sys/wl_mac80211\.c'
    defsnc 'static[ ]const[ ]u8[ ]crc8_table\[256\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(util/bcmutils\.c\|brcmutil/utils\.c\)'
    defsnc 'static[ ]const[ ]u16[ ]crc16_table\[256\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(util/bcmutils\.c\|brcmutil/utils\.c\)'
    defsnc 'static[ ]const[ ]u32[ ]crc32_table\[256\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(util/bcmutils\.c\|brcmutil/utils\.c\)'
    defsnc 'static[ ]const[ ]pmu0_xtaltab0_t[ ]pmu0_xtaltab0\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/util/hndpmu\.c'
    defsnc 'static[ ]const[ ]pmu1_xtaltab0_t[ ]pmu1_xtaltab0\(_880\(_4329\)\?\|_1760\|_1440\|_960\)\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/util/hndpmu\.c'
    defsnc 'static[ ]const[ ]s16[ ]log_table\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/\(util/qmath\.c\|brcmsmac/phy/phy_qmath\.c\)'
    blobname 'ft[12]000\.img' drivers/staging/ft1000/ft1000-pcmcia/ft1000_hw.c
    blobname 'ft3000\.img' drivers/staging/ft1000/ft1000-usb/ft1000_usb.c
    defsnc '[ ][ ][ ][ ]u8[ ]ConnectionMsg\[\][ ]='  drivers/staging/ft1000/ft1000-usb/ft1000_chdev.c
    blobname 'fw_sst_0\(80a\|82f\)\.bin' drivers/staging/intel_sst/intel_sst_common.h
    # This appends a .bin extension, but without loading the firmware
    # above, it will never arise, so leave it alone for now.
    accept '[	]len[ ][+]=[ ]snprintf[(]buf[ ][+][ ]len[,][ ]sizeof[(]buf[)][ ]-[ ]len,[ ]["][.]bin["][)][;]' drivers/staging/intel_sst/intel_sst_dsp.c
    defsnc '[	]struct[ ]sc_reg_access[ ]\(sc_acces[,][ ]\)\?sc_access\[\][ ]=' 'drivers/staging/intel_sst/intelmid_v[012]_control\.c'
    defsnc '[	]BYTE[ ]data_ptr\[36\][ ]=' 'drivers/staging/keucr/\(ms\|s[dm]\)scsi\.c'
    defsnc 'static[ ]BYTE[ ]ecctable\[256\][ ]=' drivers/staging/keucr/smilecc.c
    defsnc 'static[ ]u8[ ]MAC_REG_TABLE\[\]\[2\][ ]=' drivers/staging/rtl8187se/r8185b_init.c
    defsnc 'static[ ]u8[ ][ ]*ZEBRA_AGC\[\][ 	]=' drivers/staging/rtl8187se/r8185b_init.c
    defsnc 'static[ ]u32[ ]ZEBRA_RF_RX_GAIN_TABLE\[\][ 	]=' drivers/staging/rtl8187se/r8185b_init.c
    blob 'static[ ]const[ ]unsigned[ ]char[ ]f_array\[122328\][ ]=[ ][{]'"$sepx$blobpat*"',[\n][}][;]' drivers/staging/rtl8712/farray.h
    blob 'static[ ]u32[ ]rtl871x_open_fw[(][^)]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*f_array[^\n]*\([\n]\+[^\n}][^\n]*\)*[^\n]*[\n]\+[}]' drivers/staging/rtl8712/hal_init.c
    defsnc 'static[ ]const[ ]long[ ]frequency_list\[\][ ]=' drivers/staging/rtl8712/rtl871x_ioctl_linux.c
    defsnc 'static[ ]const[ ]unsigned[ ]short[ ]Sbox1\[2\]\[256\][ ]=' drivers/staging/rtl8712/rtl871x_security.c
    defsnc 'static[ ]const[ ]u8[ ]sbox_table\[256\][ ]=' drivers/staging/rtl8712/rtl871x_security.c
    accept '[	]119,[ ]62,[ ]6,[\n][	]0,[ ]16,[ ]20,[ ]17,[ ]32,[ ]48,[ ]0,\([\n][	][0-9]\+,\([ ][0-9]\+,\)*\)*[\n][	]0,[ ]119' drivers/staging/speakup/speakupmap.h
    defsnc 'static[ ]u32[ ]\(h_prescale\|v_gain\)\[64\][ ]=' drivers/staging/stradis/stradis.c
    accept '[/][*][ ]*\([ 1-4][0-9][ ][ ]\)*\(5[0-6][ ][ ]\)*[*][/]' drivers/staging/vt6656/channel.c
    blobname 'west[ ]bridge[ ]fw' drivers/staging/westbridge/astoria/device/cyasdevice.c
    defsnc 'static[ ]const[ ]u8[ ]gsm_fcs8\[256\][ ]=' drivers/tty/n_gsm.c
    defsnc '[	]static[ ]const[ ]struct[ ]dispc_v_coef[ ]coef_v\(up\|down\)_3tap\[8\][ ]=' drivers/video/omap2/dss/dispc.c
    blobname 'c[bt]fw_\(fc\|cna\)\.bin' drivers/scsi/bfa/bfad_im.h

    # New in 2.6.38
    blobname '%s%04x%s["][,][ ]["]fw_sst_["][,][ 	\n]*sst_drv_ctx->pci_id[,][ ]["]\.bin' drivers/staging/intel_sst/intel_sst_common.h
    accept '[ ]*[*][ ]*0[ ]1[ ]2[ ]3[ ]4[ ]5[ ]6[ ]7[ ]8[ ]9[ ]0[ ]1[ ]2[ ]3[ ]4[ ]5[ ]6[ ]7[ ]8[ ]9[ ]0[ ]1[ ]2[ ]3[ ]4[ ]5[ ]6[ ]7[ ]8[ ]9[ ]0[ ]1' 'arch/x86/crypto/aesni-intel_asm\.S\|net/l2tp/l2tp_ip6\.c'
    defsnc 'static[ ]struct[ ]aead_testvec[ ]\(aes_gcm_rfc4106\)_\(enc\|dec\)_tv_template\[\][ ]=' 'crypto/testmgr.h'
    blobname '\(sep[/]\)\?extapp\.image\.bin' drivers/staging/sep/sep_driver.c
    blobname 'radeon[/]\(BARTS\|BTC\|TURKS\|CAICOS\|%s\)_\(pfp\|rlc\|[mc][ec]\)\.bin' 'drivers/gpu/drm/radeon/[ns]i\.c'
    defsnc 'static[ ]const[ ]u32[ ]\(barts\|turks\|caicos\)_io_mc_regs\[BTC_IO_MC_REGS_SIZE\]\[2\][ ]=' drivers/gpu/drm/radeon/ni.c
    defsnc 'static[ ]int[ ]types\[0x80\][ ]=' drivers/gpu/drm/nouveau/nv50_vram.c
    blobname '\(nouveau[/]\)\?fuc4\(09\|1a\)[cd]' drivers/gpu/drm/nouveau/nvc0_graph.c
    defsnc '[	][}][ ]v_table\[\][ ]=' drivers/gpu/drm/i915/i915_dma.c
    defsnc '[}][ ]nec_8048_init_seq\[\][ ]=' drivers/video/omap2/displays/panel-nec-nl8048hl11-01b.c
    defsnc 'static[ ]const[ ]int[ ]mc13892_sw1\?\[\][ ]=' drivers/regulator/mc13892-regulator.c
    defsnc 'static[ ]const[ ]int[ ]dcdc[12]_voltages\[\][ ]=' drivers/regulator/tps6524x-regulator.c
    defsnc '[	]\(static[ ]const[ ]\)\?u8[ ]init_hash_seed\[\][ ]=' drivers/net/qlge/qlge_main.c
    blobname 'vxge[/]X3fw\(-pxe\)\?\.ncf' drivers/net/vxge/vxge-main.c
    defsnc '[ ][ ]\(static[ ]const[ ]\)\?int[ ]poly\[\]=' drivers/net/pcmcia/nmclan_cs.c
    defsnc 'static[ ]\(const[ ]\)\?int[ ]fifo_map\[\]\[MAX_TX_FIFOS\][ ]=' drivers/net/s2io.h
    defsnc 'static[ ]const[ ]struct[ ]efuse_map[ ]RTL8712_SDIO_EFUSE_TABLE\[\][ ]=' drivers/net/wireless/rtlwifi/efuse.c
    defsnc 'static[ ]const[ ]u32[ ]ofdmswing_table\[OFDM_TABLE_SIZE\][ ]=' drivers/net/wireless/rtlwifi/rtl8192ce/dm.c
    defsnc 'static[ ]const[ ]u8[ ]cckswing_table_ch\(1ch13\|14\)\[CCK_TABLE_SIZE\]\[8\][ ]=' drivers/net/wireless/rtlwifi/rtl8192ce/dm.c
    blobname 'rtlwifi[/]rtl8192cfw\.bin' drivers/net/wireless/rtlwifi/rtl8192ce/sw.c
    # This looks like pure data.
    defsnc 'static[ ]u8[ ]reserved_page_packet\[TOTAL_RESERVED_PKT_LEN\][ ]=' 'drivers/net/wireless/rtlwifi/rtl8192[cd]e/fw.c'
    defsnc 'u32[ ]RTL8192CE\(PHY_REG\|_\?RADIO[AB]\|MAC\|AGCTAB\)_\([21]T_\?ARRAY\|ARRAY_PG\)\[\(PHY_REG\|RADIO[AB]\|MAC\|AGCTAB\)_\([21]T_\?ARRAY_\?\|ARRAY_PG\)LENGTH\][ ]=' drivers/net/wireless/rtlwifi/rtl8192ce/table.c
    defsc 'static[ ]const[ ]struct[ ]ar9300_eeprom[ ]ar9300_[hx]11[236][ ]=' drivers/net/wireless/ath/ath9k/ar9003_eeprom.c
    defsnc 'static[ ]const[ ]struct[ ]b43_nphy_channeltab_entry_rev3[ ]b43_nphy_channeltab_rev\([34568]\|7_9\)\[\][ ]=' drivers/net/wireless/b43/radio_2056.c
    blobname '["]softing-4[.]6[/]["]' drivers/net/can/softing/softing_platform.h
    blobname '\(softing-4[.]6[/]\)\?\(\(b\|ld\)card2\?\|can\(card\|sja\|crd2\)\)\.bin' drivers/net/can/softing/softing_cs.c
    blobna 'which[ ]you[ ]can[ ]get[ ]at[\n][	][ ][ ]http:[/][/][^\n]*[/]socketcan[/][\n][^-]*firmware[ ]version' drivers/net/can/softing/Kconfig
    defsnc 'static[ ]struct[ ]regdata[ ]mb86a20s_init\[\][ ]=' drivers/media/dvb/frontends/mb86a20s.c
    defsnc 'static[ ]struct[ ]regdata[ ]s921_init\[\][ ]=' drivers/media/dvb/frontends/s921.c
    defsnc 'static[ ]const[ ]struct[ ]regval_list[ ]ov2640_init_regs\[\][ ]=' drivers/media/video/ov2640.c
    defsnc 'static[ ]const[ ]struct[ ]ov_i2c_regvals[ ]norm_7660\[\][ ]=' drivers/media/video/ov519.c
    defsnc '[	]static[ ]const[ ]struct[ ]ov_regvals[ ]bridge_ov7660\[2\]\[10\][ ]=' drivers/media/video/gspca/ov519.c
    defsnc '[	]static[ ]const[ ]u8[ ]fr_tb\[2\]\[6\]\[3\][ ]=' drivers/media/video/gspca/ov519.c
    defsnc '[	]static[ ]const[ ]struct[ ]ov_i2c_regvals[ ]\(brit\|contrast\|colors\)_7660\[\]\[\(6\|7\|31\)\][ ]=' drivers/media/video/gspca/ov519.c
    blobname 'radio-wl1273-fw\.bin' drivers/media/radio/radio-wl1273.c
    defsnc '[}][ ]scrubrates\[\][ ]=' drivers/edac/amd64_edac.c
    defsnc '[	]static[ ]const[ ]uint8_t[ ]branch_table\[32\][ ]=' lib/xz/xz_dec_bcj.c
    defsnc 'static[ ]const[ ]struct[ ]_pll_div[ ]codec_master_pll_div\[\][ ]=' sound/soc/codecs/alc5623.c
    defsnc '[}][ ]coeff_div\[\][ ]=' sound/soc/codecs/wm8737.c
    blobname 'rpm_firmware\(_rev11\)\?\.bin' sound/pci/rme9652/hdsp.c
    blobname 'mwl8k[/]fmimage_8366_ap-["][ ][#]api[ ]["]\.fw' drivers/net/wireless/mwl8k.c
    blobname 'rtl_nic[/]rtl8168d-[12]\.fw' drivers/net/r8169.c
    # New in 2.6.38.4
    defsnc '[	]static[ ]DEFINE_TEST_\(OK\|FAIL\)[(][^)]*[)][ ]=' lib/test-kstrtox.c

    # New in 2.6.39
    blobna 'printk[(]KERN_ERR[ ]["]r8712u:[ ]Install[^\n"]*firmware[\\]n["][)][;]' drivers/staging/rtl8712/hal_init.c
    defsnc 'static[ ]const[ ]struct[ ]phy_reg[ ]exynos4_sataphy_\(cmu\|\(com\)\?lane\)\[\][ ]=' arch/arm/mach-exynos4/dev-ahci.c
    defsnc 'static[ ]struct[ ]clk_pll_\(freq_\)\?table[ ]tegra_pll_[adpxm]_\(freq_\)\?table\[\][ ]=' arch/arm/mach-tegra/tegra2_clocks.c
    initnc '\.irp[ ]idx' arch/x86/include/asm/entry_arch.h
    initnc '\.irp[ ]idx' arch/x86/kernel/entry_64.S
    defsnc 'static[ ]const[ ]u8[ ]types\[256\][ ]=' drivers/gpu/drm/nouveau/nvc0_vram.c
    defsnc 'static[ ]__u8[ ]keytouch_fixed_rdesc\[\][ ]=' drivers/hid/hid-keytouch.c
    blobname 'dib9090\.fw' drivers/media/dvb/dvb-usb/dib0700_devices.c
    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]\(dw\(210[24]\|3101\)\|s6[3x]0\)_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\|size_of_priv\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/dw2102.c
    accept '[	]\(p1100\|s660\)->firmware[ ]=' drivers/media/dvb/dvb-usb/dw2102.c
    blobname 'dvb-usb-\(p1100\|s660\)\.fw' drivers/media/dvb/dvb-usb/dw2102.c
    blobname 'dvb-usb-lme2510c\?-s0194\.fw' drivers/media/dvb/dvb-usb/lmedm04.c
    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]technisat_usb2_devices[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\|identify_state\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/technisat-usb2.c
    blobname 'dvb-usb-SkyStar_USB_HD_FW_v17_63\.HEX\.fw' drivers/media/dvb/dvb-usb/technisat-usb2.c
    defsnc 'static[ ]const[ ]struct[ ]dib0090_pll[ ]dib0090_\(p1g_\)\?pll_table\[\][ ]=' drivers/media/dvb/frontends/dib0090.c
    defsnc '[	]static[ ]u8[ ]sine[ ]\?\[\][ ]=' drivers/media/dvb/frontends/dib7000p.c
    defsnc '\(static[ ]const[ ]\)\?u32[ ]fe_info\[44\][ ]=' drivers/media/dvb/frontends/dib9000.c
    blobname 'dvb-netup-altera-01\.fw' drivers/media/video/cx23885/cx23885-cards.c
    # These are suspicious, but the regularity suggests data.
    defsnc 'static[ ]const[ ]u8[ ]\(nw80[012]\|spacecam2\?\|cvideopro\|dlink\|ds3303\|kr651\|kritter\|mustek\|proscope\|twinkle\|dvcv6\)_start\(_\([12]\|q\?vga\)\)\?\[\][ ]=' drivers/media/video/gspca/nw80x.c
    defsnc 'static[ ]const[ ]u8[ ]\(bridge\|sensor\)_init_7\(67\|72\)x\[\]\[2\][ ]=' drivers/media/video/gspca/ov534.c
    defsnc '[	]static[ ]u8[ ]color_tb\[\]\[6\][ ]=' drivers/media/video/gspca/ov534.c
    defsnc 'static[ ]const[ ]struct[ ]isprsz_coef[ ]filter_coefs[ ]=' drivers/media/video/omap3isp/ispresizer.c
    defsnc 'static[ ]const[ ]struct[ ]ov9740_reg[ ]ov9740_defaults\[\][ ]=' drivers/media/video/ov9740.c
    defsnc 'static[ ]int[ ]therm_tbl\[\][ ]=' drivers/mfd/twl4030-madc.c
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]nandv2_hw_eccoob_\(largepage\|4k\)[ ]=' drivers/mtd/nand/mxc_nand.c
    defsnc 'static[ ]const[ ]u32[ ]ar9485\(\(C\|_c\)ommon_\(wo_xlna_\)\?rx_gain\)\?_1_[01]\(_\(radio\|baseband\|mac\)_core\)\?\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/ar9485_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9485_1_[01]_\(mac\|baseband\)_postamble\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar9485_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9485\(M\|_m\)odes_\(high\|low\|green\)\(est\)\?_\(power\|ob_db\)_tx_gain_1_[01]\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar9485_initvals.h
    defsnc '\(static[ ]\)\?const[ ]u\(8\|16\|32\)[ ]b43_ntab_\(\(adjustpower\|estimatepowerlt\|gainctl\|iqlt\|loftlt\|noisevar1\?\|tdi[24]0a\)[01]\|channelest\|frame\(lookup\|struct\)\|mcs\|pilot\|tdtrn\|tmap\)\(_r3\)\?\[\][ ]=' drivers/net/wireless/b43/tables_nphy.c
    defsnc 'struct[ ]nphy_gain_ctl_workaround_entry[ ]nphy_gain_ctl_workaround\[2\]\[3\][ ]=' drivers/net/wireless/b43/tables_nphy.c
    blobname '\(ti-connectivity[/]\)\?wl1271-\(fw\(-2\|-ap\)\?\|nvs\)\.bin' drivers/net/wireless/wl12xx/wl1271.h
    accept '#define\([ ]_\?IWL\(4965\|[156]000\(G2[AB]\)\?\|1[03]0\|5150\|6050\|20[03]\?0\)_MODULE_FIRMWARE[(]api[)]\)\+' 'drivers/net/iwlwifi/iwl-\([1256]000\|4965\)\.c'
    blobname 'rtlwifi[/]rtl8192cufw\.bin' drivers/net/wireless/rtlwifi/rtl8192cu.sw
    blobname 'rtlwifi[/]rtl8712u\.bin' drivers/staging/rtl8712/hal_init.c
    defsnc 'u32[ ]\(RTL\|Rtl\)8192CU\(PHY_REG\|_\?\(RADIO\|Radio\)[AB]\|MAC\|AGCTAB\)_\([21]T\(_HP\)\?_\?\(ARRAY\|Array\)\|\(ARRAY\|Array\)_PG\)\(_HP\)\?\[RTL8192CU\(PHY_REG\|\(RADIO\|Radio\)[AB]\|MAC\|AGCTAB\)_\([21]T\(_HP\)\?_\?\(ARRAY\|Array\)_\?\|\(ARRAY\|Array\)_PG\)\(_HP\)\?\(LENGTH\|Length\)\][ ]=' drivers/net/wireless/rtlwifi/rtl8192cu/table.c
    blobname 'rtl_nic[/]rtl8105e-1\.fw' drivers/net/r8169.c
    defsnc 'static[ ]const[ ]\(A_INT32\|s32\)[ ]wmi_rateTable\[\]\[2\][ ]=' drivers/staging/ath6kl/wmi/wmi.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]\(stk1160\|saa7113\)config[ ]\([{][^}]*[}][ ]\)\?\(stk1160\|saa7113\)config\(PAL\|NTSC\)\?\[\(256\)\?\][ ]=' drivers/staging/easycap/easycap_low.c
    defsnc 'static[ ]const[ ]ccktxbbgain_struct[ ]rtl8192_cck_txbbgain_\(ch14_\)\?table\[\][ ]=' drivers/staging/rtl8192e/r8192E_dm.c
    defsnc '[	]unsigned[ ]char[ ]data_ptr\[36\][ ]=' drivers/usb/storage/ene_ub6250.c
    blobname 'ene-ub6250[/]sd_\(init[12]\|rdwr\)\.bin' drivers/usb/storage/ene_ub6250.c
    defsnc 'static[ ]const[ ]struct[ ]hdmi_timings[ ]cea_vesa_timings\[OMAP_HDMI_TIMINGS_NB\][ ]=' drivers/video/omap2/dss/hdmi.c
    defsnc 'static[ ]struct[ ]pll_config[ ]\(cle266\|k800\|cx700\|vx855\)_pll_config\[\][ ]=' drivers/video/via/hw.c
    defsnc 'static[ ]char[ ]channel_map_unity_ss\[HDSPM_MAX_CHANNELS\][ ]=' sound/pci/rme9652/hdspm.c
    defsnc 'static[ ]const[ ]u8[ ]log_volume_table\[128\][ ]=' sound/usb/6fire/control.c
    defsnc 'static[ ]const[ ]struct[ ][{][^}]*[}][\n]init_data\[\][ ]=' drivers/usb/6fire/control.c
    blobname '6fire[/]dmx6fire\(l2\|ap\|cf\)\.\(ihx\|bin\)' sound/usb/6fire/firmware.c
    defsnc 'static[ ]const[ ]u8[ ]BIT_REVERSE_TABLE\[256\][ ]=' sound/usb/6fire/firmware.c
    initnc '[/][*][\n][ ][*][ ]\(cfa_coef\|gamma\|luma_enhance\|noise_filter\)_table\.h[\n][ ][*]\([^\n]*[\n][ ][*]\)*[/]' 'drivers/media/video/omap3isp/\(cfa_coef\|gamma\|luma_enhance\|noise_filter\)_table\.h'
    blobna 'rocess_sigma_firmwar'
    defsnc 'int[ ]process_sigma_firmware[(][^)]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*\(request\|maybe_reject\)_firmware' drivers/firmware/sigma.c
    accept 'EXPORT_SYMBOL[(]process_sigma_firmware[)]' drivers/firmware/sigma.c
    accept 'extern[ ]int[ ]process_sigma_firmware[(][^)]*[)][;]' include/linux/sigma.h
    blobname 'maxtouch\.fw' drivers/input/touchscreen/atmel_mxt_ts.c
    blobname 'fm\(c\|_[rt]x\)_ch8\(_[0-9a-f]*\.[0-9]*\.bts\)\?' drivers/media/radio/wl128x/fmdrv_common.h
    blobname '%s_%x\.%d\.bts' drivers/media/radio/wl128x/fmdrv_common.c
    blobname 'vntwusb\.fw' drivers/staging/vt6656/firmware.c
    # New in 3.0.
    accept 'resume[/]restore[,][ ]but[ ]they[ ]cannot[ ]do[ ]it[ ]by[ ]calling[ ]request_firmware[(][)]' Documentation/power/notifiers.txt
    accept '[	][	][	]interrupts[ ]=[ ]<\([\n][	][	][	][	]0xe[0-7][ ]0[ ]0[ ]0\)*>[;]' arch/powerpc/boot/dts/p1022ds.dts
    accept '[ ][ ][ ][ ]gzip[ ]-n[ ]--force[ ]-9[ ]--stdout[ ]["][$]ofile\.bin["][ ]>[ ]["][$]odir[/]otheros\.bld["]' arch/powerpc/boot/wrapper
    defsnc '\(uint32_t\|u32\)[ ]nva3_pcopy_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nva3_copy.fuc.h
    defsnc '\(uint32_t\|u32\)[ ]nvc0_pcopy_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvc0_copy.fuc.h
    accept '[	]struct[ ]nvc0_graph_fuc[ ]fuc4\(09\|1a\)[cd]' drivers/gpu/drm/nouveau/nvc0_graph.h
    defsnc 'static[ ]const[ ]u8[ ]sht15_crc8_table\[\][ ]=' drivers/hwmon/sht15.c
    defsnc 'static[ ]u8[ ]stv0288_bsbe1_d01a_inittab\[\][ ]=' drivers/media/dvb/frontends/bsbe1-d01a.h
    defsnc '[	]struct[ ]reg_val_mask[ ]tab\[\][ ]=' 'drivers/media/dvb/frontends/\(cxd2820r_\(c\|t2\)\|af9033\)\.c'
    blobname 'drxd-a2-1\.1\.fw' drivers/media/dvb/frontends/drxd_hard.c
    blobname 'drxd-b1-1\.1\.fw' drivers/media/dvb/frontends/drxd_hard.c
    blob '[/][*][	]if[ ][(]\(reject\|request\)_firmware[(][&]state->fw[,][ ]["]drxd\.fw["][,][ ]state->dev[)]<0[)][ ][*][/]'
    blobname 'drxd\.fw' drivers/media/dvb/frontends/drxd_hard.c
    defsnc '[	]static[ ]char[ ]init_values\[38\]\[3\][ ]=' drivers/media/video/usbvision/usbvision-core.c
    blobna 'www\.elandigitalsys[^\n]*download' drivers/mmc/host/Kconfig
    blobname 'vub_\(default\.bin\|%04X%04X\)' drivers/mmc/host/vub300.c
    blobna 'snprintf[(]vub300->vub_name[ ][+][^\n]*[,][ ]["]\.bin["][)][;]' drivers/mmc/host/vub300.c
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]flexonenand_oob_128[ ]=' drivers/mtd/onenand/onenand_base.c
    defsnc 'static[ ]const[ ]u32[ ]ar9340Modes_\(\(low\(est\)\?\|high\|mixed\)_ob_db\|high_power\|ub124\)_tx_gain_table_1p0\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar9340_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9340_1p0_\(radio\|baseband\|mac\)_core\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/ar9340_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9340_1p0_\(mac\|baseband\)_postamble\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar9340_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9340Common_\(wo_xlna_\)\?rx_gain_table_1p0\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/ar9340_initvals.h
    defsnc 'static[ ]u16[ ]mwifiex_data_rates\[MWIFIEX_SUPPORTED_RATES_EXT\][ ]=' drivers/net/wireless/mwifiex/cfp.c
    accept '[	]\.helper[	][	]=[ ]NULL[,][\n][	]*\.firmware' drivers/bluetooth/btmrvl_sdio.c
    blobname 'mrvl[/]sd8787_uapsta\(_w1\)\?\.bin' drivers/net/wireless/mwifiex/main.h
    blobname 'sd8787\.bin' drivers/net/wireless/mwifiex/sdio.c
    blobna 'Copy[ ]sd8787\.bin[ ]to[^.]*[.]' drivers/net/wireless/mwifiex/README
    blobname 'rtlwifi[/]rtl8192sefw\.bin' drivers/net/wireless/rtlwifi/rtl8192se/sw.c
    defsnc 'u32[ ]rtl8192sephy_reg_2t2rarray\[PHY_REG_2T2RARRAYLENGTH\][ ]=' drivers/net/wireless/rtlwifi/rtl8192se/table.c
    defsnc 'u32[ ]rtl8192sephy_changeto_1t[12]rarray\[PHY_CHANGETO_1T[12]RARRAYLENGTH\][ ]=' drivers/net/wireless/rtlwifi/rtl8192se/table.c
    defsnc 'u32[ ]rtl8192sephy_reg_array_pg\[PHY_REG_ARRAY_PGLENGTH\][ ]=' drivers/net/wireless/rtlwifi/rtl8192se/table.c
    defsnc 'u32[ ]rtl8192seradioa_1t_array\[RADIOA_1T_ARRAYLENGTH\][ ]=' drivers/net/wireless/rtlwifi/rtl8192se/table.c
    defsnc 'u32[ ]rtl8192semac_2t_array\[MAC_2T_ARRAYLENGTH\][ ]=' drivers/net/wireless/rtlwifi/rtl8192se/table.c
    defsnc 'u32[ ]rtl8192seagctab_array\[AGCTAB_ARRAYLENGTH\][ ]=' drivers/net/wireless/rtlwifi/rtl8192se/table.c
    accept 'Place[ ]isci_firmware\.bin[ ]in' drivers/scsi/isci/firmware/README
    # This is not a code blob, it is just small data structures described in create_fw.[ch].
    accept 'static[ ]const[ ]char[ ]blob_name\[\][ ]=[ ]["]isci_firmware\.bin["]' drivers/scsi/isci/create_fw.h
    accept '[	][	]orom[ ]=[ ]isci_request_firmware' drivers/scsi/isci/init.c
    accept 'MODULE_FIRMWARE[(]ISCI_FW_NAME[)][;]' drivers/scsi/isci/init.c
    accept 'struct[ ]isci_orom[ ][*]isci_request_firmware[(]' 'drivers/scsi/isci/probe_roms\.[ch]'
    accept '[	]if[ ][(]request_firmware[(][&]fw[,][ ]ISCI_FW_NAME[,]' drivers/scsi/isci/probe_roms.c
    accept '#define[ ]ISCI_FW_NAME[	][	]["]isci[/]isci_firmware\.bin["]' drivers/scsi/isci/probe_roms.h
    defsnc 'static[ ]struct[ ]pll_limit[ ]\(cle266\|k800\|cx700\|vx855\)_pll_limits\[\][ ]=' drivers/video/via/hw.c
    accept '[	][	]-e[ ]["][$]tmp_dir[/]lib[/]modules[/][$]KERNELRELEASE[/]modules\.dep\.bin["]' scripts/depmod.sh
    blobname 'wm8958_\(enh_eq\|mbc\(_vss\)\?\)\.wfw' sound/soc/codecs/wm8958-dsp2.c
    blobname 'rtl_nic[/]rtl8168e-[12]\.fw' drivers/net/r8169.c
    defsnc '[	]static[ ]const[ ]struct[ ]ephy_info[ ]e_info_8168e\[\][ ]=' drivers/net/r8169.c
    blobname 'ti-connectivity[/]wl128x-fw\(-ap\)\?\.bin' drivers/net/wireless/wl12xx/wl12xx.h
    defsnc 'static[ ]const[ ]u8[ ]tg3_tso_header\[\][ ]=' drivers/net/tg3.c
    blobname 'ath6k[/]AR6003[/]hw2\.1\.1[/]\(otp\|athwlan\|athtcmd_ram\|device\|data\.patch\|endpointping\|bdata\.\(SD3[12]\|WB31\|CUSTOM\)\)\.bin' drivers/staging/ath6kl/os/linux/include/ar6000_drv.h
    accept '[	]nvc0_graph_init_fuc[(]dev[,][ ]0x4\(09\|1a\)000[,][ ][&]priv->fuc4\(09\|1a\)c[,][ ][&]priv->fuc4\(09\|1a\)d[)][;]' drivers/gpu/drm/nouveau/nvc0_graph.c
    accept '[	][	 ]*nvc0_graph_destroy_fw[(]&priv->fuc4\(09\|1a\)[cd][)][;]' drivers/gpu/drm/nouveau/nvc0_graph.c
    accept '[	][	 ]*\(if[ ][(]\|[ ][ ][ ][ ]\)nvc0_graph_create_fw[(]dev[,][ ]["]fuc4\(09\|1a\)[cd]["][,][ ][&]priv->fuc4\(09\|1a\)[cd][)]' drivers/gpu/drm/nouveau/nvc0_graph.c
    blobname 'nouveau[/]\(nv%02x_\)\?%s' 'drivers/gpu/drm/nouveau/nv[ce]0_graph\.c'
    blobname 'radeon[/]SUMO2\?_\(pfp\|me\)\.bin' drivers/gpu/drm/radeon/r600.c
    blobname 'iwlwifi-\(105\|20[03]\?0\)-' drivers/net/iwlwifi/iwl-2000.c
    blobname '__stringify[(]api[)][ ]["]\.ucode["]' 'drivers/net/iwlwifi/iwl-\(3945.h\|\(4965\|[1256]000\)\.c\)'
    # New in 3.1
    blobname 'sdma-imx25\.bin' arch/arm/mach-imx/mm-imx25.c
    blobname 'sdma-imx31-to[12]\.bin' arch/arm/mach-imx/mm-imx31.c
    blobname 'sdma-imx35-to[12]\.bin' arch/arm/mach-imx/mm-imx35.c
    blobname 'sdma-imx5[13]\.bin' arch/arm/mach-mx5/mm.c
    blobname 'brcm[/]bcm43xx' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmsmac/mac80211_if\.c'
    blobname '%s\(_hdr\)\?-%d\.fw' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmsmac/mac80211_if\.c'
    blobname 'brcm[/]bcm4329-fullmac-4\.\(bin\|txt\)' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmfmac/bcmchip\.h'
    blobname 'mrvl[/]sd8787_uapsta\.bin' drivers/net/wireless/mwifiex/sdio.h
    defsnc 'static[ ]int[ ]omap3_batt_table\[\][ ]=' arch/arm/mach-omap2/twl-common.c
    defsnc '[	]static[ ]u8[ ]InitRegs\[\][ ]=' drivers/media/dvb/frontends/tda18271c2dd.c
    defsnc 'static[ ]struct[ ]SMapI[ ]m_RF_Cal_Map\[\][ ]=' drivers/media/dvb/frontends/tda18271c2dd_maps.h
    defsnc 'static[ ]struct[ ]SMap2[ ]m_\(Main\|Cal\)_PLL_Map\[\][ ]=' drivers/media/dvb/frontends/tda18271c2dd_maps.h
    accept '[	][ ][ ]For[ ]example,[ ]you[ ]might[ ]set[ ]CONFIG_EXTRA_FIRMWARE=["]whatever\.bin["]' drivers/base/Kconfig
    accept '[	][ ][ ]Then[ ]any[ ]request_firmware[(]\(["]whatever\.bin["]\)[)]' drivers/base/Kconfig
    blobname 'dvb-fe-xc4000-1.4.fw' drivers/media/common/tuners/xc4000.c
    defsnc 'static[ ]struct[ ]SMap2\?[ ]*m_\(GainTaper\|RF_Cal_DC_Over_DT\|CID_Target\)_Map\[\][ ]=' drivers/media/dvb/frontends/tda18271c2dd_maps.h
    defsnc '[	][}][ ]regs\[\][ ]=' drivers/media/video/em28xx/em28xx-dvb.c
    defsnc 'static[ ]struct[ ]regval_list[ ]ov5642_default_regs_\(init\|finalise\)\[\][ ]=' drivers/media/video/ov5642.c
    defsnc 'static[ ]const[ ]u8[ ]hdmiphy_conf\(27\(_027\)\?\|74\(_175\|_25\)\|148_5\)\[32\][ ]=' drivers/media/video/s5p-tv/hdmiphy_drv.c
    defsnc 'static[ ]const[ ]u8[ ]filter_y_vert_tap4\[\][ ]=' drivers/media/video/s5p-tv/mixer_reg.c
    defsnc '[	]static[ ]const[ ]char[ ][*][ ]const[ ]vui_sar_idc\[\][ ]=' drivers/media/video/v4l2-ctrls.c
    defsnc 'static[ ]const[ ]u32[ ]ar9331_\(1p[12]_\(baseband\|mac\)_postamble\|modes_\(low\(est\)\?\|high\)_\(ob_db\|power\)_tx_gain_1p[12]\)\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar9330_1p1_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9331_\(1p[12]_\(radio\|baseband\|mac\)_core\|common_\(wo_xlna_\)\?rx_gain_1p[12]\)\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/ar9330_1p1_initvals.h
    defsnc 'static[ ]const[ ]u\(16\|32\)[ ]b43_httab_0x\(1[2abcf]\(_0x\(1\?c\|[12]4\)0\)\?\|2[0-7]\)\[\][ ]=' drivers/net/wireless/b43/tables_phy_ht.c
    defsnc 'static[ ]u32[ ]targetchnl_5g\[TARGET_CHNL_NUM_5G\][ ]=' drivers/net/wireless/rtlwifi/rtl8192de/phy.c
    defsnc '[	]u8[ ]channel_\(5g\|all\|info\)\[\(45\|59\)\][ ]=' drivers/net/wireless/rtlwifi/rtl8192de/phy.c
    blobname 'rtlwifi[/]rtl8192defw[.]bin' drivers/net/wireless/rtlwifi/rtl8192de/sw.c
    defsnc 'u32[ ]rtl8192de_\(phy_reg\|radio[ab]\|mac\|agctab\)_\(\(2t\(_int_pa\)\?\|[25]g\)\?array\|array_pg\)\[\(PHY_REG\|RADIO[AB]\|MAC\|AGCTAB\)_\(\(2T\(_INT_PA\)\?_\|[25]G_\)\?ARRAY\|ARRAY_PG_\)LENGTH\][ ]=' drivers/net/wireless/rtlwifi/rtl8192de/table.c
    defsnc 'static[ ]\(const[ ]\)\?struct[ ]chan_info_basic[ ]chan_info_all\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmsmac/phy/phy_cmn\.c'
    defsnc 'struct[ ]lcnphy_rx_iqcomp[ ]lcnphy_rx_iqcomp_table_rev0\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmsmac/phy/phy_lcn\.c'
    defsnc 'static[ ]\(const[ ]\)\?struct[ ]chan_info_2064_lcnphy[ ]chan_info_2064_lcnphy\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmsmac/phy/phy_lcn\.c'
    defsnc '\(static[ ]const[ ]\)\?struct[ ]lcnphy_radio_regs[ ]lcnphy_radio_regs_2064\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmsmac/phy/phy_lcn\.c'
    defsnc '\(static[ ]const[ ]\)\?struct[ ]nphy_ipa_txrxgain[ ]nphy_ipa_rxcal_gaintbl_2GHz\(_rev7\)\?\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmsmac/phy/phy_n\.c'
    defsnc 'static[ ]\(const[ ]\)\?struct[ ]chan_info_nphy_2055[ ]chan_info_nphy_2055\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmsmac/phy/phy_n\.c'
    defsnc 'static[ ]\(const[ ]\)\?struct[ ]chan_info_nphy_radio205x[ ]chan_info_nphyrev\(3_2056\|4_2056_A1\|5_2056v5\|6_2056v6\|5n6_2056v7\|6_2056v\(8\|11\)\)\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmsmac/phy/phy_n\.c'
    defsnc 'static[ ]\(const[ ]\)\?struct[ ]chan_info_nphy_radio2057[ ]chan_info_nphyrev\(7_2057_rev4\|8_2057_rev[78]\)\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmsmac/phy/phy_n\.c'
    defsnc 'static[ ]\(const[ ]\)\?struct[ ]chan_info_nphy_radio2057_rev5[ \n]chan_info_nphyrev\(8_2057_rev5\|9_2057_rev5v1\)\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmsmac/phy/phy_n\.c'
    defsnc '\(static[ ]\)\?\(const[ ]\)\?struct[ ]radio_\(20xx_\)\?regs[ \n]regs_\(2055\|\(SYN\|[TR]X\)_205\(6\(_A1\|_rev\([5678]\|11\)\)\?\)\|2057_rev\([4578]\|5v1\)\)\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmsmac/phy/phy_n\.c'
    defsnc '[	]struct[ ]nphy_txiqcal_ladder[ ]ladder_\(lo\|iq\)\[\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmsmac/phy/phy_n\.c'
    defsnc '\(static[ ]\)\?const[ ]struct[ ]lcnphy_tx_gain_tbl_entry[ \n]dot11lcnphy_[25]GHz_\(extPA_\)\?gaintable_rev0\[128\][ ]=' 'drivers/\(staging\|net/wireless\)/brcm80211/brcmsmac/phy/phytbl_lcn\.c'
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]raw_edid\[\][ ]=' drivers/staging/gma500/mrst_hdmi.c
    defsnc 'static[ ]const[ ]u8[ ]net2272_test_packet\[\][ ]=' drivers/usb/gadget/net2272.c
    defsnc 'static[ ]const[ ]unsigned[ ]short[ ]seq_setting\[\][ ]=' drivers/video/backlight/ams369fg06.c
    defsnc 'static[ ]u8[ ]adav80x_default_regs\[\][ ]=' sound/soc/codecs/adav80x.c
    defsnc 'static[ ]const[ ]u8[ ]sta32x_regs\[STA32X_REGISTER_COUNT\][ ]=' sound/soc/codecs/sta32x.c
    defsnc '[}][ ]mclk_ratios\[3\]\[7\][ ]=' sound/soc/codecs/sta32x.c
    defsnc 'static[ ]const[ ]int[ ]vid_to_voltage\[32\][ ]=' tools/power/cpupower/debug/i386/dump_psb.c
    blobname 'dvb-usb-terratec-h5-drxk\.fw' drivers/media/video/em28xx/em28xx-dvb.c
    blobname 's5pc110-mfc\.fw' drivers/media/video/s5p-mfc/s5p_mfc_ctrl.c
    blobname 'adau1701\.bin' sound/soc/codecs/adau1701.c
    accept '[	]return[ ]process_sigma_firmware[(]codec->control_data[,][ ]ADAU1701_FIRMWARE[)]' sound/soc/codecs/adau1701.c
    # Sources for these are in the corresponding .fuc files.
    defsnc 'uint32_t[ ]nvc0_grgpc_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvc0_grgpc.fuc.h
    defsnc 'uint32_t[ ]nvc0_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvc0_grhub.fuc.h
    accept '[	][	][	]interrupts[ ]=[ ]<\([\n][	]*0x[ef][0-9a-f][ ]0[ ]0[ ]0\)*>[;]' 'arch/powerpc/boot/dts/p\(2040\|3041\|4080\|5020\)si\.dtsi'
    blobname 'dvb-netup-altera-04\.fw' drivers/media/video/cx23885/cx23885-cards.c
    blobname 'rtl_nic[/]rtl8168e-3\.fw' drivers/net/r8169.c
    defsnc '[	]static[ ]const[ ]struct[ ]ephy_info[ ]e_info_8168e_1\[\][ ]=' drivers/net/r8169.c
    blobname 'iwlwifi-135-' drivers/net/iwlwifi/iwl-2000.c
    blobname 'c[bt]2\?fw\(_\(fc\|cna\)\)\?\.bin' drivers/scsi/bfa/bfad.c
    blobname 'ene-ub6250[/]\(ms_\(init\|rdwr\)\|msp_rdwr\)\.bin' drivers/usb/storage/ene_ub6250.c
    accept '[	][	]*dsp_code->pvt->firmware[ ]=[ ]' sound/pci/asihpi/hpidspcd.c
    # New in 3.2
    blobname 'ath6k[/]AR600[0-9.]*[/]hw[0-9.]*[/][^/"]*\.\(bin\|z77\)' drivers/net/wireless/ath/ath6kl/core.h
    accept 'userspace[,][ ]using[ ]the[ ]request_firmware[(][)][ ]function' Documentation/power/suspend-and-cpuhotplug.txt
    defsnc 'static[ ]struct[ ]sh_keysc_info[ ]keysc_platdata[ ]=[ ]' arch/arm/mach-shmobile/board-kota2.c
    defsnc 'static[ ]const[ ]u32[ ]rir_offset\[MAX_RIR_RANGES\]\[MAX_RIR_WAY\][ ]=' drivers/edac/sb_edac.c
    defsnc '[	]struct[ ]tda10071_reg_val_mask[ ]tab2\[\][ ]=' drivers/media/dvb/frontends/tda10071.c
    defsnc 'static[ ]const[ ]u8[ ]\(ov965x\|ov971x\|ov562x\)_init\(_2\)\?\[\]\[2\][ ]=' drivers/media/video/gspca/ov534_9.c
    defsnc 'static[ ]const[ ]u8[ ]DQT\[17\]\[130\][ ]=' drivers/media/video/gspca/topro.c
    defsnc 'static[ ]const[ ]struct[ ]cmd[ ]tp6810_late_start\[\][ ]=' drivers/media/video/gspca/topro.c
    defsnc '[	]static[ ]const[ ]struct[ ]cmd[ ]sensor_init\[\][ ]=' drivers/media/video/gspca/topro.c
    defsnc '[	]static[ ]const[ ]u8[ ]gamma_tb\[NGAMMA\]\[3\]\[1024\][ ]=' drivers/media/video/gspca/topro.c
    defsnc 'static[ ]struct[ ]s5k6aa_regval[ ]s5k6aa_analog_config\[\][ ]=' drivers/media/video/s5k6aa.c
    defsnc 'static[ ]const[ ]u32[ ]\(ar5416Modes\(_91[06]0\)\?\|ar9280Modes\(_\(backoff_[12]3db\|original\)_rxgain\|_\(high_power\|original\)_tx_gain\)\?_9280_2\|ar9285Modes\(\(_\(high_power\|original\)_tx_gain\)\?_9285_1_2\|_XE2_0_\(normal\|high\)_power\)\|ar9287Modes\(_[tr]x_gain\)\?_9287_1_1\|ar9271Modes\(_\(normal\|high\)_power_tx_gain\)\?_9271\(_ANI_reg\)\?\)\[\]\[5\][ ]=' 'drivers/net/wireless/ath/ath9k/ar\(5008\|9002\)_initvals\.h'
    defsnc 'static[ ]const[ ]u32[ ]\(ar9\(462\|580\)_\([12]p0_\)\?\(\(baseband\|mac\|radio\)_core\(_emulation\)\?\|\(common_\)\?\(wo_xlna_\|mixed_\)\?rx_gain_table\(_ar9280\)\?\(_[12]p0\)*\)\|ar9200_ar9280_2p0_radio_core\(_1p0\)\?\)\[\]\[2\][ ]=' 'drivers/net/wireless/ath/ath9k/ar9\(462\|580\)_[12]p0_initvals\.h'
    defsnc 'static[ ]const[ ]u32[ ]ar9\(462\|580\)_\([12]p0_\)\?\(\(tx_gain_table_\)\?\(baseband\|mac\|radio\)_postamble\(_emulation\)\?\|\(modes_\)\?\(high\|low\(est\)\?\|mixed\|green\)_\(ob_db\|power\)_tx_gain_table\(_[12]p0\)\?\)\[\]\[5\][ ]=' 'drivers/net/wireless/ath/ath9k/ar9\(462\|580\)_[12]p0_initvals\.h'
    defsnc 'static[ ]const[ ]s32[ ]wmi_rate_tbl\[\]\[2\][ ]=' drivers/net/wireless/ath/ath6kl/wmi.c
    defsnc '[	]struct[ ]lcn_tx_iir_filter[ ]tx_iir_filters_\(cck\|ofdm\)\[\][ ]=' drivers/net/wireless/b43/phy_lcn.c
    defsnc 'const[ ]u32[ ]b43_httab_0x1a_0xc0_late\[\][ ]=' drivers/net/wireless/b43/tables_phy_ht.c
    defsnc 'static[ ]const[ ]u\(16\|32\)[ ]b43_lcntab_0x[01][0-9a-f]\[\][ ]=' drivers/net/wireless/b43/tables_phy_lcn.c
    defsnc '[	]b43_lcntab_tx_gain_tbl_2ghz_ext_pa_rev0\[B43_LCNTAB_TX_GAIN_SIZE\][ ]=' drivers/net/wireless/b43/tables_phy_lcn.c
    defsnc 'const[ ]u16[ ]b43_lcntab_sw_ctl_4313_epa_rev0\[\][ ]=' drivers/net/wireless/b43/tables_phy_lcn.c
    defsnc 'static[ ]const[ ]u16[ ]VCORE_VSEL_table\[\][ ]=' drivers/regulator/tps65023-regulator.c
    defsnc 'static[ ]struct[ ]channel_list[ ]ChannelPlan\[\][ ]=' drivers/staging/rtl8192e/dot11d.c
    defsnc 'u32[ ]Rtl8192PciE\(PHY_REG_1T2R\|Radio[AB]_\|AGCTAB_\)Array\[\(PHY_REG_1T2R\|Radio[AB]_\|AGCTAB_\)ArrayLengthPciE\][ ]=' drivers/staging/rtl8192e/r8192E_hwimg.c
    defsnc 'static[ ]u8[ 	]CCKSwingTable_\(Ch1_Ch13\|Ch14\)\[CCK_Table_length\]\[8\][ ]=' drivers/staging/rtl8192e/rtl_dm.c
    defsnc 'static[ ]const[ ]unsigned[ ]short[ ]XGINew_DDRDRAM_TYPE20\[12\]\[5\][ ]=' drivers/staging/xgifb/vb_init.c
    defsnc 'static[ ]const[ ]unsigned[ ]short[ ]XGINew_\(MDA\|[CEV]GA\)_DAC\[\][ ]=' drivers/staging/xgifb/vb_setmode.c
    defsnc 'static[ ]const[ ]unsigned[ ]\(power\|emif[01]\)_pins\[\][ ]=' drivers/pinctrl/pinmux-u300.c
    defsnc 'static[ ]const[ ]struct[ ]pll_div[ ]codec_\(master\|slave\)_pll_div\[\][ ]=' sound/soc/codecs/rt5631.c
    accept '[	]it913x_config\.firmware[ ]=[ ]' drivers/media/dvb/dvb-usb/it913x.c
    accept '[	]\.download_firmware[ ]=[ ]it913x_download_firmware[,][\n][	]\.firmware[ ]=[ ]["]' drivers/media/dvb/dvb-usb/it913x.c
    blobname 'dvb-usb-it9137-01\.fw' drivers/media/dvb/dvb-usb/it913x.c
    blobname '%s[/]bdata\.%s\.bin' drivers/net/wireless/ath/ath6kl/init.c
    blobna 'Used[ ][(]for[ ]now[)][^*]*\([*]\+[^/*][^*]*\)*[*]*["]bdata\.bin["][^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]' drivers/net/wireless/ath/ath6kl/init.c
    blobname 'mrvl[/]pcie8766_uapsta\.bin' 'drivers/net/wireless/mwifiex/pcie\.[ch]'
    accept '#define[ ]FIRMWARE[ \t]*["]usbduxsigma_firmware\.bin["]' drivers/staging/comedi/drivers/usbduxsigma.c
    accept 'MODULE_DESCRIPTION[(]["]Stirling[/]ITL[ ]USB-DUX[ ]SIGMA[^"]*["][)][;][\n]MODULE_LICENSE[(]["]GPL["][)][;][\n]MODULE_FIRMWARE[(]FIRMWARE[)][;]' drivers/staging/comedi/drivers/usbduxsigma.c
    blobname 'as102_data[12]_[sd]t\.hex' drivers/staging/media/as102/as102_fw.c
    blob 'u8[ ]Rtl8192PciEFw\(Boot\|Main\|Data\)Array\[\(Boot\|Main\|Data\)ArrayLengthPciE\][ ]=[ ][{][^}]*[}][;]' drivers/staging/rtl8192e/r8192E_hwimg.c
    blobna '\([&]\|sizeof[(]\)Rtl8192PciEFw\(Boot\|Main\|Data\)Array\(\[0\]\|[)]\)\(,[ 	\n]*\([&]\|sizeof[(]\)Rtl8192PciEFw\(Boot\|Main\|Data\)Array\(\[0\]\|[)]\)\)*' drivers/staging/rtl8192e/r8192E_firmware.c
    blobname 'imx[/]sdma[/]sdma-imx5[13]\.bin' 'arch/arm/boot/dts/imx5[13]-\(babbage\|ard\|evk\|qsb\|smd\)\.dts'
    blobname 'libertas[/]usb8388_olpc\.bin' drivers/net/wireless/libertas/if_usb.c
    blobname 'rtlwifi[/]rtl8192cfwU\(_B\)\?\.bin' drivers/net/wireless/rtlwifi/rtl8192ce/sw.c
    blobname 'ti-connectivity[/]wl12[78]x-fw-3\.bin' drivers/net/wireless/wl12xx/wl12xx.h
    blobname 'pcxhr[/]%s' sound/pci/pcxhr/pcxhr_hwdep.c
    blobname 'mrvl[/]sd8797_uapsta\.bin' drivers/net/wireless/mwifiex/sdio.h
    blobname 's5p-mfc\.fw' drivers/media/video/s5p-mfc/s5p_mfc_ctrl.c
    blobname 'rtl_nic[/]rtl8168f-[12]\.fw' drivers/net/ethernet/realtek/r8169.c
    accept '[	]bp->firmware[ ]=[ ]NULL[;]' drivers/net/ethernet/broadcom/bnx2x/bnx2x_main.c

    blobna '[/][*][\n][ ][*][ ]AMD[ ]microcode[ ]firmware[ ]naming[ ]convention[^*]*\([*]\+[^/*][^*]*\)*[*]*amd-ucode[/][^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]' arch/x86/kernel/microcode_amd.c
    blobname 'amd-ucode[/]microcode_amd_fam\(%\.2x\|[0-9a-f]*\)h\.bin' arch/x86/kernel/microcode_amd.c

    # New in 3.3.
    defsnc 'static[ ]const[ ]struct[ ]reg_mod_vals[ ]reg_mod_vals_tab\[\][ ]=' drivers/media/dvb/frontends/hd29l2_priv.h
    defsnc 'static[ ]struct[ ]adctable[ ]tab[1-8]\[\][ ]=' drivers/media/dvb/frontends/it913x-fe-priv.h
    defsnc 'static[ ]const[ ]struct[ ]af9013_coeff[ ]coeff_lut\[\][ ]=' drivers/media/dvb/frontends/af9013_priv.h
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]qtbl_\(lu\|chro\)minance\[4\]\[64\][ ]=' drivers/media/video/s5p-jpeg/jpeg-core.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]hactblg0\[162\][ ]=' drivers/media/video/s5p-jpeg/jpeg-core.c
    defsnc 'static[ ]const[ ]u16[ ]b43_ntab_antswctl2g_r3\[4\]\[32\][ ]=' drivers/net/wireless/b43/tables_nphy.c
    defsnc 'struct[ ]nphy_gain_ctl_workaround_entry[ ]nphy_gain_ctl_\(workaround\[2\]\[4\]\|wa_phy6_radio11_ghz2\)[ ]=' drivers/net/wireless/b43/tables_nphy.c
    defsnc 'static[ ]const[ ]u16[ ]da9052_chg_current_lim\[2\]\[DA9052_CHG_LIM_COLS\][ ]=' drivers/power/da9052-battery.c
    defsnc 'static[ ]u32[ ]const[ ]vc_tbl\[3\]\[68\]\[2\][ ]=' drivers/power/da9052-battery.c
    defsnc 'static[ ]const[ ]int[ ]PIO2_CHANNEL_BANK\[32\][ ]=' drivers/staging/vme/devices/vme_pio2.h
    defsnc 'static[ ]const[ ]struct[ ]sirfsoc_baudrate_to_regv[ ]baudrate_to_regv\[\][ ]=' drivers/tty/serial/sirfsoc_uart.c
    defsnc 'static[ ]const[ ]struct[ ]dispc_coef[ ]coef[35]_M\(1[123469]\|2[26]\|32\)\[8\][ ]=' drivers/video/omap2/dss/dispc_coefs.c
    defsnc 'const[ ]unsigned[ ]char[ ]__clz_tab\[\][ ]=' lib/clz_tab.c
    defsnc 'static[ ]struct[ ]cs42l73_mclk_div[ ]cs42l73_mclk_coeffs\[\][ ]=' sound/soc/codecs/cs42l73.c
    defsnc 'static[ ]struct[ ]reg_default[ ]wm8995_reg_defaults\[\][ ]=' sound/soc/codecs/wm8995.c
    defsnc 'static[ ]int[ ]_process_sigma_firmware[(][^)]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*\(request\|maybe_reject\)_firmware' sound/soc/codecs/sigmadsp.c
    defsnc 'int[ ]process_sigma_firmware\(_regmap\)\?[(][^)]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*_process_sigma_firmware' sound/soc/codecs/sigmadsp.c
    accept 'EXPORT_SYMBOL[(]process_sigma_firmware_regmap[)]' sound/soc/codecs/sigmadsp.c
    accept 'extern[ ]int[ ]process_sigma_firmware_regmap[(][^)]*[)][;]' sound/soc/codecs/sigmadsp.h
    accept '[	]interrupts[ ]=[ ]<\([\n][	]*0x[ef][0-9a-f][ ]0[ ]0[ ]0\)*>[;]' 'arch/powerpc/boot/dts/fsl/\(pq3\|qoriq\)-mpic\.dtsi'
    # These appear to be identifiers within the device itself,
    # used to get information from it.
    accept '#define[ ]LANCER_\(FW_DUMP\|VPD_[PV]F\)_FILE[	]*["][/]\(dbg[/]dump\.bin\|vpd[/]ntr_[pv]f\.vpd\)["]' drivers/net/ethernet/emulex/benet/be_cmds.h
    defsnc 'static[ ]struct[ ]dib0090_wbd_slope[ ]dib7090e_wbd_table\[\][ ]=' drivers/media/dvb/dvb-usb/dib0700_devices.c
    blobname 'dvb-usb-it9135-0[12]\.fw' drivers/media/dvb/dvb-usb/it913x.c
    accept '[	]*props->firmware[ ]=[ ]fw_it913\(5_v[12]\|7\)' drivers/media/dvb/dvb-usb/it913x.c
    blobname 'dvb-usb-hauppauge-hvr930c-drxk\.fw' drivers/media/video/em28xx/em28xx-dvb.c
    blobname 'brcm[/]brcmfmac\.\(bin\|txt\)' drivers/net/wireless/brcm80211/brcmfmac/dhd_sdio.c

    # New in 3.4
    blobname 'dvb-fe-xc5000-1\.6\.114\.fw' drivers/media/common/tuners/xc5000.c
    blobname 'dvb-fe-xc5000c-41\.024\.5\.fw' drivers/media/common/tuners/xc5000.c
    accept '[	]*nvidia,emc-registers[ ]=[ ]<[ ]\(0[ 	\n]*\)*>' Documentation/devicetree/bindings/arm/tegra/emc.txt
    accept '[	]*interrupts[ ]=[ ]<[ ]\(0[ ]1[345][0-9][ ]0x04[ 	\n]*\)*>[;]' Documentation/devicetree/bindings/dma/tegra20-apbdma.txt
    accept '[	]*nvidia,emc-registers[ ]=[ ]<[ ]\(0x[0-9a-f]*[ 	\n]*\)*>' arch/arm/boot/dts/tegra-seaboard.dts
    accept '[	]*interrupts[ ]=[ ]<[ ]\(0[ ]1[0-4][0-9][ ]0x04[ 	\n]*\)*>[;]' 'arch/arm/boot/dts/tegra[23]0\.dtsi'
    defsnc 'static[ ]struct[ ]clk_pll_freq_table[ ]tegra_pll_[cu]_freq_table\[\][ ]=' arch/arm/mach-tegra/tegra30_clocks.c
    defsnc '[	]static[ ]const[ ]u8[ ]snum_init_[74]6\[\][ ]=' arch/powerpc/sysdev/qe_lib/qe.c
    defsnc 'const[ ]u64[ ]camellia_sp\(10011110\|22000222\|03303033\|00444404\|02220222\|30333033\|44044404\|11101110\)\[256\][ ]=' arch/x86/crypto/camellia_glue.c
    accept 'static[ ]int[ ]_request_firmware_load[(]struct[ ]firmware_priv[ ][*]fw_priv[,]' drivers/base/firmware_class.c
    accept 'static[ ]void[ ]request_firmware_work_func[(]struct[ ]work_struct[ ][*]work[)]' drivers/base/firmware_class.c
    accept '[	]fw_priv[ ]=[ ]_request_firmware_prepare[(][&]fw[,]' drivers/base/firmware_class.c
    accept '[	][	]ret[ ]=[ ]_request_firmware_load[(]fw_priv[,]' drivers/base/firmware_class.c
    accept '[	][	]_request_firmware_cleanup[(][&]fw[)][;]' drivers/base/firmware_class.c
    defsnc 'static[ ]const[ ]u32[ ]\(tahiti\|pitcairn\|verde\)_io_mc_regs\[TAHITI_IO_MC_REGS_SIZE\]\[2\][ ]=' drivers/gpu/drm/drm/radeon/si.c
    defsnc 'static[ ]const[ ]char[ ]fake_edid_info\[\][ ]=' drivers/gpu/drm/exynos/exynos_drm_vidi.c
    defsnc 'static[ ]const[ ]u8[ ]hdmiphy_v13_conf\(27\(_027\)\?\|74_\(175\|25\)\|148_5\)\[32\][ ]=' drivers/gpu/drm/exynos/exynos_hdmi.c
    defsnc 'static[ ]char[ ][*]generic_edid_name\[GENERIC_EDIDS\][ ]=' drivers/gpu/drm/drm_edid_load.c
    defsnc 'static[ ]u8[ ]generic_edid\[GENERIC_EDIDS\]\[128\][ ]=' drivers/gpu/drm/drm_edid_load.c
    defsnc 'static[ ]int[ ]edid_load[(][^)]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*err[ ]=[ ]request_firmware[(][&]fw[,][ ]name[,][ ][&]pdev' drivers/gpu/drm/drm_edid_load.c
    blobname 'dvb-usb-terratec-h7-\(drxk\|az6007\)\.fw' drivers/media/dvb/dvb-usb/az6007.c
    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]az6007_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/gp8psk.c
    blobname 'dvb-usb-lme2510c-rs2000\.fw' drivers/media/dvb/dvb-usb/lmedm04.c
    defsnc '[	]struct[ ]rtl2830_reg_val_mask[ ]tab\[\][ ]=' drivers/media/dvb/frontends/rtl2830.c
    defsnc '[	]static[ ]u8[ ]bw_params1\[3\]\[34\][ ]=' drivers/media/dvb/frontends/rtl2830.c
    blobname 'dvb-demod-drxk-pctv\.fw' drivers/media/video/em28xx/em28xx-dvb.c
    defsnc 'static[ ]const[ ]u8[ ]\(start\|page3\)_7302\[\][ ]=' drivers/media/video/gspca/pac7302.c
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]oob_\(2048\|4096\)_ecc[48][ ]=' drivers/mtd/nand/fsl_ifc_nand.c
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]fsmc_ecc4_\(256\|224\|128\|64\)_layout[ ]=' drivers/mtd/nand/fsmc_nand.c
    defsnc '[	]static[ ]const[ ]u8[ ]dhcp_\(pattern\|mask\)\[\][ ]=' drivers/net/wireless/ath/ath6kl/cfg80211.c
    blobname 'fw-[23]\.bin' drivers/netwireless/ath/ath6kl/core.h
    blobname '\(fw\.ram\|otp\|ath\(wlan\|tcmd_ram\)\|utf\|nullTestFlow\|data\.patch\|bdata\(\.SD31\)\?\)\.bin\(\.z77\)\?' drivers/net/wireless/ath/ath6kl/core.h
    accept '[	]hif_dev->firmware[ ]=[ ]fw[;]' drivers/net/wireless/ath/ath9k/hif_usb.c
    defsnc 'static[ ]const[ ]u32[ ]b43_ntab_tx_gain_rev\(0_1_2\|3plus_2ghz\|[34]_5ghz\|5plus_5ghz\)\[\][ ]=' drivers/net/wireless/b43/tables_nphy.c
    defsnc 'static[ ]const[ ]u32[ ]txpwrctrl_tx_gain_ipa\(\|_rev[56]\|_5g\)\[\][ ]=' drivers/net/wireless/b43/tables_nphy.c
    blobname 'brcm[/]brcmfmac-sdio\.bin' drivers/net/wireless/brcm80211/brcmfmac/dhd_sdio.c
    blobname 'brcm[/]brcmfmac43236b\.bin' drivers/net/wireless/brcm80211/brcmfmac/usb.c
    blobname 'ti-connectivity[/]wl12[78]x-fw-4-\([ms]r\|plt\)\.bin' drivers/net/wireless/wl12xx/wl12xx.h
    blobname 'TINfcInit_%d\.%d\.%d\.%d\.bts' drivers/nfc/nfcwilink.c
    defsnc 'static[ ]int[ ]ab8500_\(charger\|fg_lowbat\)_voltage_map\[\][ ]=' drivers/power/ab8500_charger.c
    defsnc '[	]static[ ]const[ ]u8[ ]parity\[\][ ]=' drivers/staging/sep/sep_crypto.c
    defsnc 'static[ ]\(const[ ]\)\?struct[ ]SiS_MCLKData[ ]XGI\(340\|27\)New_MCLKData\[\][ ]=' drivers/staging/xgifb/vb_table.h
    defsnc 'static[ ]\(const[ ]\)\?struct[ ]SiS_ModeResInfo_S[ ]XGI330_ModeResInfo\[\][ ]=' drivers/staging/xgifb/vb_table.h
    defsnc 'static[ ]const[ ]u8[ ]dim_table\[101\][ ]=' drivers/video/backlight/ot200_bl.c
    defsnc '[	]static[ ]const[ ]unsigned[ ]char[ ]data_to_send\[\][ ]=' drivers/video/exynos/s6e8ax0.c
    accept '[	]ret[ ]=[ ]request_firmware\([(][&]firmware_p[,][ ]rproc->firmware[,][ ]dev[)]\|_nowait[(]THIS_MODULE[,][ ]FW_ACTION_HOTPLUG[,][\n][	 ]*rproc->firmware[,][ ]dev[,][ ]GFP_KERNEL[,][\n][ 	]*rproc[,][ ]rproc_fw_config_virtio[)]\)[;][\n][	]if[ ][(]ret[ ]<[ ]0[)][ ][{][\n][	][	]dev_err[(]dev[,][ ]["]request_firmware\(_nowait\)\?[ ]failed' drivers/remoteproc/remoteproc_core.c
    accept '[	]rproc->firmware[ ][=][ ]firmware[;]' drivers/remoteproc/remoteproc_core.c
    blobname 'ql\(2600\|8300\)_fw\.bin' drivers/scsi/qla2xxx/qla_os.c
    defsnc 'static[ ]u8[ ]__attribute__[(][(]__aligned__[(]8[)][)][)][ ]test_buf\[\][ ]=' lib/crc32.c
    defsnc '[}][ ]test\[\][ ]=' lib/crc32.c
    defsnc 'static[ ]struct[ ]reg_default[ ]da7210_reg_defaults\[\][ ]=' sound/soc/codecs/da7210.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm2200_reva_patch\[\][ ]=' sound/soc/codecs/wm2200.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm8753_reg_defaults\[\][ ]=' sound/soc/codecs/wm8753.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm8978_reg_defaults\[\][ ]=' sound/soc/codecs/wm8978.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm8988_reg_defaults\[\][ ]=' sound/soc/codecs/wm8988.c

    # New in 3.5:
    accept '[	]*linux,keymap[ ]=[ ][<][ ]\(0x[0-9a-f]*[ 	\n]*\)*>[;]' 'arch/arm/boot/dts/spear\(13[14]\|30\)0-evb\.dts'
    accept '[	]*nvidia,emc-registers[ ]=[ ]<\(0x[0-9a-f]*[ 	\n]*\)*>[;]' arch/arm/boot/dts/tegra-seaboard.dts
    accept '[	]*interrupts[ ]=[ ]<\(0[ ]1[0-4][0-9][ ]0x04[ 	\n]*\)*>[;]' 'arch/arm/boot/dts/tegra[23]0\.dtsi'
    defsnc 'static[ ]u8[ ]zero_message_\(hash\|hmac\)_sha256\[SHA256_DIGEST_SIZE\][ ]=' drivers/crypto/ux500/hash/hash_core.c
    defsnc 'static[ ]const[ ]struct[ ]ast_dramstruct[ ]ast[12][01]00_dram_table_data\[\][ ]=' drivers/gpu/drm/ast/ast_dram_tables.h
    defsc 'static[ ]struct[ ]ast_vbios_stdtable[ ]vbios_stdtable\[\][ ]=' drivers/gpu/drm/ast/ast_tables.h
    defsc 'static[ ]const[ ]struct[ ]minimode[ ]est3_modes\[\][ ]=' drivers/gpu/drm/drm_edid_modes.h
    defsnc 'static[ ]const[ ]u8[ ]hdmiphy_conf74_176\[32\][ ]=' drivers/gpu/drm/exynos/exynos_hdmi.c
    defsnc 'static[ ]const[ ]struct[ ]wrpll_tmds_clock[ ]wrpll_tmds_clock_table\[\][ ]=' drivers/gpu/drm/i915/intel_ddi.c
    blobname 'dvb-usb-af9035-02\.fw' drivers/media/dvb/dvb-usb/af9035.c
    blobname 'dvb-usb-it9135-01\.fw' drivers/media/dvb/dvb-usb/af9035.c
    defsnc 'static[ ]const[ ]struct[ ]coeff[ ]coeff_lut\[\][ ]=' drivers/media/dvb/frontends/af9033_priv.h
    defsnc 'static[ ]const[ ]struct[ ]val_snr[ ]\(qpsk\|qam\(16\|64\)\)_snr_lut\[\][ ]=' drivers/media/dvb/frontends/af9033_priv.h
    defsnc 'static[ ]const[ ]struct[ ]reg_val[ ]\(ofsm_init\|tuner_init_\(tua9001\|fc0011\|mxl5007t\|tda18218\)\)\[\][ ]=' drivers/media/dvb/frontends/af9033_priv.h
    defsnc '[	]*static[ ]u8[ ]color_tb\[\]\[6\][ ]=' drivers/media/video/gspca/ov534.c
    defsnc 'static[ ]const[ ]u16[ ]bridge_init\[\]\[2\][ ]=' drivers/media/video/gspca/sn9c20x.c
    defsnc 'static[ ]const[ ]struct[ ]i2c_reg_u8[ ]\(soi968\|ov\(7670\|965[05]\)\|hv7131r\)_init\[\][ ]=' drivers/media/video/gspca/sn9c20x.c
    defsnc 'static[ ]const[ ]struct[ ]i2c_reg_u16[ ]\(mt9v[01]1[12]\)_init\[\][ ]=' drivers/media/video/gspca/sn9c20x.c
    defsnc 'static[ ]const[ ]struct[ ]hdmiphy_conf[ ]hdmiphy_conf_\(s5pv210\|exynos4[24]1[02]\)\[\][ ]=' drivers/media/video/s5p-tv/hdmiphy_drv.c
    defsnc 'static[ ]const[ ]int32_t[ ]tbat_lookup\[255\][ ]=' drivers/mfd/da9052-core.c
    defsnc 'static[ ]const[ ]struct[ ]atl1c_platform_patch[ ]plats\[\][ ]__devinitdata[ ]=' drivers/net/ethernet/atheros/atl1c/atl1c_main.c
    defsnc '[	][}][ ]hw_config\[\][ ]=' drivers/nfc/pn544_hci.c
    defsnc 'static[ ]const[ ]unsigned[ ]\(rgmii\|smii_0_1_2\|nand_8bit\|mcif\|pci_sata\|clcd\|arm_trace\|miphy_dbg\|emi\)_pins\[\][ ]=' drivers/pinctrl/spear/pinctrl-spear1310.c
    defsnc 'static[ ]const[ ]long[ ]chan_freq_list\[\]\[2\][ ]=' drivers/staging/wlags49_h2/wl_util.c
    defsnc '[	]static[ ]const[ ]unsigned[ ]char[ ]data_to_send_panel_reverse\[\][ ]=' drivers/video/exynos/s6e8ax0.c
    defsnc 'static[ ]const[ ]unsigned[ ]short[ ]__devinitconst[ ]SiS_DRAMType\[17\]\[5\][ ]=' drivers/video/sis/sis_main.c
    defsnc 'static[ ]struct[ ]reg_default[ ]lm49453_reg_defs\[\][ ]=' sound/soc/codecs/lm49453.c
    accept '-[ ]Replace[ ]hard-coded[ ]firmware[ ]paths[ ]with[ ]request_firmware' drivers/staging/gdm72xx/TODO
    blobname '\([/]lib[/]firmware[/]\)\?\(gdm72xx[/]\)\?gdms\(krn\|rfs\)\.bin' drivers/staging/gdm72xx/sdio_boot.c
    blobname '\([/]lib[/]firmware[/]\)\?gdm72xx[/]gdmuimg\.bin' drivers/staging/gdm72xx/usb_boot.c
    blobname 'mrvl[/]usb8797_uapsta\.bin' 'drivers/net/wireless/mwifiex/usb\.[ch]'
    # This is compiled and assembled out of actual sources as part of the build.
    accept '[	]\.incbin[	]["]arch[/]x86[/]realmode[/]rm[/]realmode\.bin["]' arch/x86/realmode/rmpiggy.S
    # Sources for these are in the corresponding .fuc files.
    defsc 'uint32_t[ ]nv98_pcrypt_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nv98_crypt.fuc.h
    accept '[	]nve0_graph_init_fuc[(]dev[,][ ]0x4\(09\|1a\)000[,][ ][&]priv->fuc4\(09\|1a\)c[,][ ][&]priv->fuc4\(09\|1a\)d[)][;]' drivers/gpu/drm/nouveau/nve0_graph.c
    accept '[	][	 ]*nve0_graph_destroy_fw[(]&priv->fuc4\(09\|1a\)[cd][)][;]' drivers/gpu/drm/nouveau/nve0_graph.c
    accept '[	][	 ]*\(if[ ][(]\|[ ][ ][ ][ ]\)nve0_graph_create_fw[(]dev[,][ ]["]fuc4\(09\|1a\)[cd]["][,][ ][&]priv->fuc4\(09\|1a\)[cd][)]' drivers/gpu/drm/nouveau/nve0_graph.c
    accept '[	]struct[ ]nve0_graph_fuc[ ]fuc4\(09\|1a\)[cd]' drivers/gpu/drm/nouveau/nve0_graph.h
    accept '[	]memset[(][&]fw[,][ ]0[,][ ]sizeof[(]struct[ ]mwifiex_fw_image[)][)][;][\n][	]adapter->firmware[ ]=[ ]firmware[;]' drivers/net/wireless/mwifiex/main.c
    # nouveau_vbios is a user-supplied parameter
    accept '[	][	]snprintf[(]fname[,][ ]sizeof[(]fname[)][,][ ]["]nouveau[/]%s["][,][ ]nouveau_vbios[)][;][\n][	][	]ret[ ]=[ ]request_firmware[(]' drivers/gpu/drm/nouveau/nouveau_bios.c
    accept '[	][	]\.download_firmware[ ]=[ ]af9035_download_firmware\(_it9135\)\?[,][\n][	][	]\.firmware[ ]=[ ]' drivers/media/dvb/dvb-usb/af9035.c
    blobname 'rtl_nic[/]rtl8402-1\.fw' drivers/net/ethernet/realtek/r8169.c
    blobname 'rtl_nic[/]rtl8411-1\.fw' drivers/net/ethernet/realtek/r8169.c
    blobname 'bdata\(\.\(SD3[12]\|WB31\|CUSTOM\|DB132\)\)\?\.bin' drivers/net/wireless/ath/ath6kl/core.h
    blobname 'mrvl[/]sd8786_uapsta\.bin' 'drivers/net/wireless/mwifiex/sdio\.[ch]'
    accept '[	][ ][*][ ]the[ ]isl3886[+]net2280' drivers/net/wireless/p54/p54usb.c

    # New in 3.6:
    defsnc 'static[ ]unsigned[ ]char[ ]mcf_host_slot2sid\[32\][ ]=' arch/m68k/platform/coldfire/pci.c
    defsnc 'static[ ]struct[ ]aead_testvec[ ]hmac_sha\(1\|256\|512\)_aes_cbc_enc_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]struct[ ]hash_testvec[ ]bfin_crc_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc '[	]static[ ]u8[ ]bw_params\[3\]\[32\][ ]=' drivers/media/dvb/frontends/rtl2832.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm51\(02\|10\)_reva_patch\[\][ ]=' drivers/mfd/wm5102-tables.c
    defsnc 'static[ ]const[ ]u32[ ]ar955x_1p0_\(radio\|baseband\|mac\)_postamble\[\]\[5\][ ]' drivers/net/wireless/ath/ath9k/ar955x_1p0_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar955x_1p0_\(\(radio\|mac\|baseband\)_core\|common_\(wo_xlna_\)\?rx_gain_table\)\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/955x_1p0_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar955x_1p0_modes_\(no_\)\?xpa_tx_gain_table\[\]\[9\][ ]=' drivers/net/wireless/ath/ath9k/955x_1p0_initvals.h
    blobname 'ti-connectivity[/]wl12[78]x-fw-5-\([ms]r\|plt\)\.bin' drivers/net/wireless/wl12xx/main.c
    blobname 'ti-connectivity[/]wl18xx-\(fw\|conf\)\.bin' drivers/net/wireless/wl18xx/main.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]\(ldo5\|buck1\)_voltage_map\[\][ ]=' drivers/regulator/lp3972.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]\(lp872x_ldo\|lp8720_ldo4\|lp8725_\(lilo\|buck\)\)_vtbl\[\][ ]=' drivers/regulator/lp872x.c
    defsnc '\(static[ ]\)\?const[ ]int[ ]lp8788_dldo1239_vtbl\[\][ ]=' drivers/regulator/lp8788-ldo.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]mc13892_sw1\?\[\][ ]=' drivers/regulator/mc13892-regulator.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]VCORE_VSEL_table\[\][ ]=' drivers/regulator/tps65023-regulator.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]VDCDCx_VSEL_table\[\][ ]=' drivers/regulator/tps6507x-regulator.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]dcdc[12]_voltages\[\][ ]=' drivers/regulator/tps6524x-regulator.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]tps6586x_\(ldo4\|sm2\|dvm\)_voltages\[\][ ]=' drivers/regulator/tps6586x-regulator.c
    defsnc 'static[ ]struct[ ]bcm_ddr_setting[ ]asT3\(LP\)\?B\?_DDRSetting\(160\|133\|100\|80\)MHz\[\][ ]\?=' drivers/staging/bcm/DDRInit.c
    defsnc '[ ]*static[ ]const[ ]u8[ ]arp_req\[36\][ ]=' drivers/staging/csr/sme_sys.c
    defsnc 'omap4430_adc_to_temp\[OMAP4430_ADC_END_VALUE[ ]-[ ]OMAP4430_ADC_START_VALUE[ ][+][ ]1\][ ]=' drivers/staging/oma-thermal/omap4-thermal.c
    defsnc 'omap4460_adc_to_temp\[OMAP4460_ADC_END_VALUE[ ]-[ ]OMAP4460_ADC_START_VALUE[ ][+][ ]1\][ ]=' drivers/staging/oma-thermal/omap4-thermal.c
    defsnc 'omap5430_adc_to_temp\[OMAP5430_ADC_END_VALUE[ ]-[ ]OMAP5430_ADC_START_VALUE[ ][+][ ]1\][ ]=' drivers/staging/oma-thermal/omap5-thermal.c
    defsnc 'static[ ]struct[ ]vesa_mode[ ]vesa_mode_table\[\][ ]=' drivers/staging/sm7xxfb/sm7xxfb.c
    defsnc 'static[ ]unsigned[ ]char[ ]rdesc\[\][ ]=' samples/uhid/uhid-example.c
    defsnc 'static[ ]struct[ ]reg_default[ ]isabelle_reg_defs\[\][ ]=' sound/soc/codecs/isabelle.c
    blobname 'dvb-usb-terratec-htc-stick-drxk\.fw' drivers/media/video/em28xx/em28xx-dvb.c
    blobname 'rtl_nic[/]rtl8106e-1\.fw' drivers/net/ethernet/realtek/r8169.c
    blobname 'rtl_nic[/]rtl8168g-1\.fw' drivers/net/ethernet/realtek/r8169.c
    defsnc '[	]static[ ]const[ ]u16[ ]mac_ocp_patch\[\][ ]=' in drivers/net/ethernet/realtek/r8169.c
    blobname 'rt3290\.bin\(\.[\n][	][ ][*][/]\)\?' drivers/net/wireless/rt2x00/rt2800pci.h

    # New in 3.7:
    blobname 'imx[/]sdma[/]sdma-imx6q-to1\.bin' arch/arm/boot/dts/imx6q.dtsi
    accept 'AES_T[ed]:\([\n]\.word[	]0x[0-9a-f]*\([,][ ]0x[0-9a-f]*\)*\)*[\n][@][ ]T[ed]4\[256\]\([\n]\.byte[	]0x[0-9a-f]*\([,][ ]0x[0-9a-f]*\)*\)*\([\n][@][ ]rcon\[\]\([\n]\.word[	]0x[0-9a-f]*\([,][ ]0x[0-9a-f]*\)*\)*\([,][ ]0\)*\)\?' arch/arm/crypto/aes-armv4.S
    defsnc 'const[ ]u32[ ]cast5_s[1234]\[256\][ ]=' crypto/cast5_generic.c
    defsnc 'const[ ]u32[ ]cast6_s[1234]\[256\][ ]=' crypto/cast6_generic.c
    accept '[ ][*][ ]Once[ ]it[ ]returns[ ]successfully[,][ ]driver[ ]can[ ]use[ ]request_firmware' drivers/base/firmware_class.c
    accept 'int[\n ]cache_firmware[(]const[ ]char[ ][*]fw_name[)][\n][{]\([\n]\+[^\n}][^\n]*\)*ret[ ]=[ ]request_firmware[(][^\n]*\([\n]\+[^\n}][^\n]*\)*[\n]\+[}][\n]' drivers/base/firmware_class.c
    accept '[ ][*][ ]If[ ]one[ ]device[ ]called[ ]request_firmware' drivers/base/firmware_class.c
    defsnc 'static[ ]const[ ]struct[ ]mV_pos[ ]__cpuinitconst[ ]\(vrm85\|mobilevrm\)_mV\[32\][ ]=' drivers/cpufreq/longhaul.h
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]__cpuinitconst[ ]mV_\(vrm85\|mobilevrm\)\[32\][ ]=' drivers/cpufreq/longhaul.h
    # Sources for these are in the corresponding .fuc files.
    defsnc 'static[ ]u32[ ]nva3_pcopy_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/copy/fuc/nva3.fuc.h
    defsnc 'static[ ]u32[ ]nvc0_pcopy_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/copy/fuc/nvc0.fuc.h
    defsnc 'static[ ]uint32_t[ ]nv98_pcrypt_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/crypt/fuc/nv98.fuc.h
    defsnc 'uint32_t[ ]nve0_grgpc_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/fuc/gpcnve0.fuc.h
    defsnc 'uint32_t[ ]nve0_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/fuc/hubnve0.fuc.h
    defsnc 'nv04_graph_ctx_regs\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nv04.c
    accept '[	]*ret[ ]=[ ]request_firmware[(]&fw[,][ ]source[,][ ]&nv_device[(]bios[)]->pdev->dev[)][;]' drivers/gpu/drm/nouveau/core/subdev/bios/base.c
    defsnc 'static[ ]u8[ ][*]edid_load[(][^)]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*err[ ]=[ ]request_firmware[(][&]fw[,][ ]name[,][ ][&]pdev' drivers/gpu/drm/drm_edid_load.c
    defsnc 'static[ ]const[ ]RegInitializer[ ]initData\[\][ ]__initconst[ ]=' drivers/ide/ali14xx.c
    defsnc 'static[ ]const[ ]struct[ ]reg_val[ ]tuner_init_fc2580\[\][ ]=' drivers/media/dvb-frontends/af9033_priv.h
    defsnc '[	]static[ ]const[ ]u8[ ]bw_params1\[3\]\[34\][ ]=' drivers/media/dvb-frontends/rtl2830.c
    blobname 's5k4ecgx\.bin' drivers/media/i2c/s5k4ecgx.c
    blobname 'v4l-coda\(dx6-imx27\|7541-imx53\)\.bin' drivers/media/platform/coda.c
    blobname 's5p-mfc\(-v6\)\?\.fw' drivers/media/platform/s5p-mfc/s5p_mfc.c
    defsnc 'static[ ]const[ ]struct[ ]e4000_lna_filter[ ]e400_lna_filter_lut\[\][ ]=' drivers/media/tuners/e4000_priv.h
    defsnc 'static[ ]const[ ]struct[ ]e4000_if_filter[ ]e4000_if_filter_lut\[\][ ]=' drivers/media/tuners/e4000_priv.h
    defsnc 'static[ ]const[ ]struct[ ]fc2580_reg_val[ ]fc2580_init_reg_vals\[\][ ]=' drivers/media/tuners/fc2580_priv.h
    defsnc 'static[ ]const[ ]struct[ ]fc2580_freq_regs[ ]fc2580_freq_regs_lut\[\][ ]=' drivers/media/tuners/fc2580_priv.h
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm5110_revb_patch\[\][ ]=' drivers/mfd/wm5110-tables.c
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]lpc32xx_nand_oob[ ]=' drivers/mtd/nand/lpc32xx_mlc.c
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]flctl_4secc_oob_64[ ]=' drivers/mtd/nand/sh_flctl.c
    defsnc 'static[ ]const[ ]struct[ ]atl1c_platform_patch[ ]plats\[\][ ]__devinitconst[ ]=' drivers/net/ethernet/atheros/atl1c/atl1c_main.c
    defsnc 'static[ ]const[ ]u32[ ]ar9565_1p0_\(\(mac\|baseband\|radio\)_core\|[Cc]ommon_\(wo_xlna_\)\?rx_gain_table\)\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/ar9565_1p0_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9565_1p0_\(\(mac\|baseband\)_postamble\|[Mm]odes_\(low\(est\)\?\|high\)_\(ob_db\|power\)_tx_gain_table\)\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar9565_1p0_initvals.h
    defsnc 'static[ ]u16[ ]r2057_rev[4578]a\?_init\[[45][245]\]\[2\][ ]=' drivers/net/wireless/b43/radio_2057.c
    defsnc '[	]*tbl_rf_control_override_rev7_over[01]\[\][ ]=' drivers/net/wireless/b43/tables_nphy.c
    defsnc 'static[ ]const[ ]unsigned[ ]pci_pins\[\][ ]=' drivers/pinctrl/spear/pinctrl-spear1310.c
    defsnc 'static[ ]int[ ]array_soc\[\]\[2\][ ]=' drivers/power/88pm860x_battery.c
    defsnc 'static[ ]const[ ]int[ ]mc13783_sw[12]x_val\[\][ ]=' drivers/regulator/mc13783-regulator.c
    # remoteproc uses request_firmware, but it is generic and names
    # no blobs of its own, so we change it to maybe_request_firmware.
    accept '[	]ret[ ]=[ ]request_firmware_nowait[(]THIS_MODULE[,][ ]FW_ACTION_HOTPLUG[,][\n][	 ]*rproc->firmware[,][ ][&]rproc->dev[,][ ]GFP_KERNEL[,][\n][ 	]*rproc[,][ ]rproc_fw_config_virtio[)][;][\n][	]if[ ][(]ret[ ]<[ ]0[)][ ][{][\n][	][	]dev_err[(][&]rproc->dev[,][ ]["]request_firmware_nowait[ ]err' drivers/remoteproc/remoteproc_core.c
    # This remoteproc client does name blobs, but we discard it
    # with undefine_macro.
    blob 'SPROC_MODEM_NAME[ ]["]-fw\.bin["]' drivers/remoteproc/ste_modem_rproc.c
    accept '[	]if[ ][(]request_firmware[(]&fw_entry,[ ]fname,[ ]&ioa_cfg->pdev->dev[)][)]' drivers/scsi/ipr.c
    blobname 'daqboard2000_firmware\.bin' drivers/staging/comedi/drivers/daqboard2000.c
    blobname 'me2600_firmware\.bin' drivers/staging/comedi/drivers/me_daq.c
    blobname 'ni6534a\.bin' drivers/staging/comedi/drivers/ni_pcidio.c
    blobname 'niscrb0[12]\.bin' drivers/staging/comedi/drivers/ni_pcidio.c
    defsnc 'static[ ]const[ ]struct[ ]SiS_TVData[ ]XGI_\(St\|Ext\)\(PAL\|NTSC\|YPbPr\(525\|750\)[ip]\)Data\[\][ ]=' drivers/staging/xgifb/vb_table.h
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]XGI330_\(NTSC\|PAL\|HiTV\(Ext\|St[12]\|Text\)\|YPbPr\(525\|750\)[ip]\)Timing\[\][ ]=' drivers/staging/xgifb/vb_table.h
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]XGI330_\(HiTV\|Ren\(525\|750\)p\)Group3\(Data\|Simu\|Text\)\?\[\][ ]=' drivers/staging/xgifb/vb_table.h
    accept 'static[ ]inline[ ]int[\n]\(maybe_\)\?reject_ihex_firmware\(_nowait\)\?[(][^{;]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*[\n]\+[}]' include/linux/firmware.h
    defsnc '[/][*][ ]callback[ ]from[ ]request_firmware_nowait' sound/pci/hda/hda_intel.c
    defsnc 'static[ ]int[ ]\(__devinit[ ]\)\?azx_probe[(][^)]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*request_firmware[^\n]*' sound/pci/hda/hda_intel.c
    defsnc 'static[ ]struct[ ]reg_default[ ]da9055_reg_defaults\[\][ ]=' sound/soc/codecs/da9055.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]sta32x_regs\[\][ ]=' sound/soc/codecs/sta32x.c
    blobname 'wm0010\(_stage2\.bin\|\.dfw\)' sound/soc/codecs/wm0010.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm5102_sysclk_reva_patch\[\][ ]=' sound/soc/codecs/wm5102.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm8510_reg_defaults\[\][ ]=' sound/soc/codecs/wm8510.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm8580_reg_defaults\[\][ ]=' sound/soc/codecs/wm8580.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm8776_reg_defaults\[\][ ]=' sound/soc/codecs/wm8776.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm8900_reg_defaults\[\][ ]=' sound/soc/codecs/wm8900.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm8960_reg_defaults\[\][ ]=' sound/soc/codecs/wm8960.c
    accept '[	][	]priv->firmware[ ]=[ ]true[;]' drivers/gpu/drm/nouveau/core/engine/graph/nvc0.c
    accept '[	][	 ]*\(if[ ][(]\|[ ][ ][ ][ ]\)nvc0_graph_ctor_fw[(]priv[,][ ]["]fuc4\(09\|1a\)[cd]["][,][ ][&]priv->fuc4\(09\|1a\)[cd][)]' 'drivers/gpu/drm/nouveau/core/engine/graph/nv[ce]0\.c'
    accept '[	][	 ]*nvc0_graph_dtor_fw[(]&priv->fuc4\(09\|1a\)[cd][)][;]' 'drivers/gpu/drm/nouveau/nv[ce]0\.c'
    accept '[	][	]*nvc0_graph_init_fw[(]priv[,][ ]0x4\(09\|1a\)000[,][ ][&]priv->fuc4\(09\|1a\)c[,][ \n	]*[&]priv->fuc4\(09\|1a\)d[)][;]' 'drivers/gpu/drm/nouveau/core/engine/graph/nv[ce]0\.c'
    blobname 'dvb-fe-xc5000c-4\.1\.30\.7\.fw' drivers/media/tuners/xc5000.c
    accept '[	]\.firmware[ ]=[ ]AF9015_FIRMWARE' drivers/media/usb/dvb-usb-v2/af9015.c
    accept '[	]\.firmware[ ]=[ ]AF9035_FIRMWARE' drivers/media/usb/dvb-usb-v2/af9035.c
    accept '[	]\.firmware[ 	]*=[ ]AZ6007_FIRMWARE' drivers/media/usb/dvb-usb-v2/az6007.c
    accept '[	]\.firmware[ ]=[ ]EC168_FIRMWARE' drivers/media/usb/dvb-usb-v2/ec168.c
    blobname 'brcm[/]brcmfmac43\(143\|242a\)\.bin' drivers/net/wireless/brcm80211/brcmfmac/usb.c
    accept '[	]priv->firmware[ ]=[ ]fw[;]' drivers/net/wireless/p54/p54pci.c
    blobname 'c[bt]2\?fw-3\.1\.0\.0\.bin' drivers/scsi/bfa/bfad.c
    blobname 'gdmuimg\.bin' drivers/staging/gdm72xx/usb_boot.c
    blobname 'CMV4[pi]\.bin\(\.v2\)\?' drivers/usb/atm/ueagle-atm.c
    blobname 'dvb-fe-tda10071\.fw' drivers/media/dvb/frontends/tda10071_priv.h
    accept '[	]st->it913x_config\.firmware[ ]=' drivers/media/usb/dvb-usb-v2/it913x.c
    blobname 'ar3k[/]\(AthrBT_0x%08x\.dfu\|ramps_0x%08x_%d%s\)' drivers/bluetooth/ath3k.c

    # New in 3.8
    accept 'K_table:\([\n][ \t]*\.\(quad\|long\)[ \t]*0x[0-9a-f]*[,][ ]\?0x[0-9a-f]*\)*' arch/x86/crypto/crc32c-pcl-intel-asm_64.S
    defsnc 'const[ ]u32[ ]cast_s[1234]\[256\][ ]=' crypto/cast_common.c
    accept '[ ]request_firmware[ ]can[ ]be[ ]called[ ]safely' Documentation/firmware_class/README
    defsnc 'static[ ]const[ ]int[ ]__initconst[ ]armada_370_xp_\(nb\|h\|dram\)clk_ratios\[32\]\[2\][ ]=' drivers/clk/mvebu/clk-core.c
    defsnc 'static[ ]const[ ]int[ ]__initconst[ ]\(dove\|kirkwood\)_cpu_ddr_ratios\[16\]\[2\][ ]=' drivers/clk/mvebu/clk-core.c
    defsnc 'static[ ]const[ ]int[ ]h_coef_8t\[GSC_COEF_RATIO\]\[GSC_COEF_ATTR\]\[GSC_COEF_H_8T\][ ]=' drivers/gpu/drm/exynos/exynos_drm_gsc.c
    defsnc 'static[ ]const[ ]int[ ]v_coef_4t\[GSC_COEF_RATIO\]\[GSC_COEF_ATTR\]\[GSC_COEF_V_4T\][ ]=' drivers/gpu/drm/exynos/exynos_drm_gsc.c
    defsnc 'static[ ]const[ ]struct[ ]atl1c_platform_patch[ ]plats\[\][ ]=' drivers/net/ethernet/atheros/atl1c/atl1c_main.c
    defsnc 'u32[ ]RTL8723EPHY_REG_1TARRAY\[RTL8723E_PHY_REG_1TARRAY_LENGTH\][ ]=' drivers/net/wireless/rtlwifi/rtl8723ae/table.c
    defsnc 'u32[ ]RTL8723EPHY_REG_ARRAY_PG\[RTL8723E_PHY_REG_ARRAY_PGLENGTH\][ ]=' drivers/net/wireless/rtlwifi/rtl8723ae/table.c
    defsnc 'u32[ ]RTL8723E_RADIOA_1TARRAY\[Rtl8723ERADIOA_1TARRAYLENGTH\][ ]=' drivers/net/wireless/rtlwifi/rtl8723ae/table.c
    defsnc 'u32[ ]RTL8723EMAC_ARRAY\[RTL8723E_MACARRAYLENGTH\][ ]=' drivers/net/wireless/rtlwifi/rtl8723ae/table.c
    defsnc 'u32[ ]RTL8723EAGCTAB_1TARRAY\[RTL8723E_AGCTAB_1TARRAYLENGTH\][ ]=' drivers/net/wireless/rtlwifi/rtl8723ae/table.c
    defsnc 'static[ ]struct[ ]abx500_v_to_cap[ ]cap_tbl\(_[AB]_thermistor\)\?\[\][ ]=' drivers/power/ab8500_bmdata.c
    defsnc 'static[ ]u16[ ]rx51_temp_table2\[\][ ]=' drivers/power/rx51_battery.c
    defsnc 'static[ ]const[ ]u32[ ]runnable_avg_yN_\(inv\|sum\)\[\][ ]=' kernel/sched/fair.c
    defsnc '[	]static[ ]const[ ]u32[ ]base\[4\]\[10\][ ]=' net/wireless/util.c
    defsnc 'static[ ]unsigned[ ]short[ ]init[1234]\[128\][ ]=' sound/isa/sb/emu8000.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm8750_reg_defaults\[\][ ]=' sound/soc/codecs/wm8750.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm8770_reg_defaults\[\][ ]=' sound/soc/codecs/wm8770.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm8971_reg_defaults\[\][ ]=' sound/soc/codecs/wm8971.c
    blobname 'nouveau[/]nv%02x_fuc%03x[dc]\?' drivers/gpu/drm/nouveau/core/core/falcon.c
    blobname 'ar5523\.bin' drivers/net/wireless/ath/ar5523/ar5523.h
    blobname 'rtlwifi[/]rtl8723\(ae\)\?fw\(_B\)\?\.bin' drivers/net/wireless/rtlwifi/rtl8723ae/sw.c
    blobname '%s-dsp%d\.\(wmfw\|bin\)' sound/soc/codecs/wm_adsp.c
    blobname 'fw-4\.bin' drivers/net/wireless/ath/ath6kl/core.h
    accept '[	]hdsp->firmware[ ]=[ ]fw' sound/pci/rme9652/hdsp.c

    # ath9k firmware is now Free Software.
    accept '[	]err[ ]=[ ]request_firmware_nowait[(]THIS_MODULE[,][ ]1[,][ ]name[,][ ]sc->dev[,][ ]GFP_KERNEL[,][\n][ 	]*[&]ec[,][ ]ath9k_eeprom_request_cb[)][;]' drivers/net/wireless/ath/ath9k/init.c
    accept '[#]define[ ]FIRMWARE_AR7010_1_1[ 	]*["]htc_7010\.fw["]' drivers/net/wireless/ath/ath9k/hif_usb.c
    accept '[#]define[ ]FIRMWARE_AR9271[ 	]*["]htc_9271\.fw["]' drivers/net/wireless/ath/ath9k/hif_usb.c
    accept 'MODULE_FIRMWARE[(]FIRMWARE_AR7010_1_1[)][;]' drivers/net/wireless/ath/ath9k/hif_usb.c
    accept 'MODULE_FIRMWARE[(]FIRMWARE_AR9271[)][;]' drivers/net/wireless/ath/ath9k/hif_usb.c
    accept '[	]ret[ ]=[ ]request_firmware_nowait[(]THIS_MODULE[,][ ]true[,][ ]hif_dev->fw_name[,][\n][ 	]*[&]hif_dev->udev->dev[,][ ]GFP_KERNEL[,][\n][ 	]*hif_dev[,][ ]ath9k_hif_usb_firmware_cb[)][;]' drivers/net/wireless/ath/ath9k/hif_usb.c
    accept '[	]ret[ ]=[ ]request_firmware[(][&]hif_dev->firmware[,][ ]hif_dev->fw_name[,][\n][ 	]*[&]hif_dev->udev->dev[)][;]' drivers/net/wireless/ath/ath9k/hif_usb.c
    accept '[	][	]ret[ ]=[ ]request_firmware[(][&]fw[,][ ]hif_dev->fw_name[,][\n][ 	]*[&]hif_dev->udev->dev[)][;]' drivers/net/wireless/ath/ath9k/hif_usb.c
    # as in 2.6.39
    accept '[#]define[ ]FIRMWARE_AR7010[ 	]*["]ar7010\.fw["]' drivers/net/wireless/ath/ath9k/hif_usb.c
    accept '[#]define[ ]FIRMWARE_AR7010_1_1[ 	]*["]ar7010_1_1\.fw["]' drivers/net/wireless/ath/ath9k/hif_usb.c
    accept '[#]define[ ]FIRMWARE_AR9271[ 	]*["]ar9271\.fw["]' drivers/net/wireless/ath/ath9k/hif_usb.c
    accept 'MODULE_FIRMWARE[(]FIRMWARE_AR7010[)][;]' drivers/net/wireless/ath/ath9k/hif_usb.c
    # as in 2.6.35
    accept '[	]ATH9K_FW_USB_DEV[(]0x\(9271\|1006\)[,][ ]["]ar9271\.fw["][)][,]' drivers/net/wireless/ath/ath9k/hif_usb.c
    accept '[	]dev_info[(][&]hif_dev->udev->dev[,][ ]["]ath9k_htc:[^\n"]*["][,][\n][	 ]*["]ar9271\.fw["][,]' drivers/net/wireless/ath/ath9k/hif_usb.c
    accept '[	]ret[ ]=[ ]request_firmware[(][&]hif_dev->firmware[,][ ]fw_name[,][ ][&]hif_dev->udev->dev[)][;]' drivers/net/wireless/ath/ath9k/hif_usb.c

    # New in 3.9
    blobname 'imx[/]sdma[/]sdma-imx6q\.bin' arch/arm/boot/dts/imx6qdl.dtsi
    accept '[	]*nvidia,emc-registers[ ]=[ 	]*<\(0x[0-9a-f]*[ 	\n]*\)*>[;]' arch/arm/boot/dts/tegra20-colibri-512.dtsi
    blobname 'kernel[/]x86[/]microcode[/]GenuineIntel\.bin' arch/x86/kernel/microcode_intel_early.c
    accept '[0-9][0-9]*[	][0-3][	][0-3][	]0\([\n][0-9][0-9]*[	][0-3][	][0-3][	]0\)*' Documentation/thermal/intel_powerclamp.txt
    accept '[	]return[ ]_request_firmware_load[(]fw_priv[,]' drivers/base/firmware_class.c
    accept 'static[ ]int[\n]_request_firmware_prepare[(]struct[ ]firmware[ ][*][*]\?firmware_p' drivers/base/firmware_class.c
    accept '[/][*][ ]called[ ]from[ ]request_firmware[(][)][ ]and[ ]request_firmware_work_func[(][)][ ][*][/]' drivers/base/firmware_class.c
    accept '[	]_request_firmware[(][&]fw[,][ ]fw_work->name' drivers/base/firmware_class.c
    accept '[	]put_device[(]fw_work->device[)][;][ ][/][*][ ]taken[ ]in[ ]request_firmware_nowait[(][)][ ][*][/]' drivers/base/firmware_class.c
    defsnc 'static[ ]const[ ]u16[ ]x[48]_vectors\[\][ ]=' drivers/edac/amd64_edac.c
    defsnc 'static[ ]const[ ]struct[ ]hdmiphy_config[ ]hdmiphy_v14_configs\[\][ ]=' drivers/gpu/drm/exynos/exynos_hdmi.c
    defsnc 'static[ ]const[ ]u32[ ]oland_io_mc_regs\[TAHITI_IO_MC_REGS_SIZE\]\[2\][ ]=' drivers/gpu/drm/radeon/si.c
    defsnc 'static[ ]const[ ]u8[ ]sixaxis_rdesc_fixup2\?\[\][ ]=' drivers/hid/hid-sony.c
    defsnc 'static[ ]const[ ]struct[ ]reg_val[ ]tuner_init_fc0012\[\][ ]=' drivers/media/dvb-frontends/af9033_priv.h
    defsnc '\(static[ ]\)\?struct[ ]linear_segments[ ]cnr_\(to_db\|\(64\|16\)qam\|qpsk\)_table\[\][ ]=' drivers/media/dvb-frontends/mb86a20s.c
    blobname 'SlimISP_\(%\.2s\|..\)\.bin' drivers/media/i2c/s5c73m3/s5c73m3-core.c
    defsc 'static[ ]const[ ]struct[ ]i2c_rv[ ]ov965x_init_regs\[\][ ]=' drivers/media/i2c/ov9650.c
    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]vp7049_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/m920x.c
    blobname 'dvb-usb-vp7049-0\.95\.fw' drivers/media/dvb/dvb-usb/m920x.c
    # The blob name is just the chip name, so no point in deblobbing;
    # more so considering the number of false positives this would
    # bring about.
    # blobname 'lp5521' drivers/leds/leds-lp5521.c
    # blobname 'lp55231\?' drivers/leds/leds-lp5523.c
    blobname 'lattice-ecp3\.bit' drivers/misc/lattice-ecp3-config.c
    defsnc '[	]*static[ ]const[ ]uint8_t[ ]rss_key\[UPT1_RSS_MAX_KEY_SIZE\][ ]=' drivers/net/vmxnet3/vmxnet3_drv.c
    defsnc 'static[ ]const[ ]u32[ ]ar9300Modes_\(mixed_ob_db\|type5\)_tx_gain_table_2p2\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar9003_2p2_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9340Modes_low_ob_db_and_spur_tx_gain_table_1p0\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar9340_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9485Modes_green_spur_ob_db_tx_gain_1_1\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar9485_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9580_1p0_type6_tx_gain_table\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar9580_1p0_initvals.h
    blobname 'iwlwifi-\(7260\|3160\)-' drivers/net/wireless/iwlwifi/pcie/7000.c
    blobname 'mrvl[/]pcie8897_uapsta\.bin' drivers/net/wireless/mwifiex/pcie.h
    accept 'static[ ]const[ ]struct[ ]mwifiex_pcie_device[ ]mwifiex_pcie\(8766\|8897\)[ ]=[ ][{][\n][	]\.firmware[ 	]*=' drivers/net/wireless/mwifiex/pcie.h
    accept '[	][	]card->pcie\.firmware[ ]=' drivers/net/wireless/mwifiex/pcie.c
    accept '[	][	]\.per_chan_pwr_limit_arr_11abg[ 	]*=[ ][{][	 0xf,\n]*' drivers/net/wireless/ti/wl18xx/main.c
    blobname 'ti-connectivity[/]wl18xx-fw-2\.bin' drivers/net/wireless/ti/wl18xx/main.c
    blobname '%s-dsp%d-%s\.\(wmfw\|bin\)' sound/soc/codecs/wm_adsp.c
    defsnc 'static[ ]const[ ]struct[ ]reg_addr[ ]\(idle_\)\?reg_addrs\[\][ ]=' drivers/net/ethernet/broadcom/bnx2x/bnx2x_dump.h
    blobname '83xx_fw\.bin' drivers/net/ethernet/qlogic/qlcnic/qlcnic_83xx_hw.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]dump_num_registers\[NUM_CHIPS\]\[NUM_PRESETS\][ ]=' drivers/net/ethernet/broadcom/bnx2x/bnx2x_dump.h
    defsnc 'static[ ]int[ ]pm2xxx_charger_voltage_map\[\][ ]=' drivers/power/pm2301_charger.c
    accept '[ ][*][ ]comedi[ ]drivers\.[ ]The[ ]request_firmware[(][)][ ]hotplug' drivers/staging/comedi/comedi.h
    blobname 'rp2\.fw' drivers/tty/serial/rp2.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]seq_\(w\|rgb\)_gamma\[\][ ]=' drivers/video/backlight/lms501kf03.c
    defsnc '[#]include[ ]<video[/]mmp_disp\.h>[\n]*static[ ]u16[ ]init\[\][ ]=' drivers/video/mmp/panel/tpo_tj032md01bw.c
    defsnc 'static[ ]struct[ ]tegra_clk_pll_freq_table[ ]pll_[mpadcu]_freq_table\[\][ ]=' 'drivers/clk/tegra/clk-tegra[23]0\.c'
    blobname 'ctefx\.bin' sound/pci/hda/patch_ca0132.c
    defsnc 'static[ ]unsigned[ ]int[ ]\(voice_focus\|mic_svm\|equalizer\)_vals_lookup\[\][ ]=' sound/pci/hda/patch_ca0132.c
    defsnc 'static[ ]struct[ ]hda_verb[ ]ca0132_init_verbs0\[\][ ]=' sound/pci/hda/patch_ca0132.c
    defsnc 'static[ ]const[ ]int[ ]dmic_comp\[6\]\[6\][ ]=' sound/soc/codecs/max98090.c

    # New in 3.10
    accept '[ \t]*edid[ ]=[ ]\[00[ ]FF[ 0-9A-F\n\t]*\]' arch/powerpc/boot/dts/ac14xx.dts
    accept 'K256:[\n][\t]\.long[ ]0x428a2f98[,][0-9a-f0x,]*\([\n][\t]\.long[ ][0-9a-f0x,]*\)*' arch/x86/crypto/sha256-avx-asm.S
    accept 'K256:[\n][\t]\.long[\t]0x428a2f98[,][0-9a-f0x,]*\([\n][\t]\.long[\t][0-9a-f0x,]*\)*' arch/x86/crypto/sha256-avx2-asm.S
    accept 'K256:[\n][ ]*\.long[ ]0x428a2f98[,][0-9a-f0x,]*\([\n][ ]*\.long[ ][0-9a-f0x,]*\)*' arch/x86/crypto/sha256-ssse3-asm.S
    accept 'K512:[\n][\t]\.quad[ ]0x428a2f98d728ae22[,][0-9a-f0x,]*\([\n][\t]\.quad[ ][0-9a-f0x,]*\)*' 'arch/x86/crypto/sha512-\(avx\|ssse3\)-asm\.S'
    accept 'K512:[\n][\t]\.quad[\t]0x428a2f98d728ae22[,][0-9a-f0x,]*\([\n][\t]\.quad[\t][0-9a-f0x,]*\)*' 'arch/x86/crypto/sha512-avx2-asm.S'
    defsnc 'static[ ]const[ ]uint32_t[ ]axi_clkgen_lock_table\[\][ ]=' drivers/clk/clk-axi-clkgen.c
    defsnc 'static[ ]const[ ]int[ ]arizona_micd_levels\[\][ ]=' drivers/extcon/extcon-arizona.c
    defsnc 'static[ ]const[ ]struct[ ]hdmiphy_config[ ]hdmiphy_v13_configs\[\][ ]=' drivers/gpu/drm/exynos/exynos_hdmi.c
    defsnc '[	][}][ ]common_modes\[\][ ]=' drivers/gpu/drm/qxl/qxl_display.c
    defsnc 'static[ ]const[ ]u32[ ]\(evergreen\|cedar\|supersumo\|wrestler\|barts\|turks\|caicos\)_golden_registers2\?\[\][ ]=' drivers/gpu/drm/radeon/evergreen.c
    defsnc 'static[ ]const[ ]u32[ ]\(cypress\|redwood\|cedar\|juniper\)_mgcg_init\[\][ ]=' drivers/gpu/drm/radeon/evergreen.c
    defsnc 'static[ ]const[ ]u32[ ]\(cayman\|dvst\|scrapper\)_golden_registers2\?\[\][ ]=' drivers/gpu/drm/radeon/ni.c
    defsnc 'static[ ]const[ ]u32[ ]cayman_io_mc_regs\[BTC_IO_MC_REGS_SIZE\]\[2\][ ]=' drivers/gpu/drm/radeon/si.c
    defsnc 'static[ ]const[ ]u32[ ]\(r7xx\|rv7[1347]0\)_\(golden_registers\|mgcg_init\)\[\][ ]=' drivers/gpu/drm/radeon/rv770.c
    defsnc 'static[ ]const[ ]u32[ ]\(tahiti\|pitcairn\|verde\|oland\|hainan\)_\(golden_registers\|mgcg_cgcg_init\)\[\][ ]=' drivers/gpu/drm/radeon/si.c
    defsnc 'static[ ]\(const[ ]\)\?u32[ ]verde_pg_init\[\][ ]=' drivers/gpu/drm/radeon/si.c
    defsnc 'static[ ]const[ ]u32[ ]hainan_io_mc_regs\[TAHITI_IO_MC_REGS_SIZE\]\[2\][ ]=' drivers/gpu/drm/radeon/si.c
    defsnc 'static[ ]const[ ]s16[ ]temp_lut\[\][ ]=' drivers/hwmon/via686a.c
    defsnc 'static[ ]const[ ]u8[ ]via_lut\[\][ ]=' drivers/hwmon/via686a.c
    defsnc 'static[ ]const[ ]uint64_t[ ]crc_table\[256\][ ]=' drivers/md/bcache/util.c
    defsnc 'static[ ]const[ ]struct[ ]reg_val[ ]ofsm_init_it9135_v[12]\[\][ ]=' drivers/media/dvb-frontends/af9033_priv.h
    defsnc 'static[ ]const[ ]struct[ ]reg_val[ ]tuner_init_it9135_\(38\|51\|52\|60\|61\|62\)\[\][ ]=' drivers/media/dvb-frontends/af9033_priv.h
    defsc 'static[ ]struct[ ]regdata[ ]mb86a20s_init2\[\][ ]=' drivers/media/dvb-frontends/mb86a20s.c
    defsnc 'static[ ]const[ ]u8[ ]channel_registers\[\][ ]=' drivers/media/i2c/tw2804.c
    defsnc '[\t]static[ ]const[ ]struct[ ]si476x_property_range[ ]valid_ranges\[\][ ]=' drivers/mfd/si476x-prop.c
    defsnc '[\t]static[ ]const[ ]unsigned[ ]int[ ]t[45]_reg_ranges\[\][ ]=' drivers/net/ethernet/chelsio/cxgb4/cxgb4_main.c
    defsnc 'static[ ]const[ ]u16[ ]b43_ntab_antswctl_r3\[4\]\[32\][ ]=' drivers/net/wireless/b43/tables_nphy.c
    defsnc 'static[ ]struct[ ]nphy_gain_ctl_workaround_entry[ ]nphy_gain_ctl_wa_phy6_radio11_ghz2[ ]=' drivers/net/wireless/b43/tables_nphy.c
    defsc 'static[ ]struct[ ]nphy_gain_ctl_workaround_entry[ ]nphy_gain_ctl_workaround\[2\]\[4\][ ]=' drivers/net/wireless/b43/tables_nphy.c
    defsnc 'static[ ]const[ ]u16[ ]b43_lcntab_sw_ctl_4313_epa_rev0\[\][ ]=' drivers/net/wireless/b43/tables_phy_lcn.c
    defsc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_5592_xtal[24]0\[\][ ]=' drivers/net/wireless/rt2x00/rt2800lib.c
    defsnc 'u32[ ]RTL8188EEPHY_REG_\(1TARRAY\|ARRAY_PG\)\[\][ ]=' drivers/net/wireless/rtlwifi/rtl8188ee/table.c
    defsnc 'u32[ ]RTL8188EE_RADIOA_1TARRAY\[\][ ]=' drivers/net/wireless/rtlwifi/rtl8188ee/table.c
    defsnc 'u32[ ]RTL8188EEMAC_1T_ARRAY\[\][ ]=' drivers/net/wireless/rtlwifi/rtl8188ee/table.c
    defsnc 'u32[ ]RTL8188EEAGCTAB_1TARRAY\[\][ ]=' drivers/net/wireless/rtlwifi/rtl8188ee/table.c
    defsc 'static[ ]const[ ]struct[ ]pinmux_cfg_reg[ ]pinmux_config_regs\[\][ ]=' 'drivers/pinctrl/sh-pfc/pfc-\(r8a77\(40\|79\)\|sh72\(03\|69\)\)\.c'
    defsnc 'static[ ]const[ ]struct[ ]abx500_v_to_cap[ ]cap_tbl\(_[ab]_thermistor\)\?\[\][ ]=' drivers/power/ab8500_bmdata.c
    defsnc 'static[ ]int[ ]ab8540_charge_\(output\|input\)_curr_map\[\][ ]=' drivers/power/ab8500_bmdata.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]ldo_vaux56_ab8540_voltages\[\][ ]=' drivers/regulator/ab8500.c
    accept '[\t]rproc->firmware[ ]=[ ]p[;]' drivers/remoteproc/remoteproc_core.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]jpeg_header\[\][ ]=' drivers/staging/media/solo6x10/solo6x10-jpeg.h
    defsnc 'const[ ]unsigned[ ]char[ ]jpeg_dqt\[4\]\[DQT_LEN\][ ]=' drivers/staging/media/solo6x10/solo6x10-jpeg.h
    defsnc 'static[ ]unsigned[ ]char[ ]vop_6010_\(ntsc\|pal\)_\(d1\|cif\)\[\][ ]=' drivers/staging/media/solo6x10/solo6x10-v4l2-enc.c
    defsnc 'u8[ ]\(sbox\|dot[23]\)_table\[256\][ ]=' drivers/staging/vt6656/aes_ccmp.c
    defsnc 'static[ ]const[ ]u32[ ]s_adwCrc32Table\[256\][ ]=' drivers/staging/vt6656/tcrc.c
    defsnc 'const[ ]u8[ ]TKIP_Sbox_\(Lower\|Upper\)\[256\][ ]=' drivers/staging/vt6656/tkip.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]tas5086_reg_defaults\[\][ ]=' sound/soc/codecs/tas5086.c
    accept '[\t]\.firmware[\t]=[ ]' drivers/bluetooth/btmrvl_sdio.c
    blobname 'mrvl[/]sd8688\(_helper\)\?\.bin' drivers/bluetooth/btmrvl_sdio.c
    blobname 'mrvl[/]sd8897_uapsta\.bin' drivers/bluetooth/btmrvl_sdio.c
    blobname '\(\(atsc\|tdmb\)_denver\|cmmb_\(ming_app\|venice_12mhz\)\|dvbh\?_rio\|fm_radio\(_rio\)\?\|isdbt_\(pele\|rio\)\)\.inp' drivers/media/common/siano/smscoreapi.h
    blobname 'tigon[/]tg357766\.bin' drivers/net/ethernet/broadcom/tg3.c
    blobname 'cxgb4[/]t5fw\.bin' drivers/net/ethernet/chelsio/cxgb4/cxgb4_main.c
    blobname 'rtl_nic[/]rtl8106e-2\.fw' drivers/net/ethernet/realtek/r8169.c
    blobname 'rtl_nic[/]rtl8168g-[23]\.fw' drivers/net/ethernet/realtek/r8169.c
    blobname 'mwl8k[/]fmimage_8764_ap-["][ ][#]api[ ]["]\.fw' drivers/net/wireless/mwl8k.c
    blobname 'go7007[/]go7007fw\.bin' drivers/staging/media/go7007/go7007-driver.c
    blobname 'go7007[/]go7007tv\.bin' drivers/staging/media/go7007/go7007-fw.c
    blobname 'go7007[/]\(s2250-[12]\|px-\(m\|tv\)402u\|lr192\|wis-startrek\)\.fw' drivers/staging/media/go7007/go7007-loader.c
    blobname 'intel[/]ibt-hw-%x\.%x\(\.%x-fw-%x\.%x\.%x\.%x\.%x\)\?\.bseq' drivers/bluetooth/btusb.c
    blobname 'radeon[/]\(RV710\|CYPRESS\|SUMO\|TAHITI\)_uvd\.bin' drivers/gpu/drm/radeon/radeon_uvd.c
    blobname 'imspcu\.fw' drivers/input/misc/ims-pcu.c
    blobname 'fimc_is_fw\.bin' drivers/media/platform/exynos4-is/fimc-is.h
    blobname 'setfile\.bin' drivers/media/platform/exynos4-is/fimc-is.h
    blobname 'rtlwifi[/]rtl8188efw\.bin' drivers/net/wireless/rtlwifi/rtl8188ee/sw.c

    # New in 3.11.
    blobname 'imx[/]sdma[/]sdma-imx6sl\.bin' arch/arm/boot/dts/imx6sl.dtsi
    initnc '[	]linux,keymap[ ]=[ ]<' 'arch/arm/boot/dts/nspire-\(clp\|cx\|tp\)\.dts'
    blobname '\(kernel[/]x86[/]microcode[/]\)\?AuthenticAMD\.bin' arch/x86/kernel/microcode_amd_early.c
    initnc '[	 ]*FMC:[ ]poor[ ]dump[ ]of[ ]sdb[ ]first[ ]level:' Documentation/fmc/parameters.txt
    accept 'static[ ]int[\n ]cache_firmware[(]const[ ]char[ ][*]fw_name[)][\n][{]\([\n]\+[^\n}][^\n]*\)*ret[ ]=[ ]request_firmware[(][^\n]*\([\n]\+[^\n}][^\n]*\)*[\n]\+[}][\n]' drivers/base/firmware_class.c
    defsnc 'static[ ]const[ ]int[ ]__initconst[ ]a370_\(nb\|h\|dram\)clk_ratios\[32\]\[2\][ ]=' drivers/clk/mvebu/armada-370.c
    defsnc 'static[ ]const[ ]int[ ]__initconst[ ]axp_\(nb\|h\|dram\)clk_ratios\[32\]\[2\][ ]=' drivers/clk/mvebu/armada-xp.c
    defsnc 'static[ ]const[ ]struct[ ]mV_pos[ ]\(vrm85\|mobilevrm\)_mV\[32\][ ]=' drivers/cpufreq/longhaul.h
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]mV_\(vrm85\|mobilevrm\)\[32\][ ]=' drivers/cpufreq/longhaul.h
    accept '[][ 0-9.]*fake-fmc-carrier:[ ]Mezzanine[ ]0:[ ]eeprom[ ]["]fdelay-eeprom\.bin["]' Documentation/fmc/fmc-fakedev.txt
    accept '[][ 0-9.]*spec[ ][024:.]*[ ]got[ ]file[ ]["]fmc[/]spec-init\.bin["]' Documentation/fmc/fmc-write-eeprom.txt
    defsnc 'static[ ]char[ ]ff_eeimg\[FF_MAX_MEZZANINES\]\[FF_EEPROM_SIZE\][ ]=' drivers/fmc/fmc-fakedev.c
    accept '[	]ret[ ]=[ ]request_firmware[(][&]fw[,][ ]gw[,][ ][&]fmc->dev[)][;]' drivers/fmc/fmc-fakedev.c
    accept '[	][	]ret[ ]=[ ]request_firmware[(][&]fw[,][ ]ff_eeprom\[i\][,][ ][&]ff->dev[)][;]' drivers/fmc/fmc-fakedev.c
    accept '[	]if[ ][(][!]strcmp[(]last4[,][ ]["]\.bin["][)][)]' drivers/fmc/fmc-write-eeprom.c
    accept '[	]err[ ]=[ ]request_firmware[(][&]fw[,][ ]s[,][ ]dev[)][;]' drivers/fmc/fmc-write-eeprom.c
    defsnc 'nvc0_grctx_init_\(icmd\|9097\|902d\|90c0\|unk40xx\|unk46xx\|unk78xx\|gpc_[01]\|tpc\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnvc0.c
    defsnc 'nvc1_grctx_init_\(icmd\|9097\|gpc_0\|tpc\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnvc1.c
    defsnc 'nvc3_grctx_init_tpc\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnvc3.c
    defsnc 'nvc8_grctx_init_\(icmd\|tpc\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnvc8.c
    defsnc 'nvd7_grctx_init_\(unk40xx\|unk58xx\|gpc_0\|tpc\|unk\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnvd7.c
    defsnc 'nvd9_grctx_init_\(icmd\|90c0\|unk40xx\|unk58xx\|gpc_0\|tpc\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnvd9.c
    defsnc 'nve4_grctx_init_\(icmd\|a097\|unk40xx\|unk46xx\|unk58xx\|unk64xx\|rop\|gpc_0\|tpc\|unk\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnve4.c
    defsnc 'nvf0_grctx_init_\(unk40xx\|unk64xx\|unk88xx\|gpc_0\|tpc\|unk\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnvf0.c
    defsnc 'uint32_t[ ]nvd7_grgpc_code\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/fuc/gpcnvd7.fuc.h
    defsnc 'uint32_t[ ]nvf0_grgpc_code\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/fuc/gpcnvf0.fuc.h
    defsnc 'uint32_t[ ]nvd7_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/fuc/hubnvd7.fuc.h
    defsnc 'uint32_t[ ]nvf0_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/fuc/hubnvf0.fuc.h
    defsnc 'nvc0_graph_init_\(regs\|[gt]pc\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nvc0.c
    defsnc 'nvc1_graph_init_[gt]pc\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nvc1.c
    defsnc 'nvc3_graph_init_tpc\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nvc3.c
    defsnc 'nvc8_graph_init_[gt]pc\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nvc8.c
    defsnc 'nvd7_graph_init_[gt]pc\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nvd7.c
    defsnc 'nvd9_graph_init_[gt]pc\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nvd9.c
    defsnc 'nve4_graph_init_\(regs\|[gt]pc\|unk\|unk88xx\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nve4.c
    defsnc 'nvf0_graph_init_[gt]pc\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nvf0.c
    defsnc '[	][}][ ]magic\[\][ ]=[ ][{][\n][	][	][{][ ]0x020520[,]' drivers/gpu/drm/nouveau/core/engine/graph/nvf0.c
    blobname 'nouveau[/]nv84_xuc%03x' drivers/gpu/drm/nouveau/core/engine/graph/xtensa.c
    defsnc 'nv50_fb_memtype\[0x80\][ ]=' drivers/gpu/drm/nouveau/core/subdev/fb/nv50.c
    defsnc 'static[ ]const[ ]u32[ ]\(barts\|caicos\|turks\)_\(\(cgcg_cgls\|sysls\)_\(default\|disable\|enable\)\|mgcg_default\)\[\][ ]=' drivers/gpu/drm/radeon/btc_dpm.c
    defsnc 'u32[ ]btc_valid_sclk\[40\][ ]=' drivers/gpu/drm/radeon/btc_dpm.c
    defsnc 'static[ ]const[ ]u32[ ]\(bonaire\|spectre\|kalindi\)_\(golden_registers\|mgcg_cgcg_init\)\[\][ ]=' drivers/gpu/drm/radeon/cik.c
    defsnc 'static[ ]const[ ]u32[ ]bonaire_io_mc_regs\[BONAIRE_IO_MC_REGS_SIZE\]\[2\][ ]=' drivers/gpu/drm/radeon/cik.c
    blobname 'radeon[/]\(BONAIRE\|KAVERI\|KABINI\|%s\)_\(pfp\|[mc]ec\?\|rlc\|s\?mc\|sdma\)\.bin' drivers/gpu/drm/radeon/cik.c
    defsnc 'static[ ]u32[ ]sumo_rlc_save_restore_register_list\[\][ ]=' drivers/gpu/drm/radeon/evergreen.c
    defsnc 'static[ ]u32[ ]tn_rlc_save_restore_register_list\[\][ ]=' drivers/gpu/drm/radeon/ni.c
    blobname 'radeon[/]\(BARTS\|BTC\|TURKS\|CAICOS\|%s\)_\(pfp\|m[ec]\|rlc\|smc\)\.bin' 'drivers/gpu/drm/radeon/[ns]i\.c'
    defsnc 'static[ ]const[ ]struct[ ]ni_cac_weights[ ]cac_weights_cayman_\(xt\|pro\|le\)[ ]=' drivers/gpu/drm/radeon/ni_dpm.c
    blobname 'radeon[/]\(R\([67]0\|V6[1237]\|S7[1378]\)[05]\|CEDAR\|REDWOOD\|JUNIPER\|CYPRESS\|SUMO2\?\|%s\)_\(pfp\|[mc]e\|rlc\|s\?mc\)\.bin' drivers/gpu/drm/radeon/r600.c
    defsnc 'static[ ]const[ ]u32[ ]cayman_\(\(cgcg_cgls\|sysls\)_\(default\|disable\|enable\)\|mgcg_default\)\[\][ ]=' drivers/gpu/drm/radeon/ni_dpm.c
    blobname 'radeon[/]BONAIRE_uvd\.bin' drivers/gpu/drm/radeon/radeon_uvd.c
    blobname 'radeon[/]\(TAHITI\|PITCARIN\|VERDE\|OLAND\|HAINAN\|%s\)_\(pfp\|[mc]e\|rlc\|s\?mc\)\.bin' drivers/gpu/drm/radeon/si.c
    defsnc 'static[ ]struct[ ]dll_speed_setting[ ]dll_speed_table\[16\][ ]=' drivers/gpu/drm/radeon/rv740_dpm.c
    defsnc 'static[ ]const[ ]u8[ ]\(rv7[7314]0\|cedar\|redwood\|juniper\|cypress\|barts\|turks\|caicos\|cayman\)_smc_int_vectors\[\][ ]=' drivers/gpu/drm/radeon/rv770_smc.c
    defsnc 'static[ ]const[ ]struct[ ]si_dte_data[ ]dte_data_\(tahiti\(_le\|_pro\)\?\|new_zealand\|aruba_pro\|malta\|pitcairn\|curacao_\(xt\|pro\)\|neptune_xt\|cape_verde\|venus_\(xtx\?\|pro\)\|oland\|mars_pro\|sun_xt\)[ ]=' drivers/gpu/drm/radeon/si_dpm.c
    defsnc 'static[ ]const[ ]u32[ ]trinity_\(mgcg_shls_default\|sysls_\(default\|disable\|enable\)\|override_mgpg_sequences\)\[\][ ]=' drivers/gpu/drm/radeon/trinity_dpm.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]hex_table\[256\][ ]=' drivers/md/dm-switch.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm5102_revb_patch\[\][ ]=' drivers/mfd/wm5102-tables.c
    blobname 'c\(b\|t2\?\)fw-3\.2\.1\.0\.bin' 'drivers/\(net/ethernet/brocade/bna/cna\.h\|scsi/bfa/bfad\.c\)'
    blobname 'rtl_nic[/]rtl8411-2\.fw' drivers/net/ethernet/realtek/r8169.c
    blobname 'ath10k[/]QCA988X[/]hw[12]\.0' drivers/net/wireless/ath/ath10k/hw.h
    blobname '\(ath10k[/]QCA988X[/]hw[12]\.0[/]\)\?\(firmware\|otp\|board\)\.bin' drivers/net/wireless/ath/ath10k/hw.h
    defsnc 'static[ ]const[ ]u32[ ]ar9462_modes_mix_ob_db_tx_gain_table_2p0\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar9462_2p0_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9462_2p0_5g_xlna_only_rxgain\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/ar9462_2p0_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9462_2p1_\(\(mac\|baseband\|radio\)_core\|common_\(mixed_\|wo_xlna_\|5g_xlna_only_\)\?rx_gain\)\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/ar9462_2p1_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9462_2p1_\(\(mac\|baseband\)_postamble\|modes_\(low\|high\|mix\)_ob_db_tx_gain\)\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar9462_2p1_initvals.h
    blobname '\(boot_cw1x60\|\(wsm\|sdd\)_\(cw1x60\|22\|20\|11\|10\)\)\.bin' drivers/net/wireless/cw1200/fwio.h
    accept '[ ][*][ ]4\.[ ]save[ ]as[ ]["]iNVM_xxx\.bin["]' drivers/net/wireless/iwlwifi/mvm/nvm.c
    accept 'static[ ]const[ ]struct[ ]mwifiex_sdio_device[ ]mwifiex_sdio_sd[^ ]*[ ]=[ ][{][\n][ 	]*\.firmware[ ]=' drivers/net/wireless/mwifiex/sdio.h
    blobname 'sdd_sagrad_1091_1098\.bin' 'drivers/net/wireless/cw1200/cw1200_sdio\.c\|include/linux/platform_data/net-cw1200\.h'
    accept '[/][*][ ]An[ ]example[^*]*[\n][	 ]*\.sdd_file[ ]=[ ]["]sdd_\(sagrad_1091_1098\|myplatform\)\.bin["][,]' include/linux/platform_data/net-cw1200.h
    defsnc 'static[ ]unsigned[ ]const[ ]score_pins\[BYT_NGPIO_SCORE\][ ]=' drivers/pinctrl/pinctrl-baytrail.c
    defsnc 'static[ ]unsigned[ ]const[ ]sus_pins\[BYT_NGPIO_SUS\][ ]=' drivers/pinctrl/pinctrl-baytrail.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]bsc_data32_pins\[\][ ]=' drivers/pinctrl/pinctrl-baytrail.c
    blobname 'mt76\(50\|62\)\.bin' drivers/staging/btmtk_usb/btmtk_usb.c
    accept '[	 ]*data->firmware[ ]=[ ]firmware[;]' drivers/staging/btmtk_usb/btmtk_usb.c
    accept '[	]\[CODA_IMX\(27\|53\)\][ ]=[ ][{][\n][	][	]\.firmware[ ]*=' drivers/media/platform/coda.c
    blobname 'exynos4_\(fimc_is_fw\|s5k6a3_setfile\)\?\.bin' drivers/media/platform/exynos4-is/fimc-is.h
    accept '[ 	]*ret[ ]=[ ]process_sigma_firmware[(]client[,][ ]ADAU1701_FIRMWARE[)][;]' sound/soc/codecs/adau1701.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt5640_reg\[RT5640_VENDOR_ID2[ ][+][ ]1\][ ]=' sound/soc/codecs/rt5640.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]ssm2518_reg_defaults\[\][ ]=' sound/soc/codecs/ssm2518.c

    # New in 3.12.
    blobname 's5p-mfc-v7\.fw' drivers/media/platform/s5p-mfc/s5p_mfc.c
    blobname 'ct2\?fw-3\.2\.1\.1\.bin' drivers/net/ethernet/brocade/bna/cna.h
    blobname 'c[bt]2\?fw-3\.2\.1\.1\.bin' drivers/scsi/bfa/bfad.c
    blobname '84xx_fw\.bin' drivers/net/ethernet/qlogic/qlcnic/qlcnic_83xx_hw.c
    accept '[	]interrupts[ ]=[ ]<\([\n][	]*0x\([ef]\|1[01]\)[0-9a-f][ ]0[ ]0[ ]0\)*>[;]' arch/powerpc/boot/dts/fsl/qoriq-mpic4\.3\.dtsi
    defsnc '__visible[ ]const[ ]u64[ ]camellia_sp\(10011110\|22000222\|03303033\|00444404\|02220222\|30333033\|44044404\|11101110\)\[256\][ ]=' arch/x86/crypto/camellia_glue.c
    defsnc '__visible[ ]const[ ]u32[ ]crypto_[fi][tl]_tab\[4\]\[256\][ ]=' crypto/aes_generic.c
    defsnc '__visible[ ]const[ ]u32[ ]cast_s[1234]\[256\][ ]=' crypto/cast_common.c
    accept '[	]*interrupts[ ]=[ ]<[ ]*\(0[ ]2[012][0-9][ ]4[ 	\n]*\)*>[;]' Documentation/devicetree/bindings/dma/shdma.txt
    accept '[	][	]interrupts[ ]=[ ]<\([\n][	]*0x\([ef]\|1[01]\)[0-9a-f][ ]0[ ]0[ ]0\)*>[;]' Documentation/devicetree/bindings/powerpc/fsl/msi-pic.txt
    defsnc 'static[ ]const[ ]int[ ]a370_\(nb\|h\|dram\)clk_ratios\[32\]\[2\][ ]__initconst[ ]=' drivers/clk/mvebu/armada-370.c
    defsnc 'static[ ]const[ ]int[ ]axp_\(nb\|h\|dram\)clk_ratios\[32\]\[2\][ ]__initconst[ ]=' drivers/clk/mvebu/armada-xp.c
    defsnc 'static[ ]const[ ]int[ ]\(dove\|kirkwood\)_cpu_ddr_ratios\[16\]\[2\][ ]__initconst[ ]=' drivers/clk/mvebu/clk-core.c
    defsnc 'static[ ]const[ ]u8[ ]zero_message_\(hash\|hmac\)_sha256\[SHA256_DIGEST_SIZE\][ ]=' drivers/crypto/ux500/hash/hash_core.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]a3xx_registers\[\][ ]=' drivers/gpu/drm/msm/adreno/a3xx_gpu.c
    blobname 'a3[03]0_p\(m4\|fp\)\.fw' drivers/gpu/drm/msm/adreno/a3xx_gpu.c
    defsnc 'static[ ]const[ ]struct[ ]ci_pt_defaults[ ]defaults_\(bonaire\|saturn\)_\(xt\|pro\)[ ]=' drivers/gpu/drm/radeon/ci_dpm.c
    defsnc 'static[ ]const[ ]u32[ ]sumo_rlc_save_restore_register_list\[\][ ]=' drivers/gpu/drm/radeon/evergreen.c
    defsnc 'static[ ]const[ ]struct[ ]kv_lcac_config_values[ ]cpl_local_cac_cfg_kv\[\][ ]=' drivers/gpu/drm/radeon/kv_dpm.c
    defsnc 'static[ ]const[ ]u32[ ]tn_rlc_save_restore_register_list\[\][ ]=' drivers/gpu/drm/radeon/ni.c
    defsnc 'static[ ]struct[ ]imx_i2c_clk_pair[ ]\(imx\|vf610\)_i2c_clk_div\[\][ ]=' drivers/i2c/busses/i2c-imx.c
    defsnc 'static[ ]const[ ]u16[ ]apds9300_lux_ratio\[\][ ]=' drivers/iio/light/apds9300.c
    accept '[	]ar->firmware[ ]=[ ]\(NULL\|ath10k_fetch_fw_file\)' drivers/net/wireless/ath/ath10k/core.c
    defsnc 'static[ ]const[ ]u16[ ]dot11lcn_sw_ctrl_tbl_4313_ipa_rev0_combo\[\][ ]=' drivers/net/wireless/brcm80211/brcmsmac/phy/phytbl_lcn.c
    accept '[	][	]adapter->firmware[ ]=[ ]NULL' drivers/net/wireless/mwifiex/main.c
    defsc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_3053\[\][ ]=' drivers/net/wireless/rt2x00/rt2800lib.c
    defsnc 'static[ ]const[ ]int[ ]bq24190_\(ccc_ichg\|cvc_vreg\)_values\[\][ ]=' drivers/power/bq24190_charger.c
    blobname '[(]i\.e\.[ ]["]asfep\.bin["][)][ ][*][/]' drivers/staging/dgap/downlod.c
    blobname '[(]["][/]etc[/]dgap[/]xrfep\.bin["][)][;][ ][*][/]' drivers/staging/dgap/downlod.c
    blobname '["][/]lib[/]firmware[/]dgap[/]["]' drivers/staging/dgap/downld.c
    blobname '\(fx\|cx\|cxp\|ibm\(cx\|en\)\|xr\|sx\|pci\)\(bios\|fep\|con\|host\)\.bin' drivers/staging/dgap/downld.c
    defsnc 'static[ ]const[ ]struct[ ]msi3101_gain[ ]msi3101_gain_lut_\(120\|245\|1000\)\[\][ ]=' drivers/staging/media/msi3101/sdr-msi3101.c
    defsnc 'static[ ]struct[ ]ch_freq[ ]ch_freq_map\[\][ ]=' drivers/staging/rtl8188eu/core/rtw_rf.c
    defsnc 'static[ ]\(const\)\?[ ]\?u8[ ]sbox_table\[256\][ ]=' drivers/staging/rtl8188eu/core/rtw_security.c
    defsnc 'static[ ]const[ ]unsigned[ ]short[ ]Sbox1\[2\]\[256\][ ]=' drivers/staging/rtl8188eu/core/rtw_security.c
    defsnc 'const[ ]u32[ ]T[ed]0\[256\][ ]=' drivers/staging/rtl8188eu/core/rtw_security.c
    defsnc 'const[ ]u8[ ]Td4s\[256\][ ]=' drivers/staging/rtl8188eu/core/rtw_security.c
    defsnc 'static[ ]u32[ ]array_\(agc_tab\|phy_reg\)_\(1t\|pg\)_8188e\[\][ ]=' drivers/staging/rtl8188eu/hal/HalHWImg8188E_BB.c
    defsnc 'static[ ]u32[ ]array_MAC_REG_8188E\[\][ ]=' drivers/staging/rtl8188eu/hal/HalHWImg8188E_MAC.c
    defsnc 'static[ ]u32[ ]Array_RadioA_1T_8188E\[\][ ]=' drivers/staging/rtl8188eu/hal/HalHWImg8188E_RF.c
    defsnc '[	]u8[	]channel_all\[ODM_TARGET_CHNL_NUM_2G_5G\][ ]=' drivers/staging/rtl8188eu/hal/HalPhyRf.c
    defsnc 'static[ ]const[ ]u16[ ]dB_Invert_Table\[8\]\[12\][ ]=' drivers/staging/rtl8188eu/hal/odm.c
    blobname 'rtl8188E[/\\]*rtl8188efw\.bin' drivers/staging/rtl8188eu/include/rtl8188e_hal.h
    defsnc 'static[ ]const[ ]unsigned[ ]long[ ]K\[64\][ ]=' drivers/staging/rtl8188eu/include/rtw_security.h
    defsnc '[	]static[ ]const[ ]struct[ ]msm_baud_map[ ]table\[\][ ]=' drivers/tty/serial/msm_serial.c
    defsnc 'static[ ]u8[ ]hx8369_seq_gamma_curve_related\[\][ ]=' drivers/video/backlight/hx8357.c
    defsnc 'static[ ]const[ ]wchar_t[ ]t2_\(0[012345]\|1[def]\|2[14cd]\|a[67]\|ff\)\[256\][ ]=' fs/cifs/winucase.c
    accept '[	]*\(\(el\)\?if[ ]\[[ ]-f\|cp[ ]-v[ ]--\)[ ]["][$][{]objtree[}][/]arch[/]mips[/]boot[/]\(compressed[/]\)\?vmlinux\.bin["]' scripts/package/buildtar
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]pcm1681_reg_defaults\[\][ ]=' sound/soc/codecs/pcm1681.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm8997_sysclk_reva_patch\[\][ ]=' sound/soc/codecs/wm8997.c
    blob '[\t]0xE1[,][ ]0x88[,][ ]0x10[,][ ]0x00[,][ ]0x0B[,][ ]0x00[,][ ]0x01[,][ ]0x00[,]\([\n][\t][0-9xA-F, ]*\)*' drivers/staging/rtl8188eu/hal/Hal8188EFWImg_CE.c

    # New in 3.13
    defsnc 'static[ ]const[ ]u32[ ]hawaii_\(golden_registers\|mgcg_cgcg_init\)\[\][ ]=' drivers/gpu/drm/radeon/cik.c
    defsnc 'static[ ]const[ ]u32[ ]hawaii_io_mc_regs\[HAWAII_IO_MC_REGS_SIZE\]\[2\][ ]=' drivers/gpu/drm/radeon/cik.c
    blobname 'dvb-demod-drxk-01\.fw' drivers/media/video/em28xx/em28xx-dvb.c
    blobname '\(ath10k[/]QCA988X[/]hw[12]\.0[/]\)\?firmware-2\.bin' drivers/net/wireless/ath/ath10k/hw.h
    blobname 'brcm[/]brcmfmac43\(143\|241b[04]\|29\|3[045]\)-sdio\.bin' drivers/net/wireless/brcm80211/brcmfmac/dhd_sdio.c
    blobname 'iwlwifi-7265-' drivers/net/wireless/iwlwifi/pcie/7000.c
    accept '[\t][\t]brightness-levels[ ][=][ ][<][0-9 \t\n]*[>][;]' arch/arm/boot/dts/imx28-tx28.dts
    accept '[\t]echo[ ]["]mic[/]uos\.img["][ ]' Documentation/mic/mpssd/micctrl
    accept '[\t]mdev->firmware[ ]=[ ]kmalloc' drivers/misc/mic/host/mic_sysfs.c
    accept '[\t]rc[ ]=[ ]request_firmware[(][&]fw[,][ \t\n]*mdev->\(ramdisk\|firmware\)[,][ ]mdev->sdev->parent[)][;]' drivers/misc/mic/host/mic_x100.c
    accept '[\t]*["]\(ramdisk\|firmware\)[ ]request_firmware[ ]failed' drivers/misc/mic/host/mic_x100.c
    defsnc 'static[ ]const[ ]struct[ ]dsi_clock_table[ ]dsi_clk_tbl\[\][ ]=' drivers/gpu/drm/i915/intel_dsi_pll.c
    defsnc 'uint32_t[ ]nv108_pwr_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/core/subdev/pwr/fuc/nv108.fuc.h
    defsnc 'uint32_t[ ]nva3_pwr_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/core/subdev/pwr/fuc/nva3.fuc.h
    defsnc 'uint32_t[ ]nvc0_pwr_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/core/subdev/pwr/fuc/nvc0.fuc.h
    defsnc 'uint32_t[ ]nvd0_pwr_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/core/subdev/pwr/fuc/nvd0.fuc.h
    defsnc 'static[ ]const[ ]struct[ ]ci_pt_defaults[ ]defaults_hawaii_\(xt\|pro\)[ ]=' drivers/gpu/drm/radeon/ci_dpm.c
    accept '[\t]["]edid[/]\(1024x768\|1280x1024\|1600x1200\|1680x1050\|1920x1080\)\.bin["]' drivers/gpu/drm/drm_edid_load.c
    defsnc 'static[ ]const[ ]u8[ ]generic_edid\[GENERIC_EDIDS\]\[128\][ ]=' drivers/gpu/drm/drm_edid_load.c
    defsnc '[\t]unsigned[ ]char[ ]buf\[\][ ]=' drivers/hid/hid-sony.c
    blobname 'dvb-fe-cx24117\.fw' drivers/media/dvb-frontends/cx24117.c
    blobname 'vpdma-1b8\.bin' drivers/media/platform/ti-vpe/vpdma.c
    defsnc 'static[ ]const[ ]u8[ ]ov361x_start_\(2048\|1600\|1024\|640\|320\|160\)\[\]\[2\][ ]=' drivers/media/usb/gspca/ov534_9.c
    defsnc 'static[ ]const[ ]u8[ ]tuning_blk_pattern_[48]bit\[\][ ]=' drivers/mmc/host/dw_mmc.c
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]oob_8192_ecc[48][ ]=' drivers/mtd/nand/fsl_ifc_nand.c
    defsnc '[\t]static[ ]u8[ ]PN9Data\[\][ ]=' drivers/net/wireless/ath/ath9k/main.c
    blobname 'wlan[/]prima[/]WCNSS_qcom_wlan_nv\.bin' drivers/net/wireless/ath/wcn36xx/wcn36xx.h
    defsnc 'static[ ]s32[ ]expected_tpt_\(siso\|mimo2\)_[248]0MHz\[4\]\[IWL_RATE_COUNT\][ ]=' drivers/net/wireless/iwlwifi/mvm/rs.c
    blobname 'rtlwifi[/]rtl8188eufw\.bin' drivers/staging/rtl8188eu/hal/rtl8188e_hal_init.c
    defsnc 'static[ ]unsigned[ ]char[ ]\(sbox\|dot[23]\)_table\[256\][ ]=' drivers/staging/vt6656/aes_ccmp.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]TKIP_Sbox_\(Lower\|Upper\)\[256\][ ]=' drivers/staging/vt6656/tkip.c
    defsnc 'static[ ]u32[ ]\(al2230_txvga_data\|w89rf242_txvga_old_mapping\)\[\]\[2\][ ]=' drivers/staging/winbond/reg.c
    defsnc '[}][ ]test2\[\][ ]=' lib/random32.c
    defsnc 'static[ ]const[ ]struct[ ]hda_verb[ ]hp_bnb13_eq_verbs\[\][ ]=' sound/pci/hda/patch_sigmatel.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]aic3x_reg\[\][ ]=' sound/soc/codecs/tlv320aic3x.c
    blobname 'radeon[/]HAWAII_\(pfp\|[mc]e\|me\?c\|rlc\|sdma\|smc\)\.bin' drivers/gpu/drm/radeon/cik.c
    blobname 'ti-connectivity[/]wl1251-\(fw\|nvs\)\.bin' 'drivers/net/wireless/wl12\(51\|xx\)/wl1251.h'

    # New in 3.13.2
    blobname 'rtlwifi[/]rtl8192cufw_\([AB]\|TMSC\)\.bin' drivers/net/wireless/rtlwifi/rtl8192cu.sw

    # New in 3.14
    blobname 'dvb-usb-technisat-cablestar-hdci-drxk\.fw' drivers/media/usb/dvb-usb-v2/az6007.c
    blobname 'ctfw-3\.2\.3\.0\.bin' drivers/net/ethernet/brocade/bna/cna.h
    blobname 'ct2fw-3\.2\.3\.0\.bin' drivers/net/ethernet/brocade/bna/cna.h
    blobname 'brcm[/]brcmfmac43362-sdio\.bin' drivers/net/wireless/brcm80211/brcmfmac/dhd_sdio.c
    blobname 'brcm[/]brcmfmac4339-sdio\.bin' drivers/net/wireless/brcm80211/brcmfmac/dhd_sdio.c
    blobname 'mrvl[/]usb8897_uapsta\.bin' drivers/net/wireless/mwifiex/usb.h
    blobname 'cbfw-3\.2\.3\.0\.bin' drivers/scsi/bfa/bfad.c
    blobname 'ctfw-3\.2\.3\.0\.bin' drivers/scsi/bfa/bfad.c
    blobname 'ct2fw-3\.2\.3\.0\.bin' drivers/scsi/bfa/bfad.c

    # New in 3.14.6
    blobname 'radeon[/]\(%s\|BONAIRE\|HAWAII\|TAHITI\|PITCAIRN\|VERDE\|OLAND\|HAINAN\)_mc2\.bin' 'drivers/gpu/drm/radeon/\(cik\|si\)\.c'

    # New in 3.15
    defsnc '\(static[ ]\)\?const[ ]struct[ ]nvc0_graph_init[\n]nvc0_graph_init_\(main\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nvc0.c
    defsnc 'static[ ]const[ ]u32[ ]godavari_golden_registers\[\][ ]=' drivers/gpu/drm/radeon/cik.c
    blobname 'brcm[/]brcmfmac4354-sdio\.bin' drivers/net/wireless/brcm80211/brcmfmac/dhd_sdio.c
    blobname '%s%s\.ucode' drivers/net/wireless/iwlwifi/iwl-drv.c
    blobname 'ti-connectivity[/]wl18xx-fw-3\.bin' drivers/net/wireless/ti/wl18xx/main.c
    blobname 'ql2700_fw\.bin' drivers/scsi/qla2xxx/qla_os.c

    # New in 3.16
    defsnc '[\t]*atmel[,]pll-clk-output-ranges[ ]=[ ]<' 'Documentation/devicetree/bindings/clock/at91-clock\.txt\|arch/arm/boot/dts/at91sam9x5\.dtsi'
    blobname 'imx[/]sdma[/]sdma-imx25\.bin' arch/arm/boot/dts/imx25.dtsi
    blobname 'imx[/]sdma[/]sdma-imx35\.bin' arch/arm/boot/dts/imx35.dtsi
    blobname 'imx[/]sdma[/]sdma-imx50\.bin' arch/arm/boot/dts/imx50.dtsi
    blobname 'sdma-imx53\.bin' arch/arm/boot/dts/imx53-tx53.dtsi
    defsnc 'struct[ ]sock_filter[ ]code\[\][ ]=' Documentation/networking/filter.txt
    initnc '\.L\(Forward\|Reverse\)_Sbox:[\n][\t]\.byte[\t]*' arch/arm64/crypto/aes-neon.S
    initnc '\.Lsha2_rcon:[\n][\t]\.word[\t]*' arch/arm64/crypto/sha2-ce-core.S
    defsnc 'static[ ]const[ ]u8[ ]sata_phy_config[12]\[\][ ]*=' arch/mips/netlogic/xlp/ahci-init-xlp2.c
    accept '[	]*interrupts[ ]=[ ]<108[ ]0\([\n][	 ]*1[012][0-9][ ]0\)*>[;]' arch/powerpc/boot/dts/akebono.dts
    defsnc '[\t]static[ ]int[ ]sysdiv_code_to_x2\[\][ ]=' arch/powerpc/platforms/512x/clock-commonclk.c
    accept '[#][#][ ]*0[ ]1[ ]2[ ]3[ ]4[ ]5[ ]6[ ]7[ ]8[ ]9[ ]0[ ]1[ ]2[ ]3[ ]4[ ]5[ ]6[ ]7[ ]8[ ]9[ ]0[ ]1[ ]2[ ]3[ ]4[ ]5[ ]6[ ]7[ ]8[ ]9[ ]0[ ]1' arch/x86/crypto/aesni-intel_avx-x86_64.S
    defsc 'static[ ]struct[ ]aead_testvec[ ]hmac_sha\(1\|224\|256\|384\|512\)_\(aes\|des\|des3_ede\)_cbc_enc_tv_temp\[\][ ]=' crypto/testmgr.h
    accept '#define[ \t]*ACPI_TABLE_FILE_SUFFIX[\t ]*["]\.dat["]' drivers/acpi/acpica/acapps.h
    accept '[ ][*][ ]request_firmware\(_direct\)\?:[ ]-[ ]load[ ]firmware[ ]directly[ ]without[ ]usermode[ ]helper' drivers/base/firmware_class.c
    accept '[ ][*][ ]This[ ]function[ ]works[ ]pretty[ ]much[ ]like[ ]request_firmware[(][)]' drivers/base/firmware_class.c
    accept 'int[ ]request_firmware_direct[(]' 'drivers/base/firmware_class\.c\|include/linux/firmware\.h'
    accept '[\t]ret[ ]=[ ]_request_firmware[(]firmware_p[,][ ]name[,][ ]device[,][ ]FW_OPT_UEVENT[)][;]' drivers/base/firmware_class.c
    accept 'EXPORT_SYMBOL_GPL[(]request_firmware_direct[)][;]' drivers/base/firmware_class.c
    defsnc 'static[ ]const[ ]int[ ]armada_375_cpu_\(l2\|ddr\)_ratios\[32\]\[2\][ ]__initconst[ ]=[ ]' drivers/clk/mvebu/armada-375.c
    defsnc 'static[ ]const[ ]int[ ]armada_38x_cpu_\(l2\|ddr\)_ratios\[32\]\[2\][ ]__initconst[ ]=[ ]' drivers/clk/mvebu/armada-38x.c
    defsnc 'static[ ]struct[ ]cpufreq_frequency_table[ ]s3c64xx_freq_table\[\][ ]=' drivers/cpufreq/s3c64xx-cpufreq.c
    defsnc 'static[ ]const[ ]u8[ ]ccp_sha\(1\|224\|256\)_zero\[CCP_SHA_CTXSIZE\][ ]=' drivers/crpto/ccp/ccp-ops.c
    blobname 'ast_dp501_fw\.bin' drivers/gpu/drm/ast/ast_dp501.c
    accept '[\t]["]edid[/]\(800x600\)\.bin["]' drivers/gpu/drm/drm_edid_load.c
    defsnc 'static[ ]void[ ][*]edid_load[(][^)]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*err[ ]=[ ]request_firmware[(][&]fw[,][ ]name[,][ ][&]pdev' drivers/gpu/drm/drm_edid_load.c
    defsnc 'static[ ]const[ ]struct[ ]hdmiphy_config[ ]hdmiphy_5420_configs\[\][ ]=' drivers/gpu/drm/exynos/exynos_hdmi.c
    # These seem too sparse to be code.
    defsnc 'static[ ]const[ ]u32[ ]gen6_null_state_batch\[\][ ]=' drivers/gpu/drm/i915/intel_renderstate_gen6.c
    defsnc 'static[ ]const[ ]u32[ ]gen7_null_state_batch\[\][ ]=' drivers/gpu/drm/i915/intel_renderstate_gen7.c
    defsnc 'static[ ]const[ ]u32[ ]gen8_null_state_batch\[\][ ]=' drivers/gpu/drm/i915/intel_renderstate_gen8.c
    defsnc 'nv50_disp_\(mast_mthd_head\|\(sync\|ovly\)_mthd_base\)[ ]=' drivers/gpu/drm/nouveau/core/engine/disp/nv50.c
    defsnc 'nv84_disp_\(mast_mthd_head\|\(sync\|ovly\)_mthd_base\)[ ]=' drivers/gpu/drm/nouveau/core/engine/disp/nv84.c
    defsnc 'nva0_disp_ovly_mthd_base[ ]=' drivers/gpu/drm/nouveau/core/engine/disp/nva0.c
    defsnc 'nvd0_disp_\(mast_mthd_head\|\(sync\|ovly\)_mthd_base\)[ ]=' drivers/gpu/drm/nouveau/core/engine/disp/nvd0.c
    defsnc 'nve0_disp_\(mast_mthd_head\|ovly_mthd_base\)[ ]=' drivers/gpu/drm/nouveau/core/engine/disp/nve0.c
    defsnc 'gm107_grctx_init_\(\(icmd\|b097\|fe\|ds\|pd\|be\|setup\|tex\|mpc\|sm\|wwdx\)_0\|gpc_unk_2\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxgm107.c
    defsnc 'nv108_grctx_init_\(icmd\|fe\|ds\|pd\|rstr2d\|be\|prop\|setup\|crstr\|tex\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnv108.c
    defsnc 'nvc0_grctx_init_\(icmd\|9097\|902d\|90c0\|fe\|memfmt\|rstr2d\|prop\|setup\|crstr\|zcullr\|wwdx\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnvc0.c
    defsnc 'nvc1_grctx_init_\(icmd\|9097\|setup\|wwdx\|tex\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnvc1.c
    defsnc 'nvc4_grctx_init_\(tex\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnvc4.c
    defsnc 'nvc8_grctx_init_\(icmd\|setup\)_0\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnvc8.c
    defsnc 'nvd7_grctx_init_\(ds\|pd\|setup\|tex\|wwdx\)_0\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnvd7.c
    defsnc 'nvd9_grctx_init_\(icmd\|90c0\|fe\|ds\|prop\|setup\|crstr\|tex\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnvd9.c
    defsnc 'nve4_grctx_init_\(icmd\|a097\|fe\|memfmt\|ds\|pd\|be\|setup\|tex\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnve4.c
    defsnc 'nvf0_grctx_init_\(icmd\|a197\|fe\|pd\|be\|setup\|tex\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/ctxnvf0.c
    defsnc 'uint32_t[ ]gm107_grgpc_code\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/fuc/gpcgm107.fuc5.h
    defsnc 'uint32_t[ ]nv108_grgpc_code\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/fuc/gpcnv108.fuc5.h
    defsnc 'uint32_t[ ]gm107_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/fuc/hubgm107.fuc5.h
    defsnc 'uint32_t[ ]nv108_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/fuc/hubnv108.fuc5.h
    defsnc 'gm107_graph_init_\(main\|tpccs\|tex\|sm\|be\)_0\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/gm107.c
    defsnc 'nv108_graph_init_\(main\|l1c\)_0\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nv108.c
    defsnc 'nvc4_graph_init_sm_0\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nvc4.c
    defsnc 'nvc8_graph_init_sm_0\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nvc8.c
    defsnc 'nvd9_graph_init_\(gpc_unk_1\|sm_0\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nvd9.c
    defsnc 'nve4_graph_init_\(\(main\|l1c\|sm\|be\)_0\|gpc_unk_1\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nve4.c
    defsnc 'nvf0_graph_init_\(\(l1c\|sm\)_0\|gpc_unk_1\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nvf0.c
    defsnc 'static[ ]u8[ ]const[ ]ld9040_gammas\[25\]\[22\][ ]=' drivers/gpu/drm/panel/panel-ld9040.c
    defsnc 'static[ ]void[ ]s6e8aa0_panel_cond_set[(][^)]*[)][\n][{]\([\n]\+[^\n}][^\n]*\)*[^\n]*s6e8aa0_dcs_write_seq_static[(]ctx[,][\n\t0x0-9a-f, ]*[)][;]' drivers/gpu/drm/panel/panel-s6e8aa0.c
    defsnc 'static[ ]const[ ]s6e8aa0_gamma_table[ ]s6e8aa0_gamma_tables_v\(142\|96\|32\)\[GAMMA_LEVEL_NUM\][ ]=' drivers/gpu/drm/panel/panel-s6e8aa0.c
    blobname 'radeon[/]BONAIRE_vce\.bin' drivers/gpu/drm/radeon/radeon_vce.c
    defsnc '[\t]static[ ]const[ ]__u8[ ]sixaxis_leds\[10\]\[4\][ ]=' drivers/hid/hid-sony.c
    defsnc '[\t]union[ ]sixaxis_output_report_01[ ]report[ ]=' drivers/hid/hid-sony.c
    defsnc 'static[ ]int[ ]twl4030_therm_tbl\[\][ ]=' drivers/iio/adc/twl4030-madc.c
    defsnc 'static[ ]struct[ ]linear_segments[ ]strength_to_db_table\[\][ ]=' drivers/media/dvb-frontends/dib8000.c
    blobname 'dvb-fe-drxj-mc-1\.0\.8\.fw' drivers/media/dvb-frontends/drx39xyj/drxj.c
    defsnc 'static[ ]const[ ]u16[ ]nicam_presc_table_val\[43\][ ]=' drivers/media/dvb-frontends/drx39xyj/drxj.c
    accept '[\t][\t]*demod->firmware[ ]=[ ]\(fw\|NULL\)[;]' drivers/media/dvb-frontends/drx39xyj/drxj.c
    blobname 'dvb-demod-m88ds3103\.fw' drivers/media/dvb-frontends/m88ds3103_priv.h
    defsnc 'static[ ]const[ ]struct[ ]m88ds3103_reg_val[ ]m88ds3103_dvbs2\?_init_reg_vals\[\][ ]=' drivers/media/dvb-frontends/m88ds3103_priv.h
    blobname 'dvb-demod-si2168-02\.fw' drivers/media/dvb-frontends/si2168_priv.h
    blobname 's5k5baf-cfg\.bin' drivers/media/i2c/s5k5baf.c
    defsnc 'static[ ]const[ ]u16[ ]scaler_[hv]s_coeffs\[1[35]\]\[SC_NUM_PHASES[ ][*][ ]2[ ][*][ ]SC_[HV]_NUM_TAPS\][ ]=' drivers/media/platform/ti-vpe/sc_coeff.h
    defsnc 'static[ ]const[ ]struct[ ]si4713_start_seq_table[ ]start_seq\[\][ ]=' drivers/media/radio/si4713/radio-usb-si4713.c
    defsnc 'static[ ]const[ ]struct[ ]e4000_if_gain[ ]e4000_if_gain_lut\[\][ ]=' drivers/media/tuners/e4000_priv.h
    defsnc 'static[ ]const[ ]struct[ ]dtcs033_usb_requests[ ]dtcs033_start_reqs\[\][ ]=' drivers/media/usb/gspca/dtcs033.c
    defsnc 'static[ ]struct[ ]idxdata[ ]tbl_\(\(middle\|end\)_hvflip\(_\(low\|big\)\)\?\|init_post_alt_\(low[123]\|big\|3B\)\)\[\][ ]=' drivers/media/usb/gspca/gl860/gl860-mi2020.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm5110_revd_patch\[\][ ]=' drivers/mfd/wm5110-tables.c
    defsnc 'static[ ]const[ ]u32[ ]tuning_block_128\[\][ ]=' drivers/mmc/host/sdhci-msm.c
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]hwecc4_2048[ ]=' drivers/mtd/nand/davinci_nand.c
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]ecc_layout_[24]KB_bch[48]bit[ ]=' drivers/mtd/nand/pxa3xx_nand.c
    defsnc '[\t]static[ ]char[ ]packet\[\][ ]=' drivers/net/ethernet/intel/i40e/i40e_txrx.c
    defsnc 'u8[ ]netvsc_hash_key\[HASH_KEYLEN\][ ]=' drivers/net/hyperv/rndis_filter.c
    defsnc 'static[ ]const[ ]u32[ ]ar9300Modes_high_power_tx_gain_table_buffalo\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar9003_buffalo_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9340_cus227_tx_gain_table_1p0\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar9340_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9462_2p0_common_\(mixed_\)\?rx_gain\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/ar9462_2p0_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]ar9462_2p0_modes_\(low\|mix\|high\)_ob_db_tx_gain\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar9462_2p0_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]qca953x_1p[01]_\(\(mac\|baseband\|radio\)_core\|modes_\(no_\)\?xpa_tx_gain_table\)\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/ar953x_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]qca953x_1p0_\(baseband\|radio\)_postamble\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar953x_initvals.h
    accept '[	]err[ ]=[ ]request_firmware_nowait[(][^\n]*,[ ]CARL9170FW_NAME,' drivers/net/wireless/carl9170/usb.c
    defsnc 'static[ ]const[ ]struct[ ]b43_nphy_channeltab_entry_rev3[ ]b43_nphy_channeltab_\(phy\|radio\)_rev\([34568]\|7_9\|11\)\[\][ ]=' drivers/net/wireless/b43/radio_2056.c
    defsnc 'static[ ]const[ ]u32[ ]b43_ntab_noisevar_r3\[\][ ]=' drivers/net/wireless/b43/tables_nphy.c
    blobname 'iwlwifi-8000C\?-' drivers/net/wireless/intel/iwlwifi/iwl-8000.c
    blobname 'iwl_nvm_8000\.bin' drivers/net/wireless/iwlwifi/iwl-8000.c
    defsnc 'static[ ]const[ ]u8[ ]iwl_nvm_channels_family_8000\[\][ ]=' drivers/net/wireless/iwlwifi/iwl-nvm-parse.c
    defsnc 'static[ ]const[ ]u16[ ]expected_tpt_\(siso\|mimo2\)_[248]0MHz\[4\]\[IWL_RATE_COUNT\][ ]=' drivers/net/wireless/iwlwifi/mvm/rs.c
    blobname 'rsi_91x\.fw' drivers/net/wireless/rsi/rsi_common.h
    defsnc 'static[ ]const[ ]u32[ ]RF_GAIN_TABLE\[\][ ]=' drivers/net/wireless/rtl818x/rtl8180/rtl8225se.c
    defsnc 'static[ ]const[ ]u8[ ]\(cck_ofdm_gain_settings\|rtl8225se_tx_power_cck\(_ch14\)\?\|ZEBRA_AGC\|OFDM_CONFIG\)\[\][ ]=' drivers/net/wireless/rtl818x/rtl8180/rtl8225se.c
    defsnc '[\t]u16[ ]toshiba_smid1\[\][ ]=' drivers/net/wireless/rtlwifi/rtl8723be/hw.c
    blobname 'rtlwifi[/]rtl8723befw\.bin' drivers/net/wireless/rtlwifi/rtl8723be/sw.c
    defsnc 'u32[ ]RTL8723BE\(PHY_REG\|_RADIOA\|MAC\|AGCTAB\)_\(1T_\?ARRAY\|ARRAY_PG\)\[\][ ]=' drivers/net/wireless/rtlwfi/rtl8723be/table.c
    defsnc 'static[ ]\(const[ ]unsigned[ ]\)\?int[ ]tps65864[03]_sm2_voltages\[\][ ]=' drivers/regulator/tps6586x-regulator.c
    defsnc 'static[ ]const[ ]uint32_t[ ]ql27xx_fwdt_default_template\[\][ ]=' drivers/scsi/qla2xxx/qla_tmpl.c
    blobname 'dgap[/]\(sx\|cxp\|pci\|xr\)\(bios\|fep\)\.bin' drivers/staging/dgap/dgap.c
    accept '[\t][ ]*kernel[ ]firmware[ ]framework[,][ ]request_firmware[(][)]' drivers/staging/gs_fpgaboot/README
    defsnc 'static[ ]u8[ ]ecctable\[256\][ ]=' drivers/staging/keucr/smilecc.c
    defsnc '[\t]u8[ ]data_ptr\[36\][ ]=' drivers/staging/keucr/smscsi.c
    # This is a default for the user-supplied fpga configuration; it
    # is overridable with a module parameter.
    accept 'static[ ]char[ \t]*[*]file[ ]=[ ]["]xlinx_fpga_firmware\.bit["][;]' drivers/staging/gs_fpgaboot/gs_fpgaboot.c
    accept '[\t]pr_info[(]["]load[ ]fpgaimage[ ]%s[\\]n["][,][ ]file[)][;][\n]*[\t]err[ ]=[ ]request_firmware[(][&]fimage->fw_entry[,]' drivers/staging/gs_fpgaboot/gs_fpgaboot.c
    blobname '\(ti1273\(_\(pre\)\?le\)\?\|bc[m4]fw\)\.bin' drivers/staging/nokia_h4p/nokia_fw.c
    defsnc '[\t]u8[ ]channel5g\[CHANNEL_MAX_NUMBER_5G\][ ]=' drivers/staging/rtl8192ee/rtl8192ee/hw.c
    blobname 'rtlwifi[/]rtl8192eefw\.bin' drivers/staging/rtl8192ee/rtl8192ee/sw.c
    defsnc 'u32[ ]RTL8192EE_\(PHY_REG\|RADIO[AB]\|MAC\|AGC_TAB\)_ARRAY\(_PG\)\?\[\][ ]=' drivers/staging/rtl8192ee/rtl8192ee/table.c
    defsnc '[\t]u8[ ]Channel_5G\[45\][ ]=' drivers/staging/rtl8723au/core/rtw_mlme_ext.c
    defsnc 'static[ ]const[ ]unsigned[ ]short[ ]Sbox1\[2\]\[256\]=' drivers/staging/rtl8723au/core/rtw_security.c
    defsnc 'u32[ ]Rtl8723UPHY_REG_Array_PG\[Rtl8723UPHY_REG_Array_PGLength\][ ]=' drivers/staging/rtl8723au/hal/Hal8723UHWImg_CE.c
    defsnc 'static[ ]u32[ ]Array_\(AGC_TAB\|PHY_REG\)_\(1T\|PG\)_8723A\[\][ ]=' drivers/staging/rtl8723au/hal/HalHWImg8723A_BB.c
    defsnc 'static[ ]u32[ ]Array_MAC_REG_8723A\[\][ ]=' drivers/staging/rtl8723au/hal/HalHWImg8723A_MAC.c
    defsnc 'static[ ]u32[ ]Array_RadioA_1T_8723A\[\][ ]=' drivers/staging/rtl8723au/hal/HalHWImg8723A_RF.c
    blobname 'rtlwifi[/]rtl8723aufw_\(A\|B\(_NoBT\)\?\)\.bin' drivers/staging/rtl8723au/hal/rtl8723a_hal_init.c
    defsnc 'u8[ ]rtl88\(12\|21\)ae_delta_swing_table_idx_5g[ab]_[np]_txpwrtrack\[\]\[DELTA_SWINGIDX_SIZE\][ ]=' drivers/staging/rtl8821ae/rtl8821ae/dm.c
    defsnc 'static[ ]u8[ ]reserved_page_packet_8821\[TOTAL_RESERVED_PKT_LEN_8821\][ ]=' drivers/staging/rtl8821ae/rtl8821ae/fw.c
    defsnc 'static[ ]u8[ ]reserved_page_packet_8812\[TOTAL_RESERVED_PKT_LEN_8812\][ ]=' drivers/staging/rtl8821ae/rtl8821ae/fw.c
    defsnc '[\t]u8[ ]channel_5g\[CHANNEL_MAX_NUMBER_5G\][ ]=' 'drivers/staging/rtl8821ae/rtl8821ae/\(hw\|phy\)\.c'
    defsnc '[\t]u8[ ]channel_all\[TARGET_CHNL_NUM_2G_5G_8812\][ ]=' drivers/staging/rtl8821ae/rtl8821ae/phy.c
    blobname 'rtlwifi[/]rtl8821aefw\.bin' drivers/staging/rtl8821ae/rtl8821ae/sw.c
    defsnc 'u32[ ]RTL88\(12\|21\)AE_\(\(PHY\|MAC\)_REG\|RADIO[AB]\|AGC_TAB\)_ARRAY\(_PG\)\?\[\][ ]=' drivers/staging/rtl8821ae/rtl8821ae/table.c
    accept '#define[ ]CONFIG_PATH[\t]*["][/]etc[/]vntconfiguration[.]dat["]' drivers/staging/vt6656/device.h
    defsnc 'static[ ]const[ ]u8[ ]TKIP_Sbox_\(Lower\|Upper\)\[256\][ ]=' drivers/staging/vt6656/tkip.c
    blobname 'moxa[/]moxa-\(%04x\|[0-9a-f][0-9a-f][0-9a-f][0-9a-f]\)\.fw' drivers/usb/serial/mxuport.c
    accept '#define[ \t]request_firmware_direct[ \t]request_firmware' include/linux/firmware.h
    accept '[\t]report_missing_free_firmware[^\n]*[\n][\t]retval[ ]=[ ]request_firmware_direct[(]' include/linux/firmware.h
    defsnc 'const[ ]u8[ ]crc7_be_syndrome_table\[256\][ ]=' lib/crc7.c
    defsnc 'static[ ]struct[ ]bpf_test[ ]tests\[\][ ]=' lib/test_bpf.c
    defsnc '[\t]static[ ]struct[ ]sock_filter[ ]ptp_filter\[\][ ]__initdata[ ]=' net/core/ptp_classifier.c
    blobname 'adau1761\.bin' sound/soc/codecs/adau1761.c
    accept '[\t][\t]ret[ ]=[ ]adau17x1_load_firmware[(]adau[,][ ]codec->dev[,][\n][\t ]*ADAU1761_FIRMWARE[)][;]' sound/soc/codecs/adau1761.c
    blobname 'adau1[37]81\.bin' sound/soc/codecs/adau1781.c
    accept '[\t][\t]firmware[ ]=[ ]ADAU1[37]81_FIRMWARE[;]\([\n][\n]*[\t][^\n]*\)*ret[ ]=[ ]adau17x1_load_firmware[(]adau[,][ ]codec->dev[,][ ]firmware[)][;]' sound/soc/codecs/adau1781.c
    blobna 'adau17x1_load_firmware' sound/soc/codecs/adau17x1.c
    accept 'int[ ]adau17x1_load_firmware[(]' 'sound/soc/codecs/adau17x1\.[ch]'
    accept 'EXPORT_SYMBOL_GPL[(]adau17x1_load_firmware[)][;]' sound/soc/codecs/adau17x1.c
    accept '[ 	]*ret[ ]=[ ]process_sigma_firmware_regmap[(]dev[,][ ]adau->regmap[,][ ]firmware[)][;]' sound/soc/codecs/adau17x1.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]adau1977_reg_defaults\[\][ ]=' sound/soc/codecs/adau1977.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]ak4641_reg_defaults\[\][ ]=' sound/soc/codecs/ak4641.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]ak464[28]_reg\[\][ ]=' sound/soc/codecs/ak4642.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt5640_reg\[\][ ]=' sound/soc/codecs/rt5640.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt5645_reg\[\][ ]=' sound/soc/codecs/rt5645.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt5651_reg\[\][ ]=' sound/soc/codecs/rt5651.c
    defsnc 'int[ ]_process_sigma_firmware[(]' sound/soc/codecs/sigmadsp.c
    accept 'EXPORT_SYMBOL_GPL[(]_process_sigma_firmware[)]' sound/soc/codecs/sigmadsp.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]sta350_regs\[\][ ]=' sound/soc/codecs/sta350.c
    defsnc 'static[ ]const[ ]struct[ ]aic31xx_rate_divs[ ]aic31xx_divs\[\][ ]=' sound/soc/codecs/tlv320aic31xx.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm5110_sysclk_revd_patch\[\][ ]=' sound/soc/codecs/wm5110.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm8974_reg_defaults\[\][ ]=' sound/soc/codecs/wm8974.c
    blobname 'intel[/]IntcSST[12]\.bin' sound/soc/intel/sst-acpi.c
    blobname 'intel[/]fw_sst_0f28\.bin-i2s_master' sound/soc/intel/sst-acpi.c
    defsnc 'static[ ]unsigned[ ]char[ ]bcd2000_init_sequence\[\][ ]=' sound/usb/bcd2000/bcd2000.c
    blobna '[ ][*][ ]xxd[ ]-r[ ]-p[ ]mXTXXX[^\n]*maxtouch\.fw[\n][ \t]*[*][/]' drivers/input/touchscreen/atmel_mxt_ts.c
    blobname 's5p-mfc-v8\.fw' drivers/media/platform/s5p-mfc/s5p_mfc.c

    # New in 3.17
    blobname 'radeon[/]\(%s\|kaveri\|KAVERI\)_mec2\.bin' drivers/gpu/drm/radeon/cik.c
    blobname 'dvb-demod-si2168-\(\(a[23]\|b4\)0-01\|-02\)\.fw' drivers/media/dvb-frontends/si2168_priv.h
    accept '[	]\[CODA_IMX6\(Q\|DL\)\][ ]=[ ][{][\n][	][	]\.firmware[ ]*=' drivers/media/platform/coda.c
    blobname 'v4l-coda960-imx6\(q\|dl\)\.bin' drivers/media/platform/coda.c
    blobname 's5p-mfc-v6-v2\.fw' drivers/media/platform/s5p-mfc/s5p_mfc.c
    blobname 'dvb-fe-xc4000-1\.4\(\.1\)\?\.fw' drivers/media/tuners/xc4000.c
    blobname 'ti-connectivity[/]TIInit_\(\(%d\|[0-9]\+\)[.]\)\+bts' drivers/misc/ti-st/st_kim.c
    blobname 'fw-5\.bin' drivers/net/wireless/ath/ath6kl/core.h
    blobname 'brcm[/]brcmfmac43569\.bin' drivers/net/wireless/brcm80211/brcmfmac/usb.c
    blobname '3826\.eeprom' drivers/net/wireless/p54/p54spi.c
    defsnc 'static[ ]const[ ]u64[ ]sha512_k\[\][ ]=' arch/arm/crypto/sha512_neon_glue.c
    accept 'K_table:\([\n][ \t]*\.\(quad\|long\)[ \t]*0x[0-9a-f]*[,][ ]\?0x[0-9a-f]*\)\*' arch/x86/crypto/crc32c-pcl-intel-asm_64.S
    accept '\.L_s[12345678]:\([\n][ 	]*\.quad[ 	]*0x[0-9a-f]*[,][ ]0x[0-9a-f]*\)*' arch/x86/crypto/des3_ede-asm_64.S
    defsnc '[\t]const[ ]unsigned[ ]char[ ][*]K[ ]=[ ][(]unsigned[ ]char[ ][*][)]' crypto/drbg.c
    accept '[\t]ret[ ]=[ ]_request_firmware[(]firmware_p[,][ ]name[,][ ]device[,]' drivers/base/firmware_class.c
    defsnc 'static[ ]const[ ]uint64_t[ ]inst\[\][ ]=' drivers/crypto/qat/qat_common/qat_hal.c
    defsnc 'gk110b_\(grctx\|graph\)_init_\(sm\|l1c\)_0\[\][ ]=' drivers/gpu/dm/nouveau/core/engine/graph/ctxgk110b.c
    defsnc '[\t]const[ ]u16[ ]map\[\][ ]=' drivers/hwmon/asc7621.c
    defsnc '[}][ ]samp_freq_table\[\][ ]=' drivers/iio/accel/kxcjk-1013.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]jpeg_dqt\[4\]\[DQT_LEN\][ ]=' drivers/media/pci/solo6x10/solo6x10-jpeg.h
    defsnc 'static[ ]const[ ]u32[ ]qca953x_2p0_baseband_core\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/ar953x_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]qca953x_2p0_baseband_postamble\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar953x_initvals.h
    defsnc 'static[ ]u16[ ]r2057_rev\(4\|5a\?\|[789]\|14\)_init\[\]\[2\][ ]=' drivers/net/wireless/b43/radio_2057.c
    defsnc 'static[ ]const[ ]u32[ ]b43_ntab_\(\(tmap\|noisevar\)_r7\|tx_gain_\(epa\|ipa\(_2057\)\?\)_rev\([34569]\|14\)_\(hi_pwr_\)\?\(2g\|5g\)\)\[\][ ]=' drivers/net/wireless/b43/tables_nphy.c
    accept '[	]ret[ ]=[ ]request_firmware[(][&]pm8001_ha->fw_image,' drivers/scsi/pm8001/pm8001_ctl.c
    defsnc 'static[ ]unsigned[ ]char[ ]byVT3253InitTab_RFMD\[CB_VT3253_INIT_FOR_RFMD\]\[2\][ ]=' drivers/staging/vt6655/baseband.c
    defsnc 'static[ ]unsigned[ ]char[ ]byVT3253B0_RFMD\[CB_VT3253B0_INIT_FOR_RFMD\]\[2\][ ]=' drivers/staging/vt6655/baseband.c
    defsnc 'static[ ]unsigned[ ]char[ ]byVT3253B0_AGC4_RFMD2959\[CB_VT3253B0_AGC_FOR_RFMD2959\]\[2\][ ]=' drivers/staging/vt6655/baseband.c
    defsnc 'static[ ]unsigned[ ]char[ ]byVT3253B0_AIROHA2230\[CB_VT3253B0_INIT_FOR_AIROHA2230\]\[2\][ ]=' drivers/staging/vt6655/baseband.c
    defsnc 'static[ ]unsigned[ ]char[ ]byVT3253B0_UW2451\[CB_VT3253B0_INIT_FOR_UW2451\]\[2\][ ]=' drivers/staging/vt6655/baseband.c
    defsnc 'static[ ]unsigned[ ]char[ ]byVT3253B0_AGC\[CB_VT3253B0_AGC\]\[2\][ ]=' drivers/staging/vt6655/baseband.c
    defsnc 'static[ ]u8[ ]al2230_init_table\[CB_AL2230_INIT_SEQ\]\[3\][ ]=' drivers/staging/vt6656/rf.c
    defsnc 'static[ ]u8[ ]\(al2230\|vt3226\)_channel_table[012]\[CB_MAX_CHANNEL_24G\]\[3\][ ]=' drivers/staging/vt6656/rf.c
    defsnc 'static[ ]u8[ ]al7230_init_table\(_amode\)\?\[CB_AL7230_INIT_SEQ\]\[3\][ ]=' drivers/staging/vt6656/rf.c
    defsnc 'static[ ]u8[ ]\(al7230\|vt3342\)_channel_table[012]\[CB_MAX_CHANNEL\]\[3\][ ]=' drivers/staging/vt6656/rf.c
    defsnc 'static[ ]u8[ ]vt3226\(d0\)\?_init_table\[CB_VT3226_INIT_SEQ\]\[3\][ ]=' drivers/staging/vt6656/rf.c
    defsnc 'static[ ]u8[ ]vt3342a0_init_table\[CB_VT3342_INIT_SEQ\]\[3\][ ]=' drivers/staging/vt6656/rf.c
    defsnc 'static[ ]const[ ]u32[ ]al2230_power_table\[AL2230_PWR_IDX_LEN\][ ]=' drivers/staging/vt6656/rf.c
    accept 'static[ ]inline[ ]int[ ]request_firmware_direct[(]const[ ]struct[ ]firmware[ ][*][*]fw[,]' include/linux/firmware.h
    defsnc 'static[ ]u8[ ]const[ ]__aligned[(]8[)][ ]test_buf\[\][ ]__initconst[ ]=' lib/crc32.c
    defsnc 'static[ ]struct[ ]crc_test[ ][{][^}]*[}][ ]const[ ]test\[\][ ]__initconst[ ]=' lib/crc32.c
    accept '[\t]rc[ ]=[ ]request_firmware[(][&]test_firmware[,]' lib/test_firmware.c
    defsnc 'static[ ]struct[ ]reg_default[ ]rt286_index_def\[\][ ]=' sound/soc/codecs/rt286.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt286_reg\[\][ ]=' sound/soc/codecs/rt286.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt5670_reg\[\][ ]=' sound/soc/codecs/rt5670.c
    accept 'FW=["][$]FWPATH[/]test-firmware\.bin["]' 'tools/testing/selftests/firmware/fw_\(filesystem\|userhelper\)\.sh'
    blobname 'qat_895xcc\.bin' drivers/crypto/qat/qat_dh895xcc/adf_dh895xcc_hw_data.h
    blobname 'dvb-demod-si2165\.fw' drivers/media/dvb-frontends/si2165_priv.h
    blobname 'dvb-tuner-si2158-a20-01\.fw' drivers/media/tuners/si2157_priv.h
    blobname 'brcm[/]brcmfmac43\(602\|5[46]\|570\)-pcie\.bin' drivers/net/wireless/brcm80211/brcmfmac/pcie.c
    blobname 'r8a779x_usb3_v1\.dlmem' drivers/usb/host/xhci-rcar.c
    blobname 'iwlwifi-3165-' drivers/net/wireless/iwlwifi/iwl-7000.c

    # New in 3.18.
    accept '[\t	]*interrupts[ ]=[ ]<\([ \n\t]*0[ ][4567][0-9][ ]0xf04\)*>[;]' Documentation/devicetree/bindings/soc/ti/keystone-navigator-qmss.txt
    accept '[\t ]*<\([ \t\n]*[ 1-9][0-9 ][0-9]\)*>[;]' arch/arm/boot/dts/tegra124-nyan-big.dts
    blobname 'keystone[/]qmss_pdsp_acc48_k2_le_1_0_0_8\.fw' Documentation/devicetree/bindings/soc/ti/keystone-navigator-qmss.txt
    defsnc 'static[ ]struct[ ]comp_testvec[ ]lz4\(hc\)\?_\(de\)\?comp_tv_template\[\][ ]=' crypto/testmgr.h
    blobname 'mrvl[/]sd8887_uapsta\.bin' 'drivers/\(bluetooth/btmrvl_sdio\.c\|net/wireless/mwifiex/sdio.h\)'
    blobname 'radeon[/]\(R600\|RS780\|RV770\)_uvd\.bin' drivers/gpu/drm/radeon/radeon_uvd.c
    defsnc '[}][ ]wake_odr_data_rate_table\[\][ ]=' drivers/iio/accel/kxcjk-1013.c
    defsnc 'static[ ]const[ ]struct[ ]linear_segments[ ]cnr_\(to_db\|\(64\|16\)qam\|qpsk\)_table\[\][ ]=' drivers/media/dvb-frontends/mb86a20s.c
    defsnc 'static[ ]u8[ ]lgtdqcs001f_inittab\[\][ ]=' drivers/media/pci/mantis/mantis_vp1033.c
    blobname 'go7007[/]go7007tv\.bin' drivers/media/pci/saa7134/saa7134-go7007.c
    defsnc 'static[ ]const[ ]u8[ ]vivid_hdmi_edid\[256\][ ]=' drivers/media/platform/vivid/vivid-core.c
    defsnc 'static[ ]const[ ]s8[ ]sin\[257\][ ]=' drivers/media/platform/vivid/vivid-tpg.c
    defsnc 'static[ ]const[ ]struct[ ]shf[ ]shf_tab\[\][ ]=' drivers/media/tuners/mxl301rf.c
    defsnc 'static[ ]const[ ]u8[ ]reg_initval\[QM1D1C0042_NUM_REGS\][ ]=' drivers/media/tuners/qm1d1c0042.c
    accept '[\t]*priv->firmware[ ]=[ ]fw[;][\n][\t][}][ ]else[\n][\t]*fw[ ]=[ ]priv->firmware[;]' drivers/media/tuners/xc5000.c
    blobname 'dvb-usb-it9303-01\.fw' drivers/media/usb/dvb-usb-v2/af9035.h
    defsnc 'const[ ]u8[ ]tuning_blk_pattern_4bit\[MMC_TUNING_BLK_PATTERN_4BIT_SIZE\][ ]=' drivers/mmc/core/mmc.c
    defsnc 'const[ ]u8[ ]tuning_blk_pattern_8bit\[MMC_TUNING_BLK_PATTERN_8BIT_SIZE\][ ]=' drivers/mmc/core/mmc.c
    defsnc 'static[ ]const[ ]u16[ ]fm10k_crc_16b_table\[256\][ ]=' drivers/net/ethernet/intel/fm10k/fm10k_mbx.c
    accept '[\t ]*[*][ ][ ]1[ ]0[ ]9[ ]8[ ]7[ ]6[ ]5[ ]4[ ]3[ ]2[ ]1[ ]0[ ]9[ ]8[ ]7[ ]6[ ]5[ ]4[ ]3[ ]2[ ]1[ ]0[ ]9[ ]8[ ]7[ ]6[ ]5[ ]4[ ]3[ ]2[ ]1[ ]0' drivers/net/ethernet/intel/fm10k/fm10k_mbx.h
    blobname '83xx_post_fw\.bin' drivers/net/ethernet/qlogic/qlcnic/qlcnic_83xx_hw.h
    blobname 'rtl_nic[/]rtl\(8168h\|8107e\)-[12]\.fw' drivers/net/ethernet/realtek/r8169.c
    blobname 'firmware-3\.bin' drivers/net/wireless/ath/ath10k/hw.h
    blobname 'utf\.bin' drivers/net/wireless/ath/ath10k/testmode.c
    accept '[ ][*][ ]wil_request_firmware[ ]-[ ]Request[ ]firmware' drivers/net/wireless/ath/wil6210/fw_inc.c
    accept 'int[ ]wil_request_firmware[(]' 'drivers/net/wireless/ath/wil6210/\(fw_inc\.c\|wil6210\.h\)'
    accept '[\t]*rc[ ]=[ ]wil_request_firmware[(]wil[,][ ]WIL_FW_NAME[)][;]' drivers/net/wireless/ath/wil6210/fw_inc.c
    blobname 'wil6210\.fw' drivers/net/wireless/ath/wil6210/wil6210.h
    blobna 'FW[ ]Version:[ ]%d_%d_%d' drivers/net/wireless/broadcom/bnx2x/bnx2x_main.c
    blobna '\([,][\n \t]*BCM_5710_FW_\(MAJOR\|MINOR\|REVISION\|ENGINEERING\)_VERSION\)\+' drivers/net/wireless/broadcom/bnx2x/bnx2x_main.c
    blobname 'iwlwifi-8000' drivers/net/wireless/iwlwifi/iwl-8000.c
    blobname '["]-["][ ]__stringify[(]api[)][ ]["]\.ucode["]' drivers/net/wireless/iwlwifi/iwl-8000.c
    blobname '%s%s-%s\.ucode' drivers/net/wireless/iwlwifi/iwl-drv.c
    blobname 'rtlwifi[/]rtl8723efw\.bin' drivers/net/wireless/rtlwifi/rtl8723ae/sw.c
    defsnc 'u32[ ]RTL8723E_RADIOA_1TARRAY\[RTL8723ERADIOA_1TARRAYLENGTH\][ ]=' drivers/net/wireless/rtlwifi/rtl8723ae/table.c
    defsnc '[\t]u8[ ]channel_all\[TARGET_CHNL_NUM_2G_5G\][ ]=' drivers/net/wireless/rtlwifi/rtl8723be/phy.c
    blobname 'rtlwifi[/]rtl88\(21\|12\)aefw\(_wowlan\)\?\.bin' drivers/net/wireless/rtlwifi/rtl8821ae/sw.c
    defsnc 'static[ ]u8[ ]rtl88\(12\|21\)ae_delta_swing_table_idx_5g[ba]_[np]\[\]\[DEL_SW_IDX_SZ\][ ]=' drivers/net/wireless/rtlwifi/rtl8821ae/dm.c
    defsnc '[\t]u8[ ]channel_all\[ODM_TARGET_CHNL_NUM_2G_5G\][ ]=' drivers/staging/rtl8188eu/hal/phy.c
    # Present before 3.18, but changes to reject_firmware shell
    # function to make it match request_firmware only require us to
    # recognize these as false positives.
    accept 'static[ ]int[ ]lp55xx_request_firmware[(]' drivers/leds/leds-lp55xx-common.c
    accept '[\t]*ret[ ]=[ ]lp55xx_request_firmware[(]' drivers/leds/leds-lp55xx-common.c
    accept 'static[ ]int[ ]flexcop_fe_request_firmware[(]' drivers/media/common/b2c2/flexcop-fe-tuner.c
    accept '[\t]\.request_firmware[ ]=[ ]flexcop_fe_request_firmware[,]' drivers/media/common/b2c2/flexcop-fe-tuner.c
    accept '[\t]if[ ][(][(]ret[ ]=[ ]st->config->request_firmware[(]' drivers/media/dvb-frontends/bcm3510.c
    accept '[\t][\t]ret[ ]=[ ]config->request_firmware[(]' drivers/media/dvb-frontends/or51211.c
    accept '[\t]if[ ][(]state->config->request_firmware[(]' drivers/media/dvb-frontends/sp8870.c
    accept '[\t][\t]ret[ ]=[ ]state->config->request_firmware[(]' drivers/media/dvb-frontends/sp887x.c
    accept '[\t]int[ ][(][*]request_firmware[)][(]' drivers/media/dvb-frontends/sp887x.h
    accept '[\t]ret[ ]=[ ]state->config->request_firmware[(]' drivers/media/dvb-frontends/tda1004x.c
    accept '[\t]if[ ][(]state->config->request_firmware[ ]' drivers/media/dvb-frontends/tda1004x.c
    accept '[\t][\t][\t]*ret[ ]=[ ]state->config->request_firmware[(]' drivers/media/dvb-frontends/tda1004x.c
    accept 'static[ ]int[ ]alps_tdhd1_204_request_firmware[(]' drivers/media/dvb-frontends/tdhd1.h
    accept '[\t]\.request_firmware[ ]=[ ]alps_tdhd1_204_request_firmware' drivers/media/dvb-frontends/tdhd1.h
    accept 'static[ ]int[ ]microtune_mt7202dtf_request_firmware[(]' drivers/media/pci/bt8xx/dvb-bt8xx.c
    accept '[\t]\.request_firmware[ ]=[ ]microtune_mt7202dtf_request_firmware[,]' drivers/media/pci/bt8xx/dvb-bt8xx.c
    accept 'static[ ]int[ ]or51211_request_firmware[(]' drivers/media/pci/bt8xx/dvb-bt8xx.c
    accept '[\t]\.request_firmware[ ]=[ ]or51211_request_firmware[,]' drivers/media/pci/bt8xx/dvb-bt8xx.c
    accept 'static[ ]int[ ]pluto2_request_firmware[(]' drivers/media/pci/pluto2/pluto2.c
    accept '[\t]\.request_firmware[ ]=[ ]pluto2_request_firmware[,]' drivers/media/pci/pluto2/pluto2.c
    accept 'static[ ]int[ ]philips_tda1004x_request_firmware[(]' drivers/media/pci/saa7134/saa7134-dvb.c
    accept '[\t]\.request_firmware[ ]=[ ]philips_tda1004x_request_firmware' drivers/media/pci/saa7134/saa7134-dvb.c
    accept 'static[ ]int[ ]alps_tdlb7_request_firmware[(]' drivers/media/pci/ttpci/av7110.c
    accept '[\t]\.request_firmware[ ]=[ ]alps_tdlb7_request_firmware[,]' drivers/media/pci/ttpci/av7110.c
    accept 'static[ ]int[ ]philips_tu1216_request_firmware[(]' drivers/media/pci/ttpci/budget-av.c
    accept '[\t]\.request_firmware[ ]=[ ]philips_tu1216_request_firmware[,]' drivers/media/pci/ttpci/budget-av.c
    accept 'static[ ]int[ ]philips_tdm1316l_request_firmware[(]' drivers/media/pci/ttpci/budget-ci.c
    accept '[\t]\.request_firmware[ ]=[ ]philips_tdm1316l_request_firmware[,]' drivers/media/pci/ttpci/budget-ci.c
    accept 'static[ ]int[ ]alps_tdhd1_204_request_firmware[(]' drivers/media/pci/ttpci/budget.c
    accept 'static[ ]int[ ]fimc_is_request_firmware[(]' drivers/media/platform/exynos4-is/fimc-is.c
    accept '[\t]ret[ ]=[ ]fimc_is_request_firmware[(]' drivers/media/platform/exynos4-is/fimc-is.c
    accept 'static[ ]int[ ]philips_tdm1316l_request_firmware[(]' drivers/media/usb/ttusb-budget/dvb-ttusb-budget.c
    accept '[\t]\.request_firmware[ ]=[ ]philips_tdm1316l_request_firmware[,]' drivers/media/usb/ttusb-budget/dvb-ttusb-budget.c
    accept '[\t][\t]pr_err[(]["][ ]request_firmware[ ]failed' drivers/misc/ti-st/st_kim.c
    accept 'typhoon_request_firmware[(]' drivers/net/ethernet/3com/typhoon.c
    accept '[\t]err[ ]=[ ]typhoon_request_firmware[(]' drivers/net/ethernet/3com/typhoon.c
    accept '[\t][\t]goto[ ]request_firmware_exit[;]' drivers/net/ethernet/broadcom/bnx2x/bnx2x_main.c
    accept '[\t]BNX2X_ALLOC_AND_SET[(]init_data[,][ ]request_firmware_exit[,]' drivers/net/ethernet/broadcom/bnx2x/bnx2x_main.c
    accept 'request_firmware_exit:' drivers/net/ethernet/broadcom/bnx2x/bnx2x_main.c
    accept 'static[ ]int[ ]bnx2_request_firmware[(]' drivers/net/ethernet/broadcom/bnx2.c
    accept '[\t]rc[ ]=[ ]bnx2_request_firmware[(]' drivers/net/ethernet/broadcom/bnx2.c
    accept 'static[ ]int[ ]tg3_request_firmware[(]' drivers/net/ethernet/broadcom/tg3.c
    accept '[\t][\t]err[ ]=[ ]tg3_request_firmware[(]' drivers/net/ethernet/broadcom/tg3.c
    accept 'static[ ]const[ ]struct[ ]firmware[ ][*]e100_request_firmware[(]' drivers/net/ethernet/intel/e100.c
    accept '[\t]fw[ ]=[ ]e100_request_firmware[(]' drivers/net/ethernet/intel/e100.c
    accept '[/][*][ ]Call[ ]this[]function[ ]from[ ]process[ ]context[,][ ]it[ ]will[ ]sleep[ ]in[ ]request_firmware[.]' drivers/net/wireless/ipw2x00/ipw2200.c
    accept '[ ][*][ ]@request_firmware_complete:' drivers/net/wireless/iwlwifi/iwl-drv.c
    accept '[\t][\t]lbs_deb_fw[(]["]request_firmware_nowait[ ]error' drivers/net/wireless/libertas/firmware.c
    accept 'void[ ]netxen_request_firmware[(]' 'drivers/net/ethernet/qlogic/netxen/netxen_nic\(\.h\|_init\.c\)'
    accept '[\t]netxen_request_firmware[(]' drivers/net/ethernet/qlogic/netxen/netxen_nic_main.c
    accept 'void[ ]qlcnic_request_firmware[(]' 'drivers/net/ethernet/qlogic/qlcnic/qlcnic\(\.h\|_init\.c\)'
    accept '[\t][\t]qlcnic_request_firmware[(]' drivers/net/ethernet/qlogic/qlcnic/qlcnic_main.c
    accept 'static[ ]void[ ]rtl_request_firmware[(]' drivers/net/ethernet/realtek/r8169.c
    accept '[\t]rtl_request_firmware[(]' drivers/net/ethernet/realtek/r8169.c
    accept 'static[ ]void[ ]b43_request_firmware[(]' drivers/net/wireless/b43/main.c
    accept '[\t]INIT_WORK[(][&]wl->firmware_load[,][ ]b43_request_firmware[)]' drivers/net/wireless/b43/main.c
    accept 'static[ ]void[ ]b43legacy_request_firmware[(]' drivers/net/wireless/b43legacy/main.c
    accept '[\t]INIT_WORK[(][&]wl->firmware_load[,][ ]b43legacy_request_firmware[)]' drivers/net/wireless/b43legacy/main.c
    accept 'il4965_request_firmware[(]' drivers/net/wireless/iwlegacy/4965-mac.c
    accept '[\t]if[ ][(]il4965_request_firmware[(]' drivers/net/wireless/iwlegacy/4965-mac.c
    accept '[\t]err[ ]=[ ]il4965_request_firmware[(]' drivers/net/wireless/iwlegacy/4965-mac.c
    accept 'static[ ]int[ ]iwl_request_firmware[(]' drivers/net/wireless/iwlwifi/iwl-drv.c
    accept '[\t]if[ ][(]iwl_request_firmware[(]' drivers/net/wireless/iwlwifi/iwl-drv.c
    accept '[\t]ret[ ]=[ ]iwl_request_firmware[(]' drivers/net/wireless/iwlwifi/iwl-drv.c
    accept '[ ][*][ ]@request_firmware_complete:' drivers/net/wireless/iwlwifi/iwl-drv.c
    accept '[\t]struct[ ]completion[ ]request_firmware_complete[;]' drivers/net/wireless/iwlwifi/iwl-drv.c
    accept '[\t]\(complete\|\(init\|wait_for\)_completion\)[(][&]drv->request_firmware_complete[)]' drivers/net/wireless/iwlwifi/iwl-drv.c
    accept '[\t][ ][*][ ]Obtain[ ]NVM[ ]image[ ]via[ ]request_firmware[.]' drivers/net/wireless/iwlwifi/mvm/nvm.c
    accept 'static[ ]int[ ]mwl8k_request_firmware[(]' drivers/net/wireless/mwl8k.c
    accept '[\t]rc[ ]=[ ]mwl8k_request_firmware[(]' drivers/net/wireless/mwl8k.c
    accept 'static[ ]int[ ]p54spi_request_firmware[(]' drivers/net/wireless/p54/p54spi.c
    accept '[\t]ret[ ]=[ ]p54spi_request_firmware[(]' drivers/net/wireless/p54/p54spi.c
    accept 'static[ ]int[ ]rt2x00lib_request_firmware[(]' drivers/net/wireless/rt2x00/rt2x00firmware.c
    accept '[\t][\t]retval[ ]=[ ]rt2x00lib_request_firmware[(]' drivers/net/wireless/rt2x00/rt2x00firmware.c
    accept '[\t][\t]*wl1271_error[(]["]request_firmware_nowait[ ]failed' drivers/net/wireless/ti/wlcore/main.c
    accept '[\t][\t]nfc_err[(][&]drv->pdev->dev[,][ ]["]request_firmware[ ]failed' drivers/nfc/nfcwilink.c
    accept '[\t][\t][\t]["]request_firmware[ ]returned' drivers/nfc/nfcwilink.c
    accept '[\t][\t]dev_err[(][&]rproc->dev[,][ ]["]request_firmware_nowait[ ]err' drivers/remoteproc/remoteproc_core.c
    accept '[\t][\t]dev_err[(]dev[,][ ]["]request_firmware[ ]failed' drivers/remoteproc/remoteproc_core.c
    accept 'static[ ]int[ ]asd_request_firmware[(]' drivers/scsi/aic94xx/aic94xx_seq.c
    accept '[\t]err[ ]=[ ]asd_request_firmware[(]' drivers/scsi/aic94xx/aic94xx_seq.c
    accept '[\t]uint32_t[ ]cfg_request_firmware_upgrade[;]' drivers/scsi/lpfc/lpfc.h
    accept '[ ][*][ ]lpfc_request_firmware_store[ ]-[ ]' drivers/scsi/lpfc/lpfc_attr.c
    accept 'lpfc_request_firmware_upgrade_store[(]' drivers/scsi/lpfc/lpfc_attr.c
    accept 'lpfc_param_show[(]request_firmware_upgrade[)]' drivers/scsi/lpfc/lpfc_attr.c
    accept '[\t]rc[ ]=[ ]lpfc_sli4_request_firmware_update[(]' drivers/scsi/lpfc/lpfc_attr.c
    accept '[ ][*][ ]lpfc_request_firmware_upgrade_init[ ]-[ ]' drivers/scsi/lpfc/lpfc_attr.c
    accept 'lpfc_request_firmware_upgrade_init[(]' drivers/scsi/lpfc/lpfc_attr.c
    accept '[\t][\t]phba->cfg_request_firmware_upgrade[ ]=' drivers/scsi/lpfc/lpfc_attr.c
    accept '[\t][\t][ ]*lpfc_request_firmware_upgrade_\(show\|store\)[,)]' drivers/scsi/lpfc/lpfc_attr.c
    accept '[\t]lpfc_request_firmware_upgrade_init[(]' drivers/scsi/lpfc/lpfc_attr.c
    accept 'int[ ]lpfc_sli4_request_firmware_update[(]' drivers/scsi/lpfc/lpfc_crtn.h
    accept '[ ][*][ ]@fw:[ ]pointer[ ]to[ ]firmware[ ]image[ ]returned[ ]from[ ]request_firmware[.]' drivers/scsi/lpfc/lpfc_init.c
    accept '[ ][*][ ]lpfc_sli4_request_firmware_update[ ]-[ ]' drivers/scsi/lpfc/lpfc_init.c
    accept 'lpfc_sli4_request_firmware_update[(]' drivers/scsi/lpfc/lpfc_init.c
    accept '[\t]if[ ][(]phba->cfg_request_firmware_upgrade[)]' drivers/scsi/lpfc/lpfc_init.c
    accept '[\t][\t]ret[ ]=[ ]lpfc_sli4_request_firmware_update[(]' drivers/scsi/lpfc/lpfc_init.c
    accept '[ ][*][ ]qla1280_request_firmware' drivers/scsi/qla1280.c
    accept 'qla1280_request_firmware[(]' drivers/scsi/qla1280.c
    accept '[\t]fw[ ]=[ ]qla1280_request_firmware[(]' drivers/scsi/qla1280.c
    accept 'extern[ ]struct[ ]fw_blob[ ][*]qla2x00_request_firmware[(]' drivers/scsi/qla2xxx/qla_gbl.h
    accept '[\t]blob[ ]=[ ]qla2x00_request_firmware[(]' drivers/scsi/qla2xxx/qla_init.c
    accept '[\t]blob[ ]=[ ]ha->hablob[ ]=[ ]qla2x00_request_firmware[(]' drivers/scsi/qla2xxx/qla_nx.c
    accept 'qla2x00_request_firmware[(]' drivers/scsi/qla2xxx/qla_os.c
    accept '[\t]-[ ]change[ ]firmware[ ]loading[ ]for[ ]usb[ ]driver[ ]to[ ]proper[ ]kernel[ ]method[ ][(]request_firmware[)]' drivers/staging/ft1000/TODO
    accept '[\t][\t]pr_err[(]["]rtl8723au:[ ]request_firmware[ ]load' drivers/staging/rtl8723au/hal/rtl8723a_hal_init.c
    accept '[\t ]*[*][ ]We[ ]call[ ]request_firmware_nowait[ ]instead[ ]of[ \t\n*]*request_firmware[ ]so[ ]that' drivers/tty/serial/ucc_uart.c
    accept '[\t][\t]dev_err[(][&]dev->dev[,][ ]["]%d[,][ ]request_firmware[ ]failed' sound/pci/asihpi/hpidspcd.c
    accept 'static[ ]int[ ]snd_ymfpci_request_firmware[(]' sound/pci/ymfpci/ymfpci_main.c
    accept '[\t]err[ ]=[ ]snd_ymfpci_request_firmware[(]' sound/pci/ymfpci/ymfpci_main.c
    # New in 3.19
    blobname 'a420_p\(m4\|fp\)\.fw' drivers/gpu/drm/msm/adreno/adreno_device.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]a4xx_registers\[\][ ]=' drivers/gpu/drm/msm/adreno/a4xx_gpu.c
    defsnc 'static[ ]const[ ]u32[ ]gen9_null_state_batch\[\][ ]=' drivers/gpu/drm/i915/intel_renderstate_gen9.c
    defsnc 'nv50_disp_\(core_mthd_head\|base_mthd_base\)[ ]=[ ][{]\([\n][ \t]*\.\(mthd\|addr\)[ ]=[ ]0x00*\([04]0\|54\)0[,]\)*[\n][ \t]*\.data[ ]=' drivers/gpu/drm/nouveau/core/engine/disp/nv50.c
    defsnc 'nv84_disp_\(core_mthd_head\|base_mthd_base\)[ ]=[ ][{]\([\n][ \t]*\.\(mthd\|addr\)[ ]=[ ]0x00*\([04]0\|54\)0[,]\)*[\n][ \t]*\.data[ ]=' drivers/gpu/drm/nouveau/core/engine/disp/nv84.c
    defsnc 'nvd0_disp_\(core_mthd_head\|base_mthd_base\)[ ]=[ ][{]\([\n][ \t]*\.\(mthd\|addr\)[ ]=[ ]0x00*\(300\)\?[,]\)*[\n][ \t]*\.data[ ]=' drivers/gpu/drm/nouveau/core/engine/disp/nvd0.c
    defsnc 'nve0_disp_\(core_mthd_head\|base_mthd_base\)[ ]=[ ][{]\([\n][ \t]*\.\(mthd\|addr\)[ ]=[ ]0x00*300[,]\)*[\n][ \t]*\.data[ ]=' drivers/gpu/drm/nouveau/core/engine/disp/nve0.c
    # This reads from user-supplied filenames.
    accept 'shadow_fw_init[(]struct[ ]nouveau_bios[ ][*]bios[,][ ]const[ ]char[ ][*]name[)][\n][{][\n]\(\([^}\n][^\n]*\)\?[\n]\)*[\t]int[ ]ret[ ]=[ ]request_firmware[(][&]fw[,][ ]name[,][ ]dev[)][;]' drivers/gpu/drm/nouveau/core/subdev/bios/shadow.c
    defsnc 'static[ ]const[ ]u32[ ]coef_lut_\(a_legacy\|b\|[cdef]_[yc]_legacy\)\[NB_COEF\][ ]=' drivers/gpu/drm/sti/sti_hqvdp_lut.h
    blobname 'hqvdp-stih407\.bin' drivers/gpu/drm/sti/sti_hqvdp.c
    defsnc '[\t]static[ ]const[ ]union[ ]sixaxis_output_report_01[ ]default_report[ ]=' drivers/hid/hid-sony.c
    blobname 'elan_i2c\.bin' drivers/input/mouse/elan_i2c_core.c
    blobname 'elants_i2c\.bin' drivers/input/touchscreen/elants_i2c.c
    defsnc '[}][ ]QAM256_mod_tab_zv_mode\[\][ ]=' drivers/media/dvb-frontends/au8522_dig.c
    blobname 'dvb-demod-m88rs6000\.fw' drivers/media/dvb-frontends/m88ds3103_priv.h
    defsnc 'static[ ]const[ ]struct[ ]m88ds3103_reg_val[ ]m88rs6000_dvbs2\?_init_reg_vals\[\][ ]=' drivers/media/dvb-frontends/m88ds3103_priv.h
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]\(luma\|chroma\)_ac_value\[162[ ][+][ ]2\][ ]=' drivers/media/platform/coda/coda-jpeg.c
    defsnc 'static[ ]unsigned[ ]char[ ]\(luma\|chroma\)_q\[64\][ ]=' drivers/media/platform/coda/coda-jpeg.c
    defsnc 'static[ ]const[ ]struct[ ]vin_coeff[ ]vin_coeff_set\[\][ ]=' drivers/media/platform/soc_camera/rcar_vin.c
    defsnc 'const[ ]unsigned[ ]short[ ]tpg_\(rec709_to_linear\|linear_to_rec709\)\[255[ ][*][ ]16[ ][+][ ]1\][ ]=' drivers/media/platform/vivid/vivid-tpg-colors.c
    defsnc '[\t]static[ ]const[ ]struct[ ]m88rs6000t_reg_val[ ]reg_vals\[\][ ]=' drivers/media/tuners/m88rs6000t.c
    blobna '[/][*][ ]cal-<bus>-<id>\.bin[ ][*][/]' drivers/net/wireless/ath/ath10k/core.c
    blobname 'cal-%s-%s\.bin' drivers/net/wireless/ath/ath10k/core.c
    defsnc 'static[ ]const[ ]u32[ ]qca953x_2p0_\(common_wo_xlna_rx\|modes_\(no_\)\?xpa_tx\)_gain_table\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/ar953x_initvals.h
    blobname 'mrvl[/]usb8766_uapsta\.bin' drivers/net/wireless/mwifiex/usb.h
    defsc 'static[ ]const[ ]unsigned[ ]char[ ]opcode_ind_arr\[256\][ ]=' drivers/scsi/scsi_debug.c
    defsnc 'static[ ]const[ ]struct[ ]quark_spi_rate[ ]quark_spi_rate_table\[\][ ]=' drivers/spi/spi-pxa2xx.c
    blobname 'me4000_firmware\.bin' drivers/staging/comedi/drivers/me4000.c
    defsnc '[\t]u8[ ]ConnectionMsg\[\][ ]=' drivers/staging/ft1000/ft1000-usb/ft1000_debug.c
    accept '[\t]pr_info[(]["]load[ ]fpgaimage[ ]%s[\\]n["][,][ ]fw_file[)][;][\n]*[\t]err[ ]=[ ]request_firmware[(][&]fimage->fw_entry[,]' drivers/staging/gs_fpgaboot/gs_fpgaboot.c
    blobname 'dvb-demod-mn88472-02\.fw' drivers/staging/media/mn88472/mn88472_priv.h
    blobname 'dvb-demod-mn88473-01\.fw' drivers/staging/media/mn88473/mn88473_priv.h
    accept '[\t][\t]goto[ ]err_request_firmware[;]' drivers/staging/media/mn88473/mn88473.c
    accept 'err_request_firmware[:]' drivers/staging/media/mn88473/mn88473.c
    blob 'The[ ]card[ ]requires[ ]firmware.*[\n]rm[ ]wd7296a\.sys' Documentation/scsi/wd719x.txt
    blobname 'wd719x-\(wcs\|risc\)\.bin' drivers/scsi/wd719x.c
    defsnc 'static[ ]const[ ]struct[ ]tsadc_table[ ]v2_code_table\[\][ ]=' drivers/thermal/rockchip_thermal.c
    defsnc 'static[ ]const[ ]u8[ ]debug_pk\[64\][ ]=' net/bluetooth/smp.c
    defsnc 'static[ ]const[ ]u8[ ]debug_sk\[32\][ ]=' net/bluetooth/smp.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]ad1980_reg_defaults\[\][ ]=' sound/soc/codecs/ad1980.c
    blobname 'rt5677_dsp_fw[12]\.bin' sound/soc/codecs/rt5677.c
    accept 'int[ ]sst_request_firmware_async[(]' sound/soc/intel/sst/sst.h
    blobname 'intel[/]fw_sst_0f28\.bin-48kHz_i2s_master' sound/soc/intel/sst-acpi.c
    blobname '\(intel[/]\)\?fw_sst_\(0f28\|22a8\)\.bin' sound/soc/intel/sst/sst_acpi.c
    blobname '%s%04x%s["][,][ ]["]fw_sst_["][,][\n][ \t]*sst_drv_ctx->dev_id[,][ ]["]\.bin' sound/soc/intel/sst/sst_pci.c
    accept '[\t]\?\(evsel\|machine\|thread\|comm\(_thread\)\?\|dso\|symbol\|branch_type\|sample\|[\t]call\(_path\)\?\)_file[ \t]*=[ ]open_output_file[(]["]\(evsel\|machine\|thread\|comm\(_thread\)\?\|dso\|symbol\|branch_type\|sample\|call\(_path\)\?\)_table\.bin["][)]' tools/perf/scripts/python/export-to-postgresql.py
    # accept '\([*]\.\(bin\|elf\|fw\)\|\(setup\|wakeup\)\.\(bin\|elf\)\|vmlinux\.bin\.all\|tftpboot\.img\)[\n]' Documentation/dontdiff
    # New in 4.0.
    blobname 'intel[/]ibt-11-%u\.sfi' drivers/bluetooth/btusb.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gf100_gr_init_\(main\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf100.c
    accept '[	][	]*gf100_gr_init_fw[(]priv[,][ ]0x4\(09\|1a\)000[,][ ][&]priv->fuc4\(09\|1a\)c[,][ \n	]*[&]priv->fuc4\(09\|1a\)d[)][;]' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf100.c
    accept '[	][	 ]*gf100_gr_dtor_fw[(]&priv->fuc4\(09\|1a\)[cd][)][;]' drivers/gpu/drm/nouveua/nvkm/engine/gr/gf100.c
    accept '[	][	 ]*\(if[ ][(]\|[ ][ ][ ][ ]\)gf100_gr_ctor_fw[(]priv[,][ ]["]fuc4\(09\|1a\)[cd]["][,][ ][&]priv->fuc4\(09\|1a\)[cd][)]' drivers/gpu/drm/nouveua/nvkm/engine/gr/gf100.c
    blobname 'firmware-4\.bin' drivers/net/wireless/ath/ath10k/hw.h
    blobname 'brcm[/]brcmfmac43340-sdio\.bin' drivers/net/wireless/brcm80211/brcmfmac/dhd_sdio.c
    blobname 'iwlwifi-7260-' drivers/net/wireless/iwlwifi/pcie/7000.c
    blobname 'iwlwifi-8000' drivers/net/wireless/intel/iwlwifi/iwl-8000.c
    blobname 'iwl_nvm_8000B\.bin' drivers/net/wireless/iwlwifi/iwl-8000.c
    blobname 'mrvl[/]sd8801_uapsta\.bin' drivers/net/wireless/mwifiex/sdio.h
    blobname 'mrvl[/]usb8801_uapsta\.bin' drivers/net/wireless/mwifiex/usb.h
    blobname 'ti-connectivity[/]wl18xx-fw-4\.bin' drivers/net/wireless/ti/wl18xx/main.c
    blobname 'intel[/]fw_sst_22a8\.bin' sound/soc/intel/sst_acpi.c
    defsnc 'static[ ]const[ ]struct[ ]clk_div_table[ ]z_div_table\[\][ ]=' drivers/clk/shmobile/clk-sh73a0.c
    defsnc 'uint32_t[ ]gf100_pce_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/ce/fuc/gf100.fuc3.h
    defsnc 'uint32_t[ ]gt215_pce_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/ce/fuc/gt215.fuc3.h
    defsnc '\(static[ ]\)\?const[ ]struct[ ]nv50_disp_mthd_list[\n]g84_disp_\(base\|core\|ovly\)_mthd_\(dac\|head\|base\)[ ]=' drivers/gpu/drm/nouveau/nvkm/engine/disp/g84.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]nv50_disp_mthd_list[\n]gf110_disp_\(base\|core\|ovly\)_mthd_\(dac\|head\|base\|sor\|pior\)[ ]=' drivers/gpu/drm/nouveau/nvkm/engine/disp/gf110.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]nv50_disp_mthd_list[\n]gk104_disp_\(core\|ovly\)_mthd_\(head\|base\)[ ]=' drivers/gpu/drm/nouveau/nvkm/engine/disp/gk104.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]nv50_disp_mthd_list[\n]gt200_disp_ovly_mthd_base[ ]=' drivers/gpu/drm/nouveau/nvkm/engine/disp/gt200.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gf100_grctx_init_\(icmd\|9097\|902d\|90c0\|fe\|memfmt\|rstr2d\|prop\|setup\|crstr\|zcullr\|wwdx\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/ctxgf100.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gf104_grctx_init_\(tex\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/ctxgf104.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gf108_grctx_init_\(icmd\|9097\|setup\|wwdx\|tex\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/ctxgf108.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gf110_grctx_init_\(icmd\|setup\)_0\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/ctxgf110.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gf117_grctx_init_\(ds\|pd\|setup\|tex\|wwdx\)_0\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/ctxgf117.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gf119_grctx_init_\(\(icmd\|90c0\|fe\|ds\|prop\|setup\|crstr\|tex\|sm\)_0\|gpc_unk_1\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/ctxgf119.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gk104_grctx_init_\(icmd\|a097\|fe\|memfmt\|ds\|pd\|be\|setup\|tex\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/ctxgk104.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gk110_grctx_init_\(icmd\|a197\|fe\|pd\|be\|setup\|tex\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/ctxgk110.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gk208_grctx_init_\(icmd\|fe\|ds\|pd\|rstr2d\|be\|prop\|setup\|crstr\|tex\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/ctxgk208.c
    defsnc 'uint32_t[ ]gf100_grgpc_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/gpcgf100.fuc3.h
    defsnc 'uint32_t[ ]gf117_grgpc_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/gpcgf117.fuc3.h
    defsnc 'uint32_t[ ]gk104_grgpc_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/gpcgk104.fuc3.h
    defsnc 'uint32_t[ ]gk110_grgpc_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/gpcgk110.fuc3.h
    defsnc 'uint32_t[ ]gk208_grgpc_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/gpcgk208.fuc5.h
    defsnc 'uint32_t[ ]gf100_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/hubgf100.fuc3.h
    defsnc 'uint32_t[ ]gf117_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/hubgf117.fuc3.h
    defsnc 'uint32_t[ ]gk104_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/hubgk104.fuc3.h
    defsnc 'uint32_t[ ]gk110_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/hubgk110.fuc3.h
    defsnc 'uint32_t[ ]gk208_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/hubgk208.fuc5.h
    accept '[	]struct[ ]gf100_gr_fuc[ ]fuc4\(09\|1a\)[cd]' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf100.h
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gf104_gr_init_\(ds\|tex\|pe\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf104.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gf110_gr_init_sm_0\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf110.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gf119_gr_init_\(\(pd\|ds\|prop\|gpm\|tex\|pe\|wwdx\|sm\)_0\|\(tpccs\|gpc_unk\|fe\)_1\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf119.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gk104_gr_init_\(\(main\|ds\|sked\|cwd\|tpccs\|pe\|l1c\|sm\|be\)_0\|gpc_unk_1\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/gk104.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gk110_gr_init_\(\(fe\|ds\|sked\|cwd\|tex\|l1c\|sm\)_0\|gpc_unk_1\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/gk110.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gk110b_gr_init_\(l1c\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/gk110b.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gk208_gr_init_\(\(main\|ds\|gpc_unk\|tex\|l1c\)_0\|setup_1\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/gk208.c
    defsnc '\(static[ ]\)\?const[ ]struct[ ]gf100_gr_init[\n ]gm107_gr_init_\(\(main\|ds\|scc\|sked\|prop\|zcull\|tpccs\|tex\|pe\|l1c\|sm\|pes\|wwdx\|cbm\|be\)_0\|\(setup\|gpc_unk\|l1c\|sm\)_1\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/gm107.c
    defsnc 'static[ ]u32[ \n]nv04_gr_ctx_regs\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nv04.c
    defsnc 'static[ ]int[ \n]nv10_gr_ctx_regs\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/nv10.c
    defsnc 'uint32_t[ ]g98_psec_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/sec/fuc/g98.fuc0s.h
    accept 'shadow_fw_init[(]struct[ ]nvkm_bios[ ][*]bios[,][ ]const[ ]char[ ][*]name[)][\n][{][\n]\(\([^}\n][^\n]*\)\?[\n]\)*[\t]int[ ]ret[ ]=[ ]request_firmware[(][&]fw[,][ ]name[,][ ]dev[)][;]' drivers/gpu/drm/nouveau/nvkm/subdev/bios/shadow.c
    defsnc 'uint32_t[ ]gf100_pmu_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/subdev/pmu/fuc/gf100.fuc3.h
    defsnc 'uint32_t[ ]gf110_pmu_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/subdev/pmu/fuc/gf110.fuc4.h
    defsnc 'uint32_t[ ]gk208_pmu_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/subdev/pmu/fuc/gk208.fuc5.h
    defsnc 'uint32_t[ ]gt215_pmu_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/subdev/pmu/fuc/gt215.fuc3.h
    defsnc 'static[ ]const[ ]struct[ ]dw_hdmi_mpll_config[ ]rockchip_mpll_cfg\[\][ ]=' drivers/gpu/drm/rockchip/dw_hdmi-rockchip.c
    defsnc '[}][ ]kmx61_\(samp_freq\|wake_up_odr\)_table\[\][ ]=' drivers/iio/imu/kmx61.c
    defsnc 'static[ ]const[ ]u8[ ]jpeg_header\[\][ ]=' drivers/staging/media/solo6x10/solo6x10-jpeg.h
    defsnc 'static[ ]const[ ]u8[ ]jpeg_dqt\[4\]\[DQT_LEN\][ ]=' drivers/media/pci/solo6x10/solo6x10-jpeg.h
    defsnc 'static[ ]u8[ ]vop_6010_\(ntsc\|pal\)_\(d1\|cif\)\[\][ ]=' drivers/staging/media/solo6x10/solo6x10-v4l2-enc.c
    defsnc '[\t]static[ ]const[ ]struct[ ]rate_s[ ]rate_1\[\][ ]=' drivers/media/usb/gspca/ov534.c
    defsnc 'static[ ]struct[ ]serdes_cfg[ ]cfg_phyb_10p3125g_\(156p25mhz_cmu1\|16bit_lane\|comlane\)\[\][ ]=' drivers/net/ethernet/ti/netcp_xgbepcsr.c
    defsnc 'static[ ]const[ ]u32[ ]qca956x_1p0_\(baseband\|radio\)_core\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/ar956x_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]qca956x_1p0_\(baseband\|radio\)_postamble\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar956x_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]qca956x_1p0_modes_\(no_\)\?xpa_\(low_ob_db_\|green_\)\?tx_gain_table\[\]\[3\][ ]=' drivers/net/wireless/ath/ath9k/ar956x_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]qca956x_1p0_common_rx_gain_table\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/ar956x_initvals.h
    defsnc 'static[ ]const[ ]u32[ ]qca956x_1p0_xlna_only\[\]\[5\][ ]=' drivers/net/wireless/ath/ath9k/ar956x_initvals.h
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]smc0_nor_pins\[\][ ]=' drivers/pinctrl/pinctrl-zynq.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]gamma_correction_table\[\][ ]=' drivers/staging/fbtft/fb_agm1264k-fl.c
    defsnc '[\t]write_reg[(]par[,][ ]0x2D[,]' drivers/staging/fbtft/fb_hx8353d.c
    defsnc '[#]define[ ]DEFAULT_GAMMA' 'drivers/staging/fbtft/fb_ssd13[35]1\.c'
    defsnc 'static[ ]struct[ ]fbtft_device_display[ ]displays\[\][ ]=' drivers/staging/fbtft/fbtft_device.c
    defsnc 'struct[ ]ModeInit[ ]vgamode\[\][ ]=' drivers/staging/sm7xxfb/sm7xx.h
    defsnc 'static[ ]const[ ]u8[ ]\(\(priv\|pub\)_[ab]\|dhkey\)_[123]\[\(32\|64\)\][ ]__initconst[ ]=' net/bluetooth/selftest.c
    defsnc '[\t]const[ ]u8[ ][uvw]\[32\][ ]=' net/bluetooth/smp.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm8995_reg_defaults\[\][ ]=' sound/soc/codecs/wm8995.c

    # CYAPA_FW_NAME, defined to this string, is not used anywhere, and
    # firmware requests are issued with user-supplied names.  So,
    # deblob the unused name, but keep the request active.
    blobname 'cyapa\.bin' drivers/input/mouse/cyapa.c
    accept 'static[ ]int[ ]cyapa_firmware[(]struct[ ]cyapa[ ][*]cyapa[,][ ]const[ ]char[ ][*]fw_name[)][\n][{][\n]\(\([^}\n][^\n]*\)\?[\n]\)*[\t]error[ ]=[ ]request_firmware[(][&]fw[,][ ]fw_name[,][ ]dev[)][;]' drivers/input/mouse/cyapa.c

    # There are blob names here, but no apparent load mechanism.
    blobname 'ssp_B2\.fw' drivers/iio/common/ssp_sensors/ssp_dev.c
    blobname 'ssp_crashed\.fw' drivers/iio/common/ssp_sensors/ssp_dev.c
    blobname 'thermostat_B2\.fw' drivers/iio/common/ssp_sensors/ssp_dev.c

    # New in 4.1.
    defsnc 'uint8_t[ ]default_tx\[\][ ]=' Documentation/spi/spidev_test.c
    accept '[#][ ]cat[ ][/]sys[/]kernel[/]debug[/]zsmalloc[/]zram0[/]classes[\n][\n][ ]class[^\n]*\([\n][ ][0-9. \t]*\)*' Documentation/vm/zsmalloc.txt
    accept '[\t]*nvidia[,]emc-configuration[ ]=[ ][<][\n][\t]*\(0x[0-9a-f]*[\n][\t]*\)*[>][;]' 'arch/arm/boot/dts/tegra124-\(jetson-tk1\|nyan-\(big\|blaze\)\)-emc.dtsi'
    initnc '\.Lsha256_rcon:[\n][\t]\.word[\t]*' arch/arm64/crypto/sha2-ce-core.S
    accept 'K256:[\n]\.word[\t]0x428a2f98[,][0-9a-f0x,]*\([\n]\.word[\t][0-9a-f0x,]*\)*' 'arch/arm/crypto/sha256-\(armv4\.pl\|core\.S_shipped\)'
    initnc 'PPC_AES_4K_DECTAB2:[\n][/][*][ ]decryption[ ]table[,][ ]same[ ]as[ ]crypto_il_tab[ ]in[ ]crypto[/]aes-generic\.c[ ][*][/]' arch/powerpc/crypto/aes-tab-4k.S
    initnc 'PPC_SPE_SHA256_K:' arch/powerpc/crypto/sha256-spe-asm.S
    defsnc 'static[ ]const[ ]u8[ ]initial_parm_block\[32\][ ]__initconst[ ]=' arch/s390/crypto/prng.c
    defsnc '[\t]static[ ]const[ ]u8[ ]\(seed\|[VC]0\|random\)\[\][ ]__initconst[ ]=' arch/s390/crypto/prng.c
    defsnc 'gm204_grctx_init_\(icmd\|b197\|fe\|ds\|pd\|be\|prop\|setup\|tex\|mpc\|sm\)_0\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/ctxgm204.c
    defsnc 'gm204_gr_init_\(main\|tpccs\|pe\|sm\|be\)_0\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/ctxgm204.c
    defsnc 'static[ ][ ]*\(const[ ]\)\?struct[ ]sensor_register[ ]ov2659_\(init_regs\|[us]\?xga\|[sq]\?vga\)\[\][ ]=' drivers/media/i2c/ov2659.c
    defsnc 'static[ ]const[ ]struct[ ]pll_ctrl_reg[ ]ctrl1\[\][ ]=' drivers/media/i2c/ov2659.c
    defsnc 'static[ ]const[ ]u16[ ]aic_lin_table\[ATH_AIC_MAX_AIC_LIN_TABLE\][ ]=' drivers/net/wireless/ath/ath9k/ar9003_aic.c
    defsc 'static[ ]struct[ ]ModeInit[ ]vgamode\[\][ ]=' drivers/staging/sm7xxfb/sm7xx.h
    defsnc 'static[ ]const[ ]s32[ ]sin_table\[\][ ]=' include/linux/fixp-arith.h
    defsnc 'static[ ]int64_t[ ]__RH_LH_tbl\[128[*]2[+]2\][ ]=' net/ceph/crush/crush_ln_table.h
    defsnc 'static[ ]int64_t[ ]__LL_tbl\[256\][ ]=' net/ceph/crush/crush_ln_table.h
    blobname 'rtl_bt[/]rtl8723[ab]_fw\.bin' drivers/bluetooth/btusb.c
    blobname 'rtl_bt[/]rtl8821a_fw\.bin' drivers/bluetooth/btusb.c
    blobname 'rtl_bt[/]rtl8761a_fw\.bin' drivers/bluetooth/btusb.c
    blobname 'brcm[/]\(%s\(-%4\.4x-%4\.4x\)\?[^ "\n]*\)\.hcd' drivers/bluetooth/btbcm.c
    blobname 'cxgb4[/]aq1202_fw\.cld' drivers/net/ethernet/chelsio/cxgb4/cxgb4_main.c
    accept 'static[ ]int[ ]set_flash[(]struct[ ]net_device[ ][*]netdev[,][ ]struct[ ]ethtool_flash[ ][*]ef[)][\n][{]\([\n]\+[^\n}][^\n]*\)*ret[ ]=[ ]request_firmware[(][&]fw[,][ ]ef->data[,][ ]adap->pdev_dev[)][;]\([\n]\+[^\n}][^\n]*\)*[\n]\+[}][\n]' drivers/net/ethernet/chelsio/cxgb4/cxgb4_ethtool.c
    blobname 'brcm[/]\(%s\|.*\)-\(%04x\|[0-9a-f]*\)-\(%04x\|[0-9a-f]*\)\.hcd' drivers/bluetooth/btusb.c
    blobname 'qca[/]\(rampatch\|nv\(ra\)\?m\)_usb_\(%08x\|[0-9a-f]*\)\.bin' drivers/bluetooth/btusb.c
    blobname 'elants_i2c_\(%04x\|[0-9a-f]*\)\.bin' drivers/input/touchscreen/elants_i2c.c
    blobname 'ct2\?fw-3\.2\.5\.1\.bin' drivers/net/ethernet/brocade/bna/cna.h
    blobname 'brcm[/]brcmfmac43\(4\(30\|55\)\|54\)-sdio\.bin' drivers/net/wireless/brcm80211/brcmfmac/sdio.c
    blobname 'iwlwifi-7265D-' drivers/net/wireless/iwlwifi/iwl-7000.c
    blobname '%s%c-%s\.ucode' drivers/net/wireless/iwlwifi/iwl-drv.c
    blobname 'intel[/]IntcPP01\.bin' sound/soc/intel/haswell/sst-haswell-ipc.c
    accept '[\t]*rc[ ]=[ ]wil_request_firmware[(]wil[,][ ]WIL_FW2\?_NAME[)][;]' drivers/net/wireless/ath/wil6210/main.c
    blobname 'nvmData-8000[BC]' drivers/net/wireless/iwlwifi/iwl-8000.c

    # New in 4.2.
    accept '[\t	]*interrupts[ ]=[ ]<\([ \n\t]*0x0[ ]0x1[0-9a-f][ ]0x4\)*>[;]' Documentation/devicetree/bindings/remoteproc/wkup_m3_rproc.txt
    accept '[\t]*bool[ ]["]vmlinu[xz]\.bin["]' arch/mips/Kconfig
    defsnc 'static[ ]struct[ ]hash_testvec[ ]\(ghash\|poly1305\|crc32\)_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]struct[ ]aead_testvec[ ]rfc7539\(esp\)\?_\(enc\|dec\)_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]struct[ ]cipher_testvec[ ]chacha20_enc_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]const[ ]struct[ ]iproc_pll_vco_param[ ]mipipll_vco_params\[\][ ]=' drivers/clk/bcm/clk-cygnus.c
    defsnc 'static[ ]const[ ]struct[ ]clk_div_table[ ]ahb_div_table\[\][ ]=' drivers/clk/clk-stm32f4.c
    defsnc '[\t]static[ ]u8[ ]padded_hash\[64\][ ]=' drivers/crypto/talitos.c
    defsnc 'static[ ]const[ ]int[ ]stk3310_it_table\[\]\[2\][ ]=' drivers/iio/light/stk3310.c
    defsnc 'static[ ]const[ ]u8[ ]drv2665_sine_wave_form\[\][ ]=' drivers/input/misc/drv2665.c
    defsnc 'static[ ]const[ ]char[ ]ipr_bit\[\][ ]=' drivers/irqchip/irq-renesas-h8300h.c
    defsnc 'static[ ]const[ ]struct[ ]multiplier[ ]multipliers\[\][ ]=' drivers/media/pci/cobalt/cobalt-cpld.c
    defsnc 'static[ ]u8[ ]edid\[256\][ ]=' drivers/media/pci/cobalt/cobalt-driver.c
    defsnc 'static[ ]const[ ]struct[ ]bdisp_filter_[hv]_spec[ ]bdisp_[hv]_spec\[\][ ]=' drivers/media/platform/sti/bdisp/bdisp-filter.h
    defsnc '[\t]struct[ ]init_command[ ]genius_vcam_live_start_commands\[\][ ]=' drivers/media/usb/gspca/sn9c2028.c
    defsnc '[\t]static[ ]const[ ]unsigned[ ]int[ ]t6_reg_ranges\[\][ ]=' drivers/net/ethernet/chelsio/cxgb4/t4_hw.c
    defsnc 'static[ ]const[ ]struct[ ]mt76_reg_pair[ ]bbp_\(common\|chip\)_vals\[\][ ]=' drivers/net/wireless/mediatek/mt7601u/initvals.h
    defsnc '[\t]static[ ]const[ ]u8[ ]freq_plan\[14\]\[FREQ_PLAN_REGS\][ ]=' drivers/net/wireless/mediatek/mt7601u/phy.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]\(lcd_vip_gpio\|visbus_dout\)_pins\[\][ ]=' drivers/pinctrl/sirf/pinctrl-atlas7.c
    defsnc 'static[ ]const[ ]u32[ ]bq24257_vbat_map\[\][ ]=' drivers/power/bq24257_charger.c
    defsnc 'static[ ]const[ ]int[ ]rt9455_\(voreg\|boost_voltage\)_values\[\][ ]=' drivers/power/rt9455_charger.c
    defsnc '[\t]write_reg[(]par[,][ ]HX8357D_SETGAMMA[,][\n][\t][\t]' drivers/staging/fbtft/fb_hx8357d.c
    defsnc '[}][ ]isl29018_scales\[4\]\[4\][ ]=' drivers/staging/iio/light/isl29018.c
    defsnc 'const[ ]u32[ ]dm_tx_bb_gain\[TxBBGainTableLength\][ ]=' drivers/staging/rtl8192e/rtl8192e/rtl_dm.c
    defsnc 'const[ ]u8[ ]dm_cck_tx_bb_gain\(_ch14\)\?\[CCKTxBBGainTableLength\]\[8\][ ]=' drivers/staging/rtl8192e/rtl8192e/rtl_dm.c
    defsnc 'static[ ]const[ ]struct[ ]vesa_mode[ ]vesa_mode_table\[\][ ]=' drivers/staging/sm7xxfb/sm7xxfb.c
    defsnc 'static[ ]const[ ]struct[ ]modeinit[ ]vgamode\[\][ ]=' drivers/staging/sm7xxfb/sm7xxfb.c
    defsnc 'static[ ]const[ ]uint8_t[ ]crc7_syndrome_table\[256\][ ]=' drivers/staging/wilc1000/wilc_spi.c
    defsnc 'static[ ]__s64[ ]__RH_LH_tbl\[128[*]2[+]2\][ ]=' net/ceph/crush/crush_ln_table.h
    defsnc 'static[ ]__s64[ ]__LL_tbl\[256\][ ]=' net/ceph/crush/crush_ln_table.h
    defsnc 'static[ ]const[ ]u8[ ]vol_quot_table\[\][ ]=' sound/soc/codecs/sgtl5000.c
    blobname 'radeon[/]TAHITI_vce\.bin' drivers/gpu/drm/radeon/radeon_vce.c
    blobname 'elan_i2c_["][ ]ETP_PRODUCT_ID_FORMAT_STRING[ ]["]\.bin' drivers/input/mouse/elan_i2c.h
    # Is this too broad?
    blobname '%s%s%s_%s%s' drivers/net/ethernet/cavium/liquidio/libquidio_main.c
    accept '#define[ ]LIO_FW_NAME_SUFFIX[\t ]*["]\.bin["]' drivers/net/ethernet/cavium/liquidio/liquidio_image.h
    blobname 'cxgb4[/]\(t6fw\|bcm8483\)\.bin' drivers/net/ethernet/chelsio/cxgb4/cxgb4_main.c
    blobname 'board-%s-%s\.bin' drivers/net/wireless/ath/ath10k/core.c
    accept '[\t][/][*][ ]Don.t[ ]trust[ ]error[ ]code[ ]from[ ]otp\.bin[ ][*][/]' drivers/net/wireless/ath/ath10k/core.h
    blobname 'firmware-5\.bin' drivers/net/wireless/ath/ath10k/hw.h
    blobname 'brcm[/]brcmfmac4358-pcie\.bin' drivers/net/wireless/brcm80211/brcmfmacpcie.c
    blobname 'brcm[/]brcmfmac43241b5-sdio\.bin' drivers/net/wireless/brcm80211/brcmfmac/sdio.c
    # http://arago-project.org/git/projects/?p=am33x-cm3.git contains
    # source code and the Texas Instruments, Inc Software License
    # Agreeent even looks like a Free Software license, but there are
    # provisions about trade secrets that might be contained in blobs
    # therein.  Furthermore, the license hasn't been reviewed by the
    # FSF.  So let's keep on assuming it's non-Free, until we get a
    # definitive answer.
    blobname 'am335x-pm-firmware\.elf' Documentation/devicetree/bindings/remoteproc/wkup_m3_rproc.txt
    blobname 'rtl_bt[/]rtl\(8723[ab]\|8821a\|8761a\)_fw\.bin' drivers/bluetooth/btrtl.c
    blobname 'radeon[/]\(bonaire\|kabini\|kaveri\|hawaii\|mullins\)_uvd\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_uvd.c
    blobname 'amdgpu[/]\(tonga\|carrizo\)_uvd\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_uvd.c
    blobname 'radeon[/]\(bonaire\|kabini\|kaveri\|hawaii\|mullins\)_vce\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vce.c
    blobname 'amdgpu[/]\(tonga\|carrizo\)_vce\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vce.c
    blobname 'radeon[/]\(bonaire\|hawaii\|%s\)_smc\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_dpm.c
    blobname 'radeon[/]\(bonaire\|kabini\|kaveri\|hawaii\|mullins\|%s\)_sdma1\?\.bin' drivers/gpu/drm/amd/amdgpu/cik_sdma.c
    accept '[\t][/][*][ ]request_firmware[ ][*][/]' drivers/gpu/drm/amd/amdgpu/amdgpu_ucode.h
    blobname 'amdgpu[/]\(bonaire\|kabini\|kaveri\|hawaii\|mullins\|%s\)_\(pfp\|me\|ce\|rlc\|mec2\?\|mc\)\.bin' drivers/gpu/drm/amd/amdgpu/gfx_v7_0.c
    blobname 'amdgpu[/]\(tonga\|topaz\|%s\)_mc\.bin' drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c
    blobname 'amdgpu[/]topaz_smc\.bin' drivers/gpu/drm/amd/amdgpu/iceland_dpm.c
    blobname 'amdgpu[/]\(topaz\|%s\)_sdma1\?\.bin' drivers/gpu/drm/amd/amdgpu/sdma_v2_4.c
    blobname 'amdgpu[/]\(tonga\|carrizo\|%s\)_sdma1\?\.bin' drivers/gpu/drm/amd/amdgpu/sdma_v3_0.c
    blobname 'amdgpu[/]tonga_smc\.bin' drivers/gpu/drm/amd/amdgpu/tonga_dpm.c
    blobname 'i915[/]skl_dmc_ver1\.bin' drivers/gpu/drm/i915/intel_csr.c
    blobname 'wdt87xx_\(fw\|cfg\)\.bin' drivers/input/touchscreen/wdt87xx_i2c.c
    blobname 'dvb-fe-cx24120-1\.20\.58\.2\.fw' drivers/media/dvb-frontends/cx24120.c
    # FIXME: LIO_... drivers/net/ethernet/cavium/liquidio/lio_main.c
    blobname 'mt7601u\.bin' drivers/net/wireless/media/tek/mt7601u/usb.h
    accept '[\t ]*["]request_firmware_nowait[ ]error' drivers/net/wireless/mwifiex/main.c
    blobname 'atmel[/]wilc1000\(_ap\|_p2p\)\?_fw\.bin' drivers/staging/wilc1000/Makefile
    blobname 'wifi_firmware\(_ap\|_p2p_concurrency\)\?\.bin' drivers/staging/wilc1000/linux_wlan.c
    blob 'This[ ]directory[ ]is[ ]_NOT_[ ]for[ ]adding[ ]arbitrary[ ]new[ ]firmware[ ]images.*git[ ]pull[ ]request[ ]to:[\n][^\n]*linux-firmware@kernel\.org[\n][^\n]*mailing[ ]lists\.' firmware/README.AddingFirmware

    # New in 4.2.1 and 4.1.8.
    defsnc '[}][ ]common_modes\[\][ ]=' drivers/gpu/drm/qxl/qxl_display.c

    # New in 4.3.
    accept '[\t]*operating-points[ ]=[ ]<[\n\t 0-9]*>[;]' arch/arm/boot/dts/exynos5250.dtsi
    defsnc 'static[ ]struct[ ]aead_testvec[ ]aes_ccm_rfc4309_\(enc\|dec\)_tv_template\[\][ \t]=' crypt/testmgr.h
    defsnc 'static[ ]const[ ]u8[ ]const_tab\[1024\][ ]=' drivers/crypt/qat/qat_common/adf_admin.c
    defsnc '[\t]static[ ]const[ ]int[ ]even_dividers\[\][ ]=' drivers/gpu/drm/i915/intel_ddi.c
    defsnc 'static[ ]const[ ]struct[ ]bxt_clk_div[ ]bxt_dp_clk_val\[\][ ]=' drivers/gpu/drm/i915/intel_ddi.c
    defsnc 'uint32_t[ ]gf100_ce_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/ce/fuc/gf100.fuc3.h
    defsnc 'uint32_t[ ]gt215_ce_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/ce/fuc/gf215.fuc3.h
    defsnc 'gf119_disp_\(base\|core\|ovly\)_mthd_\(base\|head\)[ ]=' drivers/gpu/drm/nouveau/nvkm/engine/disp/basegf119.c
    defsnc 'uint32_t[ ]g98_sec_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/ce/fuc/gf98.fuc0s.h
    defsnc 'uint32_t[ ]gf119_pmu_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/ce/fuc/gf119.fuc4.h
    defsnc '[\t]static[ ]const[ ]u16[ ]\(display_mode\|gamma\)_settings\[\][ ]=' drivers/gpu/drm/panel/panel-lg-lg4573.c
    defsnc 'static[ ]const[ ]struct[ ]cxd2841er_cnr_data[ ]s2\?_cn_data\[\][ ]=' drivers/media/dvb-frontends/cxd2841er.c
    defsnc 'static[ ]const[ ]struct[ ]dvb_pll_desc[ ]dvb_pll_\(unknown_1\|opera1\|samsung_dtos403ih102a\)[ ]=' drivers/media/dvb-frontends/dvb-pll.c
    defsnc 'static[ ]const[ ]u8[ ]zigzag\[\][ ]=' drivers/media/platform/rcar_jpu.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]qtbl_\(lum\|chr\)\[JPU_MAX_QUALITY\]\[QTBL_SIZE\][ ]=' drivers/media/platform/rcar_jpu.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]hactbl_\(lum\|chr\)\[HACTBL_SIZE\][ ]=' drivers/media/platform/rcar_jpu.c
    defsnc 'static[ ]const[ ]struct[ ]reg_sequence[ ]wm5102_rev[ab]_patch\[\][ ]=' drivers/mfd/wm5102-tables.c
    defsnc 'static[ ]const[ ]struct[ ]reg_sequence[ ]wm5110_rev[abd]_patch\[\][ ]=' drivers/mfd/wm5110-tables.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm8998_rev_a_patch\[\][ ]=' drivers/mfd/wm8998-tables.c
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]hwecc4_4096[ ]=' drivers/mtd/nand/davinci_nand.c
    defsnc 'static[ ]const[ ]unsigned[ ]adinter_\(pins\|muxvals\)\[\][ ]=' drivers/pinctrl/uniphier/pinctrl-ph1-ld6b.c
    defsnc '[\t]write_csr[(]dd[,][ ]DCC_CFG_SC_VL_TABLE_\(15_0\|31_16\)' drivers/staging/rdma/hfi1/chip.c
    defsnc '\(static[ ]\)\?const[ ]u8[ ]pcie_\(serdes\|pcs\)_addrs\[2\]\[NUM_PCIE_SERDES\][ ]=' drivers/staging/rdma/hfi1/firmware.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]ak4643_reg\[\][ ]=' sound/soc/codecs/ak4642.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]da7210_reg_defaults\[\][ ]=' sound/soc/codecs/da7210.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]da9055_reg_defaults\[\][ ]=' sound/soc/codecs/da9055.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]isabelle_reg_defs\[\][ ]=' sound/soc/codecs/isabelle.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]lm49453_reg_defs\[\][ ]=' sound/soc/codecs/lm49453.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt286_index_def\[\][ ]=' sound/soc/codecs/rt286.c
    defsnc 'static[ ]\(const[ ]\)\?struct[ ]reg_default[ ]rt298_\(index_def\|reg\)\[\][ ]=' sound/soc/codecs/rt298.c
    defsnc 'static[ ]const[ ]struct[ ]reg_sequence[ ]wm2200_reva_patch\[\][ ]=' sound/soc/codecs/wm2200.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm5110_sysclk_reve_patch\[\][ ]=' sound/soc/codecs/wm5110.c
    blobname 'qat_mmp\.bin' drivers/crypto/qat/qat_dh895xcc/adf_dh895xcc_hw_data.h
    blobname 'amdgpu[/]fiji_uvd\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_uvd.c
    blobname 'amdgpu[/]fiji_vce\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vce.c
    blobname 'amdgpu[/]fiji_\(ce\|pfp\|me\(c2\?\)\?\|rlc\)\.bin' drivers/gpu/drm/amd/amdgpu/gfx_v8_0.c
    blobname 'amdgpu[/]fiji_mc\.bin' drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c
    blobname 'amdgpu[/]fiji_sdma1\?\.bin' drivers/gpu/drm/amd/amdgpu/sdma_v3_0.c
    accept '[	][	]*gf100_gr_init_fw[(]gr[,][ ]0x4\(09\|1a\)000[,][ ][&]gr->fuc4\(09\|1a\)c[,][ \n	]*[&]gr->fuc4\(09\|1a\)d[)][;]' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf100.c
    accept '[	][	 ]*gf100_gr_dtor_fw[(]&gr->fuc4\(09\|1a\)[cd][)][;]' drivers/gpu/drm/nouveua/nvkm/engine/gr/gf100.c
    accept '[	][	 ]*\(if[ ][(]\|[ ][ ][ ][ ]\)gf100_gr_ctor_fw[(]gr[,][ ]["]\(fecs\|gpccs\)_\(inst\|data\)["][,][ ][&]gr->fuc4\(09\|1a\)[cd][)]' drivers/gpu/drm/nouveua/nvkm/engine/gr/gf100.c
    blobname 'nvidia[/]%s[/]%s\.bin' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf100.c
    accept '[\t]gr->firmware[ ]=[ ]nvkm_boolopt' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf100.c
    blobname 'mrvl[/]pcie8997_uapsta\.bin' drivers/net/wireless/mwifiex/pcie.h
    accept 'static[ ]const[ ]struct[ ]mwifiex_pcie_device[ ]mwifiex_pcie8997[ ]=[ ][{][\n][	]\.firmware[ 	]*=' drivers/net/wireless/mwifiex/pcie.h
    blobname 'mrvl[/]sd8997_uapsta\.bin' drivers/net/wireless/mwifiex/sdio.h
    blobname 'mrvl[/]usb8997_uapsta\.bin' drivers/net/wireless/mwifiex/usb.h
    blobname 'intel[/]ibt-11-5\.\(sfi\|ddc\)' drivers/bluetooth/btintel.c
    blobname 'qca[/]\(rampatch\|nvm\)_%08x\.bin' drivers/bluetooth/btqca.c
    blobname 'intel[/]ibt-11-%u\.sfi' drivers/bluetooth/hci_intel.c
    blobname 'amdgpu[/]fiji_smc\.bin' drivers/gpu/drm/adm/amdgpu/fiji_dpm.c
    blobname 'pti_memdma_h407\.elf' drivers/media/platform/sti/c8sectpfe/c8sectpfe-core.c
    blobname 'sec_s3fwrn5_\(firmware\|rfreg\)\.bin' drivers/nfc/s3fwrn5/core.c
    blobname 'hfi_dc8051\.bin' drivers/staging/rdma/hfi1/firmware.c
    blobname 'hfi1_\(dc8051\|fabric\|sbus\|pcie\)\.fw' drivers/staging/rdma/hfi1/firmware.c
    blobname 'hfi1_platform\.dat' drivers/staging/rdma/hfi1/firmware.c
    blobname 'dsp_fw_release\.bin' sound/soc/intel/skylake/skl-sst.c
    accept '[\t]*dev_err[(]fei->dev[,][ ]["]request_firmware_nowait[ ]err:' drivers/media/platform/sti/c8sectpfe/c8sectpfe-core.c
    accept 'static[ ]int[ ]s3fwrn5_fw_request_firmware[(]struct[ ]s3fwrn5_fw_info' drivers/nfc/s3fwrn5/firmware.c
    accept '[\t]ret[ ]=[ ]s3fwrn5_fw_request_firmware[(]fw_info[)][;]' drivers/nfc/s3fwrn5/firmware.c

    # New in 4.4.
    blobna 'More[ ]description[ ]on[ ]the[ ]firmware.*make[ ]sure[ ]to[ ]copy[ ]firmware[\n]to[ ]file[ ]system[ ]before[ ]using[ ]these[ ]queue[ ]types[.]' Documentation/arm/keystone/knav-qmss.txt
    accept '[\t	]*interrupts[ ]=[ ]<\([\n\t ]*\([0-9xa-f]*\|[/]\([*]\+[^*/][^*]*\)\+[*]\+[/]\)\)*>[;]' arch/arm64/boot/dts/hisilicon/hip05_hns.dtis
    accept '[ ][ ][ ][ ]run_cmd[ ]dd[ ]if=["][$]ofile\.bin["][ ]of=["][$]ofile\.bin["]' arch/powerpc/boot/wrapper
    accept '#define[ ]XCHAL_BYTE0_FORMAT_LENGTHS[ \t238,\\\n]*' arch/xtensa/variants/de212/include/variant/tie.h
    defsnc 'static[ ]const[ ]struct[ ]reg_sequence[ ]wm8998_rev_a_patch\[\][ ]=' drivers/mfd/wm8998-tables.c
    defsnc 'static[ ]struct[ ]nand_ecclayout[ ]vf610_nfc_ecc\(45\|60\)[ ]=' drivers/mtd/nand/vf610_nfc.c
    defsnc 'static[ ]const[ ]struct[ ]iro[ ]iro_arr\[31\][ ]=' drivers/net/ethernet/qlogic/qed/qed_hsi.h
    defsnc 'static[ ]struct[ ]rtl8xxxu_reg8val[ ]rtl8723a_mac_init_table\[\][ ]=' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu.c
    defsnc 'static[ ]struct[ ]rtl8xxxu_reg32val[ ]rtl\(\(8723a_phy_1t\|8192cu_phy_2t\)_init\|8188ru_phy_1t_highpa\|8xxx_agc_\(standard\|highpa\)\)_table\[\][ ]=' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu.c
    defsnc 'static[ ]struct[ ]rtl8xxxu_rfregval[ ]rtl\(\(8723au_radioa_1t\|8192cu_radio[ab]_[12]t\)_init\|8188ru_radioa_1t_highpa\)_table\[\][ ]=' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu.c
    defsnc 'static[ ]const[ ]int[ ]base_to_fuse_addr_mappings\[\]\[2\][ ]=' drivers/nvmem/vf610-ocotp.c
    defsnc 'static[ ]const[ ]u8[ ]crc7_syndrome_table\[256\][ ]=' drivers/staging/wilc1000/wilc_spi.c
    defsnc 'static[ ]const[ ]struct[ ]tsadc_table[ ]v3_code_table\[\][ ]=' drivers/thermal/rockchip_thermal.c
    defsnc 'omap3[46]xx_adc_to_temp\[128\][ ]=' drivers/thermal/ti-soc-thermal/omap3-thermal-data.c
    accept '[\t]*[ ][*][ ]*0[ ]1[ ]2[ ]3[ ]4[ ]5[ ]6[ ]7[ ]8[ ]9[ ]0[ ]1[ ]2[ ]3[ ]4[ ]5[ ]6[ ]7[ ]8[ ]9[ ]0[ ]1[ ]2[ ]3[ ]4[ ]5[ ]6[ ]7[ ]8[ ]9[ ]0[ ]1' net/6lowpan/iphc.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]ak4613_reg\[\][ ]=' sound/soc/codecs/ak4613.c
    accept '[	]\.helper[ 	]*=[ ]NULL[,][\n][	]*\.firmware' drivers/bluetooth/btmrvl_sdio.c
    blobname 'amdgpu[/]stoney_uvd\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_uvd.c
    blobname 'amdgpu[/]stoney_vce\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vce.c
    blobname 'i915[/]bxt_dmc_ver1\.bin' drivers/gpu/drm/i915/intel_csr.c
    blobname '\(utf\|board\)\(-2\)\?\.bin' drivers/net/wireless/ath/ath10k/hw.h
    blobname 'brcm[/]brcmfmac43\(50\|6[56]b\|71\)-pcie\.bin' drivers/net/wireless/brcm80211/brcmfmac/pcie.c
    accept '[\t]g_linux_wlan->firmware[ ]=' drivers/staging/wilc1000/linux_wlan.c
    accept '#define[ \t]*FILE_SUFFIX_BINARY_TABLE[\t ]*["]\.dat["]' drivers/acpi/acpica/acapps.h
    blobname 'i915[/]skl_guc_ver4\.bin' drivers/gpu/drm/i915/intel_guc_loader.c
    blobname 'bu21023\.bin' drivers/input/touchscreen/rohm_bu21023.c
    # These are user-supplied.
    accept '[\t]cdev->firmware[ ]=[ ]kmalloc' drivers/misc/mic/cosm/cosm_sysfs.c
    accept '[\t]rc[ ]=[ ]request_firmware[(][&]fw[,][ ]mdev->cosm_dev->' drivers/misc/mic/host/mic_x100.c
    accept '[\t]if[ ][(]bnxt_dir_type_is_executable[^\n]*[\n][\t]*return[ ]-EINVAL[;][\n][\n]*[\t]rc[ ]=[ ]request_firmware[(][&]' drivers/net/ethernet/broadcom/bnxt/bnxt_ethtool.c
    blobname 'qed[/]qed_init_values_zipped-["][ ]FW_FILE_VERSION[ ]["]\.bin' drivers/net/ethernet/qlogic/qed/qed_main.c
    accept 'MODULE_FIRMWARE[(]HTC_7010_MODULE_FW[)][;]' drivers/net/wireless/ath/ath9k/hif_usb.c
    accept 'MODULE_FIRMWARE[(]HTC_9271_MODULE_FW[)][;]' drivers/net/wireless/ath/ath9k/hif_usb.c
    accept '\(static[ ]int[ ]\|[\t]*ret[ ]=[ ]\)ath9k_hif_request_firmware[(]' drivers/net/wireless/ath/ath9k/hif_usb.c
    accept '[\t ]*["]%s[/]htc_%s-%d\.%s\.0\.fw["]' drivers/net/wireless/ath/ath9k/hif_usb.c
    accept '#define[ ]HTC_\(9271\|7010\)_MODULE_FW[ \t]*HTC_FW_PATH[ ]["][/]htc_\(9271\|7010\)-["][ ][\\][\n][ \t]*__stringify[(]MAJOR_VERSION_REQ[)][ ][\\][\n][ \t]*["]\.["][ ]__stringify[(]FIRMWARE_MINOR_IDX_MAX[)][ ]["]\.0\.fw["]' drivers/net/wireless/ath/ath9k/hif_usb.h
    blobname 'rtlwifi[/]rtl8723aufw_\(A\|B\|B_NoBT\)\.bin' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu.c
    blobname 'rtlwifi[/]rtl8192cufw_\(A\|B\|TMSC\)\.bin' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu.c
    blobname '\(otp\|ram\)\.bin' drivers/nfc/fdp/fdp.c
    accept '\(static[ ]int[ ]\|[\t]r[ ]=[ ]\)fdp_nci_request_firmware[(]' drivers/nfc/fdp/fdp.c
    accept '[\t][\t]lpfc_sli4_request_firmware_update[(]' drivers/scsi/lpfc/lpfc_init.c
    blobname 'ks2_qmss_pdsp_acc48\.bin' drivers/soc/ti/knav_qmss_queue.c
    blobname 'dfw_sst\.bin' sound/soc/intel/skylake/skl-topology.c
    # This seems to be designed to load a user-supplied fpga
    # configuration file, but there aren't any callers to this
    # function in the kernel tree.  Presumably users who program FPGAs
    # are supposed to write their own drivers and call this function.
    accept '[\t]ret[ ]=[ ]request_firmware[(][&]fw[,][ ]image_name[,][ ]' drivers/fpga/fpga-mgr.c
    blobname 'fpga_mgr_firmware_load' drivers/fpga/fpga-mgr.c
    accept '[\t ]*\(int\|ret[ ]=\)[ ]fpga_mgr_firmware_load[(]' drivers/fpga/fpga-mgr.[ch]
    accept '[ ][*][ ]fpga_mgr_firmware_load[ ]-' drivers/fpga/fpga-mgr.c
    accept 'EXPORT_SYMBOL_GPL[(]fpga_mgr_firmware_load[)][;]' drivers/fpga/fpga-mgr.c
    accept '[\t ]*CHIP_IS_E2[(]bp[)][ ][?][ ]["]everest2["][ ]:[ ]["]everest3["][/][*][(]DEBLOBBED[)][*][/][)][;]' drivers/net/ethernet/broadcom/bnx2x/bnx2x_main.c

    # New in 4.5.
    blobname 'qat_895xcc_mmp\.bin' drivers/crypto/qat/qat_dh895xcc/adf_dh895xcc_hw_data.h
    # These could use some assembly comments, but they're so simple
    # and regular that disassembly should suffice to make them transparent.
    defsnc 'static[ ]const[ ]u32[ ][vs]gpr_init_compute_shader\[\][ ]=' drivers/gpu/drm/amd/amdgpu/gfx_v8_0.c
    blobname 'brcmfmac43\(602\|50\(\|c2\)\|56\|570\|5[89]\|6[56]b\|71\)-pcie\.bin' drivers/net/wireless/broadcom/brcm80211/brcmfmac/pcie.c
    blobname 'brcmfmac43\(143\|241b[045]\|29\|3[0459]\|340\|362\|430\|455\|54\)-sdio\.bin' drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
    blobname 'brcmfmac43\(143\|236b\|242a\|569\)\.bin' drivers/net/wireless/broadcom/brcm80211/brcmfmac/usb.c
    blobname 'hfi1_\(dc8051\|fabric\|sbus\|pcie\)_d\.fw' drivers/staging/rdma/hfi1/firmware.c
    blobname '%s%s%s["][,][\n \t]*["]intel[/]dsp_fw_["][,][ ]guid[,][ ]["]\.bin' sound/soc/intel/skylake/skl-sst.c
    accept '[\t]*fsl[,]tmu-calibration[ ]=[ ][<][0-9a-fx \t\n]*>[;]' 'Documentation/devicetree/bindings/thermal/qoriq-thermal.txt\|arch/powerpc/boot/dts/fsl/t10\(23\|40\)si-post.dtsi'
    defsnc 'const[ ]u8[ ]sha256_zero_message_hash\[SHA256_DIGEST_SIZE\][ ]=' crypto/sha256_generic.c
    defsc 'static[ ]struct[ ]tegra_clk_pll_freq_table[ ]pll_e_freq_table\[\][ ]=' drivers/clk/tegra/clk-tegra210.c
    blobname 'qat_c3xxx\(\|_mmp\)\.bin' drivers/crypto/qat/qat_c3xxx/adf_c3xxx_hw_data.h
    blobname 'qat_c62x\(\|_mmp\)\.bin' drivers/crypto/qat/qat_c62x/adf_c62x_hw_data.h
    defsnc 'uint32_t[ ]fiji_clock_stretcher_ddt_table\[2\]\[4\]\[4\][ ]=' drivers/gpu/drm/amd/powerplay/hwmgr/fiji_hwmgr.c
    defsnc 'uint32_t[ ]PP_ClockStretcherDDTTable\[2\]\[4\]\[4\][ ]=' drivers/gpu/drm/amd/powerplay/hwmgr/tonga_hwmgr.c
    defsc 'struct[ ]SMU73_Discrete_GraphicsLevel[ ]avfs_graphics_level\[8\][ ]=' drivers/gpu/drm/amd/poewrplay/smumgr/fiji_smumgr.c
    defsnc 'static[ ]const[ ]struct[ ]dphy_pll_testdin_map[ ]dptdin_map\[\][ ]=' drivers/gpu/drm/rockchip/dw-mipi-dsi.c
    defsnc 'static[ ]const[ ]u16[ ]iproc_msi_reg_paxb\[NR_HW_IRQS\]\[IPROC_MSI_REG_SIZE\][ ]=' drivers/pci/host/pcie-iproc-msi.c
    defsnc 'static[ ]const[ ]int[ ]pv88090_buck1_limits\[\][ ]=' drivers/regulator/pv88090-regulator.c
    accept '[\t]wilc->firmware[ ]=' drivers/staging/wilc1000/linux_wlan.c
    defsnc 'static[ ]const[ ]struct[ ]tsadc_table[ ]v[14]_code_table\[\][ ]=' drivers/thermal/rockchip_thermal.c
    defsnc 'static[ ]const[ ]u8[ ]degrade_factor\[CPU_LOAD_IDX_MAX\]\[DEGRADE_SHIFT[ ][+][ ]1\][ ]=' kernel/sched/fair.c
    accept '[\t ]*rm[ ]-f[ ]["][/]boot[/]initramfs-[$]f\.img["]' scripts/prune-kernel
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt5616_reg\[\][ ]=' sound/soc/codecs/rt5616.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt5650_reg\[\][ ]=' sound/soc/codecs/rt5645.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt5659_reg\[\][ ]=' sound/soc/codecs/rt5659.c
    accept '[\t ]*["][ ]*-i[ ]--input[ \t]*input[ ]data[ ]from[ ]a[ ]file[ ][(]e\.g\.[ ][\\]["]test\.bin[\\]["]' tools/spi/spidev_test.c
    accept '[\t ]*["][ ]*-o[ ]--output[ \t]*output[ ]data[ ]to[ ]a[ ]file[ ][(]e\.g\.[ ][\\]["]results\.bin[\\]["]' tools/spi/spidev_test.c
    accept '[ ][*][ ]directly[ ]from[ ]probe[ ]or[ ]from[ ]request_firmware_\(no\)\?wait[ ]callback\.' drivers/input/touchscreen/goodix.c
    accept '[ ][*][ ]request_firmware_wait[ ]callback' drivers/input/touchscreen/goodix.c
    blobname 'goodix_\(%d\|[0-9]*\)_cfg\.bin' drivers/input/touchscreen/goodix.c
    blobname 'adf7242_firmware\.bin' drivers/net/ieee802154/adf7242.c
    blobna '[/][*][ ]get[ ]ADF7242[ ]addon[^*]*\([*]\+[^/*][^*]*\)*[*][*]*[/]' drivers/net/ieee802154/adf7242.c
    blobname 'wlan[/]prima[/]WCNSS_qcom_wlan_nv\.bin' drivers/soc/qcom/wcnss_ctrl.c
    blobname 'r8a779x_usb3_v[12]\.dlmem' drivers/usb/host/xhci-rcar.h
    blobname 'moxa[/]moxa-\(%04x\|11[135][01]\|[0-9a-f]*\)\.fw' drivers/usb/serial/mxu11x0.c
    blobname 'intel[/]dsp_fw_release\.bin' sound/soc/intel/skylake/skl.c
    accept '[\t]rc[ ]=[ ]request_firmware_nowait[(]THIS_MODULE[,][ ]1[,][ ]name[,][ ]dev[,][ ]GFP_KERNEL[,][\n][ \t]*NULL[,][ ]trigger_async_request_cb[)][;]' lib/test_firmware.c
    blobname 'nvidia[/]gk\(100\|20a\)[/]\(\(fecs\|gpccs\)_\(data\|inst\)\|sw_\(\(bundle\|method\)_init\|\(\|non\)ctx\)\)\.bin' drivers/gpu/drm/nouveau/nouveau_platform.c

    # New in 4.6.
    blobname 'atmel[/]wilc100[23]_firmware\.bin' drivers/staging/wilc1000/Makefile
    accept '[\t]*dev->firmware[ ]=[ ]1[;]' drivers/media/platform/coda/coda-common.c
    blobname 'vpu_fw_imx\(27_TO2\|53\|6[qd]\)\.bin' drivers/media/platform/coda/coda-common.c
    blobname 'brcmfmac4366c-pcie\.bin' drivers/net/wireless/broadcom/brcm80211/brcmfmac/pcie.c
    defsnc 'static[ ]struct[ ]rtl8xxxu_reg8val[ ]rtl8723b_mac_init_table\[\][ ]=' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu.c
    defsnc 'static[ ]struct[ ]rtl8xxxu_reg32val[ ]rtl8723b_phy_1t_init_table\[\][ ]=' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu.c
    defsnc 'static[ ]struct[ ]rtl8xxxu_reg32val[ ]rtl8xxx_agc_8723bu_table\[\][ ]=' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu.c
    defsnc 'static[ ]struct[ ]rtl8xxxu_rfregval[ ]rtl8723bu_radioa_1t_init_table\[\][ ]=' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu.c
    blobname 'rtlwifi[/]rtl8723bu_\(bt\|nic\)\.bin' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu.c
    blobname 'rtlwifi[/]rtl8192eu_nic\.bin' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu.c
    blobname 'intel[/]dsp_fw_bxtn\.bin' sound/soc/intel/skylake/skl.c
    accept 'CONFIG_EXTRA_FIRMWARE=["][/][*][(]DEBLOBBED' Documentation/x86/early-microcode.txt
    blob '[/]lib[/]firmware[/]\([\n][^\n][^\n]*\)*[\n][ ]*\.\.\.' Documentation/x86/'\(early-microcode\.txt\|microcode\.\(txt\|rst\)\)'
    blobname 'https[:][/][/]01\.org[/]linuxgraphics[/]intel-[^"\n]*' drivers/gpu/drm/i915/intel_csr.c
    accept '[\t ]*["]genroms[/]kvmvapic\.bin' Documentation/ABI/testing/sysfs-firmware-qemu_fw_cfg
    accept '#define[ ]XCHAL_BYTE0_FORMAT_LENGTHS[ \t238,\\\n]*' arch/xtensa/variants/test_kc705_hifi/include/variant/tie.h
    defsnc 'static[ ]const[ ]int[ ]supported_data_lane_swaps\[\]\[4\][ ]=' drivers/gpu/drm/msm/dsi/dsi_host.c
    accept '[\t ]*\(if[ ][(]\)\?[(]ret[ ]=[ ]gf100_gr_ctor_fw[(]gr[,][ ]["]gr[/]\(fecs\|gpccs\)_\(data\|inst\)["][,][ ][&]gr->fuc4\(09\|1a\)[cd][)]' drivers/gpu/drm/nouveau/nvkm/engine/gr/gm200.c
    defsnc '[\t]static[ ]const[ ]u8[ ]sixaxis_leds\[10\]\[4\][ ]=' drivers/hid/hid-sony.c
    defsnc 'static[ ]const[ ]struct[ ]afe440x_val_table[ ]afe4403_cap_table\[\][ ]=' drivers/iio/health/afe4403.c
    defsnc 'static[ ]const[ ]u16[ ]sunxi_nfc_randomizer_\(page\|ecc\(512\|1024\)\)_seeds\[\][ ]=' drivers/mtd/nand/sunxi_nand.c
    defsnc 'static[ ]const[ ]struct[ ]iro[ ]iro_arr\[44\][ ]=' drivers/net/ethernet/qlogic/qed/qed_hsi.h
    defsnc 'static[ ]const[ ]u32[ ]qca953x_1p1_modes_no_xpa_low_power_tx_gain_table\[\]\[2\][ ]=' drivers/net/wireless/ath/ath9k/ar953x_initvals.h
    defsnc '[\t]write_reg[(]par[,][ ]MIPI_DCS_WRITE_LUT[,]' drivers/staging/fbtft/fb_hx8353d.c
    defsnc 'static[ ]const[ ]struct[ ]tsadc_table[ ]rk3\(\(2[28]\|36\)8\|399\)_code_table\[\][ ]=' drivers/thermal/rockchip_thermal.c
    accept 'echo[ ]["]new-kernel-pkg[ ]--remove[ ][$]KERNELRELEASE[ ]--rminitrd[ ]--initrdfile=[/]boot[/]initramfs-[$]KERNELRELEASE\.img["]' scripts/package/mkspec
    defsnc '[}][ ]ni_div\[\][ ]=' sound/soc/codecs/max9867.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]max9867_reg\[\][ ]=' sound/soc/codecs/max9867.c
    defsnc 'static[ ]const[ ]struct[ ]reg_sequence[ ]rt5514_i2c_patch\[\][ ]=' sound/soc/codecs/rt5514.c
    defsnc '__thread[ ]vector[ ]int[ ]varray\[\][ ]=' 'tools/testing/selftests/poewrpc/math/vmx_\(preempt\|signal\)\.c'
    defsnc 'vector[ ]int[ ]varray\[\][ ]=' tools/testing/selftests/poewrpc/math/vmx_syscall.c
    blobname '%x-%\.6s-%\.8s-%d%s[^;]*-tplg\.bin' sound/soc/intel/skylake/skl-nhlt.c
    blobname 'intel[/]ibt-hw-%x\.%x\.bddata' drivers/bluetooth/hci_ag6xx.c
    blobname 'intel[/]ibt-hw-%x\.%x\.%x-fw-%x\.%x\.%x\.%x\.%x\.pbn' drivers/bluetooth/hci_ag6xx.c
    blobname 'melfas_mip4\.fw' drivers/input/touchscreen/melfas_mip4.c
    blobname 'iwlwifi-8000C-' drivers/net/wireless/intel/iwlwifi/iwl-8000.c

    # New in 4.7
    blobname 'amdgpu[/]polaris1[01]_smc\(_sk\)\?\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_cgs.c
    blobname 'amdgpu[/]polaris1[01]_uvd\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_uvd.c
    blobname 'amdgpu[/]polaris1[01]_vce\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vce.c
    blobname 'amdgpu[/]polaris1[01]_\(ce\|pfp\|me\|mec\|mec2\|rlc\)\.bin' drivers/gpu/drm/amd/amdgpu/gfx_v8_0.c
    blobname 'amdgpu[/]polaris1[01]_mc\.bin' drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c
    blobname 'amdgpu[/]polaris1[01]_sdma1\?\.bin' drivers/gpu/drm/amd/amdgpu/sdma_v_0.c
    blobname 'i915[/]skl_guc_ver6\.bin' drivers/gpu/drm/i915/intel_guc_loader.c
    accept '[\t]ar->normal_mode_fw\.fw_file\.firmware[ ]=[ ]NULL' drivers/net/wireless/ath/ath10k/core.c
    blobname 'pre-cal-%s-%s\.bin' drivers/net/wireless/ath/ath10k/core.c
    accept '[\t]fw_file->firmware[ ]=[ ]ath10k_fetch_fw_file' drivers/net/wireless/ath/ath10k/core.c
    blobname 'brcmfmac4356-sdio\.bin' drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
    blobname 'iwlwifi-9000\(-pu-[ab]0-\(jf\|lc\)-[ab]0-\|-\|\)' drivers/net/wireless/intel/iwlwifi/iwl-9000.c
    blobname 'iwlwifi-9260-th-a0-\(jf\|lc\)-a0-' drivers/net/wireless/intel/iwlwifi/iwl-9000.c
    blobname 'mrvl[/]pcie8897_uapsta_a0\.bin' drivers/net/wireless/marvell/mwifiex/pcie.h
    blobname 'mrvl[/]pcieuart8997_combo\(_v2\)\?\.bin' drivers/net/wireless/marvell/mwifiex/pcie.h
    blobname 'mrvl[/]pcieusb8997_combo\(_v2\)\?\.bin' drivers/net/wireless/marvell/mwifiex/pcie.h
    defsnc 'struct[ ]rtl8xxxu_reg8val[ ]rtl8xxxu_gen1_mac_init_table\[\][ ]=' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_core.c
    blobname '%s%pUL%s["][,][\n \t]*["]intel[/]dsp_fw_["][,][ ]uuid_mod[,][ ]["]\.bin' sound/soc/intel/skylake/skl-sst.c
    accept 'pm8994:[\n\t ,lvs0-9]*' Documentation/devicetree/bindings/regulator/qcom,spmi-regulator.txt
    defsnc '[\t]brightness-levels[ ]=[ ]<[0-9 \t\n]*>[;]' 'arch/arm/boot/dts/rk288-veyron-\(jaq\|minnie\).dts'
    defsc 'static[ ]const[ ]struct[ ]i2s_pll_cfg[ ]i2s_pll_cfg_2[78]m\[\][ ]=' drivers/clk/axs10x/i2s_pll_clock.c
    defsnc 'static[ ]const[ ]u8[ ]const_tab\[1024\][ ]__aligned[(]1024[)][ ]=' drivers/crypto/qat/qat_common/adf_admin.c
    defsnc 'static[ ]const[ ]uint32_t[ ]fiji_clock_stretcher_ddt_table\[2\]\[4\]\[4\][ ]=' drivers/gpu/drm/amd/powerplay/hwmgr/fiji_hwmgr.c
    defsnc 'static[ ]const[ ]uint32_t[ ]polaris10_clock_stretcher_ddt_table\[2\]\[4\]\[4\][ ]=' drivers/gpu/drm/amd/powerplay/hwmgr/polaris10_hwmgr.c
    defsc 'static[ ]const[ ]struct[ ]polaris10_pt_defaults[ ]polaris10_power_tune_data_set_array\[POWERTUNE_DEFAULT_SET_MAX\][ ]=' drivers/gpu/drm/amd/powerplay/hwmgr/polaris10_powertune.c
    defsnc 'static[ ]const[ ]uint32_t[ ]PP_ClockStretcherDDTTable\[2\]\[4\]\[4\][ ]=' drivers/gpu/drm/amd/powerplay/hwmgr/tonga_hwmgr.c
    defsc 'static[ ]const[ ]struct[ ]SMU73_Discrete_GraphicsLevel[ ]avfs_graphics_level\[8\][ ]=' drivers/gpu/drm/amd/powerplay/smumgr/fiji_smumgr.c
    defsc 'static[ ]const[ ]SMU74_Discrete_GraphicsLevel[ ]avfs_graphics_level_polaris10\[8\][ ]=' drivers/gpu/drm/amd/powerplay/smumgr/polaris10_smumgr.c
    defsnc 'static[ ]const[ ]struct[ ]hdmiphy_config[ ]hdmiphy_5433_configs\[\][ ]=' drivers/gpu/drm/exynos/exynos_hdmi.c
    defsnc 'static[ ]const[ ]struct[ ]dsi_phy_range[ ]dphy_range_info\[\][ ]=' drivers/gpu/drm/hisilicon/kirin/dw_drm_dsi.c
    defsnc 'static[ ]const[ ]struct[ ]bmi160_odr[ ]bmi160_accel_odr\[\][ ]=' drivers/iio/imu/bmi160/bmi160_core.c
    defsnc 'reg_initval\[QM1D1C0042_NUM_REG_ROWS\]\[QM1D1C0042_NUM_REGS\][ ]=' drivers/media/tuners/qm1d1c0042.c
    accept '[\t ]*[*][ ]*24[ ]*16[ ]*8[ ]*0[\n][\t ]*[*][ ]\([ ][0-7]\)*' drivers/net/ethernet/intel/fm10k/fm10k_pf.c
    accept '[\t]ar->testmode\.utf_mode_fw\.fw_file\.firmware[ ]=[ ]NULL' drivers/net/wireless/ath/ath10k/testmode.c
    defsnc 'static[ ]struct[ ]rtl8xxxu_reg8val[ ]rtl8192e_mac_init_table\[\][ ]=' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_8192e.c
    defsc 'static[ ]struct[ ]rtl8xxxu_reg32val[ ]rtl8192eu_phy_init_table\[\][ ]=' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_8192e.c
    defsnc 'static[ ]struct[ ]rtl8xxxu_reg32val[ ]rtl8xxx_agc_8192eu_\(std\|highpa\)_table\[\][ ]=' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_8192e.c
    defsc 'static[ ]struct[ ]rtl8xxxu_rfregval[ ]rtl8192eu_radio[ab]_init_table\[\][ ]=' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_8192e.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]byt_score_pins_map\[BYT_NGPIO_SCORE\][ ]=' drivers/pinctrl/intel/pinctrl-baytrail.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]byt_sus_pins_map\[BYT_NGPIO_SUS\][ ]=' drivers/pinctrl/intel/pinctrl-baytrail.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]byVT3253InitTab_RFMD\[CB_VT3253_INIT_FOR_RFMD\]\[2\][ ]=' drivers/staging/vt6655/baseband.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]byVT3253B0_RFMD\[CB_VT3253B0_INIT_FOR_RFMD\]\[2\][ ]=' drivers/staging/vt6655/baseband.c
    accept '[\t]*wilc->firmware[ ]=' drivers/staging/wilc1000/linux_wlan.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]max98371_reg\[\][ ]=' sound/soc/codecs/max98371.c
    blobname 'rtlwifi[/]rtl8192cufw_\(TMSC\|[AB]\)\.bin' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_8192c.c
    blobname 'rtlwifi[/]rtl8192eu_nic\.bin' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_8192e.c
    blobname 'rtlwifi[/]rtl8723aufw_\([AB]\|B_NoBT\)\.bin' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_8723a.c
    blobname 'rtlwifi[/]rtl8723bu_\(bt\|nic\)\.bin' drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_8723b.c
    blobname 'nvidia[/]tegra\(124\|210\)[/]xusb\.bin' drivers/usb/host/xhci-tegra.c
    accept '[\t]*ath10k_info[(]ar[,][ ]["][/][*][(]DEBLOBBED[)][*][/][ ]didn.t' drivers/net/wireless/ath/ath10k/testmode.c
    accept 'static[ ]const[ ]struct[ ]tegra_xusb_soc[ ]tegra\(124\|210\)_soc[ ]=[ ][{][\n][\t][.]firmware[ ]=' drivers/usb/host/xhci-tegra.c
    blobname 'i915[/]kbl_dmc_ver1\.bin' drivers/gpu/drm/i915/intel_csr.c

    # New in 4.8.
    blobname 'intel[/]dsp_fw_kbl\.bin' sound/soc/intel/skylake/skl.c
    blobname 'brcmfmac4365c-pcie\.bin' drivers/net/wireless/broadcom/brcm80211/brcmfmac/pcie.c
    blobname 'radeon[/]\(%s\|tahiti\|pitcairn\|verde\|oland\|hainan\)_\(pfp\|me\|ce\|mc\|rlc\|smc\|k_smc\)\.bin' drivers/gpu/drm/radeon/si.c
    blobname 'radeon[/]\(%s\|bonaire\|hawaii\|kaveri\|kabini\|mullins\)_\(pfp\|me\|ce\|mec\|mec2\|mc\|rlc\|sdma\|smc\|k_smc\)\.bin' 'drivers/gpu/drm/radeon/ci\(k\|_dpm\).c'
    blobname 'i915[/]skl_guc_ver6_1\.bin' drivers/gpu/drm/i915/intel_guc_loader.c
    blobname 'i915[/]bxt_guc_ver8_7\.bin' drivers/gpu/drm/i915/intel_guc_loader.c
    blobname 'i915[/]kbl_guc_ver9_14\.bin' drivers/gpu/drm/i915/intel_guc_loader.c
    blobname 'i915[/]kbl_dmc_ver1_01\.bin' drivers/gpu/drm/i915/intel_csr.c
    blobname 'i915[/]skl_dmc_ver1_26\.bin' drivers/gpu/drm/i915/intel_csr.c
    blobname 'i915[/]bxt_dmc_ver1_07\.bin' drivers/gpu/drm/i915/intel_csr.c
    blobname 'intel[/]ibt-%u-%u\.sfi' drivers/bluetooth/btusb.c
    accept '[\t]*ranges[ ]=[ ]<[ \t\n0-9xa-f]*>[;]' arch/arm/boot/dts/ep7209.dtsi
    accept '[\t]*nvidia[,]emc-configuration[ ]=[ ]<[ \t\n0-9xa-f]*>[;]' arch/arm/boot/dts/tegra124-apalis-emc.dtsi
    accept '[\t]*bool[ ]["]vmlinux\.bin[ ]or[ ]vmlinuz\.bin["]' arch/mips/Kconfig
    accept 'K256_8:\([\n][ 	]*\.octa[ 	]*0x[0-9a-f]*\)*' arch/x86/crypto/sha256-mb/sha256_x8_avx2.S
    accept 'K256:\([\n][ 	]*\.int[ 	]*0x[0-9a-f,x]*\)*' arch/x86/crypto/sha256-mb/sha256_x8_avx2.S
    accept 'K512_4:\([\n][ 	]*\.octa[ 	]*0[x0-9a-f,\\\t\n]*\)*' arch/x86/crypto/sha256-mb/sha256_x8_avx2.S
    accept '[ ][*][ ]request_firmware_into_buf[ ]-' drivers/base/firmware_class.c
    accept 'request_firmware_into_buf[(]const[ ]struct[ ]firmware[ ]' drivers/base/firmware_class.c
    accept 'EXPORT_SYMBOL[(]request_firmware_into_buf[)]' drivers/base/firmware_class.c
    defsc 'static[ ]const[ ]int[ ]mma8452_hp_filter_cutoff\[4\]\[8\]\[4\]\[2\][ ]=' drivers/iio/accel/mma8452.c
    defsnc '[\t]static[ ]const[ ]u8[ ]cmd\[7\]\[6\][ ]=' drivers/input/touchscreen/raydium_i2c_ts.c
    defsnc '[\t]static[ ]const[ ]u8[ ]cmd\[5\]\[11\][ ]=' drivers/input/touchscreen/raydium_i2c_ts.c
    blobname 'raydium\.fw' drivers/input/touchscreen/raydium_i2c_ts.c
    blobname '\(silead[/]\)\?%s\.fw' drivers/input/touchscreen/silead.c
    blobna 'snprintf[(]data->fw_name[,][ ]sizeof[(]data->fw_name[)][,][ \n\t]*["]\(silead[/]\)\?%s["][,][ ]str[)]' drivers/input/touchscreen/silead.c
    blobname 'vpu_[pd]\.bin' drivers/media/platform/mtk-vpu/mtk_vpu.c
    accept '[\t]if[ ][(]dir_type[ ]!=[ ]BNX_DIR_TYPE_UPDATE[ ][&][&][\n\t ]*bnxt_dir_type_is_executable[^\n]*[\n][\t]*return[ ]-EINVAL[;][\n][\n]*[\t]rc[ ]=[ ]request_firmware[(][&]' drivers/net/ethernet/broadcom/bnxt/bnxt_ethtool.c
    defsnc 'static[ ]const[ ]struct[ ]iro[ ]iro_arr\[46\][ ]=' drivers/net/ethernet/qlogic/qed/qed_hsi.h
    blobname 'iwlwifi-Qu-a0-jf-b0-' drivers/net/wireless/intel/iwlwifi/iwl-a000.c
    blobname 'ks7010sd\.rom' drivers/staging/ks7010/ks7010_sdio.h
    defsnc 'static[ ]const[ ]u16[ ]expected_tpt_\(siso\|mimo2\)_160MHz\[4\]\[IWL_RATE_COUNT\][ ]=' drivers/net/wireless/intel/iwlwifi/mvm/rs.c
    defsnc 'static[ ]const[ ]int[ ]adinter_muxvals\[\][ ]=' drivers/pinctrl/uniphier/pinctrl-uniphier-ld6b.c
    accept '\(static[ ]inline[ ]\)\?int[ ]request_firmware_into_buf[(]const[ ]struct[ ]firmware[ ]' include/linux/firmware.h
    accept 'static[ ]inline[ ]int[ ]mod_firmware_load[(]const[ ]char[ ][*]fn[,]' sound/oss/sound_firmware.h
    defsnc 'static[ ]const[ ]struct[ ]pll_macro_entry[ ]pll_predef_mclk\[\][ ]=' sound/soc/bcm/cygnus-ssp.c
    defsnc 'static[ ]const[ ]struct[ ]_ssp_clk_coeff[ ]ssp_clk_coeff\[\][ ]=' sound/soc/bcm/cygnus-ssp.c
    defsnc 'static[ ]const[ ]struct[ ]cs35l33_mclk_div[ ]cs35l33_mclk_coeffs\[\][ ]=' sound/soc/codecs/cs35l33.c
    defsnc 'static[ ]struct[ ]reg_default[ ]max98504_reg_defaults\[\][ ]=' sound/soc/codecs/max98504.c
    blobname 'rt5514_dsp_fw[12]\.bin' sound/soc/codecs/rt5514.h
    blobname 'modem\.mdt' drivers/remoteproc/qcom_q6v5_pil.c
    blobname 'mba\.b00' drivers/remoteproc/qcom_q6v5_pil.c

    # New in 4.9.
    blobname 'rtl_bt[/]rtl\(8723b\|8821a\|8761a\|8822b\)_\(config\|fw\)\.bin' drivers/bluetooth/btrtl.c
    blobname 'amdgpu[/]\(topaz\|tonga\)_k_smc\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_cgs.c
    blobname 'i915[/]["][^"]*["]_guc_ver["][^"]*["]_["][^"]*["]\.bin' drivers/gpu/drm/i915/intel_guc_loader.c
    blobname 'mrvl[/]pcie\(uart\|usb\)8997_combo_v4\.bin' drivers/net/wireless/marvell/mwifiex/pcie.h
    blobname 'mrvl[/]pcie8997_wlan_v4\.bin' drivers/net/wireless/marvell/mwifiex/pcie.h
    blobname 'mrvl[/]usbusb8997_combo_v4\.bin' drivers/net/wireless/marvell/mwifiex/usb.h
    accept '[ ]*[/]Widths[ ]\[[0-9 ]*\]' Documentation/media/media_api_files/typical_media_device.pdf
    accept '[ ]*:widths:[0-9 ]*' Documentation/media/uapi/v4l/subdev-formats.rst
    defsc 'static[ ]const[ ]struct[ ]iceland_pt_defaults[ ]defaults_iceland\(xt\|pro\)\?[ ]=' drivers/gpu/drm/amd/powerplay/smumgr/iceland_smc.c
    defsc 'static[ ]const[ ]struct[ ]tonga_pt_defaults[ ]tonga_power_tune_data_set_array\[POWERTUNE_DEFAULT_SET_MAX\][ ]=' drivers/gpu/drm/amd/poewrplay/smumgr/tonga_smc.c
    defsnc 'static[ ]const[ ]uint32_t[ ]tonga_clock_stretcher_ddt_table\[2\]\[4\]\[4\][ ]=' drivers/gpu/drm/amd/powerplay/smumgr/tonga_smc.c
    defsnc 'static[ ]const[ ]u16[ ]\(forward\|inverse\)_quantization_table\[QUANTIZATION_TABLE_LEN\][ ]=' drivers/media/pci/tw5864/tw5864-video.c
    defsnc 'static[ ]const[ ]u16[ ]encoder_vlc_lookup_table\[VLC_LOOKUP_TABLE_LEN\][ ]=' drivers/media/pci/tw5864/tw5864-video.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]\(lambda_lookup_table\|intra4x4_lambda3\)\[\][ ]=' drivers/media/pci/tw5864/tw5864-video.c
    defsnc 'static[ ]const[ ]struct[ ]iro[ ]iro_arr\[47\][ ]=' drivers/net/ethernet/qlogic/qed/qed_hsi.h
    defsnc 'static[ ]const[ ]u8[ ]netvsc_hash_key\[\][ ]=' drivers/net/hyperv/rndis_filter.c
    defsc 'static[ ]const[ ]struct[ ]cs42l73_mclk_div[ ]cs42l73_mclk_coeffs\[\][ ]=' sound/soc/codecs/cs42l73.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt5660_reg\[\][ ]=' sound/soc/codecs/rt5660.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt566[38]_reg\[\][ ]=' sound/soc/codecs/rt5663.c
    defsnc '__thread[ ]vector[ ]int[ ]varray\[24\][ ]=' tools/testing/selftests/powerpc/math/vsx_preempt.c
    defsnc 'vector[ ]int[ ]vms\[\][ ]=' tools/testing/selftests/powerpc/tm/tm-signal-context-chk-vmx.c
    defsnc 'vector[ ]int[ ]vss\[\][ ]=' tools/testing/selftests/powerpc/tm/tm-signal-context-chk-vsx.c
    blobname 'imx[/]sdma[/]sdma-imx7d\.bin' arch/arm/boot/dts/imx7s.dtsi
    blobname 'gsl3675-gt90h\.fw' arch/arm/boot/dts/sun8i-a23-gt90h-v4.dts
    blobname 'gsl1680-inet86dz\.fw' arch/arm/boot/dts/sun8i-a23-inet86dz.dts
    blobname 'gsl1680-polaroid-mid2407pxe03\.fw' arch/arm/boot/dts/sun8i-a23-polaroid-mid2407pxe03.dts
    blobname 'gsl3670-polaroid-mid2809pxe04\.fw' arch/arm/boot/dts/sun8i-a23-polaroid-mid2809pxe04.dts
    blobname 'gsl3675-ga10h\.fw' arch/arm/boot/dts/sun8i-a33-ga10h-v1.1.dts
    blobname 'mrvl[/]helper_uart_3000000\.bin' drivers/bluetooth/hci_mrvl.c
    blobname 'mrvl[/]uart8897_bt\.bin' drivers/bluetooth/hci_mrvl.c
    accept 'static[ ]int[ ]bnxt_flash_\(firmware\|package\)_from_file[(][ \t\na-z0-9_,*]*[)][\n][{][\n][\t]\([^\n]*[\n]\+[\t]\)*rc[ ]=[ ]request_firmware[(][&]fw' drivers/net/ethernet/broadcom/bnxt/bnxt_ethtool.c
    accept '[\t]*\(rc[ ]=[ ]\)\?wil_request_firmware[(]wil[,][ ]WIL_FW2\?_NAME[,][ ]\(true\|false\)[)][;]' drivers/net/wireless/ath/wil6210/main.c
    blobname 'mwifiex_mfg\.bin' drivers/net/wireless/marvell/mwifiex/main.c
    accept '[\t]*mwifiex_dbg[(]adapter[,][ ]ERROR[,][\n][\t ]*["]request_firmware[ ]error' drivers/net/wireless/marvell/mwifiex/main.c
    blobname 'ti-connectivity[/]wl12[78]x-nvs\.bin' 'drivers/net/wireless/ti/wlcore/\(sdio\|spi\)\.c'
    blobname 'ti-connectivity[/]wl18xx-conf\.bin' 'drivers/net/wireless/ti/wlcore/\(sdio\|spi\)\.c'
    blobname 'ziirave_wdt\.fw' drivers/watchdog/wiirave_wdt.c
    blobna '["]gmp_["]' drivers/staging/greybus/firmware.h
    blobna '["]FW_NAME_PREFIX["]["]%08x_%08x_%08x_%08x_%s\.tftf["][\n][^*]*\([*]\+[^/*][^*]*\)*[*]\+[/]' drivers/staging/greybus/firmware.h
    blobname '\(gmp_\)\?%08x_%08x_%08x_%08x_s2l\.tftf' drivers/staging/greybus/bootrom.c
    blobname '\(gmp_\)\?%08x_%08x_%08x_%08x_\(%s\|[^"]*\)\.tftf' drivers/staging/greybus/fw-download.c
    # Long-needed b43 cleanup.  These are actually cleaned up with
    # custom code in deblob-<kver>.  Only ucode5, b0g0initvals5 and
    # b0g0bsinitvals5 are provided by openfwwf, and only b43 (not
    # b43legacy) can use the openfwwf files, so anything else in b43
    # and b43legacy ought to be cleaned up.
    accept '[\t]*filename[ ]=[ ]["]\(ucode\|b0g0\(bs\)\?initvals\)5["][;]' drivers/net/wireless/broadcom/b43.c
    blobna '["]\(ucode\|[^ "\n]*initvals\)[0-9][^" .\n]*["]' 'drivers/net/wireless/broadcom/b43\(legacy\)\?\.c'
    # We want to be more specific than deblob0-<kver> in the pcm
    # matches, to avoid numerous false positives in sound pcm drivers.
    blobna '["]pcm[45]["]' 'drivers/net/wireless/broadcom/b43\(legacy\)\?\.c'
    blobna '[/][*][ ]What[ ]about[ ][^ \n]*initvals22[?][ ][*][/]' drivers/net/wireless/broadcom/b43.c

    # New in 4.9.2 and 4.8.17.
    accept '[\t]*fwname[ ]=[ ]["]fuc4\(09\|1a\)[cd]["][;]' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf100.c
    accept '[\t]*snprintf[(]f[,][ ]sizeof[(]f[)][,][ ]["]nouveau[/]nv%02x_%s["][,][ ]device->chipset[,][ ]fwname[)][;][\n][\t]*ret[ ]=[ ]request_firmware[(][&]fw[,][ ]f[,][ ]device->dev[)][;][\n][\t]*if[ ][(]ret[)][ ][{][\n][\t]*snprintf[(]f[,][ ]sizeof[(]f[)][,][ ]["]nouveau[/]%s["][,][ ]fwname[)][;][\n][\t]*ret[ ]=[ ]request_firmware[(][&]fw[,][ ]f[,][ ]device->dev[)][;]' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf100.c

    # New in 4.10-rc*.
    accept '[ ]*d=["]m[ ]0[,]0[ ][^z\n]*z["]' Documentation/media/uapi/v4l/crop.svg
    accept '[ ]*Kernel[ ]driver[ ]in[ ]use:[ ]serial\([\n][ ]*[0-3]0:[ 0-9a-f]*\)*' Documentation/media/v4l-drivers/ivtv.rst
    accept 'tbl_shf_table:[\n]\([/][/][^\n]*[\n]\)*[\n]*\([\n][\t]\.byte[ \t0-9xa-f]*\)*' arch/arm/crypto/crct10dif-ce-core.S
    accept '\.LK256:\([\n][ 	]*\.long[ 	]*0\(x[0-9a-f]*\([,]0x[0-9a-f]*\)*\)\?\)*[ \t]*[/][/][ ]*terminator' arch/arm64/crypto/sha256-core.S_shipped
    accept '\.LK[$]BITS:\([\n]___[\n][$]code\.=<<___[ ]if[^\n]*\([\n][ 	]*\.\(long\|quad\)[ 	]*0\(x[0-9a-f]*\([,]0x[0-9a-f]*\)*\)\?\)*[ \t]*[/][/][ ]*terminator\)*' arch/arm64/crypto/sha512-armv8.pl
    accept '\.LK512:\([\n][ 	]*\.quad[ 	]*0\(x[0-9a-f]*\([,]0x[0-9a-f]*\)*\)\?\)*[ \t]*[/][/][ ]*terminator' arch/arm64/crypto/sha512-core.S_shipped
    accept '[ ][*][ ]Concurrent[ ]request_firmware[(][)][ ]for[ ]the[ ]same' drivers/base/firmware_class.c
    defsnc 'static[ ]const[ ]struct[ ]rcar_gen2_cpg_pll_config[ ]cpg_pll_configs\[8\][ ]__initconst[ ]=' drivers/clk/renesas/r8a7745-cpg-mssr.c
    defsnc 'static[ ]unsigned[ ]int[ ]eotf_33_linear_mapping\[OSD_EOTF_LUT_SIZE\][ ]=' drivers/gpu/drm/meson/meson_viu.c
    defsnc 'static[ ]unsigned[ ]int[ ]oetf_41_linear_mapping\[OSD_OETF_LUT_SIZE\][ ]=' drivers/gpu/drm/meson/meson_viu.c
    defsnc 'static[ ]unsigned[ ]int[ ]vpp_filter_coefs_4point_bspline\[\][ ]=' drivers/gpu/drm/meson/meson_vpp.c
    defsnc 'static[ ]const[ ]u32[ ]a5xx_registers\[\][ ]=' drivers/gpu/drm/msm/adreno/a5xx_gpu.c
    defsnc '[}][ ]a5xx_sequence_regs\[\][ ]=' drivers/gpu/drm/msm/adreno/a5dxx_power.c
    defsnc 'static[ ]uint32_t[ ]gf100_ce_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/ce/fuc/gf100.fuc3.h
    defsnc 'static[ ]uint32_t[ ]gt215_ce_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/ce/fuc/gf215.fuc3.h
    defsnc 'static[ ]uint32_t[ ]gf100_grgpc_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/gpcgf100.fuc3.h
    defsnc 'static[ ]uint32_t[ ]gf117_grgpc_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/gpcgf117.fuc3.h
    defsnc 'static[ ]uint32_t[ ]gk104_grgpc_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/gpcgk104.fuc3.h
    defsnc 'static[ ]uint32_t[ ]gk110_grgpc_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/gpcgk110.fuc3.h
    defsnc 'static[ ]uint32_t[ ]gk208_grgpc_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/gpcgk208.fuc5.h
    defsnc 'static[ ]uint32_t[ ]gm107_grgpc_code\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/fuc/gpcgm107.fuc5.h
    defsnc 'static[ ]uint32_t[ ]gf100_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/hubgf100.fuc3.h
    defsnc 'static[ ]uint32_t[ ]gf117_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/hubgf117.fuc3.h
    defsnc 'static[ ]uint32_t[ ]gk104_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/hubgk104.fuc3.h
    defsnc 'static[ ]uint32_t[ ]gk110_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/hubgk110.fuc3.h
    defsnc 'static[ ]uint32_t[ ]gk208_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/fuc/hubgk208.fuc5.h
    defsnc 'static[ ]uint32_t[ ]gm107_grhub_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/core/engine/graph/fuc/hubgm107.fuc5.h
    defsnc 'static[ ]uint32_t[ ]g98_psec_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/sec/fuc/g98.fuc0s.h
    defsnc 'static[ ]uint32_t[ ]gf100_pmu_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/subdev/pmu/fuc/gf100.fuc3.h
    defsnc 'static[ ]uint32_t[ ]gf119_pmu_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/ce/fuc/gf119.fuc4.h
    defsnc 'static[ ]uint32_t[ ]gk208_pmu_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/subdev/pmu/fuc/gk208.fuc5.h
    defsnc 'static[ ]uint32_t[ ]gt215_pmu_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/subdev/pmu/fuc/gt215.fuc3.h
    defsnc 'static[ ]uint32_t[ ]g98_sec_\(data\|code\)\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/ce/fuc/gf98.fuc0s.h
    defsnc 'static[ ]const[ ]u16[ ]lmp91000_temp_lut\[\][ ]=' drivers/iio/potentiostat/lmp91000.c
    defsnc 'static[ ]const[ ]u8[ ]fdp1_mdet\[\][ ]=' drivers/media/platform/rcar_fdp1.c
    defsnc 'static[ ]struct[ ]cs35l34_mclk_div[ ]cs35l34_mclk_coeffs\[\][ ]=' sound/soc/codecs/cs35l34.c
    defsnc 'static[ ]const[ ]struct[ ]cs42l42_pll_params[ ]pll_ratio_table\[\][ ]=' sound/soc/codecs/cs42l42.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt5663_v2_reg\[\][ ]=' sound/soc/codecs/rt5663.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt5665_reg\[\][ ]=' sound/soc/codecs/rt5665.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]stac9766_reg_defaults\[\][ ]=' sound/soc/codecs/stac9766.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm9705_reg_defaults\[\][ ]=' sound/soc/codecs/wm9705.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]wm9712_reg_defaults\[\][ ]=' sound/soc/codecs/wm9712.c
    blobname 'fdma_\(%s_%d\|[^\." ,;_]*_[0-9][0-9]*\)\.elf' drivers/dma/st_fdma.c
    blobname 'amdgpu[/]polaris12_smc\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_cgs.c
    blobname 'amdgpu[/]polaris12_uvd\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_uvd.c
    blobname 'amdgpu[/]polaris12_vce\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vce.c
    blobname 'amdgpu[/]polaris12_\(ce\|pfp\|me\|mec\|mec2\|rlc\)\.bin' drivers/gpu/drm/amd/amdgpu/gfx_v8_0.c
    blobname 'amdgpu[/]polaris12_mc\.bin' drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c
    blobname 'amdgpu[/]polaris12_sdma1\?\.bin' drivers/gpu/drm/amd/amdgpu/sdma_v3_0.c
    blobname 'amdgpu[/]polaris12_smc\.bin' drivers/gpu/drm/amd/amdgpu/vi.c
    blobname 'radeon[/]si58_mc\.bin' 'drivers/gpu/drm/amd/amdgpu/gmc_v6_0\.c\|drivers/gpu/drm/radeon/si\.c'
    blobname 'a530_p\(m4\|fp\)\.fw' drivers/gpu/drm/msm/adreno/adreno_device.c
    blobname 'radeon[/]banks_k_2_smc\.bin' 'drivers/gpu/drm/amd/amdgpu/si_dpm\.c\|drivers/gpu/drm/radeon/si\.c'
    blobname 'melfas_mip4_%04X\.fw' drivers/input/touchscreen/melfas_mip4.c
    blobname 'cbfw-3\.2\.5\.1\.bin' drivers/scsi/bfa/bfad.c
    blobname 'r8a779x_usb3_v3\.dlmem' drivers/usb/host/xhci-rcar.h
    blob 'https\?:[/][/]linuxtv\.org[/][^" >]*firmware[/][^" \t\n>\\)]*' 'Documentation/media/v4l-drivers/ivtv\.rst\|drivers/media/pci/ttpci/av7110\.c\|firmware/WHENCE'
    # The firmware file name is supplied by the user.
    accept '[\t]ret[ ]=[ ]request_firmware[(][&]fw[,][ ]fw_name[,]\([^\n]*[\n]\+[^\n}]\)*ret[ ]=[ ]rmi_firmware_update[(]data[,][ ]fw[)]' drivers/input/rmi4/rmi_f34.c
    # This seems to be an example file name of something to be
    # supplied by the user in the DTS file, not the name of an actual
    # firmware file.
    accept '[\t ]*firmware-name[ ]=[ ]["]zynq-gpio\.bin["][;]' Documentation/devicetree/bindings/fpga/fpga-region.txt
    accept '[\t]if[ ][(]of_property_read_bool[(]np[,][ ]["]qca[,]no-eeprom["][)][)][ ][{][\n][\t]*[/][*][ ]ath9k-eeprom-<bus>-<id>\.bin[ ][*][/][\n][\t]*scnprintf[(]eeprom_name[,][ ]sizeof[(]eeprom_name[)][,][\n][\t ]*["]ath9k-eeprom-%s-%s\.bin["][,]' drivers/net/wireless/ath/ath9k/init.c
    blobname 'iwlwifi-3168-' drivers/net/wireless/intel/iwlwifi/iwl-7000.c
    blobname 'iwlwifi-8265-' drivers/net/wireless/intel/iwlwifi/iwl-8000.c
    blobname 'iwlwifi-[0-9][^"\n\t ]*-' drivers/net/wireless/intel/iwlwifi/iwl-8000.c
    blobname 'a530v3_gpmu\.fw2' drivers/gpu/drm/msm/adreno/adreno_device.c

    # New in 4.11.
    blobname 'amdgpu[/]polaris1[01]_k_smc\.bin' drivers/gpu/drm/amdgpu/amdgpu_cgs.c
    blobname 'i915[/]\(glk\|kbl\)_dmc_ver1_01\.bin' drivers/gpu/drm/i915/intel_csr.c
    blobname 'vpu[/]vpu_fw_imx\(27_TO2\|53\|6[qd]\)\.bin' drivers/media/platform/coda/coda-common.c
    blobname '%s-%d\.bin' drivers/net/wireless/ath/ath10k/core.c
    blobname 'wil6210_sparrow_plus\.fw' drivers/net/wireless/ath/wil6210/wil6210.h
    blobname 'iwlwifi-Qu-a0-hr-a0-' drivers/net/wireless/intel/iwlwifi/iwl-a000.c
    blobname 'intel[/]dsp_fw_glk\.bin' sound/soc/intel/skylake/skl.c
    defsnc 'unsigned[ ]char[ ]__aligned[(]16[)][ ]bootlogo_bits\[\][ ]=' 'arch/m68k/68000/bootlogo\(-vz\)\?\.h'
    defsnc 'static[ ]volatile[ ]const[ ]u8[ ]__cacheline_aligned[ ]__aesti_\(inv_\)\?sbox\[\][ ]=' crypto/aes_ti.c
    defsc 'static[ ]const[ ]struct[ ]ast_vbios_stdtable[ ]vbios_stdtable\[\][ ]=' drivers/gpu/drm/ast/ast_tables.h
    defsnc 'static[ ]const[ ]struct[ ]vadc_map_pt[ ]adcmap_100k_104ef_104fb\[\][ ]=' drivers/iio/adc/qcom-spmi-vadc.c
    defsnc 'static[ ]const[ ]int[ ]srf08_sensitivity\[\][ ]=' drivers/iio/proximity/srf80.c
    defsnc '[\t]static[ ]u8[ ]rss_key\[40\][ ]=' drivers/net/ethernet/aquantia/atlantic/aq_nic.c
    defsnc '[\t]static[ ]u32[ ]\(itr_imr_\(rxr\|txt\)\(en\)\?\|rpo_lro_ldes_max\)_\(adr\|msk\|shift\)\[32\][ ]=' drivers/net/ethernet/aquantia/atlantic/hw_atl/hw_atl_llh.c
    defsnc 'static[ ]const[ ]u32[ ]hw_atl_utils_hw_mac_regs\[\][ ]=' drivers/net/ethernet/aquantia/atlantic/hw_tl/hw_atl_utils.c
    defsnc 'static[ ]const[ ]u8[ ]netvsc_hash_key\[NETVSC_HASH_KEYLEN\][ ]=' drivers/net/hyperv/rndis_filter.c
    defsnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_3x_xtal20\[\][ ]=' drivers/net/wireless/ralink/rt2x00/rt2800lib.c
    defsnc 'unsigned[ ]long[ ]long[ ]lpfc_enable_nvmet\[LPFC_NVMET_MAX_PORTS\][ ]=' drivers/scsi/lpfc/lpfc_attr.c
    defsnc 'static[ ]const[ ]u64[ ]test_vectors_siphash\[64\][ ]=' lib/test_siphash.c
    defsnc 'static[ ]const[ ]u32[ ]test_vectors_hsiphash\[64\][ ]=' lib/test_siphash.c
    defsnc 'static[ ]yyconst[ ]YY_CHAR[ ]yy_ec\[256\][ ]=' scripts/dtc/dtc-lexer.lex.c_shipped
    defsnc 'static[ ]yyconst[ ]YY_CHAR[ ]yy_meta\[48\][ ]=' scripts/dtc/dtc-lexer.lex.c_shipped
    defsnc 'static[ ]yyconst[ ]flex_uint16_t[ ]yy_base\[180\][ ]=' scripts/dtc/dtc-lexer.lex.c_shipped
    defsnc 'static[ ]yyconst[ ]flex_uint16_t[ ]yy_nxt\[449\][ ]=' scripts/dtc/dtc-lexer.lex.c_shipped
    accept '0x1B[,][ ]0x5E[,][ ]0x78[,][ ]0x3D[,][ ]0x00[,][ ]0x00[,][ ]0x00[,][ ]0x18[,][ ][0x1-9A-F, \n]*' security/apparmor/nulldfa.in
    defsnc '[\t]struct[ ]sock_filter[ ]bpf_filter\[\][ ]=' tools/testing/selftests/net/psock_lib.h
    blobname 'cpt8x-mc-[as]e\.out' drivers/crypto/cavium/cpt/cptpf_main.c
    blobname 'i915[/]["][ ]__stringify[(]platform[)][ ]["]_huc_ver["][ ]__stringify[(]major[)][ ]["]_["][ \\\n\t]*__stringify[(]minor[)][ ]["]_["][ ]__stringify[(]bld_num[)][ ]["]\.bin' drivers/gpu/drm/i915/intel_huc.c
    accept '[	][	]*gf100_gr_init_fw[(]gr->fecs[,][ ][&]gr->fuc409c[,][ ][&]gr->fuc409d[)][;]' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf100.c
    accept '[	][	]*gf100_gr_init_fw[(]gr->gpccs[,][ ][&]gr->fuc41ac[,][ ][&]gr->fuc41ad[)][;]' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf100.c
    blobname 'rockchip[/]dptx\.bin' drivers/gpu/drm/rockchip/cdn-dp-core.c
    accept 'static[ ]int[ ]cdn_dp_request_firmware[(]' drivers/gpu/drm/rockchip/cdn-dp-core.c
    accept '[\t]ret[ ]=[ ]cdn_dp_request_firmware[(]dp[)]' drivers/gpu/drm/rockchip/cdn-cp-core.c
    blobname 'netronome[/]nic_%s' drivers/net/ethernet/netronome/nfp/nfp_main.c
    blobname 'spc[ ]-=[ ]snprintf[(][&]fw_name\[ARRAY_SIZE[(]fw_name[)][ ]-[ ]spc\][,][^;]*[)]' drivers/net/ethernet/netronome/nfp/nfp_main.c
    blobname 'netronome[/]nic_AMDA00\(81-0001_\(1x40\|4x10\)\|96-0001_2x10\|97-0001_\(2x40\|4x10_1x40\|8x10\)\|99-0001_2x\(10\|25\)\)\.nffw' drivers/net/ethernet/netronome/nfp/nfp_main.c
    accept '#define[ ]NFP_RESOURCE_NFP_NFFW[ \t]*["]nfp\.nffw["]' drivers/net/ethernet/netronome/nfp/nfp.h
    accept '[\t]*\(rc[ ]=[ ]\)\?wil_request_firmware[(]wil[,][ ]\(wil->wil_fw_name\|WIL_BOARD_FILE_NAME\)[,][ ]\(true\|false\)[)][;]' drivers/net/wireless/ath/wil6210/main.c
    blobname 'gsl3670-cube-iwork8-air\.fw' drivers/platform/x86/silead_dmi.c
    blobname 'gsl3676-jumper-ezpad-mini3\.fw' drivers/platform/x86/silead_dmi.c
    accept '[\t]*\(rc[ ]=[ ]\)\?request_firmware_nowait[(]THIS_MODULE[,][ ]FW_ACTION_NOHOTPLUG[,][ ]name[,]' lib/test_firmware.c
    accept '[ ]*mechanism[ ]is[ ]available[ ]and[ ]for[ ]the[ ]request_firmware_nowait[(][)][ ]call' Documentation/driver-api/firmware/fallback-mechanisms.rst
    accept '[ ]*except[ ]request_firmware_direct[(][)]' Documentation/driver-api/firmware/fallback-mechanisms.rst
    accept '[ ]*today[.][ ]The[ ]call[ ]request_firmware_nowait[(][)]' Documentation/driver-api/firmware/fallback-mechanisms.rst
    accept '[ ]*argument[ ]to[ ]request_firmware_nowait[(][)]' Documentation/driver-api/firmware/fallback-mechanisms.rst
    accept '[ ]*for[ ]request_firmware_nowait[(][)][ ]when[ ]uevent' Documentation/driver-api/firmware/fallback-mechanisms.rst
    accept '[ ]*supported[ ]for[ ]request_firmware_into_buf[(][)]' Documentation/driver-api/firmware/fallback-mechanisms.rst
    accept '[ ]*For[ ]details[ ]of[ ]implementation[ ]refer[ ]to[ ]_request_firmware_load[(][)]' Documentation/driver-api/firmware/fallback-mechanisms.rst
    accept '[ ]*Users[ ]of[ ]the[ ]request_firmware_nowait[(][)][ ]call' Documentation/driver-api/firmware/fallback-mechanisms.rst
    accept '[ ]*rely[ ]on[ ]the[ ]uevent[ ]flag[ ]which[ ]can[ ]be[ ]disabled[ ]by[ ]request_firmware_nowait[(][)]' Documentation/driver-api/firmware/fallback-mechanisms.rst
    accept '[ ]*Although[ ]this[ ]can[ ]disable[ ]the[ ]firmware[ ]cache[ ]for[ ]request_firmware_nowait[(][)]' Documentation/driver-api/firmware/fallback-mechanisms.rst
    accept '[ ]*uses[ ]all[ ]synchronous[ ]call[ ]except[ ]:c:func:[`]request_firmware_into_buf[`]' Documentation/driver-api/firmware/firmware_cache.rst
    accept '[ \t]*if[(]request_firmware[(][&]fw_entry[,][ ][$]FIRMWARE[,]' Documentation/driver-api/firmware/firmware_cache.rst
    accept '[ ]*device[ ]\(if[ ]\)*the[ ]second[ ]argument[ ][(]uevent[)][ ]to[ ]request_firmware_nowait[(][)]' Documentation/driver-api/firmware/firmware_cache.rst
    accept '[ ]*introduction[\n][ ]*core[\n][ ]*request_firmware[\n]' Documentation/driver-api/firmware/index.rst
    accept '\([ ]*:functions:[ ]\)\?request_firmware\([ ]API\|\|_direct\|_into_buf\|_nowait\|\)[\n]' Documentation/driver-api/firmware/request_firmware.rst
    accept 'informed[ ]through[ ]the[ ]callback[.][ ]request_firmware_nowait[(][)][ ]cannot' Documentation/driver-api/firmware/request_firmware.rst
    accept 'firmware[.][ ]For[ ]example[ ]if[ ]you[ ]used[ ]request_firmware[(][)][ ]and[ ]it[ ]returns' Documentation/driver-api/firmware/request_firmware.rst
    accept 'If[ ]something[ ]went[ ]wrong[ ]request_firmware[(][)][ ]returns[ ]non-zero' Documentation/driver-api/firmware/request_firmware.rst
    accept 'resume[/]restore[,][ ]but[ ]they[ ]cannot[ ]do[ ]it[ ]by[ ]calling[ ]:c:func:[`]request_firmware[(][)][`]' Documentation/driver-api/pm/notifiers.rst
    accept 'In[ ]this[ ]example[,][ ]the[ ][^\n]*["]ts\.out["]' tools/power/x86/turbostat/turbostat.8
    accept '[\t]if[ ][(][!]snd_card_proc_new[(]hdspm->card[,][ ]["]ports\.\(in\|out\)["][,]' sound/pci/rme9652/hdspm.c
    accept '[ \t]*print[ ]["]cat[ ]["][ ]rd[ ]cfr\[j\][ ][ ]["][/]kvm-test-1-run\.sh\.out["]' tools/testing/selftests/rcutorture/bin/kvm.sh
    # If this actually requests any firmware, it will do so using
    # disabled request_firmware calls elsewhere, but it seems to me
    # that this would just pin and unpin firmware that might have
    # already been requested before.
    accept 'static[ ]int[ ]smu7_request_firmware[(]' drivers/gpu/drm/amd/powerplay/hwmgr/smu7_hwmgr.c
    accept '[\t]\.request_firmware[ ]=[ ]smu7_request_firmware[,]' drivers/gpu/drm/amd/powerplay/hwmgr/smu7_hwmgr.c

    # New in 4.12.
    accept '[ ]*Bit\([ ]*[0-7]\)*' Documentation/input/devices/sentelic.rst
    defsnc 'static[ ]const[ ]struct[ ]hash_testvec[ ]\(ghash\|hmac_sha\(224\|256\)\|aes_xcbc128\|poly1305\|crc32\|crc32c\|bfin_crc\)_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]const[ ]struct[ ]cipher_testvec[ ]\(\(des3_ede\|bf\)_cbc\|\(tf\|cast6\|aes\)_xts\|serpent\(_xts\)\?\|tnepres\|aes\(_cbc\|_ctr_rfc3686\)\?\|x\?tea\|anubis\(_cbc\)\?\|xeta\|camellia_\(cbc\|xts\)\|salsa20_stream\|chacha20\|cts_mode\)_\(enc\|dec\)_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]const[ ]struct[ ]aead_testvec[ ]hmac_sha\(1\|256\|512\|224\|384\)_\(aes\|des3\?\(_ede\)\?\)_cbc_enc_tv_temp\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]const[ ]struct[ ]aead_testvec[ ]\(aes_\(gcm_rfc4106\|ccm_rfc4309\)\|rfc7539\(esp\)\?\)_\(enc\|dec\)_tv_template\[\][ \t]=' crypto/testmgr.h
    defsnc 'static[ ]const[ ]struct[ ]comp_testvec[ ]\(lzo\|lz4\(hc\)\?\)_\(de\)\?comp_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc '[}][ ]segments\[MALIDP_COEFFTAB_NUM_COEFFS\][ ]=' drivers/gpu/drm/arm/malidp_crtc.c
    defsnc 'static[ ]const[ ]u16[ ]dp500_se_scaling_coeffs\[\]\[SE_N_SCALING_COEFFS\][ ]=' drivers/gpu/drm/arm/malidp_hw.c
    defsnc 'static[ ]const[ ]u8[ ]gamma_tbl\[S6E3HA2_NUM_GAMMA_STEPS\]\[S6E3HA2_GAMMA_CMD_CNT\][ ]=' drivers/gpu/drm/panel/panel-samsung-s6e3ha2.c
    defsnc 'static[ ]const[ ]struct[ ]rcar_hdmi_phy_params[ ]rcar_hdmi_phy_params\[\][ ]=' drivers/gpu/drm/rcar-du/rcar_dw_hdmi.c
    defsnc 'static[ ]const[ ]int[ ]temp_map\[CPCAP_MAX_TEMP_LVL\]\[2\][ ]=' drivers/iio/adc/cpcap-adc.c
    defsnc 'static[ ]const[ ]struct[ ]reg_value[ ]ov5645_\(global_init_setting\|setting_\(sxga\|1080p\|full\)\)\[\][ ]=' drivers/media/i2c/ov5645.c
    defsnc 'static[ ]struct[ ]regval_list[ ]ov5647_640x480\[\][ ]=' drivers/media/i2c/ov5647.c
    defsc 'static[ ]const[ ]u32[ ]isc_gamma_table\[GAMMA_MAX[ ][+][ ]1\]\[GAMMA_ENTRIES\][ ]=' drivers/media/platform/atmel/atmel-isc.c
    defsnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_7620\[\][ ]=' drivers/net/wireless/ralink/rt2x00/rt2800lib.c
    defsnc 'static[ ]const[ ]u8[ ]zero_buff\[\][ ]=' drivers/staging/ccree/ssi_cipher.c
    oprepline '#define[ ]NIST_\(AES\([CG]CM\)\?\|SHA\|HMAC\)_\(SHA\)\?\(256\|512\|192\|128\|1\)_\(XTS_\|CMAC_\)\?\(KEY\|PLAIN\(_DATA\)\?\|CIPHER\|MD\|MSG\|ADATA\)' drivers/staging/ccree/ssi_fips_data.h
    defsnc 'static[ ]struct[ ]atomisp_css_macc_table[ ]\(skin_\(low\|medium\|high\)\|blue\|green\)_macc_table[ ]=' drivers/staging/media/atomisp/pci/atomisp2/atomisp_tables.h
    defsnc 'static[ ]struct[ ]atomisp_css_ctc_table[ ]vivid_ctc_table[ ]=' drivers/staging/media/atomisp/pci/atomisp2/atomisp_tables.h
    defsnc '#define[ ]S_1W_\(6X6\|9X9\|7X7\)_MATRIX_DEFAULT[ ][(][(]s_1w_.x._matrix[)][\\]' drivers/staging/media/atomisp/pci/atomisp2/css2400/hive_isp_css_include/host/ref_vector_func_types.h
    defsnc 'const[ ]struct[ ]ia_css_anr_config[ ]default_anr_config[ ]=' drivers/staging/media/atomisp/pci/atomisp2/css2400/isp/kernels/anr/anr_1.0/ia_css_anr.host.c
    defsnc 'const[ ]struct[ ]ia_css_anr_thres[ ]default_anr_thres[ ]=' drivers/staging/media/atomisp/pci/atomisp2/css2400/isp/kernels/anr/anr_2/ia_css_anr2_table.host.c
    defsnc 'default_ctc_table_data\[IA_CSS_VAMEM_[21]_CTC_TABLE_SIZE\][ ]=' drivers/staging/media/atomisp/pci/atomisp2/css2400/isp/kernels/ctc/ctc_1.0/ia_css_ctc_table.host.c
    defsnc 'default_gamma_table_data\[IA_CSS_VAMEM_[21]_GAMMA_TABLE_SIZE\][ ]=' drivers/staging/media/atomisp/pci/atomisp2/css2400/isp/kernels/gc/gc_1.0/ia_css_gc_table.host.c
    defsnc 'default_gamma_table_data\[IA_CSS_VAMEM_[21]_RGB_GAMMA_TABLE_SIZE\][ ]=' drivers/staging/media/atomisp/pci/atomisp2/css2400/isp/kernels/gc/gc_2/ia_css_gc2_table.host.c
    defsnc 'const[ ]struct[ ]ia_css_macc1_5_table[ ]default_macc1_5_table[ ]=' drivers/staging/media/atomisp/pci/atomisp2/css2400/isp/kernels/macc/macc1_5/ia_css_macc1_5_table.host.c
    defsnc 'const[ ]struct[ ]ia_css_macc_table[ ]default_macc2\?_table[ ]=' drivers/staging/media/atomisp/pci/atomisp2/css2400/isp/kernels/macc/macc_1.0/ia_css_macc_table.host.c
    defsc '#define[ ]DEFAULT_DVS_GRID_INFO[ ]' drivers/staging/media/atomisp/pci/atomisp2/css2400/isp/kernels/sdis/common/ia_css_sdis_common_types.h
    defsnc 'const[ ]int16_t[ ]g_pyramid\[8\]\[8\][ ]=' drivers/staging/media/atomisp/pci/atomisp2/css2400/isp/kernels/tdf/tdf_1.0/ia_css_tdf.host.c
    defsnc 'static[ ]const[ ]int[ ]zoom_table\[4\]\[HRT_GDC_N\][ ]=' drivers/staging/media/atomisp/pci/atomisp2/css2400/sh_css_params.c
    defsnc '[\t]static[ ]\+u8[ ]sbox_table\[256\][ ]=' drivers/staging/rtl8723bs/core/rtw_security.c
    defsnc 'static[ ]u32[ ]Array_MP_8723B_\(AGC_TAB\|PHY_REG\(_PG\)\?\)\[\][ ]=' drivers/staging/rtl8723bs/hal/HalHWImg8723B_BB.c
    defsnc 'static[ ]u32[ ]Array_MP_8723B_MAC_REG\[\][ ]=' drivers/staging/rtl8723bs/hal/HalHWImg8723B_MAC.c
    defsnc 'static[ ]u32[ ]Array_MP_8723B_RadioA\[\][ ]=' drivers/staging/rtl8723bs/hal/HalHWImg8723B_RF.c
    defsnc 'static[ ]u8[ ]gDeltaSwingTableIdx_MP_5G[BA]_[NP]_TxPowerTrack_SDIO_8723B\[\]\[DELTA_SWINGIDX_SIZE\][ ]=' drivers/staging/rtl8723bs/hal/HalHWImg8723B_RF.c
    defsnc '[\t]u8[ ]channel5G\[CHANNEL_MAX_NUMBER_5G\][ ]=' drivers/staging/rtl8723bs/hal/hal_com_phycfg.c
    defsc 'static[ ]struct[ ]cs35l35_sysclk_config[ ]cs35l35_clk_ctl\[\][ ]=' sound/soc/codecs/cs35l35.c
    blobname 'amdgpu[/]vega10_smc\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_cgs.c
    blobname 'amdgpu[/]vega10_uvd\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_uvd.c
    blobname 'amdgpu[/]vega10_vce\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vce.c
    blobname 'amdgpu[/]vega10_\(ce\|pfp\|me\(c2\?\)\?\|rlc\)\.bin' drivers/gpu/drm/amd/amdgpu/gfx_v9_0.c
    blobname 'amdgpu[/]\(vega10\|%s\)_\(sos\|asd\)\.bin' drivers/gpu/drm/amd/amdgpu/psp_v3_1.c
    blobname 'amdgpu[/]vega10_sdma1\?\.bin' drivers/gpu/drm/amd/amdgpu/sdma_v4_0.c
    blobname 'amdgpu[/]vega10_smc\.bin' drivers/gpu/drm/amd/amdgpu/soc15.c
    blobname 'i915[/]glk_dmc_ver1_04\.bin' drivers/gpu/drm/i915/intel_csr.c
    blobname 'https[:][/][/]01\.org[/]linuxgraphics[/]downloads[/][^"\n]*' drivers/gpu/drm/i915/intel_csr.c
    blobname 'dvb-demod-si2168-d60-01\.fw' drivers/media/dvb-frontends/si2168_priv.h
    blobname 'dvb-tuner-si2141-a10-01\.fw' drivers/media/tuners/si2157_priv.h
    blobname 'firmware-6\.bin' drivers/net/wireless/ath/ath10k/hw.h
    blobname '[/][*][ ]the[ ]firmware-6\.bin[ ]blob[ ][*][/]' drivers/net/wireless/ath/ath10k/hw.h
    blobname 'iwlwifi-9260-th-b0-\(jf\|lc\)-b0-' drivers/net/wireless/intel/iwlwifi/iwl-9000.c
    blobname 'iwlwifi-QuIcp-a0-hrcdb-a0-' drivers/net/wireless/intel/iwlwifi/iwl-a000.c
    blobname 'git:[/][/]git\.kernel\.org[/][^"\n]*firmware\.git' drivers/net/wireless/intel/iwlwifi/iwl-drv.c
    blobname 'rtlwifi[/]rtl8723befw_36\.bin' drivers/net/wireless/realtek/rtlwifi/rtl8723be/sw.c
    blobname 'rtlwifi[/]rtl8821aefw_29\.bin' drivers/net/wireless/realtek/rtlwifi/rtl8821ae/sw.c
    blobname 'gsl1686-dexp-ursus-7w\.fw' drivers/platform/x86/silead_dmi.c
    blobname 'gsl1686-surftab-wintron70-st70416-6\.fw' drivers/platform/x86/silead_dmi.c
    blobname 'ti-connectivity[/]TIInit_\(\(%d\|[0-9]\+\)[.]\)\+bts' drivers/bluetooth/hci_ll.c
    accept '[\t]*bt_dev_err[(]lldev->hu\.hdev[,][ ]["]request_firmware[ ]failed' drivers/bluetooth/hci_ll.c
    blobname 'nokia[/]\(bcmfw\|ti1273\)\.bin' drivers/bluetooth/hci_nokia.c
    accept '[\t ]*falcon->firmware\.\(bin_data\|firmware\)' drivers/gpu/drm/tegra/falcon.c
    accept '[\t][/][*][ ]request_firmware[ ]prints' drivers/gpu/drm/tegra/falcon.c
    accept 'static[ ]const[ ]struct[ ]vic_config[ ]vic_t\(124\|210\)_config[ ]=[ ][{][\n][	]\.firmware[ ]*=[ ]' drivers/gpu/drm/tegra/vic.c
    blobname 'nvidia[/]tegra124[/]vic03_ucode\.bin' drivers/gpu/drm/tegra/vic.c
    blobname 'nvidia[/]tegra210[/]vic04_ucode\.bin' drivers/gpu/drm/tegra/vic.c
    accept 'static[ ]int[ ]ap1302_request_firmware[(]' drivers/staging/media/atomisp/i2c/ap1302.c
    accept '[\t ]*["]ap1302_request_firmware[ ]failed' drivers/staging/media/atomisp/i2c/ap1302.c
    accept '[\t]ret[ ]=[ ]ap1302_request_firmware[(]' drivers/staging/media/atomisp/i2c/ap1302.c
    blobname 'ap1302_fw\.bin' drivers/staging/media/atomisp/i2c/ap1302.c
    blobname 'shisp_2401a0_\(legacy_\)\?v21\.bin' drivers/staging/media/atomisp/pci/atomisp2/atomisp_v4l2.c
    blobname 'shisp_2400b0_v21\.bin' drivers/staging/media/atomisp/pci/atomisp2/atomisp_v4l2.c
    accept '[\t]*isp->firmware[ ]=[ ]\(atomisp_load_firmware[(]\|NULL\)' 'drivers/staging/media/atomisp/pci/atomisp2/atomisp_\(fops\|v4l2\)\.c'
    accept '[\t]stage_desc->firmware[ ]=' drivers/staging/media/atomisp/pci/atomisp2/css2400/camera/pipe/src/pipe_stagedesc.c
    accept '[\t]stage->firmware[ ]=' drivers/staging/media/atomisp/pci/atomisp2/css2400/runtime/pipeline/src/pipeline.c
    blobname 'rtlwifi[/]rtl8723bs_\(wowlan\|nic\)\.bin' drivers/staging/rtl8723bs/hal/rtl8723b_hal_init.c
    blobname 'rtl8723b[/]FW_\(NIC\|WoWLAN\)\.bin' drivers/staging/rtl8723bs/include/rtl8723b_hal.h

    # New in 4.13
    accept '[ ]*This[ ]driver[ ]requires[ ]a[ ]patch[ ]for[ ]firmware_class\.c[^\n]*[\n][ ]*request_firmware_nowait[ ]function' Documentation/dell_rbu.txt
    accept '[\t][ ]d=["]m[ ]0[,]0[ ]0[,]1895[ ]4118[,]0[ ][-0-9, LZm]*z["]' Documentation/media/uapi/v4l/crop.svg
    defsnc 'static[ ]const[ ]struct[ ]akcipher_testvec[ ]pkcs1pad_rsa_tv_template\[\][ ]=' crypto/testmgr.h
    accept '[\t]ret[ ]=[ ]_request_firmware_load[(]fw_priv[,][ ]opt_flags[,][ ]timeout[)][;]' drivers/base/firmware_class.c
    defsnc 'static[ ]const[ ]struct[ ]cpg_pll_config[ ]cpg_pll_configs\[8\][ ]__initconst[ ]=' drivers/clk/renesas/clk-rcar-gen2.c
    blobname 'cnn55xx_se.fw' drivers/crypto/cavium/nitrox/nitrox_main.c
    defsnc 'unsigned[ ]int[ ]dsgl_ent_len\[\][ ]=' drivers/crypto/chelsio/chcr_algo.h
    blobname '\(ifpp\|ipue\)\.bin' drivers/crypto/inside-secure/safexcel.c
    blobname 'amdgpu[/]\(%s\|vega10\|raven\)_gpu_info\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_device.c
    blobname 'amdgpu[/]raven_vcn\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vcn.c
    blobname 'amdgpu[/]raven_\(ce\|pfp\|me\(c2\?\)\?\|rlc\)\.bin' drivers/gpu/drm/amd/amdgpu/gfx_v9_0.c
    blobname 'amdgpu[/]\(vega10\|raven\)_sdma1\?\.bin' drivers/gpu/drm/amdgpu/sdma_v4_0.c
    defsnc 'const[ ]struct[ ]pctl_data[ ]pctl[01]_data\[\][ ]=' drivers/gpu/drm/amd/amdgpu/mmhub_v1_0.c
    blobname 'i915[/]cnl_dmc_ver1_04\.bin' drivers/gpu/drm/i915/intel_csr.c
    defsnc '[\t]static[ ]const[ ]int[ ]dividers\[\][ ]=' drivers/gpu/drm/i915/intel_dpll_mgr.c
    defsnc 'const[ ]struct[ ]stm32h7_adc_ck_spec[ ]stm32h7_adc_ckmodes_spec\[\][ ]=' drivers/iio/adc/stm32-adc-core.c
    defsnc 'static[ ]const[ ]u8[ ]full_fm_\(eu\|na\)_1p0\[\][ ]=' drivers/media/i2c/max2175.c
    defsnc 'static[ ]const[ ]struct[ ]max2175_reg_map[ ]\(dab12\|fmeu1p2\|fmna[12]p0\)_map\[\][ ]=' drivers/media/i2c/max2175.c
    defsnc 'static[ ]const[ ]u8[ ]adc_presets\[2\]\[23\][ ]=' drivers/media/i2c/max2175.c
    defsnc 'static[ ]const[ ]struct[ ]ov13858_reg[ ]mode_\(4224x3136\|2112x\(1568\|1188\)\|1056x784\)_regs\[\][ ]=' drivers/media/i2c/ov13858.c
    defsnc 'static[ ]const[ ]struct[ ]reg_value[ ]ov5640_\(init_\)\?setting_\(30\|15\)fps_\(VGA\(_640_480\)\?\|XGA_1024_768\|QVGA_320_240\|QCIF_176_144\|NTSC_720_480\|PAL_720_576\|720P_1280_720\|1080P_1920_1080\|QSXGA_2592_1944\)\[\][ ]=' drivers/media/i2c/ov5640.c
    blobname 'qcom[/]venus-\(1\.8\|4\.2\)[/]venus\.mdt' drivers/media/platform/qcom/venus/core.c
    # The firmware file name is supplied by the user.
    accept '[\t]err[ ]=[ ]request_firmware_direct[(][&]fw[,][ ]flash->data[,]\([^\n]*[\n]\+[^\n}]\)*err[ ]=[ ]mlx5_firmware_flash[(]mdev[,][ ]fw[)]' drivers/net/ethernet/mellanox/mlx5/core/en_ethtool.c
    blobname 'mellanox[/]mlxsw_spectrum-\([0-9.]*\|["]\([ \t]*\|[\\][\n]\|__stringify[(]MLXSW_FWREV_\(MAJOR\|MINOR\|SUBMINOR\)[)]\|["].["]\)*["]\)\.mfa2' drivers/net/ethernet/mellanox/mlxsw/spectrum.c
    # This firmware file name is supplied by the user,
    # but there's another in the same source file (above) that is hardcoded.
    accept '[\t]err[ ]=[ ]request_firmware_direct[(][&]firmware[,][ ]flash->data[,]\([^\n]*[\n]\+[^\n}]\)*err[ ]=[ ]mlxsw_sp_firmware_flash[(]mlxsw_sp[,][ ]firmware[)]' drivers/net/ethernet/mellanox/mlxsw/spectrum.c
    defsnc 'static[ ]const[ ]struct[ ]iro[ ]iro_arr\[49\][ ]=' drivers/net/ethernet/qlogic/qed/qed_hsi.h
    defsc 'static[ ]const[ ]u8[ ]iwl_ext_nvm_channels\[\][ ]=' drivers/net/wireless/intel/iwlwifi/iwl-nvm-parse.c
    blobname '\(rsi[/]\)\?rs9113_wlan_qspi\.rps' drivers/net/wireless/rsi/rsi_common.h
    defsnc '[}][ ]hsfreq_map\[\][ ]=' drivers/staging/media/imx/imx6-mipi-csi2.c
    defsnc 'static[ ]const[ ]u16[ ]avc_thr_db2reg\[97\][ ]=' sound/soc/codecs/sgtl5000.c
    blob 'SD8688[ ]firmware[\n]=*[\n]*Images:[\n]*\(-[ ][/]lib[/]firmware[^\n]*[\n]*\)*The[ ]images[^:]*:[\n]*[^\n]*[/]linux-firmware[^\n]*' Documentation/btmrvl.txt
    blobname '%s-%s-%d\.bin' drivers/net/wireless/ath/ath10k/core.c
    blobname 'wil6210_\(sparrow_plus_\)\?ftm\.fw' drivers/net/wireless/ath/wil6210/wil6210.h
    blobname 'brcmfmac43430a0-sdio\.bin' drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
    blobname 'iwlwifi-9000-pu-a0-jf-b0-' drivers/net/wireless/intel/iwlwifi/cfg/9000.c
    blobname 'iwlwifi-QuIcp-z0-hrcdb-a0-' drivers/net/wireless/intel/iwlwifi/iwl-a000.c
    blobname 'qtn[/]fmac_qsr10g\.img' drivers/net/wireless/quantenna/qtnfmac/qtn_hw_ids.h
    blobname 'gsl1680-\(gp-electronic-t701\|pipo-w2s\)\.fw' drivers/platform/x86/silead_dmi.c
    blobname 'gsl3692-pov-mobii-wintab-p800w\.fw' drivers/platform/x86/silead_dmi.c
    blobname 'gsl3670-itworks-tw891\.fw' drivers/platform/x86/silead_dmi.c
    defsnc 'struct[ ]phm_fuses_default[ ]vega10_fuses_default\[\][ ]=' drivers/gpu/drm/amd/powerplay/hwmgr/pp_overdriver.c
    blobname 'a530_zap\.mdt' drivers/gpu/drm/msm/adreno/adreno_device.c
    accept '[\t]\(complete\|init_completion\|[\t]wait_for_completion\)[(][&]bus->request_firmware_complete[)]' drivers/net/wireless/quantenna/qtnfmac/pearl/pcie.c
    accept '[\t]ret[ ]=[ ]reject_firmware_nowait[(][^)]*[,][ ]qtnf_firmware_load[)][;][\n][\t]*if[ ][(]ret[ ][<][ ]0[)][\n][\t]*pr_err[(]["]request_firmware_nowait[ ]error' drivers/net/wireless/quantenna/qtnfmac/pearl/pcie.c
    blobname '\(adsp\|slpi\)\.mdt' drivers/remoteproc/qcom_adsp_pil.c
    blobname 'wcnss\.mdt' drivers/remoteproc/qcom_wcnss.c

    # New in 4.14 (up to rc5).
    blobname 'amdgpu[/]vega10_acg_smc\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_cgs.c
    blobname '\(netronome[/]\)\?\(serial-\(%pMF-%02hhx-%02hhx\|[-0-9a-f]*\)\|pci-\(%s\|[0-9a-f:.]*\)\)\.nffw' drivers/net/ethernet/netronome/nfp/nfp_main.c
    blobname 'brcmfmac4373-sdio\.bin' drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
    blobname 'brcmfmac4373\.bin' drivers/net/wireless/broadcom/brcm80211/brcmfmac/usb.c
    blobname 'iwlwifi-QuQnj-\([af]0-hr-a0\|a0-jf-b0\)-' drivers/net/wireless/intel/iwlwifi/cfg/a000.c
    blobname 'rt5514_dsp_fw3\.bin' sound/soc/codecs/rt5514.h
    blobname 'intel[/]dsp_fw_cnl\.bin' sound/soc/intel/skylake/skl.c
    initnc '__aes_arm\(64\)\?_inverse_sbox:[\n][\t]\.byte[ \t]*' arch/arm/crypto/aes-cipher-core.S
    defsnc 'static[ ]const[ ]struct[ ]hsdk_pll_cfg[ ]asdt_pll_cfg\[\][ ]=' drivers/clk/clk-hsdk-pll.c
    defsnc 'static[ ]const[ ]struct[ ]clk_div_table[ ]d1cpre_div_table\[\][ ]=' drivers/clk/clk-stm32h7.c
    defsnc 'static[ ]const[ ]struct[ ]pctl_data[ ]pctl[01]_data\[\][ ]=' drivers/gpu/drm/amd/amdgpu/mmhub_v1_0.c
    defsnc '[\t]static[ ]const[ ]u16[ ]map\[\][ ]=' drivers/hwmon/asc7621.c
    defsc 'static[ ]const[ ]struct[ ]stm32h7_adc_ck_spec[ ]stm32h7_adc_ckmodes_spec\[\][ ]=' drivers/iio/adc/stm32-adc-core.c
    defsnc 'static[ ]const[ ]int[ ]srf08_sensitivity_avail\[\][ ]=' drivers/iio/proximity/srf08.c
    defsc 'static[ ]const[ ]struct[ ]slookup[ ]\(lnagain_\(nf\|iip3\)\|gain_\(rfagc\|channel_agc_\(nf\|iip3\)\)\)_lookup\[\][ ]=' drivers/media/dvb-frontends/stv6111.c
    defsnc 'static[ ]const[ ]struct[ ]ov5670_reg[ ]mode_\(2592x1944\|1296x972\|648x486\|2560x1440\|1280x720\|640x360\)_regs\[\][ ]=' drivers/media/i2c/ov5670.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]\(gnd\|dram\|pci\|pflash\)_351[26]_pins\[\][ ]=' drivers/pinctrl/pinctrl-gemini.c
    defsc 'static[ ]const[ ]unsigned[ ]int[ ]pflash_351[26]_pins_extended\[\][ ]=' drivers/pinctrl/pinctrl-gemini.c
    defsnc 'static[ ]const[ ]u16[ ]db_invert_table\[12\]\[8\][ ]=' drivers/staging/rtlwifi/phydm/phydm.c
    defsc 'u32[ ]cck_swing_table_ch1_ch14_8723d\[CCK_TABLE_SIZE_8723D\][ ]=' drivers/staging/rtlwifi/phydm/phydm_powertracking_ce.c
    defsc 'u32[ ]cck_swing_table_ch1_ch14_8710b\[CCK_TABLE_SIZE_8710B\][ ]=' drivers/staging/rtlwifi/phydm/phydm_powertracking_ce.c
    defsnc 'static[ ]u32[ ]array_mp_8822b_\(agc_tab\|phy_reg\(_pg\)\?\|mac_reg\|radio[ab]\)\[\][ ]=' drivers/staging/rtlwifi/phydm/rtl8822b/halhwimg8822b_bb.c
    defsnc 'static[ ]u8[ ]delta_swing_index_mp_5g[ba]_[np]_txpwrtrack_\(type[01246789]_\|type3_type5_\)\?8822b[\n\t ]*\[\]\[DELTA_SWINGIDX_SIZE\][ ]=' drivers/staging/rtlwifi/phydm/rtl8822b/halhwimg8822b_rf.c
    defsnc 'static[ ]const[ ]struct[ ]tsadc_table[ ]rk3328_code_table\[\][ ]=' drivers/thermal/rockchip_thermal.c
    defsnc 'static[ ]const[ ]BYTE[ ]LL_Code\[64\][ ]=' lib/zstd/compress.c
    defsnc 'static[ ]const[ ]BYTE[ ]ML_Code\[128\][ ]=' lib/zstd/compress.c
    defsc 'static[ ]const[ ]FSE_decode_t4[ ]LL_defaultDTable\[[(]1[ ][<][<][ ]LL_DEFAULTNORMLOG[)][ ][+][ ]1\][ ]=' lib/zstd/decompress.c
    defsc 'static[ ]const[ ]FSE_decode_t4[ ]ML_defaultDTable\[[(]1[ ][<][<][ ]ML_DEFAULTNORMLOG[)][ ][+][ ]1\][ ]=' lib/zstd/decompress.c
    defsc 'static[ ]const[ ]FSE_decode_t4[ ]OF_defaultDTable\[[(]1[ ][<][<][ ]OF_DEFAULTNORMLOG[)][ ][+][ ]1\][ ]=' lib/zstd/decompress.c
    defsnc '[\t]static[ ]const[ ]U32[ ][LM]L_base\[Max[LM]L[ ][+][ ]1\][ ]=' lib/zstd/decompress.c
    defsnc 'static[ ]const[ ]U32[ ][LM]L_bits\[Max[LM]L[ ][+][ ]1\][ ]=' lib/zstd/zstd_internal.h
    defsnc 'static[ ]const[ ]S16[ ][LM]L_defaultNorm\[Max[LM]L[ ][+][ ]1\][ ]=' lib/zstd/zstd_internal.h
    defsnc 'static[ ]const[ ]struct[ ]cs43130_pll_params[ ]pll_ratio_table\[\][ ]=' sound/soc/codecs/cs43130.c
    defsnc 'static[ ]const[ ]struct[ ]reg_sequence[ ]pcm_ch_\(en\|dis\)_seq\[\][ ]=' sound/soc/codecs/cs43130.c
    defsnc 'static[ ]const[ ]struct[ ]cs43130_clk_gen[ ]cs43130_\(16\|32\|48\|64\)_clk_gen\[\][ ]=' sound/soc/codecs/cs43130.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt274_\(index_def\|reg\)\[\][ ]=' sound/soc/codecs/rt274.c
    accept '[\t]report_missing_free_firmware[^\n]*[\n][\t]retval[ ]=[ ]request_firmware_into_buf[(][&]xfw[,][ ]NONFREE_FIRMWARE' include/linux/firmware.h
    accept '[\t]if[ ][(]is_nonfree_firmware[^\n]*[\n][\t][\t]return[ ]reject_firmware_into_buf[^\n]*[\n][\t]else[\n][\t][\t]return[ ]request_firmware_into_buf[(]firmware_p[,][ ]name[,]' include/linux/firmware.h
    accept '[#]define[ ]TEST_FIRMWARE_NAME[\t]["]test-firmware\.bin["]' lib/test_firmware.c
    accept '[ ][*][\t]request_firmware_direct[(][)][ ]will[ ]be[ ]used[ ]instead' lib/test_firmware.c
    accept '[ ][*][\t]of[ ]the[ ]request_firmware[*][(][)][ ]calls[ ]used[ ]in[ ]their[ ]tests' lib/test_firmware.c
    accept '[ ][*][\t]request_firmware_direct[(][)][,][ ]otherwise[ ]request_firmware[(][)]' lib/test_firmware.c
    accept '[\t]*test_fw_config->req_firmware[ ]=[ ]\(test_fw_config->sync_direct[ ][?][\n][ \t]*request_firmware_direct[ ][:][\n][ \t]*\)\?request_firmware[;]' lib/test_firmware.c
    accept '[\t][\t]req->name[ ]=[ ]test_fw_config->name[;][\n][\t][\t]req->fw[ ]=[ ]NULL[;][\n][\t][\t]req->idx[ ]=[ ]i[;][\n][\t][\t]init_completion[(][&]req->completion[)][;][\n][\t][\t]rc[ ]=[ ]request_firmware_nowait[(]THIS_MODULE[,][ ]\([^);, \t\n]*[,][ \t\n]*\)*trigger_batched_cb[)][;]' lib/test_firmware.c
    accept '[\t]release_firmware[(]test_firmware[)][;][\n][\t]test_firmware[ ]=[ ]NULL[;][\n][\t]rc[ ]=[ ]request_firmware_nowait[(]THIS_MODULE[,][ ]1[,][ ]name[^)\n]*[\n][ \t]*NULL[,][ ]trigger_async_request_cb[)]' lib/test_firmware.c
    accept '[#][ ]name:[ ]test-firmware\.bin' tools/testing/selftests/firmware/fw_filesystem.sh
    accept '[\t]*test_\(batched_\)\?request_firmware\(_direct\|_nowait_\(uevent\|custom\)\)\?\(_nofile\)\?\([(][)]\|[ ][$]i\)' tools/testing/selftests/firmware/fw_filesystem.sh
    accept '[\t]echo[ ]-n[ ]["]Batched[ ]request_firmware\(_direct\|_nowait\)\?[(]\(uevent=\(true\|false\)\)\?[)][ ]\(nofile[ ]\)\?try[ ]#[$]1:[ ]["]' tools/testing/selftests/firmware/fw_filesystem.sh
    accept '[\t]\(config_set_name\|test_wait_and_cancel_custom_load\)[ ]nope-test-firmware\.bin' tools/testing/selftests/firmware/fw_filesystem.sh
    blobname 'amdgpu[/]%s_asd\.bin' drivers/gpu/drm/amd/amdgpu/psp_v10_0.c
    blobname 'lantiq[/]xrx[23]00_phy\(22f\|11g\)_a\(14\|2[21]\)\.bin' drivers/soc/lantiq/gphy.c
    blobname 'rtlwifi[/]rtl8822befw\.bin' drivers/staging/rtlwifi/rtl8822be/sw.c
    # This loads a file named by the user.
    accept '[\t]const[ ]char[ ][*]name[ ]=[ ]i915\.vbt_firmware[;][\n][\t]int[ ]ret[;][\n][\n][\t]if[ ][(]!name[ ][|][|][ ][!][*]name[)][\n][\t][\t]return[ ]-ENOENT[;][\n][\n][\t]ret[ ]=[ ]request_firmware[(][&]fw[,][ ]name[,]' drivers/gpu/drm/i915/intel_opregion.c
    # New in 4.14-rc6.
    defsnc '[\t]static[ ]const[ ]struct[ ]nphy_txiqcal_ladder[ ]ladder_\(lo\|iq\)\[\][ ]=' drivers/net/wireless/brcm80211/brcmsmac/phy/phy_n.c
    # New in 4.14.3.  When using python for deblobbing (default), this
    # pattern appears too late.  An earlier pattern that matches
    # iwlwifi-9000 alone and starts with 'iwlwifi-9000\(' needed
    # adjusting as well.
    blobname 'iwlwifi-9000-pu-b0-jf-b0-' drivers/net/wireless/intel/iwlwifi/cfg/9000.c

    # New in 4.15 (up to rc6).
    accept '[\t]*0[ ][ ][/][*]1\([ ][ ][23456]\)*[*][/]\([ ][ ][789]\)*\([\n][\t]*\([ ]*[1-9][0-9]*\)*\)*[\n][\t]*100' arch/arm/boot/dts/imx6q-pistachio.dts
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]table\[\][ ]=' arch/mips/math-emu/dp_sqrt.c
    defsnc 'const[ ]u8[ ]sm3_zero_message_hash\[SM3_DIGEST_SIZE\][ ]=' crypto/sm3_generic.c
    defsc 'static[ ]const[ ]struct[ ]hash_testvec[ ]sm3_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]const[ ]struct[ ]rcar_gen3_cpg_pll_config[ ]cpg_pll_configs\[8\][ ]__initconst[ ]=' drivers/clk/renesas/r8a77970-cpg-mssr.c
    defsnc 'unsigned[ ]int[ ]sgl_ent_len\[\][ ]=' drivers/crypto/chelsio/chcr_algo.h
    defsc 'static[ ]const[ ]struct[ ]pte_setting[ ]pte_settings\[mi_tiling_count\]\[mi_bpp_count\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_mem_input.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_4tap_16p_\(upscale\|117\|150\|183\)\[36\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_2tap_64p\[66\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_3tap_64p_\(upscale\|117\|150\|183\)\[99\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_4tap_64p_\(upscale\|117\|150\|183\)\[132\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_5tap_64p_\(upscale\|117\|150\|183\)\[165\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_6tap_64p_\(upscale\|117\|150\|183\)\[198\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_7tap_64p_\(upscale\|117\|150\|183\)\[231\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_8tap_64p_\(upscale\|117\|150\|183\)\[264\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]struct[ ]audio_clock_info[ ]audio_clock_info_table\[16\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_stream_encoder.c
    defsnc 'static[ ]const[ ]struct[ ]audio_clock_info[ ]audio_clock_info_table_\(36\|48\)bpc\[14\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_stream_encoder.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]dvmm_Hw_Setting_\(2DTiling\|Linear\)\[4\]\[9\][ ]=' drivers/gpu/drm/amd/display/dc/dce110/dce110_mem_input_v.c
    defsnc 'static[ ]const[ ]struct[ ]phm_fuses_default[ ]vega10_fuses_default\[\][ ]=' drivers/gpu/drm/amd/powerplay/hwmgr/pp_overdriver.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]soft_dummy_pp_table\[\][ ]=' drivers/gpu/drm/amd/powerplay/hwmgr/processpptables.c
    accept 'static[ ]const[ ]PWR_DFY_Section[ ]pwr_virus_section[123456][ ]=[ ][{]\([\n][\t]\.dfy_\(cntl\|addr_\(hi\|lo\)\)[ ]=[ ]0x[0-9a-f]*[,]\)*[\n][\t]\.dfy_data[ ]=[ ][{]\([\n]\([ \t]0x[0-9a-f]*[,]\)*\)*[\n][\t][}][,][\n][\t]\.dfy_size[ ]=[ ][0-9]*[\n][}][;]' drivers/gpu/drm/amd/powerplay/inc/polaris10_pwrvirus.h
    defsnc 'static[ ]const[ ]struct[ ]kx_odr_map[ ]samp_freq_table\[\][ ]=' drivers/iio/accel/kxcjk-1013.c
    defsc 'static[ ]const[ ]struct[ ]reg_8[ ]imx274_\(mode\(1_3840x2160\|3_1920x1080\|5_1280x720\)_raw10\|start_2\)\[\][ ]=' drivers/media/i2c/imx274.c
    defsnc '[\t]static[ ]const[ ]unsigned[ ]char[ ]\(y\|uv\)QuanTable51[18]\[\][ ]=' drivers/media/usb/gspca/ov519.c
    defsnc 'static[ ]const[ ]u32[ ]t5_tp_mib_index_array\[9\]\[IREG_NUM_ELEM\][ ]=' drivers/net/ethernet/chelsio/cxgb4/cudbg_entity.h
    defsnc 'static[ ]const[ ]struct[ ]tsadc_table[ ]rv1108_table\[\][ ]' drivers/thermal/rockchip_thermal.c
    initnc '[/][*][ ]Seth[ ]Forshee.s[ ]regdb[ ]certificate[ ][*][/]' net/wireless/certs/sforshee.hex
    initnc '\(Read\|Fill\)[ ]buffer[ ]content:' tools/testing/selftests/android/ion/README
    blobname 'amdgpu[/]%s_\(pfp\|[mc]e\|mec2\?\)_2\.bin' drivers/gpu/drm/amd/amdgpu/gfx_v8_0.c
    blobname 'nvidia[/]tegra186[/]vic04_ucode\.bin' drivers/gpu/drm/tegra/vic.c
    accept 'static[ ]const[ ]struct[ ]vic_config[ ]vic_t186_config[ ]=[ ][{][\n][\t]\.firmware[ ]=[ ]NVIDIA_TEGRA_186_VIC_FIRMWARE[,]' drivers/gpu/drm/tegra/vic.c
    blobname 'gsl3680-chuwi-hi8-pro\.fw' drivers/platform/x86/silead_dmi.c
    blobname 'gsl1686-digma_citi_e200\.fw' drivers/platform/x86/silead_dmi.c
    accept '[/][*][ ]code[ ]to[ ]directly[ ]load[ ]a[ ]firmware[ ]database[ ]through[ ]request_firmware[ ][*][/]' net/wireless/reg.c
    accept '[\t]if[ ][(]request_firmware[(][&]sig[,][ ]["]regulatory\.db\.p7s["][,]' net/wireless/reg.c
    accept '[\t]return[ ]request_firmware_nowait[(]THIS_MODULE[,][ ]true[,][ ]["]regulatory\.db["][,]' net/wireless/reg.c
    accept '[\t]err[ ]=[ ]request_firmware[(][&]fw[,][ ]["]regulatory\.db["][,]' net/wireless/reg.c
    accept '[\t][ ][*][ ]the[ ]new[ ]path[,][ ]using[ ]request_firmware_direct[(][)]' drivers/gpu/drm/msm/adreno/adreno_gpu.h
    accept '[\t][ ][*][ ]finally[ ]fall[ ]back[ ]to[ ]request_firmware[(][)]' drivers/gpu/drm/msm/adreno/adreno_gpu.h
    blobname 'hideep_ts_\(%04x\|[0-9a-f]*\)\.bin' drivers/input/touchscreen/hideep.c
    blobname 'dpfe\.bin' drivers/memory/brcmstb_dpfe.c
    accept '[\t]err[ ]=[ ]request_firmware[(][&]clm[,][ ]clm_name[,][ ]dev[)][;]' drivers/net/wireless/broadcom/brcm80211/brcmfmac/common.c
    accept '[\t]*DRM_DEBUG_DRIVER[(]["]%s[ ]fw[ ]request_firmware[ ]err=%d[\\]n["][,]' drivers/gpu/drm/i915/intel_uc_fw.c

    accept '\(The[ ]k\|K\)ernel[ ]can[ ]update[ ]microcode' Documentation/x86/microcode.txt
    accept 'requires[ ]rebuilding[ ]the[ ]kernel[ ]each[ ]time[ ]updated[ ]microcode' Documentation/x86/microcode.txt
    accept '[\t][ ][ ]If[ ]you[ ]say[ ]Y[ ]here[,][ ]you[ ]will[ ]be[ ]able[ ]to[ ]update[ ]the[ ]microcode' arch/x86/Kconfig
    blobna '[,][ ]please[ ]upgrade[ ]microcode' arch/x86/events/intel/core.c
    blobna 'please[ ]update[ ]microcode[ ]to[ ]version:[ ]0x%x[ ][(]or[ ]later[)]' arch/x86/kernel/apic/apic.c
    accept '[ ][*][ \t]*This[ ]driver[ ]allows[ ]to[ ]upgrade[ ]microcode' arch/x86/kernel/cpu/microcode/'\(amd\|core\)\.c'
    accept '[\t][ ][*][ ]operation[ ]-[ ]when[ ]the[ ]other[ ]hyperthread[ ]has[ ]updated[ ]the[ ]microcode' arch/x86/kernel/cpu/microcode/core.c
    accept '[ ][*][ ]mc_bp_resume[ ]-[ ]Update[ ]boot[ ]CPU[ ]microcode[ ]during[ ]resume' arch/x86/kernel/cpu/microcode/core.c
    blobna '[,][ ]update[ ]BIOS[ ]or[ ]microcode[ ]of[ ]the[ ]CPU[!]' drivers/hwmon/coretemp.c
    accept '[ ][*][ ]ipr_update_ioa_ucode[ ]-[ ]Update[ ]IOA[\'"'"']s[ ]microcode' drivers/scsi/ipr.c
    accept '[ ][*][ ]Initiate[ ]an[ ]adapter[ ]reset[ ]to[ ]update[ ]the[ ]IOA[\'"'"']s[ ]microcode' drivers/scsi/ipr.c
    accept '[\t]*struct[ ]xenpf_microcode_update[ ]*microcode' include/xen/interface/platform.h

    # New in 4.16
    blobname 'board-2\.bin' Documentation/devicetree/bindings/net/wireless/qcom,ath10k.txt
    accept '[ ]*microcode_update_cpu[(][)][ ]which[ ]would[ ]call[ ]microcode_init_cpu[(][)][ ]in[ ]this[ ]case' Documentation/power/suspend-and-cpuhotplug.txt
    accept '[\t]\.irp[\t]b\([,][0-9]\)*\([,][1-3][0-9]\)*' arch/arm64/crypto/sha3-ce-core.S
    accept '\.Lsha512_rcon:\([\n][\t]\.quad[\t]*[0-9a-fx, ]*\)*' arch/arm64/crypto/sha512-ce-core.S
    accept '[ ][*][ ]only[ ]when[ ]microcode[ ]has[ ]been[ ]updated[.][ ]Caller[ ]holds[ ]microcode_mutex[ ]and[ ]CPU' arch/x86/kernel/cpu/common.c
    accept '[	][ ][ ]any[ ]request_firmware[(]\(["]whatever\.bin["]\)[)]' drivers/base/Kconfig
    accept 'static[ ]int[ ]_request_firmware_load[(]struct[ ]fw_sysfs[ ][*]fw_sysfs[,]' drivers/base/firmware_class.c
    accept '[\t]ret[ ]=[ ]_request_firmware_load[(]fw_sysfs[,][ ]opt_flags[,][ ]timeout[)][;]' drivers/base/firmware_class.c
    defsnc 'static[ ]const[ ]struct[ ]pll_freq_tbl[ ]a53pll_freq\[\][ ]=' drivers/clk/qcom/a53-pll.c
    defsnc 'static[ ]unsigned[ ]int[ ]d\?sgl_ent_len\[\][ ]=' drivers/crypto/chelsio/chcr_algo.c
    # FPGA configuration/programming files are named in Device Tree
    # overlays supplied by users.
    accept 'static[ ]int[ ]fpga_mgr_firmware_load[(]' drivers/fpga/fpga-mgr.c
    accept '[\t]*return[ ]fpga_mgr_firmware_load[(]mgr[,][ ]info[,][ ]info->firmware_name[)]' drivers/fpga/fpga-mgr.c
    # Nice, asm sources are in the same file, within #if 0/#endif!  License is ok, too.
    defsnc 'static[ ]const[ ]uint32_t[ ]cwsr_trap_gfx8_hex\[\][ ]=' drivers/gpu/drm/amd/amdkfd/cwsr_trap_handler_gfx8.asm
    blobname 'i915[/]cnl_dmc_ver1_06\.bin' drivers/gpu/drm/i915/intel_csr.c
    blobname 'i915[/]kbl_dmc_ver1_04\.bin' drivers/gpu/drm/i915/intel_csr.c
    blobname 'i915[/]skl_dmc_ver1_27\.bin' drivers/gpu/drm/i915/intel_csr.c
    defsnc 'static[ ]const[ ]u32[ ]lan2coefftab16\[240\][ ]=' drivers/gpu/drm/sun4i/sun8i_ui_scaler.c
    defsnc 'static[ ]const[ ]u32[ ]\(lan3\|bicubic8\)coefftab32_\(left\|right\)\[480\][ ]=' drivers/gpu/drm/sun4i/sun8i_ui_scaler.c
    defsnc 'static[ ]const[ ]u32[ ]\(lan2\|bicubic4\)coefftab32\[480\][ ]=' drivers/gpu/drm/sun4i/sun8i_ui_scaler.c
    defsnc '[}][ ]zopt2201_scale_\(als\|uvb\)\[\][ ]=' drivers/iio/light/zopt2201.c
    blobname 'raydium_\(%#04x\|[x0-9a-f]*\)\.fw' drivers/input/touchscreen/raydium_i2c_ts.c
    defsnc '[\t]*static[ ]const[ ]u8[ ]bufs\[\][ ]=' drivers/media/dvb/dvb-usb/cxusb.c
    defsnc 'static[ ]const[ ]struct[ ]reg_sequence[ ]ov7740_vga\[\][ ]=' drivers/media/i2c/ov7740.c
    accept '[ ][*][ ]@fw_get_done[\t]*flag[ ]set[ ]when[ ]request_firmware[(][)][ ]is[ ]complete' drivers/media/platform/s5p-mfc/s5p_mfc_common.h
    defsnc 'static[ ]const[ ]struct[ ]iro[ ]iro_arr\[51\][ ]=' drivers/net/ethernet/qlogic/qed/qed_hsi.h
    defsnc 'static[ ]const[ ]struct[ ]ath10k_mem_section[ ]qca6174_hw\(21\|30\)_register_sections\[\][ ]=' drivers/net/wireless/ath/ath10k/coredump.c
    blobname 'mt7662\(_rom_patch\)\?\.bin' drivers/net/wireless/mediatek/mt76/mt76x2.h
    defsnc 'static[ ]const[ ]struct[ ]mtk_pin_field_calc[ ]mt7622_pin_\(mode\|sr\|smt\|pu\|pd\|e[48]\|[tr]dsel\)_range\[\][ ]=' drivers/pinctrl/mediatek/pinctrl-mt7622.c
    blobname 'gsl\(3670-surftab-twin-10-1-st10432-8\|3676-onda-obook-20-plus\|1680-chuwi-hi8\|3676-chuwi-vi8\|1680-trekstor-primebook-c13\|1686-teclast_x98plus2\|1680-teclast-x3-plus\)\.fw' drivers/platform/x86/silead_dmi.c
    defsnc 'static[ ]const[ ]struct[ ]xvcu_pll_cfg[ ]xvcu_pll_cfg\[\][ ]=' drivers/soc/xilinx/xlnx_vcu.c
    defsnc 'u16[ ]const[ ]crc_ccitt_false_table\[256\][ ]=' lib/crc-ccitt.c
    defsc 'static[ ]const[ ]struct[ ]aic32x4_rate_divs[ ]aic32x4_divs\[\][ ]=' sound/soc/codecs/tlv320aic32x4.c
    defsnc 'static[ ]char[ ]const[ ][*][ ]const[ ]compressor_ratio_text\[\][ ]=' sound/soc/codecs/tscs42xx.c
    defsnc '[\t]const[ ]u8[ ]norm_addrs\[\][ ]=' sound/soc/codecs/tscs42xx.c
    # The firmware file name is supplied by the user.
    accept '[\t]err[ ]=[ ]request_firmware_direct[(][&]fw[,][ ]flash->data[,]\([^\n]*[\n]\+[^\n}]\)*err[ ]=[ ]nfp_nsp_write_flash[(]nsp[,][ ]fw[)]' drivers/net/ethernet/netronome/nfp/nfp_net_ethtool.c
    accept '[\t]*\(rc[ ]=[ ]\)\?wil_request_firmware[(]wil[,][ \n\t]*\(wil->wil_fw_name\|WIL_BOARD_FILE_NAME\)[,][ \n\t]*\(true\|false\)[)][;]' drivers/net/wireless/ath/wil6210/main.c
    accept '[\t]retval0[ ]=[ ]report_missing_free_firmware[^\n]*[\n][\t]retval[ ]=[ ]request_firmware_direct[(]' include/linux/firmware.h
    accept '[\t]retval0[ ]=[ ]report_missing_free_firmware[^\n]*[\n][\t]retval[ ]=[ ]request_firmware_into_buf[(][&]xfw[,][ ]NONFREE_FIRMWARE' include/linux/firmware.h

    # New in 4.17
    defsnc 'static[ ]const[ ]u8[ ]sbox\[256\][ ]=' crypto/sm4_generic.c
    defsnc 'static[ ]const[ ]u32[ ]ck\[\][ ]=' crypto/sm4_generic.c
    defsc 'static[ ]const[ ]struct[ ]cipher_testvec[ ]speck\(128\|64\)_\(xts_\)\?\(enc\|dec\)_tv_template\[\][ ]=' crypto/testmgr.h
    accept '[ ][*][ ]request_firmware_into_buf[(][)][ ]or[ ]request_firmware_nowait[(][)][ ]with' drivers/base/firmware_loader/main.c
    defsnc 'static[ ]const[ ]struct[ ]clk_div_table[ ]mcu_div_table\[\][ ]=' drivers/clk/clk-stm32mp1.c
    defsnc 'static[ ]const[ ]struct[ ]profile_mode_setting[ ]smu7_profiling\[6\][ ]=' drivers/gpu/drm/amd/powerplay/hwmgr/smu7_hwmgr.c
    defsnc 'static[ ]const[ ]u32[ ]sun4i_frontend_vert_coef\[32\][ ]=' drivers/gpu/drm/sun4i/sun4i_frontend.c
    defsnc 'static[ ]const[ ]u32[ ]sun4i_frontend_horz_coef\[64\][ ]=' drivers/gpu/drm/sun4i/sun4i_frontend.c
    defsnc 'static[ ]const[ ]struct[ ]lv0104cs_mapping[ ]lv0104cs_calibscales\[\][ ]=' drivers/iio/light/lv0104cs.c
    defsnc '[\t]static[ ]const[ ]u8[ ]rf_init1_cdata1\[40\][ ]=' drivers/media/dvb-frontends/cxd2880/cxd2880_tnrdmd.c
    defsnc '[\t]static[ ]const[ ]u8[ ]rf_init1_cdata3\[80\][ ]=' drivers/media/dvb-frontends/cxd2880/cxd2880_tnrdmd.c
    defsnc '[\t]static[ ]const[ ]u8[ ]rf_init1_cdata5\[50\][ ]=' drivers/media/dvb-frontends/cxd2880/cxd2880_tnrdmd.c
    defsnc 'static[ ]struct[ ]regval[ ]ov2685_1600x1200_regs\[\][ ]=' drivers/media/i2c/ov2685.c
    defsnc 'static[ ]const[ ]struct[ ]regval[ ]ov5695_\(global\|2592x1944\|1920x1080\|1296x972\|1280x720\|640x480\)_regs\[\][ ]=' drivers/media/i2c/ov5695.c
    defsnc 'u_short[ ]ebc_plain_map\[NR_KEYS\][ ]=' drivers/s390/char/defkeymap.c
    defsnc 'static[ ]const[ ]int16_t[ ]g_pyramid\[8\]\[8\][ ]=' drivers/staging/media/atomisp/pci/atomisp2/css2400/isp/kernels/tdf/tdf_1.0/ia_css_tdf.host.c
    accept 'MODULE_FIRMWARE[(]["]aica_firmware\.bin["][)][;]' sound/sh/aica.c
    accept '[\t]err[ ]=[ ]request_firmware[(][&]fw_entry[,][ ]["]aica_firmware\.bin["][,]' sound/sh/aica.c
    defsnc '[\t]static[ ]const[ ]u8[ ]norm_addrs\[\][ ]=' sound/soc/codecs/tscs42xx.c
    accept '[\t]FW=["][$]FWPATH[/]test-firmware\.bin["]' tools/testing/selftests/firmware/fw_lib.sh
    accept '\([/][*][ ]0x1[ ]\[\^\\000\][*]\[\^[/]\\000\][/][/][&][ ][*][/][ ]\)\?0x1B[,][ ]0x5E[,][ ]0x78[,][ ]0x3D[,][ ]0x00[,][ ]0x00[,][ \n]0x00[,][ ]0x18[,][ ][0x1-9A-F, \n]*' 'security/apparmor/\(null\|stacksplit\)dfa.in'
    blobname 'rtl_bt[/]rtl\(8723d\|8821c\)_\(config\|fw\)\.bin' drivers/bluetooth/btrtl.c
    blobname 'amdgpu[/]vega12_smc\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_cgs.c
    blobname 'amdgpu[/]vega12_uvd\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_uvd.c
    blobname 'amdgpu[/]vega12_vce\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vce.c
    blobname 'i915[/]cnl_dmc_ver1_07\.bin' drivers/gpu/drm/i915/intel_csr.c
    defsnc 'static[ ]const[ ]struct[ ]af9013_reg_mask_val[ ]demod_init_tab\[\][ ]=' drivers/media/dvb-frontends/af9013_priv.h
    defsnc 'static[ ]const[ ]struct[ ]af9013_reg_mask_val[ ]tuner_init_tab_\(env77h11d5\|mt2060\(_2\)\?\|mxl500\(3d\|5\)\|qt1010\|mc44s803\|unknown\|tda18271\)\[\][ ]=' drivers/media/dvb-frontends/af9013_priv.h
    blobname '\(vpu[/]\)\?vpu_fw_imx51\.bin' drivers/media/platform/coda/coda-common.c
    blobname 'v4l-codahx4-imx51\.bin' drivers/media/platform/coda/coda-common.c
    blobname 's5p-mfc-v10\.fw' drivers/media/platform/s5p-mfc/s5p_mfc.c
    blobname 'example[ ]file[ ]wl1251-nvs\.bin[,][^*]*[*][/]' drivers/net/wireless/ti/wl1251/main.c
    blobname '["]brcm[/]["]' drivers/net/wireless/broadcom/brcm80211/brcmfmac/firmware.h
    blobname '\(brcm[/]\)\?brcmfmac43\(143\|241b[045]\|29\|3[0459]\|340\|362\|430\(a0\)\?\|455\|5[46]\|73\)-sdio\(\.bin\|\.txt\)\?' drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
    blobname '\(brcm[/]\)\?brcmfmac43\(602\|50\(c2\)\?\|56\|570\|5[89]\|65[bc]\|66[bc]\|71\)-pcie\(\.bin\|\.txt\)\?' drivers/net/wireless/broadcom/brcm80211/brcmfmac/pcie.c
    blobname '\(brcm[/]\)\?brcmfmac43\(143\|236b\|242a\|569\|73\)\(\.bin\|\.txt\)\?' drivers/net/wireless/broadcom/brcm80211/brcmfmac/usb.c
    accept '[\t]struct[ ]brcmf_fw_name[ ]fwnames\[\][ ]=[ ][{][\n][\t][\t][{][ ]["]\.bin["]' 'drivers/net/wireless/broadcom/brcm80211/brcmfmac/\(pcie\|sdio\|usb\)\.c'
    # We require a semicolon after MODULE_FIRMWARE, which this
    # in-macro occurrence does not have, so take the semicolon from
    # the previous in-macro declaration.
    blobname '\([;][ ]\\[\n]MODULE_FIRMWARE[(]BRCMF_FW_DEFAULT_PATH[^)]*[)]\)\+' drivers/net/wireless/broadcom/brcm80211/brcmfmac/firmware.h

    # Adjust for catching firmware_request
    accept 'static[ ]int[ ]coda_firmware_request[(]' drivers/media/platform/code/coda-common.c
    accept '[\t]*ret[ ]=[ ]coda_firmware_request[(]' drivers/media/platform/code/coda-common.c
    accept '[\t]struct[ ]gb_bootrom_get_firmware_request[ ][*]firmware_request[;]' drivers/staging/greybus/bootrom.c
    accept '[\t]*\(if[ ][(]op->request->payload_size[ ]!=[ ]\)\?sizeof[(][*]firmware_request[)]' drivers/staging/greybus/bootrom.c
    accept '[\t]firmware_request[ ]=[ ]op->request->' drivers/staging/greybus/bootrom.c
    accept '[\t]\(offset\|size\)[ ]=[ ]le32_to_cpu[(]firmware_request->' drivers/staging/greybus/bootrom.c
    accept '[\t]struct[ ]gb_fw_download_\(find\|fetch\|release\)_firmware_request[ ][*]request[;]' drivers/staging/greybus/fw-download.c

    # New in 4.18 (-rc6)
    blobname 'amdgpu[/]vega\(m\|20\)_smc\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_cgs.c
    blobname 'amdgpu[/]vega\(m\|20\)_uvd\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_uvd.c
    blobname 'amdgpu[/]vega\(m\|20\)_vce\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vce.c
    blobname 'amdgpu[/]vegam_\(ce\|pfp\|me\|mec\|mec2\|rlc\)\.bin' drivers/gpu/drm/amd/amdgpu/gfx_v8_0.C
    blobname 'amdgpu[/]\(vega\(10\|12\|20\)\|raven\)_\(ce\|pfp\|me\|mec\|mec2\|rlc\)\.bin' drivers/gpu/drm/amd/amdgpu/gfx_v9_0.C
    blobname 'amdgpu[/]vega\(10\|12\|20\)_\(sos\|asd\)\.bin' drivers/gpu/drm/amd/amdgpu/psp_v3_1.C
    blobname 'amdgpu[/]vegam_sdma1\?\.bin' drivers/gpu/drm/amd/amdgpu/sdma_v3_0.C
    blobname 'amdgpu[/]\(vega\(10\|12\|20\)\|raven\)_sdma1\?\.bin' drivers/gpu/drm/amd/amdgpu/sdma_v4_0.C
    blobname 'amdgpu[/]vega\(m\|10\|10_acg12\|20\)_smc\.bin' drivers/gpu/drm/amd/amdgpu/smumgr.c
    blobna 'https:[/][/]git\.kernel\.org[/][^"\n]*firmware\.git[/]tree[/]i915' drivers/gpu/drm/i915/intel_uc_fw.h
    blobna 'You[ ]can[ ]use[ ][^"\n]*to[ ]get[ ]the[ ]firmware\.\?' drivers/media/usb/dvb-usb/dvb-usb-firmware.c
    blob '[ ][*][ ]Firmware[ ]is:[\n][ ][*][	]Derived[ ]from[ ]proprietary[^*]*\([*]\+[^/*][^*]*\)*notice[ ]is[ ]accompanying[ ]it\.[\n][ ][*][/]' drivers/net/tg3.c
    blobname 'gsl\(3692-jumper-ezpad-6-pro\|3680-\(pov-mobii-wintab-p800w-v20\|onda-v891w-v1\)\)\.fw' drivers/platform/x86/silead_dmi.c
    blobname 'ctefx-\(sbz\|r3di\)\.bin' sound/pci/hda/patch_ca0132.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]float_\(vol_db\|zero_to_one\|xbass_xover\)_lookup\[\][ ]=' sound/pci/hda/patch_ca0132.c
    blobna '[\t][/][*][\n][\t][ ][*][ ]Use[ ]default[ ]ctefx\.bin[ ]if[^*]*\([*]\+[^/*][^*]*\)*[*][/]' sound/pci/hda/patch_ca0132.c
    defsnc 'static[ ]struct[ ]hda_verb[ ]sbz_init_verbs\[\][ ]=' sound/pci/hda/patch_ca0132.c
    accept '\([ ]*:functions:[ ]\)\?firmware_request_\(nowarn\|cache\)\([(][)]\)\?' Documentation/driver-api/firmware/request_firmware.rst
    accept 'this[ ]can[ ]be[ ]done[ ]with[ ]firmware_request_cache[(][)][ ]' Documentation/driver-api/firmware/request_firmware.rst
    accept '[ ]*[.][.][.][\n][ ]*9[ ]*176[ ]*0[ ]*1[ ]*186[ 0-9\n]*' Documentation/vm/zsmalloc.rst
    defsnc '\.Lmorus1280_\(const\|counter\):' arch/x86/crypto/morus1280-avx2-asm.S
    defsnc 'static[ ]const[ ]struct[ ]cipher_testvec[ ]\(\(des3_ede\|bf\)_cbc\|tf_xts\|serpent\|tnepres\|serpent_xts\|speck128\|speck128_xts\|speck64_xts\|cast6_xts\|aes\|aes_cbc\|aes_xts\|aes_ctr_rfc3686\|tea\|xtea\|anubis\|anubis_cbc\|xeta\|camellia_cbc\|camellia_xts\|salsa20_stream\|chacha20\|cts_mode\)_tv_template\[\][ ]=' crypto/testmgr.h
    accept '[\t ]*mechanism[ ]is[ ]request_firmware_direct[(][)][.]' drivers/base/firmware_loader/Kconfig
    accept '[ ][*][ ]request_firmware[(][)][ ]-[ ]send[ ]firmware[ ]request' drivers/base/firmware_loader/main.c
    accept 'request_firmware[(]const[ ]struct[ ]firmware[ ][*][*]firmware_p[,]' drivers/base/firmware_loader/main.c
    accept '[ ][*][ ]firmware_request_nowarn[(][)][ ]-[ ]request[ ]for[ ]an[ ]optional[ ]fw[ ]module' drivers/base/firmware_loader/main.c
    accept '[ ][*][ ]This[ ]function[ ]is[ ]similar[ ]in[ ]behaviour[ ]to[ ]request_firmware[(][)][,]' drivers/base/firmware_loader/main.c
    accept 'int[ ]firmware_request_nowarn[(]const[ ]struct[ ]firmware[ ][*][*]firmware[,]' drivers/base/firmware_loader/main.c
    accept '[\t]*ret[ ]=[ ]_request_firmware[(]firmware[,][ ]name[,][ ]device' drivers/base/firmware_loader/main.c
    accept 'EXPORT_SYMBOL_GPL[(]firmware_request_\(nowarn\|cache\)[)]' drivers/base/firmware_loader/main.c
    accept '[ ][*][ ]request_firmware_direct[(][)][ ]-[ ]load[ ]firmware[ ]directly' drivers/base/firmware_loader/main.c
    accept '[ ][*][ ]firmware_request_cache[(][)][ ]-[ ]cache[ ]firmware[ ]for[ ]suspend' drivers/base/firmware_loader/main.c
    accept 'int[ ]firmware_request_cache[(]struct[ ]device[ ][*]device[,]' drivers/base/firmware_loader/main.c
    accept '[ ][*][ ]request_firmware_into_buf[(][)][ ]-[ ]load[ ]firmware[ ]into[ ]a[ ]previously[ ]allocated[ ]buffer' drivers/base/firmware_loader/main.c
    accept '[ ][*][ ]request_firmware_nowait[(][)][ ]-[ ]asynchronous[ ]version[ ]of[ ]request_firmware' drivers/base/firmware_loader/main.c
    accept '[ ][*][ \t]*Asynchronous[ ]variant[ ]of[ ]request_firmware[(][)][ ]for[ ]user[ ]contexts:' drivers/base/firmware_loader/main.c
    accept 'int[\n]request_firmware_nowait[(][\n][\t]struct[ ]module[ ][*]module' drivers/base/firmware_loader/main.c
    accept '[\t]INIT_WORK[(][&]fw_work->work[,][ ]request_firmware_work_func[)]' drivers/base/firmware_loader/main.c
    defsnc 'static[ ]struct[ ]clk_div_table[ ]nand_div_table\[\][ ]=' drivers/clk/actions/owl-s900.c
    defsc 'static[ ]struct[ ]clk_factor_table[ ]sd_factor_table\[\][ ]=' drivers/clk/actions/owl-s900.c
    defsnc '[\t][}][ ]id\[\][ ]=' drivers/crypto/caam/ctrl.c
    defsc 'static[ ]const[ ]struct[ ]IP_BASE[ ]\(ATHUB\|CLK\|DCE\|DF\|FUSE\|GC\|HDP\|MMHUB\|MP[01]\|NBIO\|OSSSYS\|SDMA[01]\|SMUIO\|THM\|UMC\|UVD\|VCE\|XDMA\|RSMU\)_BASE[ ]*=' drivers/gpu/drm/amd/include/vega20_ip_offset.h
    defsc 'vegam_power_tune_data_set_array\[POWERTUNE_DEFAULT_SET_MAX\][ ]=' drivers/gpu/drm/amd/powerplay/smumgr/vegam_smumgr.c
    defsnc 'gv100_disp_core_mthd_head[ ]=' drivers/gpu/drm/nouveau/nvkm/engine/disp/coregv100.c
    defsnc 'gv100_disp_wndw_mthd_base[ ]=' drivers/gpu/drm/nouveau/nvkm/engine/disp/wndwgv100.c
    defsc 'gf100_grctx_alpha_beta_map\[17\]\[32\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/ctxgf100.c
    defsnc 'gv100_grctx_init_sw_veid_bundle_init_0\[\][ ]=' drivers/gpu/drm/nouveau/nvkm/engine/gr/ctxgv100.c
    defsnc 'static[ ]const[ ]struct[ ]dvb_pll_desc[ ]dvb_pll_tda665x_earth_pt1[ ]=' drivers/media/dvb-frontends/dvb-pll.c
    defsnc 'static[ ]const[ ]struct[ ]imx258_reg[ ]mode_\(4208x3118\|2104_1560\|1048_780\)_regs\[\][ ]=' drivers/media/i2c/imx258.c
    defsc 'static[ ]const[ ]struct[ ]reg_value[ ]ov7251_setting_vga_[369]0fps\[\][ ]=' drivers/media/i2c/ov7251.c
    defsnc 'static[ ]const[ ]u8[ ]va1j5jf8007[st]_2[05]mhz_configs\[\]\[2\][ ]=' drivers/media/pci/pt1/pt1.c
    defsnc 'static[ ]const[ ]struct[ ]iro[ ]iro_arr\[59\][ ]=' drivers/net/ethernet/qlogic/qed/qed_hsi.h
    defsnc 'static[ ]const[ ]int[ ]pfuze3000_sw1a\[\][ ]=' drivers/regulator/pfuze100-regulator.c
    accept 'struct[ ]gb_\(fw_download_\(find\|fetch\|release\)\|bootrom_get\)_firmware_request[ ][{]' drivers/staging/greybus/greybus_protocols.h
    accept 'int[ ]firmware_request_nowarn[(]const[ ]struct[ ]firmware[ ][*][*]fw' include/linux/firmware.h
    accept 'static[ ]inline[ ]int[ ]firmware_request_nowarn[(]const[ ]struct[ ]firmware[ ][*][*]fw' include/linux/firmware.h
    accept 'int[ ]firmware_request_cache[(]struct[ ]device[ ][*]device' include/linux/firmware.h
    accept '[\t]retval[ ]=[ ]firmware_request_nowarn[(][&]xfw[,][ ]NONFREE_FIRMWARE[,]' include/linux/firmware.h
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt1305_reg\[\][ ]=' sound/soc/codecs/rt1305.c
    defsnc 'static[ ]char[ ]const[ ][*][ ]const[ ]comp_rat_txt\[\][ ]=' sound/soc/codecs/tscs454.c
    accept '[ ]*[{]["]pid["]:21800[,]["]fd["]:5[,]["]prog_id["]:9[,]["]fd_type["]:["]uprobe["][,]["]filename["]:["][/]home[/]yhs[/]a\.out["][,]["]offset["]:1159[}]\]' tools/bpf/bpftool/Documentation/bpftool-perf.rst
    accept '[#][ ]a[ ]file[ ]whose[ ]name[ ]is[ ]that[ ]of[ ]the[ ]specified[ ]litmus[ ]test[,][ ]but[ ]with[ ]["]\.out["]' tools/memory-model/scripts/checkalllitmus.sh
    accept '[#][ ]with[ ]["]\.out["][ ]appended\.' tools/memory-model/scripts/checkalllitmus.sh
    accept 'static[ ]struct[ ]bpf_test[ ]tests\[\][ ]=[ ][{][\n]\([^}][^\n]*[\n][\n]*\)*[}][;]' tools/testing/selftests/bpf/test_verifier.c
    # Sources are in cwsr_trap_handler_gfx[89].asm.
    defsnc 'static[ ]const[ ]uint32_t[ ]cwsr_trap_gfx[89]_hex\[\][ ]=' drivers/gpu/drm/amd/amdkfd/cwsr_trap_handler.h
    blobname 'amd[/]sev\.fw' drivers/crypto/ccp/psp-dev.c
    blobname 'chipone[/]icn8505-\(%s\|[^.",)]*\)\.fw' drivers/input/touchscreen/chipone_icn8505.c
    accept '[\t]*return[ ]firmware_request_cache[(]dev->dev[,][ ]MT7601U_FIRMWARE[)]' drivers/net/wireless/mediatek/mt7601u/mcu.c

    # New in 4.19-rc7.
    accept '[\t]*reg[ ]=[ ][<]\(0x\(40\)\?[08][ ]0xd[02][01][0-9a-f]0000[ ]0x0[ ]0x10000[\n\t ]*\)*[>][;]' 'Documentation/devicetree/bindings/crypto/hisilicon,hip07-sec\.txt\|arch/arm64/boot/dts/hisilicon/hip07\.dtsi'
    defsnc 'const[ ]u8[ ]sha384_zero_message_hash\[SHA384_DIGEST_SIZE\][ ]=' crypto/sha512_generic.c
    defsnc 'const[ ]u8[ ]sha512_zero_message_hash\[SHA512_DIGEST_SIZE\][ ]=' crypto/sha512_generic.c
    defsnc 'static[ ]const[ ]char[ ]vmac64_string1\[144\][ ]=' crypto/testmgr.h
    defsc 'static[ ]struct[ ]clk_factor_table[ ]lcd_factor_table\[\][ ]=' drivers/clk/actions/owl-s700.c
    defsnc 'static[ ]int[ ]avs_map\[\][ ]=' drivers/cpufreq/armada-37xx-cpufreq.c
    defsnc 'static[ ]const[ ]u32[ ]a6xx_registers\[\][ ]=' drivers/gpu/drm/msm/adreno/a6xx_gpu.c
    defsnc '[\t]static[ ]const[ ]uint32_t[ ]off_tbl\[QSEED3_FILTERS\]\[QSEED3_LUT_REGIONS\]\[2\][ ]=' drivers/gpu/drm/msm/disp/dpu1/dpu_hw_util.c
    defsnc 'static[ ]const[ ]struct[ ]reg_value[ ]ov2680_setting_30fps_\(QUXGA_800_600\|UXGA_1600_1200\)\[\][ ]=' drivers/media/i2c/ov2680.c
    defsnc 'static[ ]const[ ]uint8_t[ ]zigzag\[64\][ ]=' drivers/media/platform/vicodec/vicodec-codec.c
    defsnc 'static[ ]const[ ]int[ ]quant_table\(_p\)\?\[\][ ]=' drivers/media/platform/vicodec/vicodec-codec.c
    defsnc '[\t]static[ ]const[ ]u8[ ]demod_init\[\]\[2\][ ]=' drivers/media/usb/dvb-usb-v2/gl861.c
    defsnc 'static[ ]const[ ]struct[ ]reg_sequence[ ]cs47l35_reva_16_patch\[\][ ]=' drivers/mfd/cs47l35-tables.c
    defsnc 'static[ ]const[ ]struct[ ]reg_sequence[ ]cs47l85_rev[ac]_\(16\|32\)_patch\[\][ ]=' drivers/mfd/cs47l85-tables.c
    defsnc 'static[ ]const[ ]struct[ ]reg_sequence[ ]cs47l90_reva_16_patch\[\][ ]=' drivers/mfd/cs47l90-tables.c
    defsnc 'static[ ]const[ ]u16[ ]rtl8366rb_init_jam_\(ver_[0123]\|f5d8235\)\[\][ ]=' drivers/net/dsa/rtl8366rb.c
    defsnc '[\t]static[ ]const[ ]int[ ]mt76x0_tx_pwr_ch_list\[\][ ]=' drivers/net/wireless/mediatek/mt76/mt76x0/phy.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]madera_pin_single_group_pins\[\][ ]=' drivers/pinctrl/cirrus/pinctrl-madera-core.c
    defsnc 'static[ ]const[ ]int[ ]adp5061_vmax\[36\][ ]=' drivers/power/supply/adp5061.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]sw2_sw4_val_tbl\[\][ ]=' drivers/regulator/cpcap-regulator.c
    defsnc '[}][ ]segdist_codes\[\][ ]=' drivers/slimbus/stream.c
    accept '#define[ ]PIOLED_GAMMA[\t]["]\([0234][ ]\|["][ ][\\][\n\t ]*["]\)*["]' drivers/staging/fbtft/fbtft_device.c
    defsnc 'static[ ]const[ ]struct[ ]cp210x_rate[ ]cp210x_an205_table1\[\][ ]=' drivers/usb/serial/cp210x.c
    defsnc 'static[ ]const[ ]u8[ ]\(precedence\|diffserv[843]\|besteffort\)\[\][ ]=' net/sched/sch_cake.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt5682_reg\[\][ ]=' sound/soc/codecs/rt5682.c
    defsnc 'static[ ]struct[ ]hda_verb[ ]ca0132_init_verbs1\[\][ ]=' sound/pci/hda/patch_ca0132.c
    blobname 'imx[/]sdma[/]sdma-imx31\.bin' arch/arm/boot/dts/imx31.dtsi
    blobname 'imx[/]sdma[/]sdma-imx6q\.bin' arch/arm/boot/dts/imx6sll.dtsi
    blobname 'mediatek[/]mt7622pr2h\.bin' drivers/bluetooth/btmtkuart.c
    blobname 'qca[/]crnv%02x\.bin' drivers/bluetooth/btqca.c
    blobname 'rtl_bt[/]rtl8723[bd]s_fw\.bin' drivers/bluetooth/btrtl.c
    blobname '%s\(-%s\)\?\.bin' drivers/bluetooth/btrtl.c
    blobname 'cf-fsi-fw\.bin' drivers/fsi/fsi-master-ast-cf.c
    blobname 'amdgpu[/]\(bonaire\|hawaii\)_\(k_\)\?smc\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_cgs.c
    blobname 'amdgpu[/]\(bonaire\|kabini\|kaveri\|hawaii\|mullins\)_uvd\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_uvd.c
    blobname 'amdgpu[/]\(bonaire\|kabini\|kaveri\|hawaii\|mullins\)_vce\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vce.c
    blobname 'amdgpu[/]%s_smc\.bin' 'drivers/gpu/drm/amd/amdgpu/[cs]i_dpm\.c'
    blobname 'amdgpu[/]si58_mc\.bin' drivers/gpu/drm/amd/amdgpu/gmc_v6_0.c
    blobname 'a630_\(sqe\.fw\|gmu\.bin\)' drivers/gpu/drm/msm/adreno/adreno_device.c
    blobname 'qcom[/]venus-5\.2[/]venus\.mdt' drivers/media/platform/qcom/venus/core.c
    blobname 'mellanox[/]mlxsw_spectrum-\(["][ ]__stringify[(]MLXSW_SP1_FWREV_[^)]*[)][ \\\n\t]*["]\.\)*mfa2' drivers/net/ethernet/mellanox/mlxsw/spectrum.c
    blobname 'wil6436\(_ftm\)\?\.fw' drivers/net/wireless/ath/wil6210/wil6210.h
    blobna '[/][*][ ]brcmfmac436\(02\|6b\)-pcie\.\(ap\.\)\?bin[ ]from[ ]linux-firmware\.git[ ]commit[ ][0-9a-f]*[ ][*][/]' drivers/net/wireless/broadcom/brcm80211/brcmfmac/feature.c
    blobname 'mediatek[/]mt7610u\.bin' drivers/net/wireless/mediatek/mt76/mt76x0/usb.h
    blobname 'mediatek[/]mt7662u\(_rom_patch\)\?\.bin' drivers/net/wireless/mediatek/mt76/mt76x2.h
    blobname 'gsl3680-chuwi-vi10\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'gsl1680-connect-tablet9\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'gsl3692-cube-knote-i1101\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'gsl1680-onda-v820w-32g\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'gsl3676-onda-v891w-v3\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'keystone-dsp%d-fw' drivers/remoteproc/keystone_remoteproc.c
    blobname 'mba\.mbn' drivers/remoteproc/qcom_q6v5_pil.c
    blobname 'IPQ8074[/]q6_fw\.mdt' drivers/remoteproc/qcom_q6v5_wcss.c
    blobname '%s-%s-%s\.bin' sound/soc/codecs/wm_adsp.c
    accept '[\t]*rc[ ]=[ ]wil_request_firmware[(]wil[,][ ]board_file[,][ ]true[)][;]' drivers/net/wireless/ath/wil6210/main.c
    blobna '[ ]\(Important[ ]Notes\|Obtaining[ ]and[ ]Creating\)[^\n]*\([\n]#\([\n]#\([\n]#[ ]*For[ ]the\)\?\)\?[ ][^\n]*\)\+' Documentation/sound/cards/multisound.sh

    # New in 4.20 up to -rc6.
    initnc '\.Lcts_permute_table:' arch/arm64/crypto/aes-modes.S
    defsnc '[\t]static[ ]const[ ]unsigned[ ]char[ ]default_colors\[\][ ]__initconst[ ]=' arch/powerpc/kernel/prom_init.c
    defsc 'static[ ]const[ ]struct[ ]cipher_testvec[ ]aes_lrw_tv_template\[\][ ]=' crypto/testmgr.h
    blobname 'rtl_bt[/]rtl8822cu_fw\.bin' drivers/bluetooth/btrtl.c
    blobname 'amdgpu[/]\(picasso\|raven2\)_vcn\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vcn.c
    blobname 'amdgpu[/]\(vega20\|%s\)_sos\.bin' drivers/gpu/drm/amd/amdgpu/psp_v11_0.c
    blobname 'amdgpu[/]raven_dmcu\.bin' drivers/gpu/drm/amd/display/amdgpu_dm/amdgpu_dm.c
    blobname 'i915[/]icl_dmc_ver1_07\.bin' drivers/gpu/drm/i915/intel_csr.c
    defsnc 'static[ ]const[ ]struct[ ]vadc_map_pt[ ]adcmap_100k_104ef_104fb_1875_vref\[\][ ]=' drivers/iio/adc/qcom-vadc-common.c
    defsc 'static[ ]const[ ]struct[ ]reg_8[ ]imx274_start_1\[\][ ]=' drivers/media/i2c/imx274.c
    defsnc 'static[ ]const[ ]struct[ ]imx319_reg[ ]\(imx319_global\|mode_\(3264x2448\|3280x2464\|1936x1096\|1920x1080\|1640x\(1232\|922\)\|1296x736\|1280x720\)\)_regs\[\][ ]=' drivers/media/i2c/imx319.c
    defsnc 'static[ ]const[ ]struct[ ]imx355_reg[ ]\(imx355_global\|mode_\(326[48]x2448\|3280x2464\|19\(40\|36\)x1096\|192[40]x1080\|1640x\(1232\|922\)\|1\(300\|296\)x736\|128[40]x720\|820x616\)\)_regs\[\][ ]=' drivers/media/i2c/imx355.c
    blobname 'lantiq[/]xrx200_phy\(22f\|11g\)_a\(14\|2[21]\)\.bin' drivers/net/dsa/lantiq_gswip.c
    defsnc 'static[ ]const[ ]struct[ ]iro[ ]iro_arr\[60\]' drivers/net/ethernet/qlogic/qed/qed_hsi.h
    blobname 'mscc_vsc8584_revb_int8051_fb48\.bin' drivers/net/phy/mscc.c
    blobname 'mscc_vsc8574_revb_int8051_29e8\.bin' drivers/net/phy/mscc.c
    defsnc '[\t]const[ ]struct[ ]reg_val[ ]\(init_eee\|pre_init1\)\[\][ ]=' drivers/net/phy/mscc.c
    defsnc '[\t][}][ ]chan_map\[\][ ]=' drivers/net/wireless/mediatek/mt76/mt76x0/eeprom.c
    blobname 'mediatek[/]mt76[15]0e\.bin' drivers/net/wireless/mediatek/mt76/mt76x0/pci_mcu.c
    defsc 'static[ ]const[ ]struct[ ]pre_pll_config[ ]pre_pll_cfg_table\[\][ ]=' drivers/phy/rockchip/phy-rockhip-inno-hdmi.c
    defsc 'static[ ]const[ ]struct[ ]post_pll_config[ ]post_pll_cfg_table\[\][ ]=' drivers/phy/rockchip/phy-rockhip-inno-hdmi.c
    defsc 'static[ ]const[ ]struct[ ]phy_config[ ]rk3[23]28_phy_cfg\[\][ ]=' drivers/phy/rockchip/phy-rockhip-inno-hdmi.c
    blobname 'gsl3676-onda-v80-plus-v3\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'gsl1680-trekstor-primebook-c11\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'gsl1680-trekstor-primetab-t13b\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'cdsp\.mdt' drivers/remoteproc/qcom_q6v5_pas.c
    defsnc '[\t]unsigned[ ]char[ ]inq\[36\][ ]=' drivers/scsi/myrb.c
    defsnc 'static[ ]const[ ]u8[ ]\(non_\)\?intra_quantization_matrix_default\[64\][ ]=' drivers/staging/media/sunxi/cedrus/cedrus_mpeg2.c
    blobname 'ctefx-desktop\.bin' sound/pci/hda/patch_ca0132.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]lpf[123]_default_tap\[\][ ]=' sound/soc/meson/axg-pdm.c
    blobname 'eboard\.bin' 'drivers/net/wireless/ath/ath10k/\(hw\.h\|core\.c\)'
    blobname 'iwlwifi-\(Qu\(Qnj\)\?-b0-hr-b0\|su-z0\|Qu-b0-jf-b0\)-' drivers/net/wireless/intel/iwlwifi/cfg/22000.c
    blobname 'modem\.b%02d' drivers/remoteproc/qcom_q6v5_mss.c
    # New in 4.20-rc7.
    blobname 'amdgpu[/]polaris1[01]_k2_smc\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_cgs.c
    blobname 'amdgpu[/]polaris12_k_smc\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_cgs.c

    # New in 5.0-rc5.
    defsnc '__visible[ ]const[ ]u32[ ]crypto_[fi][tl]_tab\[4\]\[256\][ ]__cacheline_aligned[ ]=' crypto/aes_generic.c
    defsnc 'static[ ]const[ ]u8[ ]Tau\[64\][ ]=' crypto/streebog_generic.c
    defsnc 'static[ ]const[ ]u8[ ]Pi\[256\][ ]=' crypto/streebog_generic.c
    defsnc 'static[ ]const[ ]unsigned[ ]long[ ]long[ ]Ax\[8\]\[256\][ ]=' crypto/streebog_generic.c
    defsnc 'static[ ]const[ ]struct[ ]hash_testvec[ ]hmac_streebog\(256\|512\)_tv_template\[\][ ]=' crypto/testmgr.h
    defsc 'static[ ]const[ ]struct[ ]cipher_testvec[ ]xchacha\(20\|12\)_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]const[ ]struct[ ]profile_mode_setting[ ]smu7_profiling\[7\][ ]=' drivers/gpu/drm/amd/powerplay/hwmgr/smu7_hwmgr.c
    defsnc 'static[ ]const[ ]uint32_t[ ]vpp_filter_coefs_bicubic\[\][ ]=' drivers/gpu/drm/meson/meson_vpp.c
    defsc 'static[ ]const[ ]unsigned[ ]int[ ]a\(200\|220\|225\)_registers\[\][ ]=' drivers/gpu/drm/msm/adreno/a2xx_gpu.c
    defsc 'static[ ]const[ ]u32[ ]a6xx_\(ps_cluster_rac\|vbif_registers\|gmu_[gc]x_registers\)\[\][ ]=' drivers/gpu/drm/msm/adreno/a6xx_gpu-state.h
    defsc 'static[ ]const[ ]struct[ ]cmd_set[ ]qcom_2k_panel_magic_cmds\[\][ ]=' drivers/gpu/drm/panel/panel-truly-nt35597.c
    defsnc 'static[ ]const[ ]struct[ ]dw_hdmi_mpll_config[ ]sun50i_h6_mpll_cfg\[\][ ]=' drivers/gpu/drm/sun4i/sun8i_hdmi_phy.c
    defsnc 'static[ ]const[ ]struct[ ]dw_hdmi_curr_ctrl[ ]sun50i_h6_cur_ctr\[\][ ]=' drivers/gpu/drm/sun4i/sun8i_hdmi_phy.c
    defsnc '[\t]mipi_dbi_command[(]mipi[,][ ]HX8357D_SETGAMMA[,]' drivers/gpu/drm/tinydrm/hx8357d.c
    defsnc 'static[ ]const[ ]int[ ]rm3100_samp_rates\[RM3100_SAMP_NUM\]\[3\][ ]=' drivers/iio/magnetometer/rm3100-core.c
    defsc 'static[ ]const[ ]struct[ ]reg_8[ ]mode_\(4096x2304\|1920x1080\|table_common\)\[\][ ]=' drivers/media/i2c/imx214.c
    defsnc 'static[ ]const[ ]struct[ ]reg_value[ ]ov5640_setting_\(VGA_640_480\|XGA_1024_768\|QVGA_320_240\|QCIF_176_144\|NTSC_720_480\|PAL_720_576\|720P_1280_720\|1080P_1920_1080\|QSXGA_2592_1944\)\[\][ ]=' drivers/media/i2c/ov5640.c
    defsnc 'static[ ]const[ ]u32[ ]aspeed_video_jpeg_quant\[ASPEED_VIDEO_JPEG_QUANT_SIZE\][ ]=' drivers/media/platform/aspeed-video.c
    defsnc 'static[ ]const[ ]u32[ ]aspeed_video_jpeg_dct\[ASPEED_VIDEO_JPEG_NUM_QUALITIES\][\n\t ]*\[ASPEED_VIDEO_JPEG_DCT_SIZE\][ ]=' drivers/media/platform/aspeed-video.c
    defsnc '[\t]static[ ]u8[ ]rss_key\[AQ_CFG_RSS_HASHKEY_SIZE\][ ]=' drivers/net/ethernet/aquantia/atlantic/aq_nic.c
    defsnc 'static[ ]const[ ]u16[ ]mlxsw_sp_acl_bf_crc_tab\[256\][ ]=' drivers/net/ethernet/mellanox/mlxsw/spectrum_acl_bloom_filter.c
    defsc '[\t]*ipu3_css_bds_configs\[IMGU_BDS_CONFIG_LEN\][ ]=' drivers/staging/media/ipu3/ipu3-tables.c
    defsnc 'const[ ]s16[ ]ipu3_css_gdc_lut\[4\]\[256\][ ]=' drivers/staging/media/ipu3/ipu3-tables.c
    defsnc 'const[ ]struct[ ]ipu3_uapi_bnr_static_config[ ]ipu3_css_bnr_defaults[ ]=' drivers/staging/media/ipu3/ipu3-tables.c
    defsnc 'const[ ]struct[ ]ipu3_uapi_gamma_corr_lut[ ]ipu3_css_gamma_lut[ ]=' drivers/staging/media/ipu3/ipu3-tables.c
    defsnc '[\t]*ipu3_css_tcc_gain_pcwl_lut[ ]=' drivers/staging/media/ipu3/ipu3-tables.c
    defsnc 'const[ ]struct[ ]imgu_abi_anr_config[ ]ipu3_css_anr_defaults[ ]=' drivers/staging/media/ipu3/ipu3-tables.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]\(luma\|chroma\)_\(q\|ac\)_table\[\][ ]=' drivers/staging/media/rockchip/vpu/rockchip_vpu_jpeg.c
    defsc 'static[ ]const[ ]unsigned[ ]char[ ]rockchip_vpu_jpeg_header\[JPEG_HEADER_SIZE\][ ]=' drivers/staging/media/rockchip/vpu/rockchip_vpu_jpeg.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]fontdata_ter16x32\[FONTDATAMAX\][ ]=' lib/fonts/font_ter16x32.c
    accept '[\t][\t]\([{][ ]timeout\|["]tests[/]\|[!][ ]grep[ ]-Eq\)[^\n]*[ ]["]tests\/\$[{]testname[}]\.vg\.out["]' tools/lib/lockdep/run_tests.sh
    blobname 'amdgpu[/]\(%s\|picasso\)_rlc\(_am4\)\?\.bin' drivers/gpu/drm/amd/amdgpu/gfx_v9_0.c
    blobname 'amdgpu[/]\(%s\|vega20\)_ta\.bin' drivers/gpu/drm/amd/amdgpu/psp_v11_0.c
    blobname 'yamato_\(pm4\|pfp\)\.fw' drivers/gpu/drm/msm/adreno/adreno_device.c
    blobname 'leia_\(pm4\|pfp\)_470\.fw' drivers/gpu/drm/msm/adreno/adreno_device.c
    blobname 'nvidia[/]tegra194[/]vic\.bin' drivers/gpu/drm/tegra/vic.c
    blobname 'qtn[/]\(fmac\|uboot\)_qsr1000\.img' drivers/net/wireless/quantenna/qtnfmac/qtn_hw_ids.h
    accept '\(static[ ]inline[ ]void[ ]\|[\t]*\)pqi_request_firmware_feature[(]' drivers/scsi/smartpqi/smartpqi_init.c
    blobname 'intel[/]ipu3-fw\.bin' drivers/staging/media/ipu3/ipu3-css-fw.h
    blobname 'intel[/]dsp_fw_icl\.bin' sound/soc/intel/common/soc-acpi-intel-icl-match.c
    # SOF stands for Sound Open Firmware, and it is Free Software.
    # blobname '\(sof\|reef\)-icl\(\.ri\|-rt274\.tplg\)' sound/soc/intel/common/soc-acpi-intel-icl-match.c
    blobname 'iwl-dbg-tlv\.ini' drivers/net/wireless/intel/iwlwifi/iwl-dbg-tlv.c
    accept '\(static[ ]int[ ]\|[\t]*\)brcmf_fw_request_firmware[(]' drivers/net/wireless/broadcom/brcm80211/brcmfmac/firmware.c
    blobna 'snprintf[(]version[,][ ]ETHTOOL_FWVERS_LEN[,][ ]["][ ]storm[ ]%d\.%d\.%d\.%d["]\([,][ \t\n]*BCM_5710_FW_\(MAJOR\|MINOR\|REVISION\|ENGINEERING\)_VERSION\)\+[)]' drivers/net/ethernet/broadcom/bnx2x/bnx2x_ethtool.c
    # In case the command matched by the above is changed and it then
    # fails to match, catch the snprintf format string, since the FW
    # macros will be caught and dropped by other much earlier patterns.
    blobname '[ ]storm[ ]%d\.%d\.%d\.%d' drivers/net/ethernet/broadcom/bnx2x/bnx2x_ethtool.c
    # These are probably older, we did not check for .ri and .tplg before.
    # blobname 'intel[/]\(sof\|reef\)-apl\(\.ri\|-\(rt298\|da7219\|pcm512x\|wm8804\|tdf8532\)\.tplg\)' sound/soc/intel/common/soc-acpi-intel-bxt-match.c
    # blobname 'intel[/]\(sof\|reef\)-byt\(\.ri\|-\(rt5670\|rt5640\|rt5651\|da7213\|rt5645\|max98090\)\.tplg\)' sound/soc/intel/common/soc-acpi-intel-byt-match.c
    # blobname 'intel[/]\(sof\|reef\)-cht\(\.ri\|-\(rt5645\|rt5670\|max98090\|nau8824\|da7213\|es8316\|rt5640\|rt5651\)\.tplg\)' sound/soc/intel/common/soc-acpi-intel-cht-match.c
    # blobname 'intel[/]\(sof\|reef\)-cnl\(\.ri\|-rt274\.tplg\)' sound/soc/intel/common/soc-acpi-intel-cnl-match.c
    # blobname 'intel[/]\(sof\|reef\)-glk\(\.ri\|-\(alc298\|da7219\)\.tplg\)' sound/soc/intel/common/soc-acpi-intel-glk-match.c
    # blobname 'intel[/]\(sof\|reef\)-hda-generic\.tplg' sound/soc/intel/common/soc-acpi-intel-hda-match.c
    # blobname 'intel[/]\(sof\|reef\)-hsw\(\.ri\|\.tplg\)' sound/soc/intel/common/soc-acpi-intel-hsw-bdw-match.c
    # blobname 'intel[/]\(sof\|reef\)-bdw\(\.ri\|-\(rt286\|rt5677\|rt5640\)\.tplg\)' sound/soc/intel/common/soc-acpi-intel-hsw-bdw-match.c
    accept '[\t][\t]pr_err[(]["]%s:[ ]request_firmware[ ]error' drivers/net/wireless/quantenna/qtnfmac/pcie/topaz_pcie.c

    # New in 5.0.7.
    accept '[\t]*[/]bin[/]bash[ ]["]tests[/][$][{]testname[}]\.sh["][ ][<][ ]["]tests[/][$][{]testname[}]\.vg\.out["]' tools/lib/lockdep/run_tests.sh

    # New in 5.1-rc6.
    initnc '.Lbyteshift_table:' 'arch/arm/crypto/crct10dif-\(ce-core\|pcl-asm_64\)\.S'
    defsc 'static[ ]const[ ]struct[ ]aead_testvec[ ]hmac_sha\(1\|256\|512\)_aes_cbc_tv_temp\[\][ ]=' crypto/testmgr.h
    defsc 'static[ ]const[ ]struct[ ]aead_testvec[ ]hmac_sha\(1\|224\|256\|384\|512\)_des_cbc_tv_temp\[\][ ]=' crypto/testmgr.h
    defsc 'static[ ]const[ ]struct[ ]aead_testvec[ ]hmac_sha\(1\|224\|256\|384\|512\)_des3_ede_cbc_tv_temp\[\][ ]=' crypto/testmgr.h
    defsc 'static[ ]const[ ]struct[ ]aead_testvec[ ]\(aes_\(gcm_rfc4106\|ccm_rfc4309\)\|rfc7539\(\|esp\)\)_tv_template\[\][ ]=' crypto/testmgr.h
    initnc '\t\.entries[ ]=' drivers/clk/tegra/clk-tegra124-dfll-fcpu.c
    accept '[	][	]*gf100_gr_init_fw[(]gr->fecs\.falcon[,][ ][&]gr->fuc409c[,][ ][&]gr->fuc409d[)][;]' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf100.c
    accept '[	][	]*gf100_gr_init_fw[(]gr->gpccs\.falcon[,][ ][&]gr->fuc41ac[,][ ][&]gr->fuc41ad[)][;]' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf100.c
    defsnc 'static[ ]const[ ]struct[ ]kingdisplay_panel_cmd[ ]init_code\[\][ ]=' drivers/gpu/drm/panel/panel-kingdisplay-kd097d04.c
    defsnc 'static[ ]const[ ]struct[ ]ov8856_reg[ ]mode_\(3280x2464\|1640x1232\)_regs\[\][ ]=' drivers/media/i2c/ov8856.c
    defsnc 'static[ ]const[ ]u8[ ]hclge_hash_key\[\][ ]=' drivers/net/ethernet/hisilicon/hns3/hns3pf/hclge_main.c
    defsnc 'static[ ]const[ ]u8[ ]hclgevf_hash_key\[\][ ]=' drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_main.c
    defsnc 'static[ ]const[ ]u32[ ]max77651_sbb1_regulator_volt_table\[\][ ]=' drivers/regulator/max77650-regulator.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]pv88090_buck1_limits\[\][ ]=' drivers/regulator/pv88090-regulator.c
    defsc '\t*imgu_css_bds_configs\[IMGU_BDS_CONFIG_LEN\][ ]=' drivers/staging/media/ipu3/ipu3-tables.c
    defsnc 'const[ ]s16[ ]imgu_css_gdc_lut\[4\]\[256\][ ]=' drivers/staging/media/ipu3/ipu3-tables.c
    defsc 'const[ ]struct[ ]ipu3_uapi_bnr_static_config[ ]imgu_css_bnr_defaults[ ]=' drivers/staging/media/ipu3/ipu3-tables.c
    defsnc 'const[ ]struct[ ]ipu3_uapi_gamma_corr_lut[ ]imgu_css_gamma_lut[ ]=' drivers/staging/media/ipu3/ipu3-tables.c
    defsnc '\t*imgu_css_tcc_gain_pcwl_lut[ ]=' drivers/staging/media/ipu3/ipu3-tables.c
    defsnc 'const[ ]struct[ ]imgu_abi_anr_config[ ]imgu_css_anr_defaults[ ]=' drivers/staging/media/ipu3/ipu3-tables.c
    defsnc 'static[ ]struct[ ]channel_list[ ]channel_array\[\][ ]=' drivers/staging/rtl8192e/dot11d.c
    accept '\t*sprintf[(]fname[,][ ]["]hbm\.%d\.out["]' samples/bpf/hbm.c
    accept '\tsnd_card_ro_proc_new[(]hdspm-[>]card[,][ ]["]ports\.out["]' sound/pci/rme9652/hdspm.c
    defsnc 'static[ ]const[ ]struct[ ]cs35l36_pll_config[ ]cs35l36_pll_sysclk\[\][ ]=' sound/soc/codecs/cs35l36.c
    defsnc 'static[ ]const[ ]u8[ ]table_msbc_silence\[SCO_PACKET_180\][ ]=' sound/soc/mediatek/common/mtk-btcvsd.c
    accept '[#][ ]that[ ]of[ ]the[ ]specified[ ]litmus[ ]test[,][ ]but[ ]with[ ]["]\.out["][ ]appended' tools/memory-model/scripts/checkalllitmus.sh
    accept '\t\.data[ ]=[ ][{]\([\n\t ]*0\(\|x08\|x06\|x10\)*[,]\)*\([ ]0x\(bf\|48\|d6\|43\)[,]\)*[ ]0xd6[,]' tools/testing/selftests/bpf/verifier/ld_abs.c
    blobname 'habanalabs[/]goya[/]goya-\(u-boot\.bin\|fit\.itb\)' drivers/misc/habanalabs/goya/goya.c
    blobname 'mrvl[/]sd8977_uapsta\.bin' 'drivers/bluetooth/btmrvl_sdio\.c\|drivers/net/wireless/marvell/mwifiex/sdio\.h'
    blobname 'mediatek[/]mt766[38]pr2h\.bin' drivers/bluetooth/btmtkuart.c
    blobname 'mt76\(03\|28\)_e[12]\.bin' drivers/net/wireless/mediatek/mt76/mt7603/mt7603.h
    blobname 'gsl3676-chuwi-hi8-air\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'gsl1680-chuwi-hi10-air\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'gsl3692-pov-mobii-wintab-p1006w-v10\.fw' drivers/platform/x86/touchscreen_dmi.c
    # blobname '\(sof\|reef\)-apl\(\.ri\|-\(rt298\|da7219\|pcm512x\|wm8804\|tdf8532\)\.tplg\)' sound/soc/intel/common/soc-acpi-intel-bxt-match.c
    # blobname '\(sof\|reef\)-byt\(\.ri\|-\(rt5670\|rt5640\|rt5651\|da7213\|es8316\|rt5645\|max98090\)\.tplg\)' sound/soc/intel/common/soc-acpi-intel-byt-match.c
    # blobname '\(sof\|reef\)-cht\(\.ri\|-\(rt5645\|rt5670\|rt5645\|max98090\|nau8824\|da7213\|es8316\|rt5640\|rt5651\)\.tplg\)' sound/soc/intel/common/soc-acpi-intel-cht-match.c
    # blobname '\(sof\|reef\)-cnl\(\.ri\|-rt274\.tplg\)' sound/soc/intel/common/soc-acpi-intel-cnl-match.c
    # blobname '\(sof\|reef\)-glk\(\.ri\|-\(alc298\|da7219\)\.tplg\)' sound/soc/intel/common/soc-acpi-intel-glk-match.c
    # blobname '\(sof\|reef\)-hda-generic\.tplg' sound/soc/intel/common/soc-acpi-intel-hda-match.c
    # blobname '\(sof\|reef\)-hsw\(\.ri\|\.tplg\)' sound/soc/intel/common/soc-acpi-intel-hsw-bdw-match.c
    # blobname '\(sof\|reef\)-bdw\(\.ri\|-\(rt286\|rt5677\|rt5640\)\.tplg\)' sound/soc/intel/common/soc-acpi-intel-hsw-bdw-match.c
    # blobname '\(sof\|reef\)-icl\(\.ri\|-rt274\.tplg\)' sound/soc/intel/common/soc-acpi-intel-icl-match.c
    blobna '[/][*][ ]brcmfmac4366c-pcie\.\(ap\.\)\?bin[ ]from[ ]linux-firmware\.git[ ]commit[ ][0-9a-f]*[ ][*][/]' drivers/net/wireless/broadcom/brcm80211/brcmfmac/feature.c
    blobname 'iwlwifi-[^ ]*-[ab]0-' drivers/net/wireless/intel/iwlwifi/cfg/22000.c
    blobname 'iwlwifi-\(\(QuZ-a0-hr\|QuQnj-b0-jf\|so-a0-\(jf\|hr\)\)-b0\|\(cc\|\(so\|ty\)-a0-gf\)-a0\)-' drivers/net/wireless/intel/iwlwifi/cfg/22000.c

    # New in 5.1.2, 5.0.16, 4.19.43, 4.14.119, and 4.9.176.
    accept '[ ][ ]the[ ]CPUID[ ]to[ ]the[ ]guest[.][ ]If[ ]the[ ]host[ ]has[ ]updated[ ]microcode[ ]the[ ]protection' 'Documentation/\(admin-guide/\)\?hw-vuln/mds\.rst'
    accept 'instruction[ ]in[ ]combination[ ]with[ ]a[ ]microcode[ ]update[.][ ]The[ ]microcode[ ]clears' Documentation/x86/mds.rst
    accept '[ \t]*scenarios[ ]where[ ]the[ ]host[ ]has[ ]the[ ]updated[ ]microcode[ ]but' Documentation/x86/mds.rst

    # New in 5.2.
    blobname 'nvidia[/]%s[/]%s\(-%d\)\?\.bin' drivers/gpu/drm/nouveau/nvkm/core/firmware.c
    accept '\(63\|31\|56\|24\|39\|32\|[0437][ ]\)\([ ]\([0-9 ][0-9 ]\)\)*[ ]\(56\|63\|32\|39\|24\|31\|[ ]\?[0437]\)\([\n]\(63\|31\|56\|24\|39\|32\|[0437][ ]\)\([ ]\([0-9 ][0-9 ]\)\)*[ ]\(56\|63\|32\|39\|24\|31\|[ ]\?[0437]\)\)*' Documentation/packing.txt
    blobname 'amd-ucode[/]microcode_amd[*]\.bin' Documentation/x86/microcode.rst
    accept '[ ][ ]CONFIG_EXTRA_FIRMWARE=["][/][*][(]DEBLOBBED[)][*][/][ ][/][*][(]DEBLOBBED[)][*][/]["]' Documentation/x86/microcode.rst
    blobname 'imx[/]sdma[/]sdma-imx7d\.bin' arch/arm64/boot/dts/freescale/imx8mq.dtsi
    # Still very suspicious, but it doesn't look like code, and the
    # license, if it can be trusted, makes it acceptable for magic
    # data numbers.
    defsc 'static[ ]uint32_t[ ]onyx_images\[\]\[PCXU_IMAGE_SIZE[/]sizeof[(]uint32_t[)]\][ ]__ro_after_init[ ]=' arch/parisc/kernel/perf_images.h
    defsc 'static[ ]uint32_t[ ]cuda_images\[\]\[PCXW_IMAGE_SIZE[/]sizeof[(]uint32_t[)]\][ ]__ro_after_init[ ]=' arch/parisc/kernel/perf_images.h
    defsc '[\t]struct[ ]prng_parm[ ]prng[ ]=' arch/s390/boot/kaslr.c
    defsc '[\t]u8[ ][*]pg[,][ ]pblock\[80\][ ]=' arch/s390/crypto/prng.c
    defsnc '__visible[ ]const[ ]u32[ ]crypto_[fi][tl]_tab\[4\]\[256\][ ]____cacheline_aligned[ ]=' crypto/aes_generic.c
    blobname 'mrvl[/]sd8987_uapsta\.bin' 'drivers/\(bluetooth/btmrvl_sdio\.c\|net/wireless/marvell/mwifiex/sdio\.h\)'
    blobname 'mediatek[/]mt766[38]pr2h\.bin' drivers/bluetooth/btmtksdio.c
    blobname 'amdgpu[/]%s_kicker_rlc\.bin' drivers/gpu/drm/amd/amdgpu/gfx_v9_0.c
    defsnc 'static[ ]struct[ ]profile_mode_setting[ ]smu7_profiling\[7\][ ]=' drivers/gpu/drm/amd/powerplay/hwmgr/smu7_hwmgr.c
    blobname 'a630_zap\.mdt' drivers/gpu/drm/msm/adreno/adreno_device.c
    accept '[\t]dsi_generic_write_seq[(]dsi[,][ ]ST7703_CMD_SET\(GIP[12]\|GAMMA\)\([, \t\n]*0x[0-9A-F][0-9A-F]\)*[)][;]' drivers/gpu/drm/panel/panel-rocktech-jh057n00900.c
    blobname 'intel[/]%s' drivers/hid/intel-ish-hid/ishtp-fw-loader.c
    defsnc 'const[ ]unsigned[ ]int[ ]wm831x_isinkv_values\[WM831X_ISINK_MAX_ISEL[ ][+][ ]1\][ ]=' drivers/mfd/wm831x-core.c
    # File name is supplied through ethtool.
    accept '[\t]*status[ ]=[ ]request_firmware[(][&]ddp_config[,][ ]profile_name[,]' drivers/net/ethernet/intel/i40e/i40e_ddp.c
    defsnc 'static[ ]const[ ]u16[ ]iwl_\(ext\|uhb\)_nvm_channels\[\][ ]=' drivers/net/wireless/intel/iwlwifi/iwl-nvm-parse.c
    blobname 'brcmfmac43012-sdio' drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
    blobname 'mt7615_\(cr4\|n9\|rom_patch\)\.bin' drivers/net/wireless/mediatek/mt76/mt7615/mt7615.h
    defsnc 'static[ ]const[ ]struct[ ]rf_channel[ ]rf_vals_3853\[\][ ]=' drivers/net/wireless/ralink/rt2x00/rt2800lib.c
    accept '[\t]fw->firmware[ ]=[ ]firmware[;]' drivers/net/wireless/realtek/rtw88/main.c
    defsnc 'static[ ]const[ ]u32[ ]db_invert_table\[12\]\[8\][ ]=' drivers/net/wireless/realtek/rtw88/phy.c
    blobname 'rtw88[/]rtw8822b_fw\.bin' drivers/net/wireless/realtek/rtw88/rtw8822b.c
    defsnc 'static[ ]const[ ]u32[ ]rtw8822b_\(mac\|agc\|bb\(\|_pg_type[25]\)\|rf_[ab]\)\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8822b_table.c
    defsnc 'static[ ]const[ ]u8[ ]rtw8822b_txpwr_lmt_type[25]\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8822b_table.c
    blobname 'rtw88[/]rtw8822c_fw\.bin' drivers/net/wireless/realtek/rtw88/rtw8822c.c
    defsnc 'static[ ]const[ ]u32[ ]rtw8822c_\(agc\|bb\(\|_pg_type0\)\|rf_[ab]\|array_mp_cal_init\)\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8822c_table.c
    defsnc 'static[ ]const[ ]u8[ ]rtw8822c_txpwr_lmt_type0\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8822c_table.c
    blobname 'gsl3692-jumper-ezpad-6-pro-b\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'gsl1680-myria-my8307\.fw' drivers/platform/x86/touchscreen_dmi.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]max77651_sbb1_regulator_volt_table\[\][ ]=' drivers/regulator/max77650-regulator.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]isink_cur\[\][ ]=' drivers/regulator/wm8350-regulator.c
    blobname 'ql2800_fw\.bin' drivers/scsi/qla2xxx/qla_os.c
    accept 'static[ ]const[ ]struct[ ]tegra_xusb_soc[ ]tegra186_soc[ ]=[ ][{][\n][\t][.]firmware[ ]=' drivers/usb/host/xhci-tegra.c
    blobname 'nvidia[/]tegra186[/]xusb\.bin' drivers/usb/host/xhci-tegra.c
    blobname 'ccg_\(boot\|primary\|secondary\)\.cyacd' drivers/usb/typec/ucsi/ucsi_ccg.c
    defsnc 'static[ ]const[ ]struct[ ]utf8data[ ]utf8nfdi\(cf\|\)data\[\][ ]=' fs/unicode/utf8data.h_shipped
    defsc 'static[ ]const[ ]unsigned[ ]char[ ]utf8data\[64256\][ ]=' fs/unicode/utf8data.h_shipped
    accept '[\t]*\.sof_fw_filename[ ]=[ ]["]\(intel[/]\)\?\(sof\|reef\)-[^" ;]*\.ri["]' sound/soc/intel/common/soc-acpi-intel-'\(b[xy]t\|cht\|cnl\|icl\|glk\|hda\|hsw-bdw\|kbl\|skl\)-match\.c'
    accept '[\t]*\.sof_tplg_filename[ ]=[ ]["]\(intel[/]\)\?\(sof\|reef\)-[^" ;]*\.tplg["]' sound/soc/intel/common/soc-acpi-intel-'\(b[xy]t\|cht\|cnl\|icl\|glk\|hda\|hsw-bdw\|kbl\|skl\)-match\.c'
    accept '[\t]*tplg_filename[ ]=[ ]devm_kasprintf[(]sdev->dev[,][ ]GFP_KERNEL[,][\n\t ]*["]%s-idisp\.tplg["][,][ ]split_ext[)]' sound/soc/sof/intel/hda.c
    accept '[\t]ret[ ]=[ ]request_firmware[(][&]plat_data->fw[,][ ]fw_filename[,][ ]sdev->dev[)]' sound/soc/sof/loader.c
    accept '[\t]*\.\(nocodec\|sof\)_fw_filename[ ]=[ ]["]\(sof\|reef\)-[^" ;]*\.ri["]' sound/soc/sof/'\(sof\|reef\)-\(acpi\|pci\)-dev\.c'
    accept '[\t]*\.\(nocodec\|sof\)_tplg_filename[ ]=[ ]["]\(sof\|reef\)-[^" ;]*\.tplg["]' sound/soc/sof/'\(sof\|reef\)-\(acpi\|pci\)-dev\.c'
    accept '[\t]ret[ ]=[ ]request_firmware[(][&]fw[,][ ]file[,][ ]sdev->dev[)]' sound/soc/sof/topology.c
    # blobname '\(sof\|reef\)-byt-rt5682\.tplg' sound/soc/intel/common/soc-acpi-intel-byt-match.c
    # blobname '\(sof\|reef\)-cht-rt5682\.tplg' sound/soc/intel/common/soc-acpi-intel-cht-match.c
    # blobname '\(sof\|reef\)-cml-rt5682\(-max98357a\)\?\.tplg' sound/soc/intel/common/soc-acpi-intel-cnl-match.c
    # blobname '\(sof\|reef\)-glk-rt5682\.tplg' sound/soc/intel/common/soc-acpi-intel-glk-match.c
    # blobname '\(sof\|reef\)-icl-rt5682\.tplg' sound/soc/intel/common/soc-acpi-intel-icl-match.c
    # blobname '%s-idisp\.tplg' sound/soc/sof/intel/hda.c
    # blobname '\(sof\|reef\)-\(hsw\|bdw\|byt\|cht\)\(\.ri\|\(-nocodec\)\?\.tplg\)' sound/soc/sof/'\(sof\|reef\)-acpi-dev\.c'
    # blobname '\(sof\|reef\)-\(apl\|glk\|cnl\|icl\|skl\|kbl\)\(\.ri\|\(-nocodec\)\?\.tplg\)' sound/soc/sof/'\(sof\|reef\)-pci-dev\.c'

    # New in 5.2.1, 5.1.18, and 4.19.58.
    accept '[ ][ ][ ]the[ ]latest[ ]updated[ ]microcode\.' Documentation/admin-guide/hw-vuln/spectre.rst

    # New in 5.2.3, 5.1.20, and 4.19.61.
    defsnc 'static[ ]const[ ]u32[ ]runnable_avg_yN_inv\[\][ ]__maybe_unused[ ]=' kernel/sched/sched-pelt.h

    # New in 5.3.
    accept 'int[ ]rtl_fw_request_firmware[(]' drivers/net/ethernet/realtek/r8169_firmware.c
    accept '[\t]if[ ][(]rtl_fw_request_firmware[(]' drivers/net/ethernet/realtek/r8169_main.c
    defsnc 'static[ ]const[ ]struct[ ]phy_reg[ ]rtl8168d_1_phy_reg_init_0\[\][ ]=' drivers/net/ethernet/realtek/r8169_main.c
    defsnc '[ ][ ]const[ ]char[ ]parity\[256\][ ]=' Documentation/driver-api/mtd/nand_ecc.rst
    defsc 'static[ ]const[ ]struct[ ]si5341_reg_default[ ]si5341_reg_defaults\[\][ ]=' drivers/clk/clk-si5341.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_\([56789]\|1[012]\)tap_16p_\(upscale\|117\|150\|183\)\[\(45\|54\|63\|72\|81\|9[09]\|108\)\][ ]=' drivers/gpu/drm/amd/display/dc/dcn20/dcn20_dwb_scl.c
    defsnc 'const[ ]qp_table[ \t]\+qp_table_4\(2[02]\|44\)_\(8\|1[02]\)bpc_m\(in\|ax\)[ ]=' drivers/gpu/drm/amd/display/dc/dsc/qp_tables.h
    defsnc 'static[ ]const[ ]struct[ ]IP_BASE[ ]\(DCN\|RSMU\|VCN\)_BASE[ \t]\+=' drivers/gpu/drm/amd/include/navi10_ip_offset.h
    defsnc 'rdma_dim_prof\[RDMA_DIM_PARAMS_NUM_PROFILES\][ ]=' drivers/infiniband/core/cq.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]applespi_scancodes\[\][ ]=' drivers/input/keyboard/applespi.c
    defsc 'const[ ]u32[ ]isc_gamma_table\[GAMMA_MAX[ ][+][ ]1\]\[GAMMA_ENTRIES\][ ]=' drivers/media/platform/atmel/atmel-isc.c
    defsnc 'static[ ]const[ ]struct[ ]reg_sequence[ ]cs47l92_reva_\(16\|32\)_patch\[\][ ]=' drivers/mfd/cs47l92-tables.c
    defsc 'static[ ]const[ ]unsigned[ ]char[ ]hantro_jpeg_header\[JPEG_HEADER_SIZE\][ ]=' drivers/staging/media/hantro/hantro_jpeg.c
    defsnc 'static[ ]const[ ]u8[ ]zigzag\[64\][ ]=' drivers/staging/media/hantro/hantro_mpeg2.c
    defsnc 'static[ ]u64[ ]intervals[0124]\[\][ ]__initdata[ ]=' kernel/irq/timings.c
    defsnc 'static[ ]struct[ ]etab[ ]Tab\[\][ ]=' lib/reed_solomon/test_rslib.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt1011_reg\[\][ ]=' sound/soc/codecs/rt1011.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt1308_reg\[\][ ]=' sound/soc/codecs/rt1308.c
    for n in ptwrite cbr mwait pwre exstop pwrx context_switches; do
	defsnc "$n"'_file[ \t]*=[ ]open_output_file[(]["]'"$n"'_table\.bin["][)]' tools/perf/scripts/python/export-to-postgresql.py
    done
    blobname 'nvm_00440302\.bin' Documentation/devicetree/bindings/net/qualcomm-bluetooth.txt
    blobname 'crnv21\.bin' Documentation/devicetree/bindings/net/qualcomm-bluetooth.txt
    accept 'bpp\([ ]\+[0-9]\+x[0-9]\+\)*[\n][ =]*\([\n][ ]*[0-9]\+\([ ]*0x[0-9A-F]*\)*\)*' Documentation/fb/matroxfb.rst
    accept '[ ][ ]pct[ ]confidence[ ]steady[ ]dynamic[ ][(]compensation[)]\([\n][ ]*[0-9]\([ ]\+[0123]\)\+\)\+[\n][ ]*[.]*\([\n][ ]*[34][0-9]\([ ]\+[0123]\)\+\)\+' Documentation/thermal/intel_powerclamp.rst
    blobname 'amdgpu[/]navi10_vcn\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vcn.c
    blobname 'amdgpu[/]%s_ta\.bin' drivers/gpu/drm/amd/amdgpu/psp_v11_0.c
    blobname 'i915[/]\(["][ ][\\][\n][\t]__stringify[(]KEY##_GUC_FW_\(PREFIX\|MAJOR\|MINOR\|PATCH\)[)][ ]["][^"]*\)\+' drivers/gpu/drm/i915/intel_guc_fw.c
    blobname 'a540_\(gpmu\.fw2\|zap\.mdt\)' drivers/gpu/drm/msm/adreno/adreno_device.c
    blobname 'dvb-tuner-si2157-a30-01\.fw' drivers/media/tuners/si2157_priv.h
    accept 'static[ ]struct[ ]dvb_usb_device_properties[\n]cxusb_bluebird_\(lgh064f\|dee1601\|lgz201\|dtt7579\|nano2_needsfirmware\)_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/dvb/dvb-usb/cxusb.c
    blobname 'v4l-pvrusb2-160xxx-01\.fw' drivers/media/usb/pvrusb2/pvrusb2-devattr.c
    blobname 'gsl1680-chuwi-hi10plus\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname '%s%pUL%s["][,][\n \t]*["]intel[/]dsp_fw_["][,][ ]guid[,][ ]["]\.bin' sound/soc/intel/skylake/skl-sst.c
    blobname 'qcom[/]db845c[/]\(adsp\|cdsp\)\.mdt' arch/arm64/boot/dts/qcom/sdm845-db845c.dts
    accept '[\t]rpi->firmware[ ]=[ ]' drivers/clk/bcm/clk-raspberrypi.c
    blobname 'display_hdcp_srm\.bin' drivers/gpu/drm/drm_hdcp.c
    accept '[ ][*][ ]SRM[ ]should[ ]be[ ]presented[ ]in[ ]the[ ]name[ ]of[ ]["][^"]*["]' drivers/gpu/drm/drm_hdcp.c
    accept '[\t]s6e63m0_dcs_write_seq_static[(]ctx[,][ ]0xb[579]\([, \t\n]*0x[0-9a-f][0-9a-f]\)*[)][;]' drivers/gpu/drm/panel/panel-samsung-s6e63m0.c
    # The link to "source" for this and other firmware files in
    # LibreELEC meson-firmware is broken, but I tracked it down and
    # it's just a binary blob encoded as an array initializer.
    blobname 'meson[/]vdec[/]gxl_mpeg12\.bin' drivers/staging/media/meson/vdec/vdec_platform.c
    accept '[\t]echo[ ]-n[ ]["]Batched[ ]request_firmware\(_direct\|_nowait\)\?[(]' tools/testing/selftests/firmware/fw_filesystem.sh
    # The firmware file name is supplied by the user.
    accept '[\t]err[ ]=[ ]request_firmware_direct[(][&]fw[,][ ]file_name[,]\([^\n]*[\n]\+[^\n}]\)*return[ ]mlx5_firmware_flash[(]dev[,][ ]fw[,]' drivers/net/ethernet/mellanox/mlx5/core/devlink.c
    accept '[\t]err[ ]=[ ]request_firmware_direct[(][&]fw[,][ ]flash->data[,]\([^\n]*[\n]\+[^\n}]\)*err[ ]=[ ]mlx5_firmware_flash[(]mdev[,][ ]fw[,]' drivers/net/ethernet/mellanox/mlx5/core/en_ethtool.c
    # This firmware file name is supplied by the user,
    # but there's another in the same source file (way above) that is hardcoded.
    accept '[\t]err[ ]=[ ]request_firmware_direct[(][&]firmware[,][ ]\(fw_filename\|file_name\)[,]\([^\n]*[\n]\+[^\n}]\)*err[ ]=[ ]mlxsw_sp_firmware_flash[(]mlxsw_sp[,][ ]firmware[,]' drivers/net/ethernet/mellanox/mlxsw/spectrum.c
    blobname 'al5e\(_b\)\?\.fw' drivers/staging/media/allegro-dvt/allegro-core.c
    # Sources are in cwsr_trap_handler_gfx10.asm.
    defsnc 'static[ ]const[ ]uint32_t[ ]cwsr_trap_gfx10_hex\[\][ ]=' drivers/gpu/drm/amd/amdkfd/cwsr_trap_handler.h
    blobname 'amdgpu[/]%s_mes\.bin' drivers/gpu/drm/amd/amdgpu/mes_v10_1.c
    accept 'static[ ]int[ ]allegro_firmware_request_nowait[(]' drivers/staging/media/allegro-dvt/allegro-core.c
    accept '[\t]ret[ ]=[ ]allegro_firmware_request_nowait[(]' drivers/staging/media/allegro-dvt/allegro-core.c

    # New in 5.3.4 and 5.2.19
    defsnc '[\t]static[ ]const[ ]struct[ ]hda_alc298_mbxinit[ ]dac_init\[\][ ]=' sound/pci/hda/patch_realtek.c
    blobname 'mediatek[/]mt7615_\(cr4\|n9\|rom_patch\)\.bin' drivers/net/wireless/mediatek/mt76/mt7615/mt7615.h

    # WIP: False positives of suspicious extensions followed by anything
    # other than quotes.
    accept '\(BIN\|IHEX\)[\t]:=[ ][$][(]patsubst[ ]%\.S[,][ ]%\.bin\(\.ihex\)\?' Documentation/EDID/Makefile
    accept '[\t]@rm[ ]-f[ ][*]\.o[ ][*]\.bin\.ihex[ ][*]\.bin[ ]' Documentation/EDID/Makefile
    accept '%\.bin\(\.nocrc\|\.ihex\)\?:[\t]%\.[op]' Documentation/EDID/Makefile
    accept '%\.crc:[\t]%\.bin\.nocrc' Documentation/EDID/Makefile
    accept '[ ]*[(]e\.g\.[ ]support[ ]for[ ]RAM[ ]disks[,][ ]initrd[,][ ]a\.out[,]' Documentation/admin-guide/initrd.rst
    accept '[\t]*System\.out\.println' Documentation/admin-guide/java.rst
    accept '[\t]*edid[/]1024x768\.bin[,][ ]edid[/]1280x1024\.bin[,]' Documentation/admin-guide/kernel-parameters.txt
    accept '[\t]*edid[/]1680x1050\.bin[,][ ]or[ ]edid[/]1920x1080\.bin[,]' Documentation/admin-guide/kernel-parameters.txt
    accept '[ ]*disk[ ]=[ ]\[[ ][\'"'"']file:[/]root[/]rhel5\.img[,]' Documentation/ia64/xen.rst
    accept '[\t]*[$][(]obj[)][/]vmlinux\.bin\.gz:[ ][$][(]vmlinux\.bin\.all-y[)]' Documentation/kbuild/makefiles.rst
    accept 'raw2pnm[ ]-x2560[ ]-y1920[ ]-fNV12[ ][/]tmp[/]frames\.out[ ][/]tmp[/]frames\.out\.ppm' Documentation/media/v4l-drivers/ipu3.rst
    accept 'the[ ]file[ ]is[ ]6pack\.bin\.' Documentation/networking/6pack.txt
    accept 'CMAGIC[ ]*0x0111[ ]*user[ ]*``include[/]linux[/]a\.out\.h``' 'Documentation/\(process\|translations/\(it_IT\|zh_CN\)\)/magic-number\.rst'
    accept '[ ]*[#][ ]\(echo[ ][\'"'"']\|trigger[ ]info:[ ]\)[!]\?hist:\(name=foo:\)\?keys=\(skbaddr\|call_site\)\.hex:' Documentation/trace/histogram.rst
    accept '#include[ ][<]\(linux\|uapi[/]asm\)[/]a\.out\.h[>]' 'arch/\(alpha/\(boot/tools/objstrip\.c\|include/asm/a\.out\.h\|kernel/binfmt_loader\.c\)\|x86/ia32/ia32_aout\.c\)'
    accept 'targets[ ]:=[ ]vmlinux\.bin[ ]vmlinux\.bin\.gz[ ]' arch/arc/boot/Makefile
    accept 'extra-y[ ][+]=[ ]vmlinux\.bin\.\(gz\|lzma\)' arch/arc/boot/Makefile
    accept '[$][(]obj[)][/]\(vmlinuz\.bin\(\.gz\|\.lzma\)\?\|uImage\.\(bin\|gz\|lzma\)\):[ ]\([$][(]obj[)][/]\)\?vmlinux\(\.bin\(\.gz\|\.lzma\)\?\)\?[ ]' arch/arc/boot/Makefile
    accept '[\t][ ][*][ ]using[ ]flashwriter_nand\.out[,][ ]but' arch/arm/mach-davinci/board-dm644x-evm.c
    accept '[\t]fw[ ]=[ ]am200_board\.fw[;]' arch/arm/mach-pxa/am200epd.c
    accept '[#][ ]Default[ ]to[ ]vmlinuxz.bin[,][ ]override' arch/c6x/Makefile
    accept 'vmlinux\.bin:[ ]vmlinux' 'arch/\(c6x\|ia64\)/Makefile'
    accept '[$][(]obj[)][/]vmlinux\.bin:' 'arch/\(c6x\|mips\|nios2\|parisc\|s390\|sh\|x86\)/boot/\(compressed/\)\?Makefile'
    accept 'vmlinux\.srec[ ]vmlinux\.bin[ ]zImage[ ]uImage\.bin:[ ]vmlinux' arch/h8300/Makefile
    accept '[$][(]obj[)][/]vmlinux\.srec[ ][$][(]obj[)][/]vmlinux\.bin:' arch/h8300/boot/Makefile
    accept '[$][(]obj[)][/]uImage\.bin:[ ][$][(]obj[)][/]vmlinux\.bin' arch/h8300/boot/Makefile
    accept 'targets[\t]*:=[ ]vmlinux[ ]vmlinux\.bin[ ]vmlinux\.bin\.gz' arch/h8300/boot/compressed/Makefile
    accept '[$][(]obj[)][/]\(vmlinux\.bin\(\.[$][(]suffix-y[)]\)\?\|piggy\.o\):\([ ]\([$][(]obj[)][/]\)\?vmlinux\(\.scr\|\.bin\(\.[$][(]suffix-y[)]\)\?\)\?\)*' arch/h8300/boot/compressed/Makefile
    accept 'PHONY[ ][+]=[ ]linux\.bin[ ]linux\.bin\.gz[ ]linux\.bin\.ub' arch/microblaze/Makefile
    accept 'linux\.bin\.ub[ ]linux\.bin\.gz:[ ]linux\.bin' arch/microblaze/Makefile
    accept 'linux\.bin:[ ]vmlinux' arch/microblaze/Makefile
    accept 'linux\.bin[ ]linux\.bin\.gz[ ]linux\.bin\.ub:' arch/microblaze/Makefile
    accept '[ ]*echo[ ][\'"'"'][ ]*linux.bin.\(gz\|ub\)' arch/microblaze/Makefile
    accept 'targets[ ]:=[ ]linux\.bin[ ]linux\.bin\.gz[ ]linux\.bin\.ub' arch/microblaze/boot/Makefile
    accept '[$][(]obj[)][/]linux\.bin\(\.ub\|\.gz\)\?:[ ]\([$][(]obj[)][/]\|vm\)\?linux\(\.bin\)\?[ ]' arch/microblaze/boot/Makefile
    accept '[\t]*[ ]*DTB[)][ ]appended[ ]to[ ]raw[ ]vmlinux\.bin[ ]or[ ]vmlinuz\.bin\.' arch/mips/Kconfig
    accept '[\t]*[ ]*to[ ]vmlinux\.bin\.' arch/mips/Kconfig
    accept 'extra-y[ ][+]=[ ]vmlinux\.bin\.\(bz2\|gz\|lzma\|lzo\)' arch/mips/boot/Makefile
    accept '[$][(]obj[)][/]\(vmlinux\|uImage\)\(\.\(bin\|bz2\|gz\|lzma\|lzo\)\)\+:[ ][$][(]obj[)][/]vmlinux\.bin[ ]' arch/mips/boot/Makefile
    accept '[\t][$][(]call[ ]if_changed[,]cpp_its_S[,]\(gzip\|bzip2\|lzma\|lzo\)[,]vmlinux\.bin\.\(gz\|bz2\|lzma\|lzo\)[)]' arch/mips/boot/Makefile
    accept '[$][(]obj[)][/]vmlinux\(.%\)\?\.itb:[ ][$][(]obj[])[/]vmlinux\(.%\)\?\.its[ ][$][(]obj[)][/]vmlinux\(.%\)\?\.bin[ ]' arch/mips/boot/Makefile
    accept 'targets[ ][+]=[ ]vmlinux\.bin\.z' arch/mips/boot/compressed/Makefile
    accept '[$][(]obj[)][/]vmlinux\.bin\.z:[ ][$][(]obj[)][/]vmlinux\.bin[ ]' arch/mips/boot/compressed/Makefile
    accept 'OBJCOPYFLAGS_piggy\.o[ ]:=[ ]--add-section=\.image=[$][(]obj[)][/]vmlinux\.bin\.z[ ]' arch/mips/boot/compressed/Makefile
    accept '[$][(]obj[)][/]piggy\.o:\([ ][$][(]obj[)][/]\(dummy\.o\|vmlinux\.bin\.z\)\)*' arch/mips/boot/compressed/Makefile
    accept 'vmlinuz\.bin:[ ]vmlinuz' arch/mips/boot/compressed/Makefile
    accept 'uzImage\.bin:[ ]vmlinuz\.bin[ ]' arch/mips/boot/compressed/Makefile
    accept '[\t]return[ ]read_cmd\.s\.dat[;]' arch/mips/cavium-octeon/executive/octeon-model.c
    accept '[\t]*\(\(if\|switch\)[ ][(]\|opcode[ ]=[ ]\)\(inst_mips16e\|inst\|mips16inst\)\.ri\.opcode' 'arch/mips/kernel/\(branch\|unaligned\)\.c'
    accept '[\t]*reg[ ]=[ ]reg16to32\[mips16inst\.ri\.rx\]' arch/mips/kernel/unaligned.c
    accept '[\t]*switch[ ][(]mips16inst\.ri\.imm[ ]' arch/mips/kernel/unaligned.c
    accept 'rom\.bin:[\t][$][(]obj[)][/]rom\.bin' arch/mips/lasat/image/Makefile
    accept '[$][(]obj[)][/]\(rom\|kImage\)\.bin:' arch/mips/lasat/image/Makefile
    accept 'targets[ ][:+]=\([ ]vmlinux\(\.\(lds\|bin\(\.\(gz\|bz2\|xz\|lzma\|lzo\|lz4\)\)\?\)\)\?\)*' 'arch/\(parisc\|s390\)/boot/compressed/Makefile'
    accept 'vmlinux\.bin\.all-y[ ]:=[ ][$][(]obj[)][/]vmlinuz\.bin' 'arch/\(parisc\|s390\)/boot/compressed/Makefile'
    accept '[$][(]obj[)][/]vmlinux\.bin\.\(gz\|bz2\|lz4\|lzma\|lzo\|xz\):[ ][$][(]vmlinux\.bin\.all-y[)]' 'arch/\(parisc\|s390\|sh\|x86\)/boot/compressed/Makefile'
    accept '[$][(]obj[)][/]piggy\.o:\([ ][$][(]obj[)][/]vmlinux\.\(scr\|bin\.[$][(]suffix-y[)]\)\)*' 'arch/\(parisc\|sh\)/boot/compressed/Makefile'
    accept '[\t][/][*][ ]vmlinux\.bin\.gz[ ]is[ ]here[ ][*][/]' arch/parisc/boot/compressed/vmlinux.lds.S
    accept 'zImage\.bin\.[*]' arch/powerpc/boot/.gitignore
    accept '[$][(]obj[)][/]spu_%\.bin:[ ][$][(]src[)][/]spu_%' arch/powerpc/platforms/cell/spufs/Makefile
    accept '[$][(]obj[)][/]info.bin:' arch/s390/boot/compressed/Makefile
    accept 'vmlinux\.bin\.all-y[ ]:=[ ][$][(]obj[)][/]vmlinux.bin' 'arch/\(s390\|sh\|x86\)/boot/compressed/Makefile'
    accept 'OBJCOPYFLAGS_piggy\.o[ ]:=[ ]-I[ ]binary[ ]-O[ ]elf64-s390[ ]-B[ ]s390:64-bit[ ]--rename-section[ ]\.data=\.vmlinux\.bin\.compressed' arch/s390/boot/compressed/Makefile
    accept '[\t]*[*][(]\.vmlinux\.bin\.compressed[)]' arch/s390/boot/compressed/vmlinux.lds.S
    accept 'extra-y[ ][+]=\([ ]\([\\][\n][\t][ ]*\)\?vmlinux\.bin\(\.\(bz2\|gz\|lzma\|lzo\|xz\)\)\?\)*' arch/sh/boot/Makefile
    accept '[$][(]obj[)][/]\(vmlinux\|uImage\)\(\.\(bin\|bz2\|gz\|lzma\|xz\|lzo\)\)\+:[ ][$][(]obj[)][/]vmlinux\.bin\(\.\(bz2\|gz\|lzma\|xz\|lzo\)\)\?' arch/sh/boot/Makefile
    accept 'vmlinux\.bin\.[*]' arch/sh/boot/compressed/.gitignore
    accept 'targets[ \t]*[:+]=\([ ][\\\n\t ]*vmlinux\(\.\(bin\(\.\(gz\|bz2\|xz\|lzma\|lzo\|lz4\)\)\?\)\)\?\)*' 'arch/\(parisc\|s390\|x86\)/boot/compressed/Makefile'
    accept '[$][(]obj[)][/]zeropage.bin:' arch/sh/boot/compressed/Makefile
    accept '[$][(]obj[)][/]\(image\|tftpboot\).bin:' arch/sparc/boot/compressed/Makefile
    accept '[\t]*fprintf[ ][(]stderr[,][ ]["]Not[ ]a\.out\.' arch/sparc/boot/piggyback.c
    accept '[$][(]obj[)][/]setup\.elf:' arch/x86/boot/Makefile
    accept '[$][(]obj[)][/]setup\.bin:[ ][$][(]obj[)][/]setup\.elf[ ]' arch/x86/boot/Makefile
    accept 'image_cmdline[ ]=[ ]default[ ]linux[ ][$][(]FDARGS[)][ ][$][(]if[ ][$][(]FDINITRD[)][,]initrd=initrd\.img[,][)]' arch/x86/boot/Makefile
    accept 'vmlinux\.bin\.all' arch/x86/boot/compressed/.gitignore
    accept '[#][ \t]*vmlinux\.bin\.\(all\|[(]gz\|bz2\|lzma\|\.\.\.[)]\)' arch/x86/boot/compressed/Makefile
    accept '[#][\t]compressed[ ]vmlinux\.bin\.all[ ][+][ ]u32[ ]size[ ]of[ ]vmlinux\.bin\.all' arch/x86/boot/compressed/Makefile
    accept 'targets[ ][+]=[ ][$][(]patsubst[ ][$][(]obj[)][/]%[,]%[,][$][(]vmlinux-objs-y[)][)][ ]vmlinux\.bin\.all[ ]vmlinux\.relocs' arch/x86/boot/compressed/Makefile
    accept 'vmlinux\.bin\.all-[$][(]CONFIG_X86_NEED_RELOCS[)][ ][+]=[ ][$][(]obj[)][/]vmlinux\.relocs' arch/x86/boot/compressed/Makefile
    accept '[$][(]obj[)][/]piggy\.S:[ ][$][(]obj[)][/]vmlinux\.bin\.[$][(]suffix-y[)]' arch/x86/boot/compressed/Makefile
    accept '[$][(]obj[)][/]\(rm[/]\)\?realmode\.\(elf\|bin\):\([ ][$][(]obj[)][/]realmode\.\(lsd\|elf\|relocs\)\)*' arch/x86/realmode/Makefile
    accept 'vmlinux\.bin\.gz:[ ]vmlinux\.bin' arch/xtensa/boot/Makefile
    accept 'boot-redboot:[ ]vmlinux\.bin\.gz' arch/xtensa/boot/Makefile
    accept '[$][(]obj[)][/]uImage:[ ]vmlinux\.bin\.gz' arch/xtensa/boot/Makefile
    accept '[$][(]obj[)][/]\.\.[/]Image\.elf:[ ][$][(]obj[)][/]Image\.o[ ][$][(]obj[)][/]boot\.lds' arch/xtensa/boot/boot-elf/Makefile
    accept '[$][(]obj[)][/]zImage\.o:[ ]vmlinux\.bin\.gz' arch/xtensa/boot/boot-redboot/Makefile
    accept '[\t]*--add-section[ ]image=vmlinux\.bin\.gz[ ]' arch/xtensa/boot/boot-redboot/Makefile
    accept '[$][(]obj[)][/]zImage\.elf:[ ][$][(]obj[)][/]zImage\.o' arch/xtensa/boot/boot-redboot/Makefile
    accept '[\t]*[(]unsigned[ ]long[)]op\.out[,][ ][(]long[)]op\.outlen[)][;]' drivers/crypto/nx/nx-842-pseries.c
    accept '[\t]*adev->firmware\.ucode\[AMDGPU_UCODE_ID_\(UVD1\?\|VC[EN]1\?\)\]\.fw[ ]=[ ]adev->\(uvd\|vc[en]\)\.fw[;]' drivers/gpu/drm/amd/amdgpu/'\(uvd_v7_0\|vce_v[124]_[05]\)\.c'
    accept '[\t]*\(err[ ]=[ ]\)intel_uc_fw_fetch[(][&]uc->[gh]uc\.fw[,]' drivers/gpu/drm/i915/gt/uc/intel_uc.c
    accept '[\t]*intel_uc_fw_dump[(][&]dev_priv->gt\.uc\.[hg]uc\.fw[,]' drivers/gpu/drm/i915/i915_debugfs.c
    accept '[\t]memcpy[(][&]error_uc->[gh]uc_fw[,][ ][&]uc->[gh]uc\.fw[,][ ]sizeof[(]uc->[gh]uc\.fw[)][)][;]' drivers/gpu/drm/i915/i915_gpu_error.c
    accept '[\t]error_uc->[gh]uc_fw\.path[ ]=[ ]kstrdup[(]uc->[gh]uc\.fw\.path[,]' drivers/gpu/drm/i915/i915_gpu_error.c
    accept '[\t]return[ ]le16_to_cpu[(]dp\.fw\.family_code[)]' drivers/hid/hid-led.c
    accept '[\t]*cmd->tx_buf[ ]=[ ]i3c_xfers\[i\]\.data\.out[;]' drivers/i3c/master/dw-i3c-master.c
    accept '[\t]*ccmd->tx_buf[ ]=[ ]xfers\[i\]\.data\.out[;]' drivers/i3c/master/i3c-master-cdns.c
    accept '[\t]*cmd\.valid\.out\.\(tf\|hob\)[ ][|]\?=' drivers/ide/'ide-.*\.c'
    accept '[\t]*if[ ][(]cmd->valid\.out\.tf[ ][&]' drivers/ide/ide-taskfile.c
    accept '[\t]*tp_ops->tf_load[(]drive[,][ ][&]cmd->\(tf\|hob\)[,][ ]cmd->valid\.out\.\(tf\|hob\)[)][;]' drivers/ide/ide-taskfile.c
    accept '[\t]err[ ]=[ ]mlx5_cmd_exec[(]dev->mdev[,][ ]cmd\.in[,][ ]cmd\.inlen[,][ ]cmd\.out[,]' drivers/infiniband/hw/mlx5/devx.c
    accept '[\t]devx_obj_build_destroy_cmd[(]cmd\.in[,][ ]cmd\.out[,]' drivers/infiniband/hw/mlx5/devx.c
    accept '[\t]mlx5_cmd_exec[(]obj->mdev[,][ ]obj->dinbox[,][ ]obj->dinlen[,][ ]cmd\.out[,][ ]sizeof[(]cmd\.out[)][)][;]' drivers/infiniband/hw/mlx5/devx.c
    accept '[\t]\(bl\(oc\)\?k_count\|num_of_containers\)[ ]=[ ]f34->v7\.img\.' drivers/input/rmi4/rmi_f34v7.c
    accept '[\t]f34->v7.config_\(data\|size\)[ ]=[ ]f34->v7\.img\.' drivers/input/rmi4/rmi_f34v7.c
    accept '[\t]return[ ]rmi_f34v7_write_f34v7_blocks[(]f34[,][ ]f34->v7\.img\.guest_code\.data[,][\n\t ]*f34->v7\.img\.guest_code\.size' drivers/input/rmi4/rmi_f34v7.c
    accept '[\t]return[ ]rmi_f34v7_write_f34v7_blocks[(]f34[,][ ]f34->v7\.img\.\(guest_code\|ui_firmware\)\.data[,][\n\t ]*f34->v7\.img\.\(guest_code\|ui_firmware\)\.size' drivers/input/rmi4/rmi_f34v7.c
    accept '[\t]\(if[ ][(]\|[ ]*\)f34->v7\.phyaddr\.\(ui_firmware\|ui_config\|dp_config\|guest_code\)[ ]!=[ ]f34->v7\.img\.phyaddr\.\(ui_firmware\|ui_config\|dp_config\|guest_code\)[)]' drivers/input/rmi4/rmi_f34v7.c
    accept '[\t]*addr[ ]=[ ]get_unaligned_le32[(]f34->v7\.img\.bootloader\.data[ ]' drivers/input/rmi4/rmi_f34v7.c
    accept '[\t]*[ ]*f34->v7\.img\.' drivers/input/rmi4/rmi_f34v7.c
    accept '[\t]rmi_dbg[(]RMI_DEBUG_FN[,][ ][&]f34->fn->dev[,][ ]["]%s:[ ]f34->v7\.img\.checksum' drivers/input/rmi4/rmi_f34v7.c
    accept '[\t]*__func__[,][ ]f34->v7\.img\.checksum[)]' drivers/input/rmi4/rmi_f34v7.c
    accept '[\t]memset[(][&]f34->v7\.img[,][ ]0x00[,][ ]sizeof[(]f34->v7\.img[)][)][;]' drivers/input/rmi4/rmi_f34v7.c
    accept '[\t]if[ ][(][!]f34->v7\.img\.' drivers/input/rmi4/rmi_f34v7.c
    accept '[\t]rmi_f34v7_parse_partition_table[(]f34[,][ ]f34->v7\.img\.' drivers/input/rmi4/rmi_f34v7.c
    accept '[\t]*[&]f34->v7\.img\.blkcount[,][ ][&]f34->v7\.img\.phyaddr[)][;]' drivers/input/rmi4/rmi_f34v7.c
    accept '[\t]*if[ ][(]f34->v7\.has_\(guest_code\|display_cfg\)[ ][&][&][ ]f34->v7\.img\.contains_\(guest_code\|display_cfg\)[)]' drivers/input/rmi4/rmi_f34v7.c
    blobname 'picasso_rlc\(_am4\)\?\.bin' drivers/gpu/drm/amd/amdgpu/gfx_v9_0.c
    blobna '[/][*][\n][\t][ ][*][ ]For[ ]Picasso[^*]*\([*]\+[^/*][^*]*\)*picasso_rlc[^*]*\([*]\+[^/*][^*]*\)*[*][*]*[/]' drivers/gpu/drm/amd/amdgpu/gfx_v9_0.c
    # WIP: more to come here.

    # New in 5.3.11, 4.19.84 and 4.14.154.
    accept 'CPUID[ ]to[ ]the[ ]guest[.][ ]If[ ]the[ ]host[ ]has[ ]updated[ ]microcode[ ]the[ ]protection' Documentation/admin-guide/hw-vuln/tsx_async_abort.rst
    accept '[\t *]*-[ ]Updated[ ]microcode[ ]is[ ]present' arch/x86/kvm/x86.c

    # New in 5.4-rc*.
    accept '[ ][ ]\(63\|31\|56\|24\|39\|32\|[0437][ ]\)\([ ]\([0-9 ][0-9 ]\)\)*[ ]\(56\|63\|32\|39\|24\|31\|[ ]\?[0437]\)\([\n][ ][ ]\(63\|31\|56\|24\|39\|32\|[0437][ ]\)\([ ]\([0-9 ][0-9 ]\)\)*[ ]\(56\|63\|32\|39\|24\|31\|[ ]\?[0437]\)\)*' Documentation/packing.txt
    blobname 'linux-firmware\.git' Documentation/networking/device_drivers/netronome/nfp.rst
    defsnc 'static[ ]u32[ ]vrate_adj_pct\[\][ ]=' block/blk-iocost.c
    defsnc 'static[ ]const[ ]u32[ ]crypto_[fi]l_tab\[4\]\[256\][ ]____cacheline_aligned[ ]=' crypto/aes_generic.c
    defsnc 'static[ ]const[ ]struct[ ]comp_testvec[ ]lzorle_\(de\)\?comp_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]const[ ]struct[ ]cipher_testvec[ ]essiv_aes_cbc_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]const[ ]struct[ ]aead_testvec[ ]essiv_hmac_sha256_aes_cbc_tv_temp\[\][ ]=' crypto/testmgr.h
    blobname 'cnn55xx_ae\.fw' drivers/crypto/cavium/nitrox/nitrox_main.c
    blobname 'amdgpu[/]\(arcturus\|renoir\|navi1[24]\)_vcn\.bin' drivers/gpu/dmr/amd/amdgpu/amdgpu_vcn.c
    blobname 'amdgpu[/]\(renoir\|%s\)_asd\.bin' drivers/gpu/drm/amd/amdgpu/psp_v12_0.c
    blobname 'amdgpu[/]%s_sdma%d\.bin' drivers/gpu/drm/amd/amdgpu/sdma_v4_0.C
    defsnc '\(const[ ]uin32_t[\n]\)\?[ \t]*umc_v6_1_channel_idx_tbl\[UMC_V6_1_UMC_INSTANCE_NUM\]\[UMC_V6_1_CHANNEL_INSTANCE_NUM\][ ]=' drivers/gpu/drm/amd/amdgpu/umc_v6_1.c
    # Sources are in cwsr_trap_handler_gfx9.asm.
    defsnc 'static[ ]const[ ]uint32_t[ ]cwsr_trap_arcturus_hex\[\][ ]=' drivers/gpu/drm/amd/amdkfd/cwsr_trap_handler.h
    defsnc 'static[ ]const[ ]struct[ ]abm_parameters[ ]abm_settings_config[01]\[abm_defines_max_level\][ ]=' drivres/gpu/drm/amd/display/modules/power/power_helpers.c
    defsnc 'static[ ]const[ ]struct[ ]IP_BASE[ ]\(\(NBIF\|PCIE\)0\|SDMA[234567]\|DBGU_IO\)_BASE[ \t]*=' drivers/gpu/drm/amd/include/arct_ip_offset.h
    defsnc 'static[ ]const[ ]struct[ ]IP_BASE[ ]\(DIO\|DMU\|DPCS\|HDA\|\(NBIF\|PCIE\)0\|SDMA\|USB0\|UVD0\)_BASE[ \t]*=' drivers/gpu/drm/amd/include/navi12_ip_offset.h
    defsnc 'static[ ]const[ ]struct[ ]IP_BASE[ ]\(DIO\|DMU\|DPCS\|HDA\|\(NBIF\|PCIE\)0\|SDMA\|USB0\|UVD0\)_BASE[ \t]*=' drivers/gpu/drm/amd/include/navi14_ip_offset.h
    defsnc 'static[ ]const[ ]struct[ ]IP_BASE[ ]\(ACP\|DBGU_IO0\|DIO\|DMU\|DPCS\|HDA\|IOHC0\|ISP\|L2IMU0\|\(NBIF\|PCIE\)0\|USB0\|UVD0\)_BASE[ \t]*=' drivers/gpu/drm/amd/include/renoir_ip_offset.h
    blobname 'i915[/]tgl_dmc_ver2_04\.bin' drivers/gpu/drm/i915/intel_csr.c
    defsnc '[\t][}][ ]init_data\[\][ ]=' drivers/gpu/drm/panel/panel-lg-lb035q02.c
    defsnc '[\t][}][ ]nl8048_init_seq\[\][ ]=' drivers/gpu/drm/panel/panel-nec-nl8048hl11.c
    defsnc 'static[ ]const[ ]struct[ ]cmd_set_entry[ ]manufacturer_cmd_set\[\][ ]=' drivers/gpu/drm/panel/panel-raydium-rm67191.c
    defsnc 'static[ ]const[ ]char[ ]data_\(last_\)\?block_header\[DATA_BLOCK_HEADER_SIZE\][ ]=' drivers/gpu/drm/tiny/gm12u320.c
    accept '[\t]mipi_dbi_command[(]dbi[,][ ]HX8357D_SETGAMMA\([,][\n][\t][\t][\t][ ]0x[0-9a-f][0-9a-fA-F]\)*[)][;]' drivers/gpu/drm/tiny/hx8357d.c
    defsnc 'static[ ]const[ ]unsigned[ ]short[ ]creative_sb0540_codes\[\][ ]=' drivers/hid/hid-creative-sb0540.c
    defsnc 'static[ ]const[ ]struct[ ]ov5675_reg[ ]mode_\(2592x1944\|1296x972\)_regs\[\][ ]=' drivers/media/i2c/ov5675.c
    blobname 'rtl_nic[/]rtl8125a-3\.fw' drivers/net/ethernet/realtek/r8169_main.c
    defsnc '[\t]static[ ]const[ ]u16[ ]ical\[\][ ]=' drivers/net/wireless/mediatek/mt76/mt7615/eeprom.c
    defsnc '[\t]static[ ]const[ ]u8[ ]channel_all\[TARGET_CHNL_NUM_2G_5G_8812\][ ]=' drivers/net/wireless/realtek/rtlwifi/rtl8821ae/phy.c
    defsnc 'static[ ]const[ ]struct[ ]rtw_txpwr_lmt_cfg_pair[ ]rtw8822b_txpwr_lmt_type[25]\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8822b_table.c
    defsnc 'static[ ]const[ ]struct[ ]rtw_txpwr_lmt_cfg_pair[ ]rtw8822c_txpwr_lmt_type0\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8822c_table.c
    blobname 'gsl1680-chuwi-surbook-mini\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'gsl3680-irbis_tw90\.fw' drivers/platform/x86/touchscreen_dmi.c
    defsnc 'static[ ]const[ ]u8[ ]aes_cipher_key_skeleton\[\][ ]=' drivers/s390/crypto/zcrypt_ccamisc.c
    defsnc 'const[ ]u8[ ]uni_upcase\[NUM_UPCASE[ ]<<[ ]1\][ ]=' drivers/staging/exfat/exfat_upcase.c
    defsnc 'static[ ]const[ ]u32[ ]h264_cabac_table\[\][ ]=' drivers/staging/media/hantro/hantro_h264.c
    defsnc 'static[ ]const[ ]u32[ ]zig_zag_8x8\[\][ ]=' drivers/staging/media/hantro/hantro_h264.c
    defsnc 'static[ ]volatile[ ]const[ ]u8[ ]__cacheline_aligned[ ]aes_\(inv_\)\?sbox\[\][ ]=' lib/crypto/aes.c
    defsnc 'static[ ]const[ ]u16[ ]scarlett2_mixer_values\[173\][ ]=' sound/usb/mixer_scarlett_gen2.c
    defsc 'vector[ ]int[ ]vsxs\[\][ ]=' tools/testing/selftests/powerpc/tm/tm-signal-context-chk-vsx.c
    defsnc '[\t]static[ ]const[ ]struct[ ]ephy_info[ ]e_info_8125_[12]\[\][ ]=' drivers/net/ethernet/realtek/r8169_main.c
    defsnc '[\t]static[ ]const[ ]u32[ ]wl_rx_low_gain_o\(n\|ff\)\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8822b.c
    accept '[ ][*][\t]request_firmware_into_buf[(][)]' lib/test_firmware.c
    accept '[\t]*req->rc[ ]=[ ]request_firmware_into_buf[(][&]req->fw[,][\n]' lib/test_firmware.c
    accept 'trap[ ]["]rm[ ]-f[ ][$]tmp_file\.o[ ][$]tmp_file[ ][$]tmp_file\.bin["]' scripts/tools-support-relr.sh
    accept '[\t]*\(echo[ ]-n[ ]["]\)\?\(test_batched_\|Batched[ ]\)request_firmware_into_buf\(_nofile\)\?\([(][)]\|[ ]\)' tools/testing/selftests/firmware/fw_filesystem.sh
    accept '#[ ]We[ ]need[ ]to[ ]load[ ]a[ ]different[ ]file[ ]to[ ]test[ ]request_firmware_into_buf' tools/testing/selftests/firmware/fw_lib.sh
    accept '#[ ]To[ ]reproduce[ ]rename[ ]this[ ]to[ ]test-firmware\.bin' tools/testing/selftests/firmware/fw_lib.sh
    # Since ar500X and ar92XX have Free firmware, I'm assuming this
    # initialization data file is either Free Software or pure data.
    accept '[\t]scnprintf[(]eeprom_name[,][ ]EEPROM_FILENAME_LEN[,][ ]["]ath9k-eeprom-pci-%s\.bin["]' drivers/net/wireless/ath/ath9k/ath9k_pci_owl_loader.c
    accept '[\t]err[ ]=[ ]request_firmware_nowait[(]THIS_MODULE[,][ ]true[,][ ]eeprom_name[,]' drivers/net/wireless/ath/ath9k/ath9k_pci_owl_loader.c
    blobname 'i915[/]["]\([ ][\\][\n][\t]__stringify[(]\(prefix\|major\|minor\|patch\)_[)][ ]\(\(name\|separator\)_\)\?\)*["]\.bin' drivers/gpu/drm/i915/gt/uc/intel_uc_fw.c
    blobname 'intel[/]dsp_fw_%pUL\.bin' sound/soc/intel/skylake/skl-sst.c
    accept '[\t]*tplg_filename[ ]=[ ]devm_kasprintf[(]sdev->dev[,][ ]GFP_KERNEL[,][\n][\t ]*["]%s%s%s\.tplg["][,]' sound/soc/sof/intel/hda.c
    blobname 'intel[/]ice[/]ddp[/]' drivers/net/ethernet/intel/ice/ice_main.c
    blobname '["]ice\.pkg["]' drivers/net/ethernet/intel/ice/ice_main.c
    blobname '\(intel[/]ice[/]ddp[/]\|%s\)\?ice\(-%02x%02x%02x%02x%02x%02x%02x%02x\|-[0-9A-F]*\)\?\.pkg' drivers/net/ethernet/intel/ice/ice_main.c
    accept '[\t]*marvell[,]caldata-txpwrlimit-\(2g\|5g-sub[012]\)[ ]=[ ][/]bits[/][ ]8[ ]<\([\n ]0x[0-9a-f][0-9a-f]\)*>[;]' arch/arm/boot/dts/rk3288-veyron-jerry.dts
    blobname 'amdgpu[/]%s_\(pfp\|[mc]e\|mec2\?\)%s\.bin' drivers/gpu/drm/amd/amdgpu/gfx_v10_0.c
    blobname 'amdgpu[/]navi14_\(pfp\|[mc]e\|mec2\?\)_wks\.bin' drivers/gpu/drm/amd/amdgpu/gfx_v10_0.c
    blob '6\.1\.[ ]Driver[ ]complains[^\n]*i2400m-fw[^\n]*[\n]--*\([\n][\n]*\([ ][ ][ ]\|[\t]i2400m_usb\)[^\n]*\)\+' Documentation/admin-guide/wimax/i2400m.rst
    # This is not new, just a new catch.
    blobname 'inside-secure[/]%s[/]%s' drivers/crypto/inside-secure/safexcel.c

    # New in 5.5-rc*.
    initnc '\.Lpermute_table:' arch/arm64/crypto/ghash-ce-core.S
    initnc 'SIGMA2\?:' arch/x86/crypto/blake2s-core.S
    defsnc 'static[ ]const[ ]u8[ ]blake2b_sigma\[12\]\[16\][ ]=' crypto/blake2b_generic.c
    defsc 'static[ ]const[ ]struct[ ]kpp_testvec[ ]curve25519_tv_template\[\][ ]=' crypto/testmgr.hpu
    defsnc 'static[ ]const[ ]struct[ ]hash_testvec[ ]hmac_sm3_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]const[ ]struct[ ]cipher_testvec[ ]sm4_ctr_rfc3686_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]const[ ]char[ ]blake2_ordered_sequence\[\][ ]='
    defsnc 'static[ ]const[ ]struct[ ]hash_testvec[ ]blake2b_\(256\|384\|512\)_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]const[ ]struct[ ]hash_testvec[ ]blake2b_\(256\|384\|512\)_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]const[ ]struct[ ]hash_testvec[ ]blakes2s_256_tv_template\[\][ ]=' crypto/testmgr.h
    defsnc 'static[ ]const[ ]struct[ ]clk_div_table[ ]bm1880_div_table_[01234]\[\][ ]=' drivers/clk/clk-bm1880.c
    blobname 'i915[/]icl_dmc_ver1_09\.bin' drivers/gpu/drm/i915/intel_csr.c
    defsnc 'static[ ]const[ ]u8[ ]tegra1\(24\|32\|86\)_sor_\(voltage_swing\|pre_emphasis\|post_cursor\|tx_pu\)\[4\]\[4\]\[4\][ ]=' drivers/gpu/drm/tegra/sor.c
    defsnc 'static[ ]const[ ]struct[ ]reg_sequence[ ]adux1020_def_conf\[\][ ]=' drivers/iio/light/adux1020.c
    defsnc 'static[ ]const[ ]int[ ]adux1020_led_currents\[\]\[2\][ ]=' drivers/iio/light/adux1020.c
    defsnc 'static[ ]const[ ]struct[ ]hi556_reg[ ]mipi_data_rate_874mbps\[\][ ]=' drivers/media/i2c/hi556.c
    defsnc 'static[ ]const[ ]struct[ ]hi556_reg[ ]mode_\(2592x1944\|1296x972\)_regs\[\][ ]=' drivers/media/i2c/hi556.c
    defsnc 'static[ ]const[ ]struct[ ]imx290_regval[ ]imx290_global_init_settings\[\][ ]=' drivers/media/i2c/imx290.c
    defsc 'static[ ]const[ ]struct[ ]imx290_regval[ ]imx290_\(1080\|720\)p_settings\[\][ ]=' drivers/media/i2c/imx290.c
    blobname 'rtl_nic[/]rtl8168fp-3\.fw' drivers/net/ethernet/realtek/r8169_main.c
    blobname 'rtl_nic[/]rtl8153[ab]-[234]\.fw' drivers/net/usb/r8152.c
    blobname 'iwl-debug-yoyo\.bin' drivers/net/wireless/intel/iwlwifi/iwl-dbg-tlv.c
    defsnc 'static[ ]const[ ]struct[ ]rtw_phy_pg_cfg_pair[ ]rtw8822b_bb_pg_type[235]\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8822b_table.c
    defsnc 'static[ ]const[ ]struct[ ]rtw_txpwr_lmt_cfg_pair[ ]rtw8822b_txpwr_lmt_type0\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8822b_table.c
    defsnc 'static[ ]const[ ]struct[ ]rtw_phy_pg_cfg_pair[ ]rtw8822c_bb_pg_type0\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8822b_table.c
    defsnc '[\t][}][ ]timings\[\][ ]=' drivers/phy/rockchip/phy-rockchip-inno-dsidphy.c
    defsnc 'static[ ]const[ ]struct[ ]msm_gpio_wakeirq_map[ ]sdm845_pdc_map\[\][ ]=' drivers/pinctrl/qcom/pinctrl-sdm845.c
    blobname 'gsl3692-jumper-ezpad-6-m4\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'gsl1680-schneider-sct101ctm\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'idtcm\.bin' drivers/ptp/ptp_clockmatrix.h
    defsc 'static[ ]const[ ]u32[ ]asv_arm_table\[\]\[ASV_ARM_DVFS_NUM\]\[ASV_GROUPS_NUM[ ][+][ ]1\][ ]=' drivers/soc/samsung/exynos5422-asv.c
    defsc 'static[ ]const[ ]u32[ ]asv_kfc_table\[\]\[ASV_KFC_DVFS_NUM\]\[ASV_GROUPS_NUM[ ][+][ ]1\][ ]=' drivers/soc/samsung/exynos5422-asv.c
    defsnc 'static[ ]const[ ]u8[ ]blake2s_sigma\[10\]\[16\][ ]=' lib/crypto/blake2s-generic.c
    defsnc 'static[ ]const[ ]u8[ ]blake2s_\(hmac_\)\?testvecs\[\]\[BLAKE2S_HASH_SIZE\][ ]__initconst[ ]=' lib/crypto/blake2s-selftest.c
    defsnc 'static[ ]const[ ]u8[ ]x\?\(enc\|dec\)_\(\(in\|out\)put\|key\|assoc\)[0-9]*\[\][ ]__initconst[ ]=' lib/crypto/chacha20poly1305-selftest.c
    accept '[ ][*][ ][ ][ ][ ][ ]3[ ]3[ ]2[ ]2[ ]2[ ]2[ ]2[ ]2[ ]2[ ]2[ ]2[ ]2[ ]1[ ]1[ ]1[ ]1[ ]1[ ]1[ ]1[ ]1[ ]1[ ]1[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0[ ]0' net/tipc/crypto.h
    defsnc '[\t]static[ ]const[ ]struct[ ]reg_val[ ]\(init_eee\|pre_init1\)\[\][ ]=' drivers/net/phy/mscc.c
    defsnc 'static[ ]const[ ]u32[ ]rtw8822b_txscale_tbl[RTW_TXSCALE_SIZE][ ]=' drivers/net/wireless/realtek/rtw88/rtw8822b_table.c
    defsnc 'static[ ]const[ ]u8[ \n]rtw8822b_pwrtrk_5g[ba]_[np]\[RTW_PWR_TRK_5G_NUM\]\[RTW_PWR_TRK_TBL_SZ\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8822b_table.c
    defsnc 'static[ ]const[ ]u8[ \n]rtw8822c_pwrtrk_5g[ba]_[np]\[RTW_PWR_TRK_5G_NUM\]\[RTW_PWR_TRK_TBL_SZ\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8822c.c
    accept 'static[ ]const[ ]struct[ ]tegra_xusb_soc[ ]tegra194_soc[ ]=[ ][{][\n][\t][.]firmware[ ]=' drivers/usb/host/xhci-tegra.c
    blobname 'nvidia[/]tegra194[/]xusb\.bin' drivers/usb/host/xhci-tegra.c
    blobname 'rt5677_elf_vad\([ ]file[ ][*][/]\)\?' sound/soc/codecs/rt5677.c
    blobname 'i915[/]["]\([ ][\\][\n][\t]__stringify[(]\(prefix\|major\|minor\|patch\)_[)][ ]\(\(name_\|["][.]["]\)\)\?\)*["]\.bin' drivers/gpu/drm/i915/gt/uc/intel_uc_fw.c
    blobname 'mellanox[/]mlxsw_spectrum2-\(["][ ]__stringify[(]MLXSW_SP2_FWREV_[^)]*[)][ \\\n\t]*["]\.\)*mfa2' drivers/net/ethernet/mellanox/mlxsw/spectrum.c
    accept '[\t][ ][*][ ]per-cpu[ ]cpuinfo[ ]can[ ]be[ ]updated[ ]with[ ]right[ ]microcode' arch/x86/kernel/cpu/microcode/core.c
    accept '\(static[ ]\)\?int[ ]bnxt_flash_\(firmware\|package\)_from_file[(][ \t\na-z0-9_,*]*[)][\n][{][\n]\([^}][^\n]*[\n]\+\)*[\t]rc[ ]=[ ]request_firmware[(][&]fw' drivers/net/ethernet/broadcom/bnxt/bnxt_ethtool.c
    accept 'static[ ]int[ ]rtl8152_request_firmware[(]' drivers/net/usb/r8152.c
    accept '[\t]if[ ][(]rtl8152_request_firmware[(]' drivers/net/usb/r8152.c
    accept '[\t][\t][/][*][ ]Delay[ ]execution[ ]in[ ]case[ ]request_firmware[(][)]' drivers/net/usb/r8152.c
    blobname 'rtl_nic[/]rtl8153a-[234]\.fw' drivers/net/usb/r8152.c
    blobname 'rtl_nic[/]rtl8153b-2\.fw' drivers/net/usb/r8152.c
    accept '[\t][/][*][ ]Retry[ ]in[ ]case[ ]request_firmware[(]' drivers/net/usb/r8152.c
    accept '[ ][*][ ]@context:[ ]pointer[ ]to[ ]firmware[ ]image[ ]returned[ ]from[ ]request_firmware\.' drivers/scsi/lpfc/lpfc_init.c
    accept '[ ][*][ ]request_firmware[(][)][ ]allocate[ ]data[ ]using[ ]vmalloc[(]' drivers/staging/wfx/fwio.c
    # This loads Platform Data Set pure data files.  Preconfigured
    # files, templates and tools to compress the configuration files
    # to the binary format are available.
    accept '[\t]ret[ ]=[ ]request_firmware[(]&pds,[ ]wdev->pdata\.file_pds,' drivers/staging/wfx/main.c
# .take5 rt5677.c
    # ethtool-supplied firmware to flash the virtual device.
    accept '[\t]if[ ][(]request_firmware[(]&fw[,][ ]efl->data[,][ ]&vdevice->pdev\.dev[)][)]' arch/um/drivers/vector_kern.c

    # Already present in 5.0, harmless as firmware is the first field.
    accept 'static[ ]const[ ]struct[ ]vic_config[ ]vic_t194_config[ ]=[ ][{][\n][\t]\.firmware[ ]=[ ]NVIDIA_TEGRA_194_VIC_FIRMWARE[,]' drivers/gpu/drm/tegra/vic.c

    # New in 5.5.11 and 5.4.27.
    blobname 'microchip[/]mscc_vsc8584_revb_int8051_fb48\.bin' drivers/net/phy/mscc.c
    blobname 'microchip[/]mscc_vsc8574_revb_int8051_29e8\.bin' drivers/net/phy/mscc.c

    # New in 5.6-rc7.
    initnc '[ ]*[(]gdb[)][ ]x[/]100x[ ][$]25[\n]' Documentation/virt/uml/user_mode_linux.rst
    blobname 'amdgpu[/]renoir_dmcub\.bin' drivers/gpu/drm/amd/display/amdgpu_dm/amdgpu_dm.c
    accept '[\t][ ][*][ ]the[ ][/]lib[/]firmware[/]qcom[/]\.\.\.[ ]vs[ ][/]lib[/]firmware[/]\.\.\.[ ]case' drivers/gpu/drm/msm/adreno/adreno_gpu.c
    accept '[\t]gr->firmware[ ]=[ ]' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf100.c
    accept '[\t]*snprintf[(]f[,][ ]sizeof[(]f[)][,][ ]["]nouveau[/]nv%02x_%s["][,][ ]device->chipset[,][ ]name[)][;][\n][\t]*ret[ ]=[ ]request_firmware[(][&]fw[,][ ]f[,][ ]device->dev[)][;][\n][\t]*if[ ][(]ret[)][ ][{][\n][\t]*snprintf[(]f[,][ ]sizeof[(]f[)][,][ ]["]nouveau[/]%s["][,][ ]name[)][;][\n][\t]*ret[ ]=[ ]request_firmware[(][&]fw[,][ ]f[,][ ]device->dev[)][;]' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf100.c
    accept '[	]\(if[ ][(]\|[ ][ ][ ][ ]\)gf100_gr_load_fw[(]gr[,][ ]["]fuc4\(09\|1a\)[cd]["][,][ ][&]gr->\(fecs\|gpccs\)' drivers/gpu/drm/nouveau/nvkm/engine/gr/gf100.c
    defsnc 'static[ ]const[ ]struct[ ]panel_cmd[ ]boe_himax8279d\(8\|10\)p_on_cmds\[\][ ]=' drivers/gpu/drm/panel/panel-boe-himax8279d.c
    defsnc 'static[ ]const[ ]struct[ ]ltk500hd1829_cmd[ ]init_code\[\][ ]=' drivers/gpu/drm/panel/panel-leadtek-ltk500hd1829.c
    accept '[\t]dsi_generic_write_seq[(]dsi[,][ ]XPP055C272_CMD_SET\(GIP[12]\|GAMMA\)\([, \t\n]*0x[0-9a-f][0-9a-f]\)*[)][;]' drivers/gpu/drm/panel/panel-xinpeng-xpp055c272.c
    defsc 'static[ ]const[ ]unsigned[ ]char[ ]\(luma\|chroma\)_ac\[16[ ][+][ ]162[ ][+][ ]2\]' drivers/media/platform/coda/coda-jpeg.c
    defsnc 'static[ ]const[ ]u32[ ]ice_ptypes_\(ipv[46]\|udp\|tcp\|sctp\)_\(ofos\|il\)\[\][ ]=' drivers/net/ethernet/intel/ice/ice_flow.c
    defsnc 'static[ ]const[ ]u32[ ]iro_arr\[\][ ]=' drivers/net/ethernet/qlogic/qed/qed_hsi.h
    defsnc 'static[ ]const[ ]u8[ ]dscp_tid_map\[DSCP_TID_MAP_TBL_ENTRY_SIZE\][ ]=' drivers/net/wireless/ath/ath11k/hal_tx.c
    blobname 'rtw88[/]rtw8822c_wow_fw\.bin' drivers/pinctrl/qcom/pinctrl-sc7180.c
    defsnc 'static[ ]const[ ]struct[ ]msm_gpio_wakeirq_map[ ]sc7180_pdc_map\[\][ ]=' drivers/pinctrl/qcom/pinctrl-sc7180.c
    blobname 'gsl1680-pipo-w11\.fw' drivers/platform/x86/touchscreen_dmi.c
    defsnc 'static[ ]const[ ]struct[ ]hsfreq_range[ ]rk3399_mipidphy_hsfreq_ranges\[\][ ]=' drivers/staging/media/phy-rockchip-dphy-rx0/phy-rockchip-dphy-rx0.c
    accept 'static[ ]int[ ]tegra_xusb_request_firmware[(]' drivers/usb/host/xhci-tegra.c
    accept '[\t]err[ ]=[ ]tegra_xusb_request_firmware[(]tegra[)]' drivers/usb/host/xhci-tegra.c
    defsc 'static[ ]const[ ]struct[ ]curve25519_test_vector[ ]curve25519_test_vectors\[\][ ]__initconst[ ]=' lib/crypto/curve25519-selftest.c
    defsc 'static[ ]const[ ]u8[ ]tas3004_treble_table\[\][ ]=' sound/aoa/codecs/tas-basstreble.h
    defsnc 'static[ ]const[ ]char[ ]opl3_volume_table\[128\][ ]=' sound/drivers/opl3/opl3_midi.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]snd_opl4_volume_table\[128\][ ]=' sound/drivers/opl4/opl4_synth.c
    defsnc 'static[ ]const[ ]unsigned[ ]short[ ]init[1234]\[128\][ ]=' sound/isa/sb/emu8000.c
    defsc 'static[ ]const[ ]unsigned[ ]short[ ]treble_parm\[12\]\[9\][ ]=' sound/isa/sb/emu8000.c
    defsnc 'static[ ]const[ ]u16[ ]asEqCoefsZeros\[50\][ ]=' sound/pci/au88x0/au88x0_eqdata.c
    defsnc 'static[ ]const[ ]u16[ ]asEqCoefsPipes\[64\][ ]=' sound/pci/au88x0/au88x0_eqdata.c
    defsnc 'static[ ]const[ ]auxxEqCoeffSet_t[ ]asEqCoefsNormal[ ]=' sound/pci/au88x0/au88x0_eqdata.c
    defsnc 'static[ ]const[ ]u16[ ]asEqOutStateZeros\[48\][ ]=' sound/pci/au88x0/au88x0_eqdata.c
    defsnc 'static[ ]const[ ]u16[ ]eq_levels\[64\][ ]=' sound/pci/au88x0/au88x0_eqdata.c
    defsnc '[\t]static[ ]const[ ]u32[ ]logMagTable\[128\][ ]=' sound/pci/emu10k1/io.c
    defsnc '[\t]static[ ]const[ ]char[ ]logSlopeTable\[128\][ ]=' sound/pci/emu10k1/io.c
    defsnc 'static[ ]const[ ]char[ ]coefficients\[NM_TOTAL_COEFF_COUNT[ ][*][ ]4\][ ]=' sound/pci/nm256/nm256_coef.c
    defsnc 'static[ ]const[ ]char[ ]channel_map_unity_ss\[HDSPM_MAX_CHANNELS\][ ]=' sound/pci/rme9652/hdspm.c
    defsnc 'static[ ]const[ ]short[ ]beep_wform\[256\][ ]=' sound/ppc/beep.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]\(master\|\(snapper_\)\?\(treble\|bass\|mixer\)\)_volume_table\[\][ ]=' sound/ppc/tumbler_volume.h
    defsnc 'static[ ]const[ ]u8[ ]jz4770_codec_reg_defaults\[\][ ]=' sound/soc/codecs/jz4770.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt1015_reg\[\][ ]=' sound/soc/codecs/rt1015.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt1308_reg_defaults\[\][ ]=' sound/soc/codecs/rt1308-sdw.h
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt700_reg_defaults\[\][ ]=' sound/soc/codecs/rt700-sdw.h
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt711_reg_defaults\[\][ ]=' sound/soc/codecs/rt711-sdw.h
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt715_reg_defaults\[\][ ]=' sound/soc/codecs/rt715-sdw.h
    defsnc 'static[ ]unsigned[ ]char[ ]\(in\|out\)put_clk_map_imx35\[ASRC_CLK_MAP_LEN\][ ]=' sound/soc/fsl/fsl_asrc.c
    defsc 'static[ ]unsigned[ ]char[ ]\(in\|out\)put_clk_map_imx53\[ASRC_CLK_MAP_LEN\][ ]=' sound/soc/fsl/fsl_asrc.c
    defsnc 'static[ ]unsigned[ ]char[ ]clk_map_imx8q\(m\|xp\)\[2\]\[ASRC_CLK_MAP_LEN\][ ]=' sound/soc/fsl/fsl_asrc.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]pan_volumes\[256\][ ]=' sound/synth/emux/emux_synth.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]\(voltab[12]\|expressiontab\)\[128\][ ]=' sound/synth/emux/emux_synth.c
    defsnc 'static[ ]const[ ]int[ ]log_tbl\[129\][ ]=' sound/synth/emux/soundfont.c
    defsnc 'static[ ]const[ ]short[ ]\(attack\|decay\)_time_tbl\[128\][ ]=' sound/synth/emux/soundfont.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]bcd2000_init_sequence\[\][ ]=' sound/usb/bcd2000/bcd2000.c
    defsc 'static[ ]const[ ]struct[ ]s_c2[ ]SetRate48000\[\][ ]=' sound/usb/usx2y/usbusx2yaudio.c
    accept '[\t]*\.default_fw_filename[ ]=[ ]["]\(sof\|reef\)-[^" ;]*\.ri["]' sound/soc/sof/'\(sof\|reef\)-\(acpi\|pci\)-dev\.c'
    accept '[\t]*tplg_filename[ ]=[ ]devm_kasprintf[(]sdev->dev[,][ ]GFP_KERNEL[,][\n][\t ]*["]%s-%s\.tplg["][,]' sound/soc/sof/intel/byt.c
    accept '[\t]*dev_dbg[(]sdev->dev[,][ ]["]request_firmware[ ]%s[ ]successful' sound/soc/sof/loader.c
    accept '[\t]ret[ ]=[ ]request_firmware[(][&]fw[,][ ]file[,][ ]scomp->dev[)]' sound/soc/sof/topology.c
    blobname '\(board-2\|bdwlan\|caldata\)\.bin' 'drivers/net/wireless/ath/ath11k/\(hw\|qmi\)\.h'
    blobname 'board\.bin' ddrivers/net/wireless/ath/ath11k/core.c
    blobname 'scp\.img' drivers/remoteproc/mtk_scp.c
    blobname '%s[/]%08x-%04x-%04x-%02x%02x%02x%02x%02x%02x%02x%02x\.bin' drivers/tee/amdtee/core.c
    blobname 'qcom[/]sdm845[/]\([ac]dsp\.mdt\|\(mba\|modem\)\.mbn\)' arch/arm64/boot/dts/qcom/sdm845-db845c.dts
    blobname 'brcmfmac\(43456\|4359\)-sdio' drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]\(voice_focus\|mic_svm\|equalizer\)_vals_lookup\[\][ ]=' sound/pci/hda/patch_ca0132.c
    defsnc 'static[ ]const[ ]struct[ ]hda_verb[ ]ca0132_init_verbs[01]\[\][ ]=' sound/pci/hda/patch_ca0132.c

    # New variation in 5.6.6, 5.5.19, and 5.4.34.
    # The firmware file name is supplied by the user.
    accept '[\t]err[ ]=[ ]request_firmware_direct[(][&]fw[,][ ]file_name[,]\([^\n]*[\n]\+[^\n}]\)*err[ ]=[ ]mlx5_firmware_flash[(]' drivers/net/ethernet/mellanox/mlx5/core/devlink.c

    # New in 5.7-rc7.
    accept '[\t ]*:\([ ]*[32][86420]0*\)\+\([\n][ ]*[32][86420]0*:\([ ]*[012345]\)*\)\+' Documentation/cpu-freq/cpufreq-stats.rst
    accept '\(The[ ]\)\?firmware_request_platform[(][)][ ]function' Documentation/driver-api/firmware/fallback-mechanisms.rst
    accept '[ ][ ][ ]request_firmware[\n]' Documentation/driver-api/firmware/index.rst
    accept '[ ][ ]firmware_request_platform[(][)][ ]is[ ]used' Documentation/driver-api/firmware/lookup-order.rst
    accept '\([ ][ ][ ]:functions:[ ]\)\?firmware_request_platform' Documentation/driver-api/firmware/request_firmware.rst
    accept '\(typical[ ]data[ ]at[ ]NVRAM[ ]address[ ]0x100[ ][(]53c810a[ ]NVRAM[)]\|device[ ]set[ ]up[ ][(]up[ ]to[ ]16[ ]devices[ ]-[ ]includes[ ]controller[)]\)::\([\n]\+[ ][ ][ ]\([ ][0-9a-f][0-9a-f]\)\+\([ ]-[ ]id[ ]\(0\|15\)\)\?\)*' Documentation/scsi/'\(ncr53c8xx\|sym53c8xx_2\)\.rst'
    accept 'default[ ]nvram[ ]data::\([\n]\+[ ][ ][ ]\([ ]0x[0-9a-f][0-9a-f][0-9a-f][0-9a-f]\)\+\)*' Documentation/scsi/'\(ncr53c8xx\|sym53c8xx_2\)\.rst'
    defsnc 'static[ ]const[ ]u64[ ]table_ladder\[\][ ]=' arch/x86/crypto/curve25519-x86_64.c
    defsnc 'static[ ]unsigned[ ]icx_cha_msr_offsets\[\][ ]=' arch/x86/events/intel/uncore_snbep.c
    accept '[ ][*][ ]firmware_request_platform[(][)][ ]-' drivers/base/firmware_loader/main.c
    accept '[ ][*][ ]This[ ]function[ ]is[ ]similar[ ]in[ ]behaviour[ ]to[ ]request_firmware[,]' drivers/base/firmware_loader/main.c
    accept 'int[ ]firmware_request_platform[(]' drivers/base/firmware_loader/main.c
    accept 'EXPORT_SYMBOL_GPL[(]firmware_request_platform[)]' drivers/base/firmware_loader/main.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_2tap_16p\[18\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_3tap_16p_\(upscale\|116\|149\|183\)\[27\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_4tap_16p_\(upscale\|116\|149\|183\)\[36\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_2tap_64p\[66\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_3tap_64p_\(upscale\|116\|149\|183\)\[99\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_4tap_64p_\(upscale\|116\|149\|183\)\[132\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_5tap_64p_\(upscale\|116\|149\|183\)\[165\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_6tap_64p_\(upscale\|116\|149\|183\)\[198\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_7tap_64p_\(upscale\|116\|149\|183\)\[231\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    defsnc 'static[ ]const[ ]uint16_t[ ]filter_8tap_64p_\(upscale\|116\|149\|183\)\[264\][ ]=' drivers/gpu/drm/amd/display/dc/dce/dce_scl_filters.c
    accept '#define[ ]NT35510_GAMMA_\(POS\|NEG\)_DEFAULT[ ]0x[0-9A-F][0-9A-F]\([,][ ]\([\\][\n][\t ]*\)\?0x[0-9A-F][0-9A-F]\)*' drivers/gpu/drm/panel/panel-novatek-nt35510.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]ad7124_reg_size\[\][ ]=' drivers/iio/adc/ad7124.c
    defsnc 'static[ ]const[ ]u16[ ]gp2ap002_illuminance_table\[\][ ]=' drivers/iio/light/gp2ap002.c
    defsnc 'static[ ]const[ ]struct[ ]imx219_reg[ ]mode_\(3280x2464\|1920_1080\|1640_1232\|640_480\)_regs\[\][ ]=' drivers/media/i2c/imx219.c
    defsc 'static[ ]const[ ]u16[ ]mv88e6390_serdes_regs\[\][ ]=' drivers/net/dsa/mv88e6xxx/serdes.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]zigzag\[64\][ ]=' drivers/staging/media/hantro/hantro_jpeg.c
    defsnc 'static[ ]const[ ]u32[ ]hw_reorder\[64\][ ]=' drivers/staging/media/hantro/hantro_jpeg.c
    defsnc 'static[ ]const[ ]u8[ ]eos_sequence\[SZ_4K\][ ]=' drivers/staging/media/meson/vdec/codec_h264.c
    defsnc 'static[ ]const[ ]struct[ ]v4l2_fract[ ]par_table\[\][ ]=' drivers/staging/media/meson/vdec/codec_h264.c
    defsnc 'const[ ]u16[ ]vdec_hevc_parser_cmd\[\][ ]=' drivers/staging/media/meson/vdec/codec_hevc_common.c
    defsnc 'static[ ]const[ ]unsigned[ ]short[ ]uni_def_upcase\[EXFAT_NUM_UPCASE\][ ]=' fs/exfat/nls.c
    accept 'int[ ]firmware_request_platform[(]const[ ]struct[ ]firmware[ ][*][*]fw' include/linux/firmware.h
    accept 'static[ ]inline[ ]int[ ]firmware_request_platform[(]const[ ]struct[ ]firmware[ ][*][*]fw' include/linux/firmware.h
    defsnc '[\t]static[ ]const[ ]u8[ ]test_data\[\][ ]=' lib/test_firmware.c
    defsnc 'static[ ]const[ ]struct[ ]reg_table[ ]mt6660_setting_table\[\][ ]=' sound/soc/codecs/mt6660.c
    accept '[\t]const[ ]char[ ][*]fw_name[ ]=[ ]["]test-firmware\.bin["]' tools/testing/selftests/firmware/fw_namespace.c
    defsnc 'struct[ ]reuse_opts[ ]unreusable_opts\[12\][ ]=' tools/testing/selftests/net/reuseaddr_ports_exhausted.c
    blob 'The[ ]card[ ]requires[ ]firmware.*[\n][\t]rm[ ]wd7296a\.sys' Documentation/scsi/wd719x.rst
    blobname 'rtl_bt[/]rtl8822cs_fw\.bin' drivers/bluetooth/btrtl.c
    # If this is code at all, it could use some assembly comments.
    # Most of it is so regular that disassembly of the final irregular
    # bits should suffice to make it all transparent.
    defsnc 'static[ ]const[ ]u32[ ]vgpr_init_compute_shader_arcturus\[\][ ]=' drivers/gpu/drm/amd/amdgpu/gfx_v9_0.c
    defsnc '[\t]static[ ]const[ ]u8[ ]pre_computed_values\[\][ ]=' drivers/gpu/drm/amd/display/amdgpu_dm/amdgpu_dm.c
    blobname 'i915[/]tgl_dmc_ver2_06\.bin' drivers/gpu/drm/i915/intel_csr.c
    blobname 'goodix_%s_cfg\.bin' drivers/input/touchscreen/goodix.c
    blobname 'dvb-demod-m88ds3103b\.fw' drivers/media/dvb-frontends/m88ds3103_priv.h
    blobname 'mediatek[/]mt8173[/]vpu_[pd]\.bin' drivers/media/platform/mtk-vpu/mtk_vpu.c
    blobname 'qcom[/]venus-5\.4[/]venus\.mdt' drivers/media/platform/qcom/venus/core.c
    blobname 'brcmfmac4364-pcie' drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
    blobname 'mediatek[/]mt7622_\(n9\|rom_patch\)\.bin' drivers/net/wireless/mediatek/mt76/mt7615/mt7615.h
    blobname 'mediatek[/]mt7663\(pr2h\|_n9\)_v3\.bin' drivers/net/wireless/mediatek/mt76/mt7615/mt7615.h
    blobname 'silead[/]\(gsl3680-chuwi-hi8-pro\|gsl3670-cube-iwork8-air\|gsl3676-onda-v80-plus-v3\|gsl1680-pipo-w2s\)\.fw' drivers/platform/x86/touchscreen_dmi.c
    accept '[\t]const[ ]char[ ][*]pathname[ ]=[ ]["][/]tmp[/]isst_cpu_topology\.dat["][;]' tools/power/x86/intel-speed-select/isst-config.c

    blobname 'iqs620a\.bin' Documentation/devicetree/bindings/mfd/iqs62x.yaml
    blobname 'iqs620a_coil\.bin' Documentation/devicetree/bindings/mfd/iqs62x.yaml
    blobname 'imx[/]sdma[/]sdma-imx7d\.bin' arch/arm64/boot/dts/freescale/imx8mp.dtsi
    blobname 'qcom[/]sdm845[/]\([ac]dsp\.mdt\|\(mba\|modem\)\.mbn\)' arch/arm64/boot/dts/qcom/sdm845-mtp.dts
    blobname 'cpt8x-mc\.tar' drivers/crypto/marvell/octeontx/otx_cptpf_ucode.h
    blobname 'amdgpu[/]navi12_dmcu\.bin' drivers/gpu/drm/amd/display/amdgpu_dm/amdgpu_dm.c
    blobname 'iqs62\(0a\|[1245]\)\.bin' drivers/mfd/iqs62x.c
    blobname 'ipa_fws\.mdt' drivers/net/ipa/ipa_main.c
    blobname 'microchip[/]mscc_vsc8584_revb_int8051_fb48.bin' drivers/net/phy/mscc/mscc.h
    blobname 'microchip[/]mscc_vsc8574_revb_int8051_29e8.bin' drivers/net/phy/mscc/mscc.h
    # This driver enables the user to update the non-Free BIOS, but it
    # only issues a firmware request if specifically told to.  It
    # doesn't require any non-Free firmware to function, and it
    # doesn't actually recommend users to perform updates, so I'm
    # leaving it in.
    accept '[\t]*pr_err[(]["]request_firmware_nowait[ ]failed' drivers/platform/x86/dell_rbu.c
    blobname 'idt82p33xxx\.bin' drivers/ptp/ptp_idt82p33.h
    blobname 'meson[/]vdec[/]\(gxbb_h264\|gxl_vp9\|gxl_h264\|gxm_h264\|g12a_vp9\|g12a_h264\|sm1_vp9_mmu\)\.bin' drivers/staging/media/meson/vdec/vdec_platform.c
    accept '[\t]rc[ ]=[ ]firmware_request_platform[(][&]firmware[,][ ]' lib/test_firmware.c
    accept '[ ]*device[ ]name[ ]with[ ]["]\.bin["][ ]as' Documentation/devicetree/bindings/mfd/iqs62x.yaml
    # Moved down.
    # blobname 'amdgpu[/]%s' drivers/gpu/drm/amd/amdgpu/amdgpu_psp.c
    accept '[\t][\t]\.sha256[\t ]=[ ][{][ ]0x[0-9a-f][0-9a-f]\([,][ \t\n]*0x[0-9a-f][0-9a-f]\)*[ ][}][,]' drivers/platform/x86/touchscreen_dmi.c
    # Sources added to 5.7.8, but they were available elsewhere before..
    defsnc 'static[ ]const[ ]u32[ ]ivb_clear_kernel\[\][ ]=' drivers/gpu/drm/i915/gt/ivb_clear_kernel.c
    defsnc 'static[ ]const[ ]u32[ ]hsw_clear_kernel\[\][ ]=' drivers/gpu/drm/i915/gt/hsw_clear_kernel.c

    # New in 5.8-rc5.
    blobname 'brcm[/]BCM%s\.hcd' drivers/bluetooth/btbcm.c
    accept '[ ]Package[\t]Core[\t]CPU[\t]Bzy_MHz\([\n][ ]0[\t][\t]\([0-9]\|1[0-3]\)[\t]\([0-9]\|1[0-3]\)[\t][1-9][0-9]*\)*' Documentation/admin-guide/pm/intel-speed-select.rst
    accept '[ \t]*cellwise[,]battery-profile[ ]=[ ][/]bits[/][ ]8[ ]<\([\n][ \t]*0x[0-9A-F][0-9A-F]\([ ]0x[0-9A-F][0-9A-F]\)*\)*[\n][ \t]*>[;]' Documentation/devicetree/bindings/power/supply/cw2015_battery.yaml
    blobname 'imx[/]easrc[/]easrc-imx8mn\.bin' Documentation/devicetree/bindings/sound/fsl,easrc.yaml
    defsnc '[ ]*struct[ ]sock_filter[ ]code\[\][ ]=' Documentation/networking/filter.rst
    accept '[ ]*gzip[ ]-n[ ]--force[ ]-9[ ]--stdout[ ]["][$]ofile\.bin["]' arch/powerpc/boot/wrapper
    accept '[ ][*][ ]*0[ ]-[ ]success[ ][(]no[ ]update[ ]done[ ]or[ ]microcode[ ]was[ ]updated[)]' arch/x86/kernel/cpu/microcode/core.c
    blobname 'qca[/]htnv%02x\.bin' drivers/bluetooth/btqca.c
    blobname 'rtl_bt[/]rtl8761b_fw\.bin' drivers/bluetooth/btrtl.c
    defsnc '[}][ ]postdivs\[\][ ]=' drivers/clk/mmp/clk-audio.c
    defsnc '[\t][}][ ]common_modes\[21\][ ]=' drivers/gpu/drm/amd/amdgpu/dce_virtual.c
    defsc 'static[ ]const[ ]unsigned[ ]int[ ]a405_registers\[\][ ]=' drivers/gpu/drm/msm/adreno/a4xx_gpu.c
    blobname 'a6[45]0_\(gmu\.bin\|zap\.mdt\|sqe\.fw\)' drivers/gpu/drm/msm/adreno/adreno_device.c
    defsc 'static[ ]const[ ]struct[ ]ltk050h3146w_cmd[ ]page[13]_cmds\[\][ ]=' drivers/gpu/drm/panel/panel-leadtek-ltk050h3146w.c
    defsnc '[\t]dsi_dcs_write_seq[(]dsi[,][ ]0x' drivers/gpu/drm/panel/panel-leadtek-ltk050h3146w.c
    defsnc 'static[ ]const[ ]struct[ ]ov2740_reg[ ]mode_1932x1092_regs\[\][ ]=' drivers/media/i2c/ov2740.c
    blobname 'habanalabs[/]gaudi[/]gaudi\(-boot\)\?-fit\.itb' drivers/misc/habanalabs/gaudi/gaudi.c
    blobname 'habanalabs[/]gaudi[/]gaudi_tpc\.bin' drivers/misc/habanalabs/gaudi/gaudi.c
    blobname 'habanalabs[/]goya[/]goya-boot-fit\.itb' drivers/misc/habanalabs/goya/goya.c
    defsnc 'static[ ]const[ ]u8[ ]ice_fdir_\(tc\|ud\|sct\|\|i\)p\(v[46]\|[46]_tun\)_pkt\[\][ ]=' drivers/net/ethernet/intel/ice/ice_fdir.c
    defsnc 'static[ ]const[ ]u32[ ]ice_ptypes_gre_of\[\][ ]=' drivers/net/ethernet/intel/ice/ice_flow.c
    defsc 'static[ ]const[ ]struct[ ]ath10k_index_v\?ht_data_rate_type[ ]supported_v\?ht_mcs_rate_nss[12]\[\][ ]=' drivers/net/wireless/ath/ath10k/mac.c
    defsnc '[\t]static[ ]const[ ]u16[ ]freq_list\[\][ ]=' drivers/net/wireless/mediatek/mt76/mt7615/mcu.c
    blobname 'mediatek[/]mt7663\(pr2h\|_n9\)_rebb\.bin' drivers/net/wireless/mediatek/mt76/mt7615/mt7615.h
    blobname 'mediatek[/]mt7915_\(w[am]\|rom_patch\)\.bin' drivers/net/wireless/mediatek/mt76/mt7915/mt7915.h
    defsnc 'static[ ]const[ ]u32[ ]rtw8723d_\(ofdm\|cck\)_swing_table\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8723d.c
    blobname 'rtw88[/]rtw8723d_fw\.bin' drivers/net/wireless/realtek/rtw88/rtw8723d.c
    defsnc 'static[ ]const[ ]u32[ ]rtw8723d_\(mac\|agc\|bb\|rf_a\)\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8723d_table.c
    defsnc 'static[ ]const[ ]struct[ ]rtw_phy_pg_cfg_pair[ ]rtw8723d_bb_pg\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8723d_table.c
    defsnc 'static[ ]const[ ]struct[ ]rtw_txpwr_lmt_cfg_pair[ ]rtw8723d_txpwr_lmt\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8723d_table.c
    defsnc 'static[ ]const[ ]struct[ ]rtw_txpwr_lmt_cfg_pair[ ]rtw8822c_txpwr_lmt_type5\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8723d_table.c
    blobname 'gsl3680-mpman-mpwin895cl\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'gsl3676-onda-v891-v5\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'gsl1680-techbite-arc-11-6\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'gsl1680-vinga-twizzle_j116\.fw' drivers/platform/x86/touchscreen_dmi.c
    defsc 'static[ ]struct[ ]ov2680_reg[ ]const[ ]ov2680_\(global_setting\|\(Q\?CIF\|QVGA\|656x496\|800x600\|720p\|1296x976\|1456x1096\|1616x916\|1616x1082\)_30fps\)\[\][ ]=' drivers/staging/media/atomisp/i2c/ov2680.h
    defsnc 'static[ ]struct[ ]ia_css_macc_table[ ]\(skin_\(low\|medium\|high\)\|blue\|green\)_macc_table[ ]=' drivers/staging/media/atomisp/pci/atomisp_tables.h
    defsnc 'static[ ]struct[ ]ia_css_ctc_table[ ]vivid_ctc_table[ ]=' drivers/staging/media/atomisp/pci/atomisp_tables.h
    blobname 'shisp_240\(0b\|1a\)0_v21\.bin' 'drivers/staging/media/atomisp/\(TODO\|atomisp_v4l2\.c\)'
    blobname 'shisp_2401a0_legacy_v21\.bin' drivers/staging/media/atomisp/pci/atomisp_v4l2.c
    defsnc 'static[ ]const[ ]s16[ ]g_pyramid\[8\]\[8\][ ]=' drivers/staging/media/atomisp/pci/isp/kernels/tdf/tdf_1.0/ia_css_tdf.host.c
    defsc 'static[ ]const[ ]struct[ ]vnt_threshold[ ]\(al2230\|vt3\(226\|342\)\)_vnt_threshold\[\][ ]=' drivers/staging/vt6656/baseband.c
    defsnc 'static[ ]const[ ]int[ ]k3_adc_to_temp\[\][ ]=' drivers/thermal/k3_bandgap.c
    blobname 'renesas_usb_fw\.mem' drivers/usb/host/xhci-pci.c
    defsnc 'static[ ]u8[ ]swap_bits_table\[\][ ]=' lib/bch.c
    blobname 'dsm_param\(_%s_%s\)\?\.bin' sound/soc/codecs/max98390.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt1016_reg\[\][ ]=' sound/soc/codecs/rt1016.c
    defsnc 'const[ ]struct[ ]reg_default[ ]rt5682_reg\[RT5682_REG_NUM\][ ]=' sound/soc/codecs/rt5682.c
    blobname 'zl38060\.fw' sound/soc/codecs/zl38060.c
    blobname '%s-tplg\.bin' sound/soc/intel/skylake/skl-topology.c
    defsnc 'static[ ]uint8_t[ ]default_tx\[\][ ]=' tools/spi/spidev_test.c
    # This is not used at all, but watch out for future uses thereof.
    # It is intended for use to load large register-set files rather
    # than code.  That ought to be acceptable, but let's make sure no
    # unwanted use slips through.
    blobna 'load_msr_list' drivers/staging/media/atomisp/i2c/atomisp-libmsrlisthelper.c
    accept 'int[ ]load_msr_list[(][^)]*[)][\n][{][\n][\t]*int[ ]ret[ ]=[ ]request_firmware[(]' drivers/staging/media/atomisp/i2c/atomisp-libmsrlisthelper.c
    accept '\(extern[ ]\)\?int[ ]load_msr_list[(][^)]*[)][;]' drivers/staging/media/atomisp/include/linux/libmsrlisthelper.h
    blobname 'qca[/]crbtfw%02x\.tlv' drivers/bluetooth/btqca.c
    blobname 'qca[/]htbtfw%02x\.tlv' drivers/bluetooth/btqca.c
    blobname 'qca[/]%s' drivers/bluetooth/btqca.c
    accept '[\t]quirks[ \t]*=[ ]XHCI_RENESAS_FW_QUIRK[,][\n][\t]\.firmware[ ]=' drivers/usb/host/xhci-pci.c
    accept '[\t]*dev_err[(][&]pdev->dev[,][ ]["]request_firmware[ ]failed' drivers/usb/host/xhci-pci-renesas.c
    accept 'EXPORT_SYMBOL_GPL[(]load_msr_list[)]' drivers/staging/media/atomisp/i2c/atomisp-libmsrlisthelper.c
    blobna 'for[ ]the[ ]WinTV[/]PVR[^:.]*firmware[^:.]*:[\n ][`][`]hcwamc\.rbf[^\n]*\([\n][^\n][^\n]*\)*' Documentation/admin-guide/media/bttv.rst

    # New in 5.8.2, 5.7.16, 5.4.59, and 4.19.140.
    blobname 'mrvl[/]sdsd8977_combo_v2\.bin' 'drivers/\(bluetooth/btmrvl_sdio\.c\|net/wireless/marvell/mwifiex/sdio\.h\)'
    blobname 'mrvl[/]sdsd8997_combo_v4\.bin' 'drivers/\(bluetooth/btmrvl_sdio\.c\|net/wireless/marvell/mwifiex/sdio\.h\)'

    # New in 5.9-rc6.
    accept '[ ][ ]For[ ]pm\(8841\|8916\|8941\|8994\|8994\|a8084\|i8994\|i8998\|s405\)\([,][ \n][ ]*[slv0-9]*\)*' Documentation/devicetree/bindings/regulator/qcom,smd-rpm-regulator.yaml
    initnc '[ ][ ][ ][ ][$][ ]devlink[ ]region[ ]dump[ ]pci[/][^ ]*[ ]snapshot' Documentation/networking/devlink/ice.rst
    blobname 'nvm_00440302_i2s_eu\.bin' arch/arm64/boot/dts/mediatek/mt8183-kukui-krane.dtsi
    initnc '[\t][\t]temperature-lookup-table[ ]=[ ]<' arch/arm64/boot/dts/mediatek/mt8183-kukui.dtsi
    blobname 'nvm_00440302_i2s\.bin' arch/arm64/boot/dts/mediatek/mt8183-kukui.dtsi
    defsnc 'static[ ]const[ ]u64[ ]inst\[\][ ]=' drivers/crypto/qat/qat_common/qat_hal.c
    defsnc 'static[ ]u8[ ]mci_cbc_\(enc\|dec\)_\(no_iv_\)\?array\[3\]\[MODE_CONTROL_BYTES\][ ]=' drivers/crypto/sa2ul.c
    defsnc 'static[ ]u8[ ]mci_ecb_\(enc\|dec\)_\(no_iv_\)\?array\[3\]\[27\][ ]=' drivers/crypto/sa2ul.c
    blobname 'amdgpu[/]\(tahiti\|verde\|pitcairn\|oland\)_uvd\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_uvd.c
    blobname 'amdgpu[/]\(sienna_cichlid\|navy_flounder\)_vcn\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vcn.c
    blobname 'amdgpu[/]\(sienna_cichlid\|navy_flounder\|%s\)_sdma\(%d\)\?\.bin' drivers/gpu/drm/amd/amdgpu/sdma_v5_2.c
    # Sources are in cwsr_trap_handler_gfx10.asm.
    defsnc 'static[ ]const[ ]uint32_t[ ]cwsr_trap_nv1x_hex\[\][ ]=' drivers/gpu/drm/amd/amdkfd/cwsr_trap_handler.h
    blobname 'amdgpu[/]\(sienna_cichlid\|navy_flounder\|%s\)_dmcub\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_dm.c
    blobname 'i915[/]rkl_dmc_ver2_01\.bin' drivers/gpu/drm/i915/display/intel_csr.c
    initnc '[\t]dsi_dcs_write_seq[(]dsi[,][ ]ST7703_CMD_SET\(GIP[12]\|GAMMA\)[,]' drivers/gpu/drm/panel/panel-sitronix-st7703.c
    defsnc 'static[ ]const[ ]struct[ ]vadc_map_pt[ ]adcmap7_100k\[\][ ]=' drivers/iio/adc/qcom-vadc-common.c
    defsc '[}][ ]ov10635_regs_wizard\[\][ ]=' drivers/media/i2c/rdacm20.c
    accept '[\t][/][*][ ]get[ ]reference[ ]of[ ]pdev[ ]for[ ]request_firmware[ ][*][/]' drivers/misc/ti-st/st_kim.c
    accept '[ ][*][ ]@path:[ ]the[ ]path[ ]of[ ]the[ ]firmware[ ]file[ ]to[ ]use[ ]via[ ]request_firmware' drivers/net/ethernet/intel/ice/ice_devlink.c
    blobname 'mellanox[/]mlxsw_spectrum3-\(["][ ]__stringify[(]MLXSW_SP3_FWREV_[^)]*[)][ \\\n\t]*["]\.\)*mfa2' drivers/net/ethernet/mellanox/mlxsw/spectrum.c
    blobname 'rtl_nic[/]rtl8125b-2\.fw' drivers/net/ethernet/realtek/r8169_main.c
    defsnc 'static[ ]const[ ]u8[ ]rtl88\(12\|21\)ae_delta_swing_table_idx_5g[ba]_[np]\[\]\[DEL_SW_IDX_SZ\][ ]=' drivers/net/wireless/realtek/rtlwifi/rtl8821ae/dm.c
    defsnc 'static[ ]const[ ]u32[ ]rtw8821c_txscale_tbl\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8821c.c
    defsnc 'static[ ]const[ ]u8[ ]rtw8821c_pwrtrk_5g[ba]_[np]\[\]\[RTW_PWR_TRK_TBL_SZ\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8821c.c
    blobname 'rtw88[/]rtw8821c_fw\.bin' drivers/net/wireless/realtek/rtw88/rtw8821c.c
    defsnc 'static[ ]const[ ]u32[ ]rtw8821c_\(mac\|agc\|bb\|rf_a\)\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8821c_table.c
    defsnc 'static[ ]const[ ]struct[ ]rtw_phy_pg_cfg_pair[ ]rtw8821c_bb_pg_type0\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8821c_table.c
    defsnc 'static[ ]const[ ]struct[ ]rtw_txpwr_lmt_cfg_pair[ ]rtw8821c_txpwr_lmt_type0\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8821c_table.c
    defsnc 'static[ ]const[ ]struct[ ]xpsgtr_ssc[ ]ssc_lookup\[\][ ]=' drivers/phy/xilinx/phy-zynqmp.c
    accept '[\t]*dev_err[(]dev[,][ ]["]request_firmware[ ]failed' drivers/remoteproc/remoteproc_core.c
    defsnc 'const[ ]unsigned[ ]char[ ]\(IDX_ACTIVATE_\(READ\|WRITE\)\|\(CM\|ULP\)_\(ENABLE\|SETUP\)\|DM_ACT\|IPA_PDU_HEADER\)\[\][ ]=' drivers/s390/net/qeth_core_mpc.c
    defsnc '[\t]static[ ]const[ ]u8[ ]sbox_table\[256\][ ]=' drivers/staging/rtl8723bs/core/rtw_security.c
    defsnc '[\t]static[ ]const[ ]u8[ ]rx_hash_toeplitz_key\[\][ ]=' drivers/vdpa/mlx5/net/mlx5_vnet.c
    defsnc 'static[ ]struct[ ]test_bitmap_cut[ ]test_cut\[\][ ]=' lib/test_bitmap.c
    defsnc 'static[ ]__maybe_unused[ ]const[ ]a3d_Hrtf_t[ ]A3dHrir\(Impulse\|Ones\|SatTest\|DImpulse\)[ ]=' sound/pci/au88x0/au88x0_a3ddata.c
    defsnc 'static[ ]__maybe_unused[ ]xtalk_dline_t[ ]const[ ]alXtalkDlineTest[ ]=' sound/pci/au88x0/au88x0_xtalk.c
    accept '[\t]const[ ]char[ ][*]pathname[ ]=[ ]["][/]var[/]run[/]isst_cpu_topology\.dat["]' tools/power/x86/intel-speed-select/isst-config.c
    # The firmware file name is supplied by the user.
    accept '[\t]err[ ]=[ ]request_firmware_direct[(][&]fw[,][ ]file_name[,][\n\t ]*[&]priv->hwdev->hwif->pdev->dev[)]' drivers/net/ethernet/huawei/hinic/hinic_devlink.c
    accept '[\t]err[ ]=[ ]ice_check_for_pending_update[(]pf[,][ ]component[,][ ]extack[)][;][\n][\t]if[ ][(]err[)][\n][\t][\t]return[ ]err[;][\n][\n][\t]err[ ]=[ ]request_firmware[(][&]fw[,][ ]path[,][ ]dev[)]' drivers/net/ethernet/intel/ice/ice_devlink.c
    blobname 'atmel[/]wilc1000_wifi_firmware-\([0-9]\+\.bin\)\?' drivers/net/wireless/microchip/wilc1000/netdev.c
    # We massage the file with undefine_macro before clean_blob.
    blobname '[/][*][(]DEBLOBBED[)][*][/]["][ ][#]api[ ]["]\.bin' drivers/net/wireless/microchip/wilc1000/netdev.c
    defsnc '[\t]static[ ]const[ ]struct[ ]ephy_info[ ]e_info_8125a_[12]\[\][ ]=' drivers/net/ethernet/realtek/r8169_main.c

    # New in 5.9 final.
    blobname 'gsl1680-mpman-converter9.fw' drivers/platform/x86/touchscreen_dmi.c
    defsc 'static[ ]struct[ ]font_data[ ]fontdata_ter16x32[ ]=' lib/fonts/font_ter16x32.c

    # New in 5.9.2 and 5.8.17.
    accept '[\t][\t]\.driver_data[ ]=[ ]["]\(sof\|reef\)-[^" ;]*\.tplg["]' sound/soc/sof/'\(sof\|reef\)-pci-dev\.c'

    # New in 5.9.7 and 5.4.76.
    defsc 'static[ ]const[ ]struct[ ]font_data[ ]fontdata_ter16x32[ ]=' lib/fonts/font_ter16x32.c

    # New in 5.9.9.
    defsnc 'static[ ]const[ ]struct[ ]msm_gpio_wakeirq_map[ ]sm8250_pdc_map\[\][ ]=' drivers/pinctrl/qcom/pinctrl-sm8250.c

    # New in 5.10-rc.
    defsc '\([/][*]\)\?static[ ]unsigned[ ]int[ ]\(No\)\?DbiPrbs7\[\][ ]=' drivers/gpu/drm/amd/pm/inc/smu_11_0_cdr_table.h
    defsnc 'static[ ]const[ ]struct[ ]phy_settings[ ]vc5_hdmi_phy_settings\[\][ ]=' drivers/gpu/drm/vc4/vc4_hdmi_phy.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]ad9434_scale_table\[\]\[2\][ ]=' drivers/iio/adc/ad9467.c
    defsc 'static[ ]const[ ]struct[ ]reg_default[ ]lp50\(24\|36\)_reg_defs\[\][ ]=' drivers/leds/leds-lp50xx.c
    defsc 'static[ ]const[ ]struct[ ]SMap[I2 ]\?[ ]m_\(RF_Cal\|\(Main\|Cal\)_PLL\|GainTaper\|RF_Cal_DC_Over_DT\|CID_Target\)_Map\[\][ ]=' drivers/media/dvb-frontends/tda18271c2dd_maps.h
    defsnc 'static[ ]const[ ]struct[ ]ov8856_reg[ ]mode_\(3264x2448\|1632x1224\)_regs\[\][ ]=' drivers/media/i2c/ov8856.c
    defsc 'static[ ]const[ ]u32[ ]CRC_LUT\[256\][ ]=' drivers/media/test-drivers/vidtv/vidtv_psi.c
    defsc 'static[ ]const[ ]u8[ ]reverse\[256\][ ]=' drivers/media/test-drivers/vidtv/vidtv_s302m.c
    defsnc 'static[ ]const[ ]u8[ ]r8a779\(6\(5\|_es13\)\|90\)_calib_table\[2\]\[SDHI_CALIB_TABLE_MAX\][ ]=' drivers/mmc/host/renesas_sdhi_core.c
    defsnc 'static[ ]const[ ]u16[ ]mcp251xfd_crc16_table\[\][ ]=' drivers/net/can/spi/mcp251xfd/mcp251xfd-crc16.c
    defsnc 'static[ ]const[ ]u32[ ]ice_ipv[46]_\(ofos\|il\)_no_l4\[\][ ]=' drivers/net/ethernet/intel/ice/ice_flow.c
    defsc 'static[ ]const[ ]struct[ ]ath10k_mem_section[ ]qca6174_hw30_sdio_register_sections\[\][ ]=' drivers/net/wireless/ath/ath10k/coredump.c
    accept 'const[ ]struct[ ]firmware[ ][*]ath11k_core_firmware_request[(]' drivers/net/wireless/ath/ath11k/'core\.[ch]'
    accept '[\t]*\(bd->fw\|fw_entry\|fw\)[ ]=[ ]ath11k_core_firmware_request[(]' drivers/net/wireless/ath/ath11k/qmi.c
    blobname '\(amss\|m3\)\.bin' drivers/net/wireless/ath/ath11k/hw.h
    blobname 'gsl1680-irbis-tw118\.fw' drivers/net/wireless/intel/iwlwifi/fw/pnvm.c
    blobname 'gsl3680-predia-basic\.fw' drivers/net/wireless/intel/iwlwifi/fw/pnvm.c
    accept '[\t]s->data_sz[ ][=][ ][0-9]*[;][\n][\t]s->data[ ]=[ ][(]void[ ][*][)]["]\([\\]\([0-7][0-7]*\|x[0-9a-f][0-9a-f]\|[\n]\)\)*["][;]' kernel/bpf/preload/iterators/iterators.skel.h
    accept '[ ][*][ ]@file_offset:[ ]file[ ]offset[ ]to[ ]request[ ]when[ ]calling[ ]request_firmware_into_buf' lib/test_firmware.c
    accept '[ ][*][ ]@partial:[ ]partial[ ]read[ ]opt[ ]when[ ]calling[ ]request_firmware_into_buf' lib/test_firmware.c
    accept '[\t]*req->rc[ ]=[ ]request_\(partial_\|\)firmware_into_buf[\n][\t]*[(][&]req->fw[,][\n][\t]*[ ]req->name' lib/test_firmware.c
    blobname 'qcom[/]sc7180-trogdor[/]modem[/]\(mba\|qdsp6sw\)\.mbn' arch/arm64/boot/dts/qcom/sc7180-trogdor-lte-sku.dtsi
    blobname 'qcom[/]sc7180-trogdor[/]modem-nolte[/]\(mba\|qdsp6sw\)\.mbn' arch/arm64/boot/dts/qcom/sc7180-trogdor.dtsi
    blobname 'qcom[/]sdm845[/][ac]dsp\.mdt' arch/arm64/boot/dts/qcom/sdm845-xiaomi-beryllium.dts
    blobname 'qcom[/]sdm845[/]mba\.mbn' arch/arm64/boot/dts/qcom/sdm845-xiaomi-beryllium.dts
    blobname 'qcom[/]sdm845[/]modem\.mdt' arch/arm64/boot/dts/qcom/sdm845-xiaomi-beryllium.dts
    accept '[ ][*][ ]request_partial_firmware_into_buf[(][)][ ]-[ ]load' drivers/base/firmware_loader/main.c
    accept '[ ][*][ ]This[ ]function[ ]works[ ]pretty[ ]much[ ]like[ ]request_firmware_into_buf[ ]except' drivers/base/firmware_loader/main.c
    accept 'request_partial_firmware_into_buf[(]const[ ]struct[ ]firmware' drivers/base/firmware_loader/main.c
    accept 'EXPORT_SYMBOL[(]request_partial_firmware_into_buf[)]' drivers/base/firmware_loader/main.c
    accept '\(static[ ]inline[ ]\)\?int[ ]request_partial_firmware_into_buf\([(]const[ ]struct[ ]firmware\|[\n]\)' include/linux/firmware.h
    accept '[\t]retval0[ ]=[ ]report_missing_free_firmware[^\n]*[\n][\t]retval[ ]=[ ]request_partial_firmware_into_buf[(][&]xfw[,][ ]NONFREE_FIRMWARE' include/linux/firmware.h
    accept '[\t]if[ ][(]is_nonfree_firmware[^\n]*[\n][\t][\t]return[ ]reject_partial_firmware_into_buf[^\n]*[\n][\t]else[\n][\t][\t]return[ ]request_partial_firmware_into_buf[(]firmware_p[,][ ]name[,]' include/linux/firmware.h
    accept 'test_request_partial_firmware_into_buf\(_nofile\)\?\([(][)]\|[ ][0-9]\)' tools/testing/selftests/firmware/fw_filesystem.sh
    accept '[\t]echo[ ]-n[ ]["]Test[ ]request_partial_firmware_into_buf[(][)]' tools/testing/selftests/firmware/fw_filesystem.sh
    blobname 'amdgpu[/]green_sardine_vcn\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vcn.c
    blobname 'amdgpu[/]green_sardine_dmcub\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_dm.c
    blobname 'cadence[/]mhdp8546\.bin' drivers/gpu/drm/bridge/cadence/cdns-mhdp8546-core.h
    blobname 'i915[/]rkl_dmc_ver2_02\.bin' drivers/gpu/drm/i915/display/intel_csr.c
    blobname 'i915[/]tgl_dmc_ver2_08\.bin' drivers/gpu/drm/i915/intel_csr.c
    blobname 'mrvl[/]prestera[/]mvsw_prestera_fw-v%u\.%u\.img' drivers/net/ethernet/marvell/prestera/prestera_pci.c
    # The firmware file name is supplied by the user.
    accept '[\t]err[ ]=[ ]request_firmware_direct[(][&]fw[,][ ]params->file_name' drivers/net/ethernet/huawei/hinic/hinic_devlink.c
    accept '[\t]err[ ]=[ ]request_firmware[(][&]fw[,][ ]params->file_name[,][ ]dev[)]' drivers/net/ethernet/intel/ice/ice_devlink.c
    accept '[\t]err[ ]=[ ]request_firmware_direct[(][&]fw[,][ ]params->file_name' drivers/net/ethernet/mellanox/mlx5/core/devlink.c
    accept '[\t]err[ ]=[ ]request_firmware[(][&]fw[,][ ]fw_name[,][ ]ionic->dev[)]' drivers/net/ethernet/pensando/ionic/ionic_fw.c
    accept '[\t]err[ ]=[ ]request_firmware_direct[(][&]firmware[,][ ]params->file_name' drivers/net/ethernet/mellanox/mlxsw/spectrum.c
    blobname 'intel[/]ibt-%u-%u-%u\.sfi' drivers/bluetooth/hci_intel.c
    blobname '[^ ]*[:][/][/][^ ]*linux-can[/]can-firmware' drivers/net/can/softing/Kconfig
    blobna 'which[ ]you[ ]can[ ]get[ ]at[\n][	][ ][ ]http[^\n]*[/]linux-can[/][\n][^-]*firmware[ ]version[^\n]*' drivers/net/can/softing/Kconfig
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]ca0113_mmio_init_\(address\|data\)_ae5\[\][ ]=' sound/pci/hda/patch_ca0132.c
    blobname 'qcom[/]LENOVO[/]81F1[/]qcdsp\(1v\)\?28998.mbn' arch/arm64/boot/dts/qcom/msm8998-lenovo-miix-630.dts
    blobname 'qcom[/]sdm845[/]a630_zap\.mbn' arch/arm64/boot/dts/qcom/'sdm845-\(db845c\|mtp\|xiaomi-beryllium\)\.dts'
    blobname 'qcom[/]LENOVO[/]81JL[/]qc\([ac]dsp\|dsp\(1v\)\?2\)850\.mbn' arch/arm64/boot/dts/qcom/sdm850-lenovo-yoga-c630.dts
    blobname 'qcom[/]LENOVO[/]81JL[/]qcdxkmsuc850\.mbn' 'Documentation/devicetree/bindings/display/msm/gpu.txt\|arch/arm64/boot/dts/qcom/sdm850-lenovo-yoga-c630.dts'
    blobname 'qcom[/]sm8250[/]\([ac]dsp\|slpi\).mbn' arch/arm64/boot/dts/qcom/sm8250-mtp.dts

    # New in 5.11-rc6.
    initnc '[\t][\t]dlg,mem-array[ ]=[ ]<' Documentation/devicetree/bindings/input/dlg,da7280.txt
    initnc '\.Lpermute:' arch/arm/crypto/chacha-neon-core.S
    blobname 'qca[/]crnv%02xu\.bin' drivers/bluetooth/btqca.c
    blobname 'rtl_bt[/]rtl8852au_fw\.bin' drivers/bluetooth/btrtl.c
    blobname 'qca[/]nvm_usb_%08x_%04x\.bin' drivers/bluetooth/btusb.c
    blobname 'amdgpu[/]%s_toc\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_psp.c
    # Moved down, after %s_cap and %s.bin under 5.18-rc.
    # blobname 'amdgpu[/]%s' drivers/gpu/drm/amd/amdgpu/amdgpu_psp.c
    blobname 'amdgpu[/]vangogh_vcn\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vcn.c
    blobname 'amdgpu[/]dimgrey_cavefish_vcn\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vcn.c
    blobname 'amdgpu[/]vangogh_dmcub\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_dm.c
    blobname 'amdgpu[/]dimgrey_cavefish_dmcub\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_dm.c
    defsnc 'static[ ]const[ ]struct[ ]IP_BASE[ ]VCN0_BASE[ ]=[ ]' drivers/gpu/drm/amd/include/dimgrey_cavefish_ip_offset.h
    defsnc 'static[ ]const[ ]struct[ ]IP_BASE[ ]\(FCH\|MP2\|USB\)_BASE[ ]=[ ]' drivers/gpu/drm/amd/include/vangogh_ip_offset.h
    defsnc 'static[ ]struct[ ]lt9611uxc_mode[ ]lt9611uxc_modes\[\][ ]=' drivers/gpu/drm/bridge/lontium-lt9611uxc.c
    blobname 'i915[/]dg1_dmc_ver2_02\.bin' drivers/gpu/drm/i915/display/intel_csr.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]sx9310_pthresh_codes\[\][ ]=' drivers/iio/proximity/sx9310.c
    defsc 'static[ ]const[ ]struct[ ]reg_8[ ]imx274_mode6_1280x540_raw10\[\][ ]=' drivers/media/i2c/imx274.c
    defsnc 'static[ ]const[ ]struct[ ]ov02a10_reg[ ]ov02a10_1600x1200_regs\[\][ ]=' drivers/media/i2c/ov02a10.c
    defsnc 'static[ ]const[ ]struct[ ]reg_value[ ]ov5640_setting_QQVGA_160_120\[\][ ]=' drivers/media/i2c/ov5640.c
    defsnc 'static[ ]const[ ]struct[ ]ov9734_reg[ ]mode_1296x734_regs\[\][ ]=' drivers/media/i2c/ov9734.c
    defsnc 'static[ ]const[ ]int[ ]pf8x00_sw7_voltages\[\][ ]=' drivers/regulator/pf8x00-regulator.c
    defsc 'static[ ]const[ ]u8[ ]prob_table_init\[\][ ]=' drivers/staging/media/sunxi/cedrus/cedrus_vp8.c
    defsnc 'static[ ]const[ ]u8[ ]k_mv_entropy_update_probs\[2\]\[V4L2_VP8_MV_PROB_CNT\][ ]=' drivers/staging/media/sunxi/cedrus/cedrus_vp8.c
    defsnc 'static[ ]const[ ]u32[ ]SHA256_K\[\][ ]=' lib/crypto/sha256.c
    accept '[\t]local[ ]mount_img=["][$][{]tmp_dir[}][/]test\.img' tools/testing/selftests/bpf/ima_setup.sh
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]sync_v2\[\][ ]=' tools/testing/selftests/net/timestamping.c
    accept '[\t]if[ ][(][!]encl_load[(]["]test_encl\.elf["]' tools/testing/selftests/sgx/main.c
    accept 'MZPKT_[A-Z0-9_]*=["][0-9a-f][0-9a-f]\(:\([\\][\n]\)\?[0-9a-f][0-9a-f]\)*["]' tools/testing/selftests/net/forwarding/bridge_mld.sh
    accept 'CBPF_MPTCP_SUBOPTION_ADD_ADDR=["][0-9,\n\t ]*["]' tools/testing/selftests/net/mptcp/mptcp_join.sh
    accept 'int[ ]s3fwrn5_fw_request_firmware[(]struct[ ]s3fwrn5_fw_info' drivers/nfc/s3fwrn5/'firmware\.[ch]'
    accept '[\t]ret[ ]=[ ]request_firmware[(][&]params\.fw[,][ ]file_name[,][ ]devlink->dev[)]' net/core/devlink.c
    defsnc 'static[ ]const[ ]struct[ ]coex_5g_afh_map[ ]afh_5g_8822b\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8822b.c
    blobname 'ccs[/]ccs-\(sensor\|module\)-%4.4x-%4.4x-%4.4x\.fw' drivers/media/i2c/ccs/ccs-core.c
    blobname 'lt9611uxc_fw\.bin' drivers/gpu/drm/bridge/lontium-lt9611uxc.c
    blobname 'qat_4xxx\(\|_\(mmp\|sym\|asym\|admin\)\)\.bin' drivers/crypto/qat/qat_4xxx/adf_4xxx_hw_data.h
    blobname 'qcom[/]sdx55m[/]\(sbl1\|edl\)\.mbn' drivers/bus/mhi/pci_generic.c
    blobname 'qcom[/]sm8150[/]\([ac]dsp\|slpi\)\.mbn' arch/arm64/boot/dts/qcom/sm8150-hdk.dts
    blobname 'qcom[/]sm8150[/]\([ac]dsp\|modem\|slpi\)\.mdt' arch/arm64/boot/dts/qcom/sm8150-mtp.dts
    blobname 'imx[/]xcvr[/]xcvr-imx8mp\.bin' sound/soc/fsl/fsl_xcvr.c

    # New in 5.11.3.
    accept '[\t]s6e63m0_dcs_write_seq_static[(]ctx[,][ ]MCS_[^ ,\t\n)]*\([, \t\n]*0x[0-9a-f][0-9a-f]\)*[)][;]' drivers/gpu/drm/panel/panel-samsung-s6e63m0.c

    # New in 5.12-rc5.
    blobname 'ice\.pkg' drivers/net/ethernet/intel/ice/ice_main.c
    blob 'Dynamic[ ]Device[ ]Personalization[\n]-\+[\n]\([^\n]\+[\n][\n]\?\)*of[ ]the[ ]default[ ]DDP[ ]package[ ]file[ ][(]ice\.pkg[)]\.' Documentation/networking/device_drivers/ethernet/intel/ice.rst
    initnc '[ \t]*[.]active_vlans[ ]=[ ][(]unsigned[ ]long[ ]\[64\][)]' Documentation/networking/device_drivers/qlogic/qlge.rst
    accept '[ \t]*["]values["]:[ ]\[[ ]0\([,]0\)*[ ]\]' Documentation/networking/device_drivers/qlogic/qlge.rst
    blobname 'qcom[/]sm8250[/][ac]dsp\.mbn' arch/arm64/boot/dts/qcom/qrb5165-rb5.dts
    blobname 'qcom[/]sm8250[/]a650_zap\.mbn' arch/arm64/boot/dts/qcom/'qrb5165-rb5\|sm8250-mtp\.'dts
    blobname 'qcom[/]sdm845[/]oneplus6[/]\([ac]dsp\|a630_zap\|mba\|modem\)\.mbn' arch/arm64/boot/dts/qcom/sdm845-oneplus-common.dtsi
    blobname 'oneplus6[/]crnv21\.bin' arch/arm64/boot/dts/qcom/sdm845-oneplus-common.dtsi
    blobname 'mediatek[/]BT_RAM_CODE_MT%04x_1_%x_hdr\.bin' drivers/bluetooth/btusb.c
    blobname 'mrvl[/]cpt%02d[/]%s\.out' drivers/crypto/marvell/octeontx2/otx2_cptpf_ucode.c
    blobname 'a5\(08\|12\)_zap\.mdt' drivers/gpu/drm/msm/adreno/adreno_device.c
    defsc 'static[ ]const[ ]struct[ ]khadas_ts050_panel_cmd[ ]init_code\[\][ ]=' drivers/gpu/drm/panel/panel-khadas-ts050.c
    blobname 'dvb-demod-mxl692\.fw' drivers/media/dvb-frontends/mxl692.h
    defsnc 'static[ ]const[ ]struct[ ]imx334_reg[ ]mode_3840x2160_regs\[\][ ]=' drivers/media/i2c/imx334.c
    defsnc 'static[ ]struct[ ]regval_list[ ]ov5647_\(2592x1944\|1080p30\|2x2binned\|640x480\)_10bpp\[\][ ]=' drivers/media/i2c/ov5647.c
    defsc 'static[ ]const[ ]struct[ ]ov8865_register_value[ ]ov8865_\(register_values_\(native\|binning\)\|init_sequence\)\[\][ ]=' drivers/media/i2c/ov8865.c
    blobname 'v\(k\(_[ab]0\|\)\|p\)-boot[12]\.bin' drivers/misc/bcm-vk/bcm_vk_dev.c
    defsc 'static[ ]const[ ]u8[ ]mv88e6xxx_lag_mask_table\[8\]\[8\][ ]=' drivers/net/dsa/mv88e6xxx/chip.c
    defsnc 'static[ ]const[ ]struct[ ]rtl8366rb_jam_tbl_entry[ ]rtl8366rb_init_jam_\(ver_[0123]\|f5d8235\)\[\][ ]=' drivers/net/dsa/rtl8366rb.c
    blobname 'mediatek[/]WIFI_RAM_CODE_MT7961_1\.bin' drivers/net/wireless/mediatek/mt76/mt7921/mt7921.h
    blobname 'mediatek[/]WIFI_MT7961_patch_mcu_1_2_hdr\.bin' drivers/net/wireless/mediatek/mt76/mt7921/mt7921.h
    defsnc 'static[ ]const[ ]u32[ ]rtw8821c_agc_btg_type2\[\][ ]=' drivers/net/wireless/realtek/rtw88/rtw8821c_table.c
    defsnc 'static[ ]const[ ]struct[ ]msm_gpio_wakeirq_map[ ]sc8180x_pdc_map\[\][ ]=' drivers/pinctrl/qcom/pinctrl-sc8180x.c
    blobname 'gsl3680-jumper-ezpad-7\.fw' drivers/platform/x86/touchscreen_dmi.c
    defsnc '\(static[ ]\)\?unsigned[ ]short[ ]\(plain\|shift\|altgr\|ctrl\|shift_ctrl\|alt\|ctrl_alt\)_map\[NR_KEYS\][ ]=' drivers/tty/vt/defkeymap.c_shipped
    defsnc 'static[ ]const[ ]struct[ ]xr_txrx_clk_mask[ ]xr21v141x_txrx_clk_masks\[\][ ]=' drivers/usb/serial/xr_serial.c
    defsc '[\t]static[ ]const[ ]u32[ ]base\[4\]\[12\][ ]=' net/wireless/util.c
    defsnc 'static[ ]const[ ]struct[ ]comp_coeff_val[ ]comp_coeff_table\[HPH_MODE_MAX\]\[COMP_MAX_COEFF\][ ]=' sound/soc/codecs/lpass-rx-macro.c
    accept 'ROOTFS_IMAGE=["]root\.img["]' tools/testing/selftests/bpf/vmtest.sh
    accept '[\t]img_fd[ ]=[ ]openat[(]-EBADF[,][ ]["][/]mnt[/]C[/]ext4\.img["]' tools/testing/selftests/mount_setattr/mount_setattr_test.c
    accept '[\t]ASSERT_EQ[(]system[(]["]mkfs\.ext4[ ]-q[ ][/]mnt[/]C[/]ext4\.img["][)]' tools/testing/selftests/mount_setattr/mount_setattr_test.c
    accept '[\t]echo[ ]["][ ]---[ ]make[ ]\(clean\|allmodconfig\|\)["][ ][>]\+[ ]["][$]amcdir[/]Make\.out["]' tools/testing/selftests/rcutorture/bin/torture.sh
    accept '[\t]make[ ]-j[$]MAKE_ALLOTED_CPUS[ ]\(clean[ ]\|allmodconfig[ ]\|\)[>][>][ ]["][$]amcdir[/]Make\.out["]' tools/testing/selftests/rcutorture/bin/torture.sh

    # New in 5.12.9, 5.10.42.
    blobname '\(silead[/]\)\?gsl1680-chuwi-hi10-pro\.fw' drivers/platform/x86/touchscreen_dmi.c

    # New in 5.13-rc.
    # Sources are in cwsr_trap_handler_gfx9.asm.
    defsnc 'static[ ]const[ ]uint32_t[ ]cwsr_trap_aldebaran_hex\[\][ ]=' drivers/gpu/drm/amd/amdkfd/cwsr_trap_handler.h
    defsnc '[\t]static[ ]const[ ]uint16_t[ ]prime_numbers\[\][ ]=' drivers/gpu/drm/amd/display/dc/dcn10/dcn10_hw_sequencer.c
    defsnc 'static[ ]const[ ]struct[ ]IP_BASE[ ]\(\(IO\(AGR\|APIC\)\|L1IMU\(IOAGR\|PCIE\)\)0\|WAFL[01]\|XGMI[012]\)_BASE[ ]='
    defsnc '[\t]const[ ]struct[ ]reg_sequence[ ]seq\[\][ ]=' drivers/gpu/drm/bridge/lontium-lt8912b.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]jpeg_d[qh]t\[\][ ]=' drivers/media/platform/imx-jpeg/mxc-jpeg.c
    accept '[ ][*][ ]@fw_get_done:[\t]flag[ ]set[ ]when[ ]request_firmware[(][)]' drivers/media/platform/s5p-mfc/s5p_mfc_common.h
    defsnc 'static[ ]const[ ]u8[ ]ice_fdir_\(\(udp\|tcp\|icmp\|ipv\)4_gtpu4\|ipv[46]_\(l2tpv3\|\(nat_t_\)\?esp\|ah\|pfcp_\(session\|node\)\)\)_pkt\[\][ ]=' drivers/net/ethernet/intel/ice/ice_fdir.c
    defsnc 'static[ ]const[ ]u32[ ]ice_ptypes_\(mac_ofos\|macvlan_il\|ipv[46]_ofos_all\|\(arp\|icmp\)_of\|ipv[46]_\(ofos\|il\)_no_l4\|icmp_\(of\|il\)\|mac_il\|gtpc\(_tid\)\?\|gtpu\|pppoe\|pfcp_\(node\|session\)\|l2tpv3\|\(nat_t_\)\?esp\|ah\|mac_non_ip_ofos\)\[\][ ]=' drivers/net/ethernet/intel/ice/ice_flow.c
    defsnc '[\t]static[ ]const[ ]u8[ ]chan_list_5ghz\[\][ ]=' drivers/net/wireless/mediatek/mt76/mt76_connac_mcu.c
    defsnc 'static[ ]const[ ]struct[ ]msm_gpio_wakeirq_map[ ]sc7280_pdc_map\[\][ ]=' drivers/pinctrl/gcom/pinctrl-sc7280.c
    defsnc 'static[ ]const[ ]struct[ ]msm_gpio_wakeirq_map[ ]sm8350_pdc_map\[\][ ]=' drivers/pinctrl/gcom/pinctrl-sc8350.c
    defsnc 'static[ ]const[ ]int[ ]bd7181x_wled_currents\[\][ ]=' drivers/regulator/bd71815-regulator.c
    accept '[ ][*][ ]lpfc_request_firmware_upgrade_store[ ]-[ ]Request[ ]for[ ]Linux[ ]generic[ ]firmware[ ]upgrade' drivers/scsi/lpfc/lpfc_attr.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]by_vt3253_init_tab_rfmd\[CB_VT3253_INIT_FOR_RFMD\]\[2\][ ]=' drivers/staging/vt6655/baseband.c
    defsnc '[}][ ]test_div64_results\[SIZE_DIV64_DIVISORS\]\[SIZE_DIV64_DIVIDENDS\][ ]=' lib/math/test_div64.c
    defsnc 'static[ ]const[ ]struct[ ]cs8409_i2c_param[ ]cs42l42_init_reg_seq\[\][ ]=' sound/pci/hda/patch_cirrus.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt1019_reg\[\][ ]=' sound/soc/codecs/rt1019.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt1316_reg_defaults\[\][ ]=' sound/soc/codecs/rt1316-sdw.c
    defsnc 'static[ ]const[ ]struct[ ]reg_sequence[ ]rt1316_blind_write\[\][ ]=' sound/soc/codecs/rt1316-sdw.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt711_sdca_reg_defaults\[\][ ]=' sound/soc/codecs/rt711-sdca-sdw.h
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt715_reg_defaults_sdca\[\][ ]=' sound/soc/codecs/rt715-sdca-sdw.h
    defsnc 'static[ ]const[ ]char[ ][*]mips_gpr_names\[32\][ ]=' tools/perf/arch/mips/util/dwarf-regs.c
    accept '[\t]unlink[(]["][/]var[/]run[/]isst_cpu_topology\.dat["][)]' tools/power/x86/intel-speed-select/isst-config.c
    defsnc 'const[ ]struct[ ]vm_guest_mode_params[ ]vm_guest_mode_params\[\][ ]=' tools/testing/selftests/kvm/lib/kvm_util.c
    accept '[\t]rpipwm->firmware[ ]=[ ]firmware[;]' drivers/pwm/pwm-raspberrypi-poe.c
    blobname 'qcom[/]sdm845[/][ac]dsp\.mbn' arch/arm64/boot/dts/qcom/sdm845-db845c.dts
    blobname 'qcom[/]sm8350[/]\([ac]dsp\|modem\|slpi\|\)\.mbn' arch/arm64/boot/dts/qcom/sm8350-'\(hdk\|mtp\)\.dts'
    blobname 'qcom[/]sdx65m[/]xbl\.elf' drivers/bus/mhi/pci_generic.c
    blobname 'qcom[/]sdx65m[/]edl\.mbn' drivers/bus/mhi/pci_generic.c
    blobname 'qcom[/]prog_firehose_sdx24\.mbn' drivers/bus/mhi/pci_generic.c
    blobname 'amdgpu[/]aldebaran_vcn\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vcn.c
    blobname 'amdgpu[/]aldebaran_\(sos\|ta\)\.bin' drivers/gpu/drm/amd/amdgpu/psp_v13_0.c
    blobname 'amdgpu[/]\(aldebaran\|%s\)_smc\.bin' drivers/gpu/drm/amd/pm/swsmu/smu13/smu_v13_0.c
    blobname 'i915[/]adls_dmc_ver2_01\.bin' drivers/gpu/drm/i915/display/intel_csr.c
    blobname 'qcom[/]vpu-1\.0[/]venus\.mdt' drivers/media/platform/qcom/venus/core.c
    blobname 'rtl_nic[/]rtl815\(3c-1\|6[ab]-2\)\.fw' drivers/net/usb/r8152.c
    blobname '\(silead[/]\)\?gsl3692-teclast-tbook11\.fw' drivers/platform/x86/touchscreen_dmi.c

    # New in 5.13.2, 5.12.17, 5.10.50.
    blobname 'amd[/]amd_sev_fam1[79]h_model[03]xh\.sbin' drivers/crypto/ccp/sev-dev.c
    blobname 'gt912-glavey-tm800a550l.fw' drivers/platform/x86/touchscreen_dmi.c

    # New in 5.13.4, 5.12.19.
    defsnc 'static[ ]unsigned[ ]char[ ]screen_bits\[\][ ]=' arch/m68k/68000/screen.h
    # New in 5.13.4, 5.12.19, 5.10.52.
    defsc '[\t]setrate_44100\[\][ ]=' sound/usb/usx2y/usbusx2yaudio.c
    defsc 'static[ ]const[ ]struct[ ]s_c2[ ]setrate_48000\[\][ ]=' sound/usb/usx2y/usbusx2yaudio.c

    # New in 5.13.5 and 5.10.53.
    blobna 'and[ ]booted[ ]am335x-pm-firmware\.elf\.[\n][ ][*][/]' Documentation/devicetree/bindings/remoteproc/wkup_m3_rproc.txt

    # New in 5.14-rc.
    accept '[	 ]*nvidia,emc-registers[ ]=[ 	]*<\(0x[0-9a-f]*[ 	\n]*\)*>[;]' Documentation/devicetree/bindings/memory-controllers/nvidia,tegra20-emc.yaml
    blobname 'msnv11\.bin' Documentation/devicetree/bindings/net/qualcomm-bluetooth.yaml
    blobname 'qcom[/]sm8150[/]microsoft[/]\([ac]dsp\|modem\|slpi\)\.mdt' arch/arm64/boot/dts/qcom/sm8150-microsoft-surface-duo.dts
    blobname 'qca[/]msbtfw%02x\.\(tlv\|mbn\)' drivers/bluetooth/btqca.c
    blobname 'qca[/]msnv%02x\.bin' drivers/bluetooth/btqca.c
    blobname 'rtl_bt[/]rtl8761bu_fw\.bin' drivers/bluetooth/btrtl.c
    blobname 'amdgpu[/]\(beige_goby\|yellow_carp\)_vcn\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vcn.c
    defsnc 'static[ ]const[ ]u32[ ]\(vgpr\|sgpr\(112\|96\|64\)\)_init_compute_shader_aldebaran\[\][ ]=' drivers/gpu/drm/amd/amdgpu/gfx_v9_4_2.c
    blobname 'amdgpu[/]\(beige_goby\|yellow_carp\)_dmcub\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_dm.c
    defsnc 'static[ ]const[ ]struct[ ]IP_BASE[ ]PCIE_BASE[ ]=' drivers/gpu/drm/amd/include/yellow_carp_offset.h
    blobname 'i915[/]["][ \t\\\n]*__stringify[(]platform[)][ ]["]_dmc_ver["][ \t\\\n]*__stringify[(]major[)][ ]["]_["][ \t\\\n]*__stringify[(]minor[)][ ]["]\.bin' drivers/gpu/drm/i915/display/intel_dmc.c
    defsnc 'static[ ]const[ ]u8[ ]rc_range_\(min\|max\)qp444_8bpc\[DSC_NUM_BUF_RANGES\]\[RC_RANGE_QP444_8BPC_MAX_NUM_BPP\][ ]=' drivers/gpu/drm/i915/display/intel_qp_tables.c
    defsnc 'static[ ]const[ ]u8[ ]rc_range_\(min\|max\)qp444_10bpc\[DSC_NUM_BUF_RANGES\]\[RC_RANGE_QP444_10BPC_MAX_NUM_BPP\][ ]=' drivers/gpu/drm/i915/display/intel_qp_tables.c
    defsnc 'static[ ]const[ ]u8[ ]rc_range_\(min\|max\)qp444_12bpc\[DSC_NUM_BUF_RANGES\]\[RC_RANGE_QP444_12BPC_MAX_NUM_BPP\][ ]=' drivers/gpu/drm/i915/display/intel_qp_tables.c
    blobname 'a660_sqe\.fw' drivers/gpu/drm/msm/adreno/adreno_device.c
    blobname 'a660_gmu\.bin' drivers/gpu/drm/msm/adreno/adreno_device.c
    blobname 'a660_zap\.mdt' drivers/gpu/drm/msm/adreno/adreno_device.c
    defsnc '[\t]static[ ]const[ ]unsigned[ ]int[ ]coeffs\[192\][ ]=' drivers/gpu/drm/tegra/hub.c
    defsnc 'static[ ]const[ ]struct[ ]imx208_reg[ ]mode_\(1936x1096\|968_548\)_60fps_regs\[\][ ]=' drivers/media/i2c/imx208.c
    defsnc 'static[ ]const[ ]struct[ ]ov8856_reg[ ]lane_[24]_mode_\(3280x2464\|1640x1232\)\[\][ ]=' drivers/media/i2c/ov8856.c
    defsnc 'static[ ]const[ ]struct[ ]ov8856_reg[ ]lane_4_mode_\(3264x2448\|1632x1224\)\[\][ ]=' drivers/media/i2c/ov8856.c
    defsc 'static[ ]const[ ]u32[ ]isc_sama\(5d2\|7g5\)_gamma_table\[\]\[GAMMA_ENTRIES\][ ]=' drivers/media/platform/atmel/atmel-sama5d2-isc.c
    defsnc 'static[ ]const[ ]u8[ ]mpeg2_intra_quant_matrix\[64\][ ]=' drivers/media/v4l2-core/v4l2-ctrls-core.c
    defsnc 'static[ ]u32[ ]sparx5_taxi_ports\[SPX5_DSM_CAL_TAXIS\]\[SPX5_DSM_CAL_MAX_DEVS_PER_TAXI\][ ]=' drivers/net/ethernet/microchip/sparx5/sparx5_calendar.c
    defsnc '[\t]const[ ]u32[ ]taxi_dist\[SPX5_PORTS_ALL\][ ]=' drivers/net/ethernet/microchip/sparx5/sparx5_port.c
    defsnc 'static[ ]const[ ]struct[ ]hsfreq_range[ ]rk1808_mipidphy_hsfreq_ranges\[\][ ]=' drivers/phy/rockchip/phy-rockchip-inno-csidphy.c
    defsnc 'static[ ]const[ ]struct[ ]tsadc_table[ ]rk3568_code_table\[\][ ]=' drivers/thermal/rockchip_thermal.c
    defsnc 'static[ ]const[ ]u16[ ]scarlett2_mixer_values\[SCARLETT2_MIXER_VALUE_COUNT\][ ]=' sound/usb/mixer_scarlett_gen2.c
    defsnc 'static[ ]const[ ]struct[ ]s_c2[ ]setrate_44100\[\][ ]=' sound/usb/usx2y/usbusx2yaudio.c
    accept '[\t]rc[ ]=[ ]request_firmware_nowait[(]THIS_MODULE[,][ ]FW_ACTION_NOUEVENT[,][ ]name[,][\n\t ]*dev[,][ ]GFP_KERNEL[,][ ]NULL[,][\n\t ]*trigger_async_request_cb[)][;]' lib/test_firmware.c
    # kpu_profile is derived from a user-supplied parameter
    accept '[\t]if[ ][(]!request_firmware[(][&]fw[,][ ]kpu_profile[,][ ]rvu->dev[)][)]' drivers/net/ethernet/marvell/octeontx2/af/rvu_npc.c
    accept '\(static[ ]int[ ]\|[\t]*\)\?efct_request_firmware_update[(]\(struct[ ]efct[ ][*]\)\?efct[)][;]\?' drivers/scsi/elx/efct/efct_driver.c
    blobname '%s\.grp' 'drivers/scsi/\(lpfc/lpfc_init\.c\|elx/efct/efct_driver\.c\)'

    # Blobs that we mistakenly retained up to 5.14-rc7-gnu.
    # Thanks to Legimet for bringing them to our attention!
    blob '\(static[ ]\)\?uint[ ]patch_2[0ef]00\[\][ ]\(__initdata[ ]\)\?=[ ][{][0-9xa-fA-F, \t\n]*[}][;]' 'arch/powerpc/\(sysdev\|platforms/8xx\)/micropatch\.c'
    blobna 'cpm_write_patch[(]cp[,][ ]0[xef0]*[,][ ]patch_2[0ef]00[,][ ]sizeof[(]patch_2[0ef]00[)][)][;]' 'arch/powerpc/\(sysdev\|platforms/8xx\)/micropatch\.c'
    blob 'static[ ]const[ ]u16[ ]vs6624_p1\[\][ ]=[ ][{][0-9xa-fA-F, \t\n]*[}][;]' 'drivers/media/\(video\|i2c\)/vs6624\.c'
    blobna 'vs6624_writeregs[(]sd[,][ ]vs6624_p1[)][;]' 'drivers/media/\(video\|i2c\)/vs6624\.c'

    # Here's some inducement of non-Free stuff that we clean up better now.
    blobname 'GenuineIntel\.bin' 'Documentation/x86/microcode\.\(rst\|txt\)'
    blobna 'cat[ ][/]lib[/]firmware[/]\(amd\|intel\)-ucode[/][^ ]*[ ][>][^\n]*' 'Documentation/x86/microcode\.\(rst\|txt\)'
    blobna 'cp[ ]\.\.[/]microcode\.bin[ ][^\n]*' Documentation/x86/early_microcodetxt
    blobname '[/]lib[/]firmware[/][{]intel-ucode[,]amd-ucode[}]' 'Documentation/x86/microcode\.\(rst\|txt\)'
    blobname 'microcode_amd_fam15h\.bin' 'Documentation/x86/microcode\.\(rst\|txt\)'

    # Present in 4.19, matches a later-added firmware extension pattern.
    accept '[\t]if[ ][(]!strcmp[(]last4[,][ ]["]\.tlv["][)][)]' drivers/fmc/fmc-write-eeprom.c
    # Present in 4.14, matches a later-added firmware loader interface.
    accept '[\t][\t]ret[ ]=[ ]load_msr_list[(]client[,]' drivers/staging/media/atomisp/i2c/imx/imx.c
    # Present in 4.9 and 4.4, matches a later-added firmware loader interface.
    accept '[\t]*\(return[ ]\)\?coda_firmware_request[(]' drivers/media/platform/code/coda-common.c
    # Present in 4.9 and 4.4, harmless occurrence of update.*microcode.
    accept '[ ][*][ ]Returns[:][ ]The[ ]updated[ ]number[ ]@num_saved[ ]of[ ]saved[ ]microcode[ ]patches\.' arch/x86/kernel/cpu/microcode/intel.c
    # Present in 4.9, links to Free Software.
    accept 'ARM[ ]assembly[ ]source[ ]code[ ]available[ ]at[ ]https[:][/][/]linuxtv\.org[/]downloads[/]firmware[/]Boot\.S' firmware/WHENCE

    # New in 5.14.11, 5.10.72.
    blobname '\(silead[/]\)\?gsl1680-chuwi-hi\(10plus\|book\)\.fw' drivers/platform/x86/touchscreen_dmi.c

    # New in 5.15-rc.
    blobname 'achc\.bin' 'Documentation/ABI/testing/sysfs-driver-ge-achc\|drivers/misc/gehc-achc\.c'
    blobname 'qcom[/]sdm845[/]oneplus6[/]ipa_fws\.mbn' arch/arm64/boot/dts/qcom/sdm845-oneplus-common.dtsi
    defsnc 'static[ ]__amode31_data[ ]u32[ ]__ctl_duald_amode31\[32\][ ]__aligned[(]128[)][ ]=' arch/s390/kernel/setup.c
    defsnc '[\t]umc_v6_7_channel_idx_tbl_\(second\|first\)\[UMC_V6_7_UMC_INSTANCE_NUM\]\[UMC_V6_7_CHANNEL_INSTANCE_NUM\][ ]=' drivers/gpu/drm/amd/amdgpu/umc_v6_7.c
    defsnc 'static[ ]const[ ]struct[ ]reg_sequence[ ]ej030na_init_sequence\[\][ ]=' drivers/gpu/drm/panel/panel-innolux-ej030na.c
    defsnc '[\t]static[ ]const[ ]int[ ]voltages\[\][ ]=' drivers/hid/hid-logitech-hidpp.c
    defsnc 'static[ ]const[ ]struct[ ]imx335_reg[ ]mode_2592x1940_regs\[\][ ]=' drivers/media/i2c/imx335.c
    defsnc 'static[ ]const[ ]struct[ ]imx412_reg[ ]mode_4056x3040_regs\[\][ ]=' drivers/media/i2c/imx412.c
    defsnc 'static[ ]const[ ]struct[ ]ov9282_reg[ ]mode_1280x720_regs\[\][ ]=' drivers/media/i2c/ov9282.c
    defsnc 'static[ ]const[ ]u8[ ]channel_all\[59\][ ]=' drivers/net/wireless/realtek/rtlwifi/rtl8192de/phy.c
    defsnc 'static[ ]const[ ]struct[ ]ab8500_v_to_cap[ ]cap_tbl\(_[ab]_thermistor\)\?\[\][ ]=' drivers/power/supply/ab8500_bmdata.c
    blobname 'rtlwifi\([/]\|[\\][\\]\)rtl8188eufw\.bin' drivers/staging/r8188eu/hal/rtl8188e_hal_init.c
    defsnc 'static[ ]char[ ]NEGOTIATE_GSS_HEADER\[AUTH_GSS_LENGTH\][ ]=' fs/ksmbd/auth.c
    defsnc 'const[ ]u8[ ]s_default_security\[\][ ]__aligned[(]8[)][ ]=' fs/ntfs3/fsntfs.c
    accept '[ ]*[*][ ][ ][ ]1[ ]0[ ]9[ ]8[ ]7[ ]6[ ]5[ ]4[ ]3[ ]2[ ]1[ ]0[ ]9[ ]8[ ]7[ ]6[ ]5[ ]4[ ]3[ ]2[ ]1[ ]0[ ]9[ ]8[ ]7[ ]6[ ]5[ ]4[ ]3[ ]2[ ]1[ ]0' fs/ntfs3/ntfs.h
    defsnc 'static[ ]const[ ]u32[ ]__cacheline_aligned[ ]ck\[32\][ ]=' lib/crypto/sm4.c
    defsnc 'static[ ]const[ ]u8[ ]__cacheline_aligned[ ]sbox\[256\][ ]=' lib/crypto/sm4.c
    defsnc 'static[ ]const[ ]char[ ]large_mask\[\][ ]__initconst[ ]=' lib/test_bitmap.c
    defsnc 'static[ ]const[ ]struct[ ]cs8409_i2c_param[ ]dolphin_c[01]_init_reg_seq\[\][ ]=' sound/pci/hda/patch_cs8409-tables.c
    defsnc 'const[ ]__u8[ ]nci_rf_activate_ntf\[\][ ]=' tools/testing/selftests/nci/nci_dev.c
    blobname 'brcmfmac43\(430b0\|752\)-sdio' drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
    # Catch other names likely to appear in BRCMF_FW*_DEF strings in these files.
    blobna 'brcmfmac43[^";) \t\n]*\(-sdio\|-pcie\)\?' drivers/net/wireless/broadcom/brcm80211/brcmfmac/'\(sdio\|pcie\|usb\)\.c'

    # New in 5.15.3-gnu and 5.14.19-gnu.
    blobna '[/][*][ ]linux-firmware\.git[ ]hash[ ][0-9a-f]*[ ][*][/]' drivers/gpu/drm/amd/display/amdgpu_dm/amdgpu_dm.c

    # New in 5.15.3-gnu.
    defsnc 'static[ ]const[ ]u32[ ]____cacheline_aligned[ ]ck\[32\][ ]=' lib/crypto/sm4.c
    defsnc 'static[ ]const[ ]u8[ ]____cacheline_aligned[ ]sbox\[256\][ ]=' lib/crypto/sm4.c

    # New in 5.16-rc.
    blobname 'imx[/]dsp[/]hifi4\.bin' Documentation/devicetree/bindings/dsp/fsl,dsp.yaml
    accept '[ ]*\[[ ]\(0x[1248]0*[ \n,]*\)*\]' Documentation/devicetree/bindings/leds/register-bit-led.yaml
    accept '[ ]*\[0[,][ ]\(\(1[6789]\|2[012]\)[02468]0[, \n]*\)*\]' Documentation/devicetree/bindings/net/dsa/nxp,sja1105.yaml
    blobname 'qcom[/]apq8016[/]\(\(mba\|modem\|wcnss\)\.mbn\|WCNSS_qcom_wlan_nv_sbc\.bin\)' arch/arm64/boot/dts/qcom/apq8016-sbc.dts
    blobname 'qcom[/]msm8996[/]gemini[/]\(adsp\|a530_zap\|venus\)\.mbn' arch/arm64/boot/dts/qcom/msm8996-xiaomi-gemini.dts
    blobname 'qcom[/]msm8996[/]scorpio[/]\(adsp\|a530_zap\|venus\)\.mbn' arch/arm64/boot/dts/qcom/msm8996-xiaomi-scorpio.dts
    blobname 'qcom[/]sa8155p[/][ac]dsp\.mdt' arch/arm64/boot/dts/qcom/sa8155p-adp.dts
    accept '[ ][*][ ]firmware_request_builtin\(_buf\)\?[(][)][ ]-[ ]load[ ]builtin[ ]firmware' drivers/base/firmware_loader/builtin/main.c
    accept 'bool[ ]firmware_request_builtin[(]' drivers/base/firmware_loader/builtin/main.c
    accept 'EXPORT_SYMBOL_NS_GPL[(]firmware_request_builtin[,]' drivers/base/firmware_loader/builtin/main.c
    accept '[ ][*][\t]callers[ ]such[ ]as[ ]request_firmware_into_buf[(]' drivers/base/firmware_loader/builtin/main.c
    accept '[ ][*][\t]request_partial_firmware_into_buf[(]' drivers/base/firmware_loader/builtin/main.c
    accept 'bool[ ]firmware_request_builtin_buf[(][^)]*[)][\n][{][\n][\t]if[ ][(]!firmware_request_builtin[(]' drivers/base/firmware_loader/builtin/main.c
    accept '\(static[ ]inline[ ]\)\?bool[ ]firmware_request_builtin_buf[(]' drivers/base/firmware_loader/firmware.h
    accept '[\t]if[ ][(]firmware_request_builtin_buf[(][^)]*[)][)][ ][{][\n][\t][\t]dev_dbg[(]device[,][ ]["]using[ ]built-in[ ]' drivers/base/firmware_loader/main.c
    accept '[\t]if[ ][(]firmware_request_builtin[(][^)]*[)][)][\n][\t][\t]return[ ]0[;][\n][\n][\t]fw_priv[ ]=[ ]lookup_fw_priv[(]' drivers/base/firmware_loader/main.c
    accept '[\t]retval[ ]=[ ]firmware_request_builtin[(][&]xfw[,][ ]NONFREE_FIRMWARE[)]' include/linux/firmware.h
    blobname 'amdgpu[/]ip_discovery\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_discovery.c
    defsc 'static[ ]const[ ]u16[ ]amdgpu_unsupported_pciidlist\[\][ ]=' drivers/gpu/drm/amd/amdgpu/amdgpu_drv.c
    defsnc '[\t]mipi_dbi_command[(]dbi[,][ ]S6D27A1_PANELCTL[,]' drivers/gpu/drm/panel/panel-samsung-s6d27a1.c
    defsc 'static[ ]const[ ]struct[ ]joycon_rumble_freq_data[ ]joycon_rumble_frequencies\[\][ ]=' drivers/hid/hid-nintendo.c
    defsc 'static[ ]const[ ]struct[ ]joycon_rumble_amp_data[ ]joycon_rumble_amplitudes\[\][ ]=' drivers/hid/hid-nintendo.c
    blobname 'goodix[/]%s' drivers/input/touchscreen/goodix_fwupload.c
    blobname 'ilitek[/]ili251x.bin' drivers/input/touchscreen/ili210x.c
    # These register initializers cover large contiguous regions.
    # ~180b and ~512b respectively.  It's not inconceivable that they
    # contain some code, but it doesn't quite feel like code to me, so
    # I'm tentatively leaving it in.
    defsc 'static[ ]const[ ]struct[ ]hi846_reg[ ]hi846_init_[24]lane\[\][ ]' drivers/media/i2c/hi846.c
    defsnc 'static[ ]const[ ]struct[ ]ov13b10_reg[ ]mipi_data_rate_1120mbps\[\][ ]=' drivers/media/i2c/ov13b10.c
    defsnc 'static[ ]const[ ]struct[ ]ov13b10_reg[ ]mode_\(4208x3120\|4160x\(3120\|2340\)\|2104x1560\|2080x1170\)_regs\[\][ ]=' drivers/media/i2c/ov13b10.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]jpeg_image_red\[\][ ]=' drivers/media/platform/imx-jpeg/mxc-jpeg.c
    blobname 'qcom[/]venus-4\.4[/]venus\.mdt' drivers/media/platform/qcom/venus/core.c
    blobname 'qcom[/]vpu-2\.0[/]venus\.mbn' drivers/media/platform/qcom/venus/core.c
    defsnc 'static[ ]const[ ]struct[ ]rtl8365mb_jam_tbl_entry[ ]rtl8365mb_init_jam_8365mb_vc\[\][ ]=' drivers/net/dsa/rtl8365mb.c
    defsc 'static[ ]const[ ]u8[ ]dummy_\(vlan_\)\?\(tcp\|udp\)_ipv6_packet\[\][ ]=' drivers/net/ethernet/intel/ice/ice_switch.c
    blobname 'cal-%s-%s\.bin' drivers/net/wireless/ath/ath11k/qmi.c
    blobna '[/][*][ ]cal-<bus>-<id>\.bin[ ][*][/]' drivers/net/wireless/ath/ath11k/qmi.c
    accept '[\t]*return[ ]1[;][ ][/][*][ ]not[ ]present[,][ ]try[ ]firmware_request[ ]' drivers/net/wireless/ath/ath9k/ath9k_pci_owl_loader.c
    defsnc '[\t]static[ ]const[ ]u8[ ]chan_list_6ghz\[\][ ]=' drivers/net/wireless/mediatek/mt76/mt76_connac_mcu.c
    blobname 'mediatek[/]WIFI_\(RAM_CODE_MT7922_1\|MT7922_patch_mcu_1_1_hdr\)\.bin' drivers/net/wireless/mediatek/mt76/mt7921/mt7921.h
    defsnc 'static[ ]const[ ]struct[ ]rtw89_reg2_def[ ][ ]*rtw8852a_pmac_ht20_mcs7_tbl\[\][ ]=' drivers/net/wireless/realtek/rtw89/rtw8852a.c
    blobname 'rtw89[/]rtw8852a_fw\.bin' drivers/net/wireless/realtek/rtw89/rtw8852a.c
    defsnc 'static[ ]const[ ]struct[ ]rtw89_reg2_def[ ]rtw89_8852a_phy_\(bb\|radio[ab]\|nctl\)_regs\[\][ ]=' drivers/net/wireless/realtek/rtw89/rtw8852a_table.c
    defsnc 'static[ ]const[ ]struct[ ]rtw89_txpwr_byrate_cfg[ ]rtw89_8852a_txpwr_byrate\[\][ ]=' drivers/net/wireless/realtek/rtw89/rtw8852a_table.c
    defsnc 'static[ ]const[ ]u8[ ]_txpwr_track_delta_swingidx_5g[ba]_[np]\[\]\[DELTA_SWINGIDX_SIZE\][ ]=' drivers/net/wireless/realtek/rtw89/rtw8852a_table.c
    # This names various coredump section names that resemble file
    # names, such as eeprom.bin, bootcore_trace.bin, AFAICT extracted
    # from the modem.
    defsnc 'static[ ]struct[ ]iosm_coredump_file_info[ ]list\[IOSM_NOF_CD_REGION\][ ]=' drivers/net/wwan/iosm/iosm_ipc_devlink.c
    defsnc 'static[ ]const[ ]struct[ ]msm_gpio_wakeirq_map[ ]sm6350_pdc_map\[\]' drivers/pinctrl/qcom/pinctrl-sm6350.c
    defsnc 'static[ ]const[ ]char[ ]*[*][ ]const[ ]omen_thermal_profile_boards\[\][ ]=' drivers/platform/x86/hp-wmi.c
    defsnc 'static[ ]const[ ]int[ ]mlxplat_modular_channels\[\][ ]=' drivers/platform/x86/mlx-platform.c
    blobname 'gsl3680-viglen-connect-10\.fw' drivers/platform/x86/touchscreen_dmi.c
    accept '\(static[ ]inline[ ]\)\?bool[ ]firmware_request_builtin[(]' include/linux/firmware.h
    accept '#define[ ]_MAP_0_32_ASCII_SEG14_NON_PRINTABLE[\t]*[\\][\n][\t]\(0[,]\)*' include/uapi/linux/map_to_14segment.h
    defsnc '[\t]struct[ ]some_bytes[ ]\(control\|middle\|three\|five\|overlap\(_expected\)\?\|complete\|after\|startat\)[ ]=' lib/memcpy_kunit.c
    defsnc '[ \t]*static[ ]const[ ]\(unsigned\|U32\)[ ]DeBruijnClz\[32\][ ]=' lib/zstd/common/'\(bitstream\)zstd_internal\)\.h'
    defsnc 'static[ ]const[ ]unsigned[ ]BIT_mask\[\][ ]=' lib/zstd/common/bitstream.h
    defsnc 'static[ ]UNUSED_ATTR[ ]const[ ]U32[ ]LL_bits\[MaxLL[+]1\][ ]=' lib/zstd/common/zstd_internal.h
    defsnc 'static[ ]UNUSED_ATTR[ ]const[ ]S16[ ]LL_defaultNorm\[MaxLL[+]1\][ ]=' lib/zstd/common/zstd_internal.h
    defsnc 'static[ ]UNUSED_ATTR[ ]const[ ]U32[ ]ML_bits\[MaxML[+]1\][ ]=' lib/zstd/common/zstd_internal.h
    defsnc 'static[ ]UNUSED_ATTR[ ]const[ ]S16[ ]ML_defaultNorm\[MaxML[+]1\][ ]=' lib/zstd/common/zstd_internal.h
    defsnc '[ \t]*static[ ]const[ ]BYTE[ ]LL_Code\[64\][ ]=' lib/zstd/compress/zstd_compress_internal.h
    defsnc '[ \t]*static[ ]const[ ]BYTE[ ]ML_Code\[128\][ ]=' lib/zstd/compress/zstd_compress_internal.h
    defsnc '[ \t]*static[ ]const[ ]int[ ]DeBruijnBytePos\[\(64\|32\)\][ ]=' lib/zstd/common/zstd_compress_internal.h
    defsnc '[ \t]*static[ ]unsigned[ ]const[ ]kInverseProbabilityLog256\[256\][ ]=' lib/zstd/common/zstd_compress_sequences.c
    defsnc 'static[ ]U64[ ]ZSTD_ldm_gearTab\[256\][ ]=' lib/zstd/compress/zstd_ldm_geartab.h
    defsc 'static[ ]const[ ]ZSTD_seqSymbol[ ]\(LL\|OF\|ML\)_defaultDTable\[[^]]*\][ ]=' lib/zstd/decompress/zstd_decompress_block.c
    defsnc 'static[ ]UNUSED_ATTR[ ]const[ ]U32[ ]LL_base\[MaxLL[+]1\][ ]=' lib/zstd/common/zstd_decompress_internal.h
    defsnc 'static[ ]UNUSED_ATTR[ ]const[ ]U32[ ]OF_\(base\|bits\)\[MaxOff[+]1\][ ]=' lib/zstd/common/zstd_decompress_internal.h
    defsnc 'static[ ]UNUSED_ATTR[ ]const[ ]U32[ ]ML_base\[MaxML[+]1\][ ]=' lib/zstd/common/zstd_decompress_internal.h
    defsnc 'static[ ]const[ ]struct[ ]cs35l41_pll_sysclk_config[ ]cs35l41_pll_sysclk\[\][ ]=' sound/soc/codecs/cs35l41.c
    defsnc 'static[ ]const[ ]struct[ ]cs35l41_fs_mon_config[ ]cs35l41_fs_mon\[\][ ]=' sound/soc/codecs/cs35l41.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]rt5682s_reg\[\][ ]=' sound/soc/codecs/rt5682s.c
    accept 'static[ ]int[ ]wm_adsp_request_firmware_files\?[(]' sound/soc/codecs/wm_adsp.c
    accept '[\t]*\(ret[ ]=[ ]\)\?wm_adsp_request_firmware_files\?[(]' sound/soc/codecs/wm_adsp.c
    blobname 'qcom[/]%s[/]%s-tplg\.bin' sound/soc/qcom/qdsp6/topology.c
    blobname '%s-%s-%s\.%s' sound/soc/codecs/wm_adsp.c

    # New in 5.16.3, 5.15.17, 5.10.94, 5.4.174, 4.19.226, 4.14.263.
    accept 'static[ ]struct[ ]dvb_usb_device_properties[ ]\(p1100\|s660\|p7500\)_properties[ ]=[ ][{][\n]\([	]\.\(caps\|usb_ctrl\|size_of_priv\)[ ]*=[ ][^",]*,[\n]*\)*[	]\.firmware[ ]*=[ ]' drivers/media/usb/dvb-usb/dw2102.c

    # New in 5.16.4, 5.15.18, 5.10.95.
    blob '#define[ ]BCM_5710_FW_\(\(MAJOR\|MINOR\|REVISION\|ENGINEERING\)_VERSION\|COMPILE_FLAGS\)\(_V15\)\?[ 	]*[0-9]\+\([\n]#define[ ]BCM_5710_FW_\(\(MAJOR\|MINOR\|REVISION\|ENGINEERING\)_VERSION\|COMPILE_FLAGS\)\(_V15\)\?[ 	]*[0-9]\+\)*' 'drivers/net/\(bnx2x[/]\)\?bnx2x_hsi\.h'
    blob '#define[ ]FW_FILE_VERSION\(_V15\)\?\([	 ]*[\\][\n][	]__stringify[(]BCM_5710_FW_\(MAJOR\|MINOR\|REVISION\|ENGINEERING\)_VERSION\(_V15\)\?[)]\([ ]["][.]["]\)\?\)\+' 'drivers/net/\(bnx2x/\)\?bnx2x_main\.c'
    blobname '\(bnx2x[/]\)\?bnx2x-e[12]h\?-["][ ]FW_FILE_VERSION\(_V15\)\?[ ]["]\.fw' 'drivers/net/\(bnx2x/\)\?bnx2x_main\.c'
    blobname '\(bnx2x[/]\)\?bnx2x-e[12]h\?-\([0-9.%d]*\.fw\)\?' 'drivers/net/\(bnx2x/\)\?bnx2x_main\.c'
    blobna '\([,][\n \t]*BCM_5710_FW_\(MAJOR\|MINOR\|REVISION\|ENGINEERING\)_VERSION\)\+' drivers/net/wireless/broadcom/bnx2x/bnx2x_main.c
    accept '[\t][\t][\t]goto[ ]request_firmware_exit[;]' drivers/net/ethernet/broadcom/bnx2x/bnx2x_main.c
    blobna 'bp->fw_\(major\|minor\|eng\|rev\)[ ]=[ ]BCM_5710_FW_\(MAJOR\|MINOR\|ENGINEERING\|REVISION\)_VERSION\(_V15\)\?[;]\([\n][\t]*bp->fw_\(major\|minor\|eng\|rev\)[ ]=[ ]BCM_5710_FW_\(MAJOR\|MINOR\|ENGINEERING\|REVISION\)_VERSION\(_V15\)\?[;]\)*' drivers/net/ethernet/broadcom/bnx2x/bnx2x_main.c
    blobna '\([,][\n \t]*bp->fw_\(major\|minor\|rev\)\)\+' drivers/net/wireless/broadcom/bnx2x/bnx2x_main.c

    # New in 5.16.11, 5.15.25, 5.10.102.
    blobname 'gsl1680-rwc-nanote-p8\.fw' drivers/platform/x86/touchscreen_dmi.c

    # New in 5.17-rc.
    accept '[ ]*Index\([ ]*\(CPU\|IRQ\|Thr\)-[0-9]*\)*\([\n]\([ ]*[0-9]*\)*\)*' Documentation/tools/rtla/rtla-osnoise-hist.rst
    accept '[\t]*nvidia[,]emc-configuration[ ]=[ ]*<[ \t\n0-9xa-f]*>[;]' 'arch/arm/boot/dts/tegra30-\(asus-tf\(201\|300tg\?\|700t\)\|pegatron-chagall\)\.dts'
    blobname 'qcom[/]sdm845[/]oneplus6[/]venus\.mbn' 'arch/arm64/boot/dts/qcom/sdm845-oneplus-\(common.dtsi\|beryllium\.dts\)'
    blobname 'mediatek[/]BT_RAM_CODE_MT7961_1_2_hdr\.bin' drivers/bluetooth/btmtk.h
    blobname 'qca[/]nvm_usb_%08x\(%s\(_%04x\)\?\)\?\.bin' drivers/bluetooth/btusb.c
    defsc 'static[ ]const[ ]struct[ ]rcar_gen4_cpg_pll_config[ ]cpg_pll_configs\[4\][ ]=' drivers/clk/renesas/r8a779a0-cpg-mssr.c
    blobname 'qat_4xxx_dc\.bin' drivers/crypto/qat/qat_4xxx/adf_4xxx_hw_data.h
    blobname 'a506_zap\.mdt' drivers/gpu/drm/msm/adreno/adreno_device.c
    defsnc 'static[ ]const[ ]u32[ ]hsfreqrange_table\[\]\[2\][ ]=' drivers/gpu/drm/rcar-du/rcar_mipi_dsi.c
    blobname 'nvidia[/]tegra\(210\|186\|194\)[/]nvdec\.bin' drivers/gpu/drm/tegra/nvdec.c
    accept 'static[ ]const[ ]struct[ ]nvdec_config[ ]nvdec_t\(210\|186\|194\)_config[ ]=[ ][{][\n][	]\.firmware[ ]*=[ ]' drivers/gpu/drm/tegra/nvdec.c
    defsnc 'static[ ]const[ ]unsigned[ ]int[ ]ad74413r_debounce_map\[AD74413R_DIN_DEBOUNCE_LEN\][ ]=' drivers/iio/addac/ad74413r.c
    blobname 'dvb_driver_si2141_rom6[01]\.fw' drivers/media/tuners/si2157_priv.h
    blobname 'dvb_driver_si2146_rom11\.fw' drivers/media/tuners/si2157_priv.h
    blobname 'dvb_driver_si2147_rom50\.fw' drivers/media/tuners/si2157_priv.h
    blobname 'dvb_driver_si2148_rom3[23]\.fw' drivers/media/tuners/si2157_priv.h
    blobname 'dvb_driver_si2157_rom50\.fw' drivers/media/tuners/si2157_priv.h
    blobname 'dvb_driver_si2178_rom50\.fw' drivers/media/tuners/si2157_priv.h
    blobname 'dvb_driver_si2158_rom51\.fw' drivers/media/tuners/si2157_priv.h
    blobname 'dvb_driver_si2177_rom50\.fw' drivers/media/tuners/si2157_priv.h
    defsc 'const[ ]struct[ ]v4l2_vp9_frame_context[ ]v4l2_vp9_default_probs[ ]=' drivers/media/v4l2-core/v4l2-vp9.c
    defsnc 'static[ ]const[ ]u8[ ]hclge_comm_hash_key\[\][ ]=' drivers/net/ethernet/hisilicon/hns3/hns3_common/hclge_comm_rss.c
    defsnc 'static[ ]const[ ]u16[ ]mlxsw_sp2_acl_bf_crc16_tab\[256\][ ]=' drivers/net/ethernet/mellanox/mlxsw/spectrum_acl_bloom_filter.c
    defsnc 'static[ ]const[ ]u16[ ]mlxsw_sp4_acl_bf_crc10_tab\[256\][ ]=' drivers/net/ethernet/mellanox/mlxsw/spectrum_acl_bloom_filter.c
    defsnc 'static[ ]const[ ]u8[ ]mlxsw_sp4_acl_bf_crc6_tab\[256\][ ]=' drivers/net/ethernet/mellanox/mlxsw/spectrum_acl_bloom_filter.c
    blobname 'regdb\.bin' drivers/net/wireless/ath/ath11k/hw.h
    blobname 'mediatek[/]mt7915_eeprom\(_dbdc\)\?\.bin' drivers/net/wireless/mediatek/mt76/mt7915/mt7915.h
    defsnc 'static[ ]const[ ]struct[ ]msm_gpio_wakeirq_map[ ]sdx65_pdc_map\[\][ ]=' drivers/pinctrl/qcom/pinctrl-sdx65.c
    defsnc 'static[ ]const[ ]struct[ ]msm_gpio_wakeirq_map[ ]sm8450_pdc_map\[\][ ]=' drivers/pinctrl/qcom/pinctrl-sm8450.c
    blobname 'gsl1680-chuwi-hi8\.fw' drivers/platform/x86/x86-android-tablets.c
    blobname 'gt912-tm800a550l\.fw' drivers/platform/x86/x86-android-tablets.c
    defsnc 'static[ ]const[ ]u32[ ]bq25890_tspct_tbl\[\][ ]=' drivers/power/supply/bq25890_charger.c
    defsnc 'static[ ]const[ ]struct[ ]reg_default[ ]ak4375_reg_defaults\[\][ ]=' sound/soc/codecs/ak4375.c
    defsc 'static[ ]const[ ]struct[ ]reg_default[ ]adc3xxx_defaults\[\][ ]=' sound/soc/codecs/tlv320adc3xxx.c
    # sof-rn.ri is built out of CONFIG_RENOIR from sof/ project's sources.
    accept '[\t]\([\t]\.\|\.default_\)fw_filename[ \t]=[ ]["]sof-rn\.ri["][,]' sound/soc/amd/acp-config.c
    accept '[\t]\.nocodec_tplg_filename[ \t]=[ ]["]sof-acp\.tplg["][,]' sound/soc/sof/amd/pci-rn.c
    blobna 'For[ ]both[ ]Cherrytrail[ ][(]CHT[)][ ]and[ ]Baytrail[ ][(]BHT[)][ ]the[ ]driver[\n]requires[^\n]*\([\n][^\n]\+\)*\([\n][\n][- ][^\n]*\)*' drivers/staging/media/atomisp/TODO
    blobname 'qcom[/]apq8096[/]adsp\.mbn' arch/arm64/boot/dts/qcom/apq8096-db820c.dts
    blobname 'qcom[/]sdm845[/]beryllium[/]venus\.mbn' arch/arm64/boot/dts/qcom/sdm845-xiaomi-beryllium.dts 
    blobname 'qcom[/]sm7225[/]fairphone4[/]\(adsp\|cdsp\|modem\)\.mdt' arch/arm64/boot/dts/qcom/sm7225-fairphone-fp4.dts
    blobname 'qcom[/]sm8350[/]microsoft[/]\(adsp\|cdsp\|modem\|slpi\)\.mbn' arch/arm64/boot/dts/qcom/sm8350-microsoft-surface-duo2.dts
    blobname 'qcom[/]\(adsp\|cdsp\|ipa_fws\|modem\|slpi\)\.mbn' arch/arm64/boot/dts/qcom/sm8350-sony-xperia-sagami.dtsi

    # New in 5.17.
    blobna 'if[ ][(]loaded_fw_\(major\|minor\|eng\|rev\)[ ]\(!=\|<\)[ ]BCM_5710_FW_\(MAJOR\|MINOR\|ENGINEERING\|REVISION\)_VERSION\(_V15\)\?\([ ][|][|][\n][\t ]*loaded_fw_\(major\|minor\|eng\|rev\)[ ]\(!=\|<\)[ ]BCM_5710_FW_\(MAJOR\|MINOR\|ENGINEERING\|REVISION\)_VERSION\(_V15\)\?\)*[)]' drivers/net/ethernet/broadcom/bnx2x/bnx2x_cmn.c

    # New in 5.17.4 and 5.15.35.
    accept '[ ][*][ ]enabled[ ]with[ ]updated[ ]microcode[.]' arch/x86/kernel/cpu/tsx.c

    # New in 5.17.6, 5.15.38, 5.10.114, 5.4.192.
    accept '[ ][*][ ]microcode_bsp_resume[ ]-[ ]Update[ ]boot[ ]CPU[ ]microcode[ ]during[ ]resume' arch/x86/kernel/cpu/microcode/core.c

    # New in 5.18-rc.
    defsnc 'static[ ]const[ ]u8[ ]irq_prio_[hdl]\[256\][ ]=' arch/arm/mach-rpc/irq.c
    blobname 'qcom[/]sdm845[/]axolotl[/]\([ac]dsp\|a630_zap\|ipa_fws\|mba\|modem\|venus\)\.mbn' arch/arm64/boot/dts/qcom/sdm845-shift-axolotl.dts
    blobname 'qcom[/]samsung[/]w737[/]qc\([ac]dsp\|dsp\(1v\)\?2\|vss\)850\.mbn' arch/arm64/boot/dts/qcom/sdm850-samsung-w737.dts
    blobname 'qcom[/]samsung[/]w737[/]ipa_fws\.elf' arch/arm64/boot/dts/qcom/sdm850-samsung-w737.dts
    blobname 'qcom[/]sm8450[/]\([ac]dsp\|modem\|slpi\)\.mbn' arch/arm64/boot/dts/qcom/sm8450-qrd.dts
    initnc '__nsau_data[:]' arch/xtensa/lib/modsi3.S
    blobname 'rtl_bt[/]rtl8852bu_fw\.bin' drivers/bluetooth/btrtl.c
    blobname 'amdgpu[/]%s_cap\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_psp.c
    blobname 'amdgpu[/]vcn_3_1_2\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vcn.c
    blobname 'amdgpu[/]%s\.bin' drivers/gpu/drm/amd/amdgpu/sdma_v5_2.c
    blobname 'amdgpu[/]dcn_3_1_[56]_dmcub\.bin' drivers/gpu/drm/amd/display/amdgpu_dm/amdgpu_dm.c
    blobname '%s\.bin' drivers/gpu/drm/tiny/panel-mipi-dbi.c
    defsnc 'static[ ]unsigned[ ]char[ ]blackwidow_init\[RAZER_BLACKWIDOW_TRANSFER_BUF_SIZE\][ ]=' drivers/hid/hid-razer.c
    defsnc '[\t]static[ ]const[ ]u8[ ]sine\[\][ ]=' drivers/media/dvb-frontends/dib7000p.c
    defsnc 'static[ ]const[ ]struct[ ]hi847_reg[ ]mipi_data_rate_lane_4\[\][ ]=' drivers/media/i2c/hi847.c
    defsnc 'static[ ]const[ ]struct[ ]hi847_reg[ ]mode_\(3264x2448\|1632x1224\)_regs\[\][ ]=' drivers/media/i2c/hi847.c
    defsnc 'static[ ]const[ ]struct[ ]og01a1b_reg[ ]mode_1280x1024_regs\[\][ ]=' drivers/media/i2c/og01a1b.c
    defsc 'static[ ]const[ ]struct[ ]ov08d10_reg[ ]lane_2_mode_\(3280x2460\|3264x2448\|1632x1224\)\[\][ ]=' drivers/media/i2c/ov08d10.c
    accept '[\t]dev_dbg[(]core->dev[,][ ]["]request_firmware[ ]' drivers/media/platform/amphion/vpu_core.c
    blobname 'vpu[/]vpu_fw_imx8_\(enc\|dec\)\.bin' drivers/media/platform/amphion/vpu_core.c
    defsc 'static[ ]const[ ]u8[ ]dummy_\(\(gre\|udp_tun\|ipv[46]_gtpu\)_ipv[46]_\(tcp\|udp\)\|ipv6_gtp\)_packet\[\][ ]=' drivers/net/ethernet/intel/ice/ice_switch.c
    blobname 'mediatek[/]mt79[18]6_\(w[am]\|rom_patch\|eeprom\)\(_mt797[56]\(_dual\|_dbdc\)\?\)\?\.bin' drivers/net/wireless/mediatek/mt76/mt7915/mt7915.h
    blobname 'mellanox[/]mlxsw_spectrum[23]\?-\(["][ ]__stringify[(]MLXSW_SP[123]\?_FWREV_[^)]*[)][ \\\n\t]*["]\.\)*mfa2' drivers/net/ethernet/mellanox/mlxsw/spectrum.c
    blobname 'rtw89[/]rtw8852c_fw\.bin' drivers/net/wireless/realtek/rtw89/rtw8852c.c
    defsnc 'static[ ]const[ ]struct[ ]cdns_dphy_rx_band[ ]bands\[\][ ]=' drivers/phy/cadence/cdns-dphy-rx.c
    defsnc 'static[ ]struct[ ]gbe_phy_init_data_fix[ ]gbe_phy_init_fix\[\][ ]=' drivers/phy/marvell/phy-mvebu-a3700-comphy.c
    defsnc 'static[ ]const[ ]struct[ ]wpcm450_bank[ ]wpcm450_banks\[WPCM450_NUM_BANKS\][ ]=' drivers/pinctrl/nuvoton/pinctrl-wpcm450.c
    defsnc 'static[ ]const[ ]struct[ ]msm_gpio_wakeirq_map[ ]qcm2290_mpm_map\[\][ ]=' drivers/pinctrl/qcom/pinctrl-qcm2290.c
    defsnc 'static[ ]const[ ]struct[ ]msm_gpio_wakeirq_map[ ]sc8280xp_pdc_map\[\][ ]=' drivers/pinctrl/qcom/pinctrl-sc8280xp.c
    defsc 'static[ ]const[ ]unsigned[ ]int[ ]bsc_data_pins\[\][ ]=' drivers/pinctrl/renesas/pfc-r8a7740.c
    blobname 'wpss\.mdt' drivers/remoteproc/qcom_q6v5_adsp.c
    defsnc 'static[ ]const[ ]unsigned[ ]char[ ]zigzag\[\][ ]=' drivers/staging/media/hantro/hantro_jpeg.c
    defsnc 'static[ ]const[ ]u32[ ]hw_reorder\[\][ ]=' drivers/staging/media/hantro/hantro_jpeg.c
    defsc 'static[ ]const[ ]unsigned[ ]char[ ]hantro_jpeg_header\[\][ ]=' drivers/staging/media/hantro/hantro_jpeg.c
    defsnc '[\t]opts\.\(data\|insns\)[ ]=[ ][(]void[ ][*][)]["]' kernel/bpf/preload/iterators/iterators.lskel.h
    defsnc '[\t]skel->rodata[ ]=[ ]skel_prep_map_data[(][(]void[ ][*][)]["]' kernel/bpf/preload/iterators/iterators.lskel.h
    defsnc 'static[ ]const[ ]u32[ ]____cacheline_aligned[ ]K\[64\][ ]=' lib/crypto/sm3.c
    blobname 'tas5805m_dsp_%s\.bin' sound/soc/codecs/tas5805m.c
    accept '[\t]*if[ ][(][!]wm_adsp_request_firmware_files\?[(]' sound/soc/codecs/wm_adsp.c
    accept 'int[ ]avs_request_firmware[(]' sound/soc/intel/avs/avs.h
    blobname 'dsp_basefw\.bin' sound/soc/intel/avs/loader.c
    blobname '%s[/]%s[/]dsp_mod_%pUL\.bin' sound/soc/intel/avs/loader.c
    accept '[\t]*ret[ ]=[ ]avs_request_firmware[(]' sound/soc/intel/avs/loader.c
    accept '\(int[ ]\|[ ][*][ ]\)avs_request_firmware[(]' sound/soc/intel/avs/utils.c
    accept '[\t]*tplg_filename[ ]=[ ]devm_kasprintf[(]sdev->dev[,][ ]GFP_KERNEL[,][\n][\t ]*["]%s%s["][,][\n][\t ]*sof_pdata->tplg_filename[,][\n][\t ]*["]\.tplg["]' sound/soc/sof/intel/hda.c
    blobname '%s\.sec' drivers/staging/wfx/fwio.c
    blobname '%s%s-%s-%s\(-%s\)*\.%s' sound/soc/codecs/wm_adsp.c

    # New in 5.18.3, 5.17.14, 5.15.46, 5.10.121.
    accept 'MODULE_FIRMWARE[(]["]regulatory\.db\(\.p7s\)\?["][)][;]' net/wireless/reg.c

    # New in 5.18.5, 5.15.48, 5.10.123, 5.4.199, 4.19.248, 4.14.284, 4.9.319.
    accept 'combination[ ]with[ ]a[ ]microcode[ ]update[.][ ]The[ ]microcode[ ]clears' Documentation/admin-guide/hw-vuln/processor_mmio_stale_data.rst

    # New in 5.19-rc.
    # I'm not sure the following pattern matches actual blob names, in
    # two senses: it's not clear they're software, and maybe they're
    # just examples.  I'm tentatively cleaing them up.
    blobname 'am\(335\|43\)x-evm-scale-data\.bin' Documentation/devicetree/bindings/soc/ti/wkup-m3-ipc.yaml
    blobname 'am335x-bone-scale-data\.bin' arch/arm/boot/dts/am335x-bone-common.dtsi
    blobname 'am335x-evm-scale-data\.bin' arch/arm/boot/dts/'am335x-evm\(\|sk\)\.dts'
    blobname 'am43x-evm-scale-data\.bin' arch/arm/boot/dts/'am43\(7x-\(gp\|sk\)\|x-epos\)-evm\.dts'
    blobname 'qcom[/]apq8096[/]\(mba\|modem\)\.mbn' arch/arm64/boot/dts/qcom/apq8096-db802c.dts
    blobname 'qcom[/]msm8996[/]gemini[/]\(mba\|modem\|slpi\)\.mbn' arch/arm64/boot/dts/qcom/msm8996-xiaomi-gemini.dts
    blobname 'qcom[/]msm8996[/]scorpio[/]\(mba\|modem\|slpi\)\.mbn' arch/arm64/boot/dts/qcom/msm8996-xiaomi-scorpio.dts
    blobname 'qcom[/]sdm845[/]beryllium[/]\([ac]dsp\|a630_zap\|mba\|modem\|ipa_fws\)\.mbn' arch/arm64/boot/dts/qcom/sdm845-xiaomi-beryllium.dts
    blobname 'qcom[/]sm8450[/]\([ac]dsp\|modem\|slpi\)\.mbn' arch/arm64/boot/dts/qcom/sm8450-hdk.dts
    defsnc 'static[ ]const[ ]__initconst[ ]u8[ ]certs_selftest_\(keys\|1_\(data\|pkcs7\)\)\[\][ ]=' crypto/asymmetric_keys/selftest.c
    blobname 'rtl_bt[/]rtl8852cu_fw\.bin' drivers/bluetooth/btrtl.c
    blobname 'amdgpu[/]vcn_4_0_[04]\.bin' drivers/gpu/drm/amd/amdgpu/amdgpu_vcn.c
    blobname 'amdgpu[/]\(%s\|gc_11_0_[012]\)_imu\.bin' drivers/gpu/drm/amd/amdgpu/imu_v11_0.c
    blobname 'amdgpu[/]\(%s\|gc_11_0_[012]\)_mes1\?\.bin' drivers/gpu/drm/amd/amdgpu/mes_v11_0.c
    blobname 'amdgpu[/]\(%s\|sdma_6_0_[012]\)\.bin' drivers/gpu/drm/amd/amdgpu/sdma_v6_0.c
    # The following is not new, it was just moved down to allow for
    # new patterns to match despite being prefixed by it, when using
    # non-NDA regexp engines.
    blobname 'amdgpu[/]%s' drivers/gpu/drm/amd/amdgpu/amdgpu_psp.c
    # The asm source for this is drivers/gpu/drm/amd/amdkfd/cwsr_trap_handler_gfx10.asm, there is no _gfx11.asm.
    defsnc 'static[ ]const[ ]uint32_t[ ]cwsr_trap_gfx11_hex\[\][ ]=' drivers/gpu/drm/amd/amdkfd/cwsr_trap_handler.h
    defsnc '[\t]static[ ]const[ ]u8[ ]even_dividers\[\][ ]=' drivers/gpu/drm/i915/display/intel_dpll_mgr.c
    defsnc 'static[ ]const[ ]struct[ ]nv3052c_reg[ ]nv3052c_panel_regs\[\][ ]=' drivers/gpu/drm/panel/panel-newvision-nv3052c.c
    defsc 'ICE_DECLARE_PKT_TEMPLATE[(]\(\(gre\|udp_tun\|\(vlan_\)\?\(tcp\|udp\)\|ipv[46]_gtpu\)_ipv[46]\(_\(tcp\|udp\)\)\?\|ipv6_gtp\)[)][ ]=' drivers/net/ethernet/intel/ice/ice_switch.c
    blobname 'mellanox[/]lc_ini_bundle_%u_%u\.bin' drivers/net/ethernet/mellanox/mlxsw/core_linecards.c
    blobname 'mellanox[/]lc_ini_bundle_\(["][ \\\n\t]*__stringify[(]MLXSW_SP\?_FWREV_\(SUB\)\?MINOR[)][ ]["][_.]\)*bin' drivers/net/ethernet/mellanox/mlxsw/spectrum.c
    blobname 'mrvl[/]sdiouart8997_combo_v4\.bin' drivers/net/wireless/marvell/mwifiex/sdio.h
    blobname 'plfxlc[/]lifi-x[cl]\?\.bin' drivers/net/wireless/purelifi/plfxlc/firmware.c
    accept '[\t][\t]dev_err[(][&]intf->dev[,][ ]["][Rr]equest_firmware[ ]' drivers/net/wireless/purelifi/plfxlc/firmware.c
    defsnc 'static[ ]const[ ]s8[ ]_txpwr_track_delta_swingidx_[56]g[ba]_[np]\[\]\[DELTA_SWINGIDX_SIZE\][ ]=' drivers/net/wireless/realtek/rtw89/'rtw8852[ac]_table\.c'
    defsnc 'static[ ]const[ ]struct[ ]rtw89_reg2_def[ ]rtw89_8852c_phy_bb_reg\(s\|_gain\)\[\][ ]=' drivers/net/wireless/realtek/rtw89/rtw8852c_table.c
    defsnc 'static[ ]const[ ]struct[ ]rtw89_reg2_def[ ]rtw89_8852c_phy_\(radio[ab]\|nctl\)_regs\[\][ ]=' drivers/net/wireless/realtek/rtw89/rtw8852c_table.c
    defsnc 'static[ ]const[ ]struct[ ]rtw89_txpwr_byrate_cfg[ ]rtw89_8852c_txpwr_byrate\[\][ ]=' drivers/net/wireless/realtek/rtw89/rtw8852c_table.c
    defsnc 'static[ ]const[ ]struct[ ]msm_gpio_wakeirq_map[ ]sm8150_pdc_map\[\][ ]=' drivers/pinctrl/qcom/pinctrl-sm8150.c
    # It's not clear whether this contains code, but it's presumed proprietary, so tentatively disable it.
    blobname 'intel[/]ifs[/]%02x-%02x-%02x\.scan' drivers/platform/x86/intel/ifs/load.c
    defsnc 'static[ ]const[ ]int[ ]sm5703_buck_voltagemap\[\][ ]=' drivers/regulator/sm5703-regulator.c
    blobname 'intel[/]irci_irci_ecr-master_20161208_0213_20170112_1500\.bin' drivers/staging/media/ipu3/ipu3-css-fw.h
    defsnc '[\t]static[ ]u8[ ]p\[\]\[2\][ ]=' drivers/tty/serial/8250/8250_pci.c
    defsnc '[}][ ]cs35l45_pll_refclk_freq\[\][ ]=' sound/soc/codecs/cs35l45-tables.c
    defsnc 'static[ ]const[ ]char[ ][*][ ]const[ ]max98396_thermal_thresh_text\[\][ ]=' sound/soc/codecs/max98396.c
    # Topology files are presumed not code, but since we block the
    # loading of actual firmware by this driver, there's no harm in
    # being conservative and blocking them too.  These don't seem to
    # be built out of SOF.
    blobname '\(rt286\|nau8825\|ssm4567\|max98357a\|rt298\|max98373\|da7219\|tdf8532\|i2s-test\|dmic\|hda-%08x\)-tplg\.bin' sound/soc/intel/avs/board_selection.c
    accept '[\t][\t]\[SOF_IPC\][ ]=[ ]["]sof-rn\.ri["]' sound/soc/sof/amd/pci-rn.c
    accept '[\t][\t]\[SOF_IPC\][ ]=[ ]["]sof-imx8x\?\.ri["]' sound/soc/sof/imx/imx8.c
    accept '[\t][\t]\[SOF_IPC\][ ]=[ ]["]sof-imx8m\.ri["]' sound/soc/sof/imx/imx8m.c
    accept '[\t][\t]\[SOF_IPC\][ ]=[ ]["]sof-bdw\.ri["]' sound/soc/sof/intel/bdw.c
    accept '[\t][\t]\[SOF_IPC\][ ]=[ ]["]sof-\(byt\|cht\)\.ri["]' sound/soc/sof/intel/'\(byt\|pci-tng\)\.c'
    accept '[\t][\t]\[SOF_IPC\][ ]=[ ]["]sof-\(apl\|glk\)\.ri["]' sound/soc/sof/intel/pci-apl.c
    accept '[\t][\t]\[SOF_IPC\][ ]=[ ]["]sof-\(cnl\|cfl\|cml\)\.ri["]' sound/soc/sof/intel/pci-cnl.c
    accept '[\t][\t]\[SOF_IPC\][ ]=[ ]["]sof-\(icl\|jsl\)\.ri["]' sound/soc/sof/intel/pci-icl.c
    accept '[\t][\t]\[SOF_IPC\][ ]=[ ]["]sof-\(tgl\(-h\)\?\|ehl\|adl\(-s\)\?\)\.ri["]' sound/soc/sof/intel/pci-tgl.c
    # This is a new naming convention for the sof-*.ri files.  SOF
    # zephyr build scripts will output either name depending on the
    # selected naming convention.
    accept '[\t][\t]\[SOF_INTEL_IPC4\][ ]=[ ]["]dsp_basefw\.bin["]' sound/soc/sof/intel/'pci-\(apl\|cnl\|icl\|tgl\)\.c'
    accept '[\t][\t]\[SOF_IPC\][ ]=[ ]["]sof-mt8186\.ri["]' sound/soc/sof/mediatek/mt8186/mt8186.c
    accept '[\t][\t]\[SOF_IPC\][ ]=[ ]["]sof-mt8195\.ri["]' sound/soc/sof/mediatek/mt8195/mt8195.c
    accept '\([ ]*\|[$][(]OUTPUT[)]\)test-libbpf-bpf_object__next_program\.bin' tools/build/feature/Makefile
    accept '[\t][\t]test_batched_request_firmware\(\|_into_buf\|_direct\)[$]suffix' tools/testing/selftests/firmware/fw_filesystem.sh
    accept '[\t][\t]test_request_firmware_nowait_\(uevent\|custom\)[$]suffix' tools/testing/selftests/firmware/fw_filesystem.sh
    accept '[\t]\?test_request_firmware_compressed' tools/testing/selftests/firmware/fw_filesystem.sh

    # New in 5.19.4, 5.15.63.
    accept '[\t]if[ ][(]!request_firmware_direct[(][&]fw[,][ ]kpu_profile[,][ ]rvu->dev[)][)]' drivers/net/ethernet/marvell/octeontx2/af/rvu_npc.c

    # New in 6.0-rc5, 5.19.9, 5.15.68.
    defsnc '[\t]unsigned[ ]char[ ]modified_gray_code\[\][ ]=' arch/arm/mach-at91/pm.c

# Trisquel Aramo chnages
    # New in 6.1-rc, 6.0.11, 5.15.81, 5.10.157.
    blobname 'gsl1680-rca-cambio-w101-v2\.fw' drivers/platform/x86/touchscreen_dmi.c
    blobname 'gsl1680-csl-panther-tab-hd\.fw' drivers/platform/x86/touchscreen_dmi.c
#
    ;;

  */*freedo*.patch | */*logo*.patch)
    accept 'P[13]\([\n]#[^\n]*\)*[\n]*\([\n][0-9 ]*\)\+' drivers/video/logo/logo_libre_clut224.ppm
    ;;

  */*firmware-Drop-WARN-from-usermodehelper*.patch)
    accept '_request_firmware[+]0x'
    accept '\[<[0-9a-f]*>\][ ]_\?request_firmware[+]'
    accept '[;][/][*]@@[ ]-[0-9]*,[0-9]*[ ][+][0-9]*,[0-9]*[ ]@@[ ]_request_firmware[(]const[ ]struct[ ]firmware'
    ;;

  */deblob-check-testsuite/*)
    accept 'accept[(][^)]*[)]'
    blobname 'blob[(][^)]*[)]'
    blobname 'blobeol[^\n]*[\n]'
    ;;
  esac

  # Non-specific patterns come after the patch-specific ones so that,
  # when using non-NDA left-to-right regexps (python, perl), the
  # patterns above can override matches of those below.

  blob "$blobseq"
  # We leave out the initial and final letters of request_firmware so
  # that deblobbing turns them into r/*DEBLOBBED*/e, a syntax error.
  blobna 'equest_firmwar'
  blobna 'equest_partial_firmwar'
  blobna 'equest_ihex_firmwar'
  blobna 'irmware_reques' # catch _nowarn; also caches _cache, but that's ok.
  # Catch request_firmare misdeblobbed by the above.
  blobname 'r[/][*][(]DEBLOBBED[)][*][/]e' 
  blobname 'f[/][*][(]DEBLOBBED[)][*][/]t' 
  blobna '[Uu]p\(date\|grade\)[^\n]*[Mm]icrocode'
  blobna 'MODULE_FIRMWARE[ 	]*[(][^\n;]*[)][ 	]*[;]\([ 	\n]*MODULE_FIRMWARE[ 	]*[(][^\n;]*[)][ 	]*[;]\)*'
  blobna 'DEFAULT_FIRMWARE'
  blobna '\([.]\|->\)firmware[ 	\n]*=[^=]'
  blobna 'mod_firmware_load' # sound/
  blobname '[.]\(\(fw\|bin\)[0-9]*\|hex\|frm\|co[dx]\|dat\|elf\|xlx\|rfb\|ucode\|img\|sbcf\|ctx\(prog\|vals\)\|z77\|wfw\|inp\|dlmem\|cld\|tftf\|out\|nffw\|mdt\|mfa2\?\|ri\|tplg\|itb\|cyacd\|mbn\|tlv\|sfi\|grp\)[\\]\?["]'
  # WIP ends with [\\]\?[][}{)(><,;:.!?% \t\n"`\'"'"']'
  # Catch misdeblobbed fw extension.
  blobname '["]\([^" \t\n/]*[/][/]*\)*[*][(]DEBLOBBED[)][*][/][^"\\]'
  # Ideally we'd whitelist URLs that don't recommend non-Free
  # Software, but there are just too many URLs in Linux, and most are
  # fine, so we just blacklist when we find undesirable URLs.
  # Please report if you find any inappropriate URL in Linux-libre
  # deblobbed documentation, sources or run-time log messages.
  # blobna '\(f\|ht\)tp:[/]\([/]\+[^/ \n ]\+\)\+'
}

# Regular expression that matches a literal constant.
constx="[0-9][0-9a-fA-FxX]*"
# Regular expression that matches a separator between consecutive
# literal constants.
sepx="\\([ 	\\n]*\\(\\([ 	\\n]\\|[,:{}LlUu\"\'\\\\][,:{} 	\\nLlUu\"\'\\\\]*\\)[xX\$]\\?\\|[.][a-zA-Z][a-zA-Z0-9]*[ 	][ 	]*[\$]\\?\\)\\)"

# Regular expression that matches a continuation of a blob, after an
# initial constant.  *, \+ and \? can be safely appended to it without
# \(\)s.
blobcont="\\($sepx$constx\\)"

# Regular expression that matches the initial constant of a blob plus
# its continuation.  *, \+ and \? can be safely appended to it without
# \(\)s.
blobpat="$constx$blobcont"

# Regular expression that matches a blob with at least the number of
# constants specified as sensitivity.
blobseq="$blobpat\\{$sens,\\}"

# Regular expression that matches the beginning of the pattern or a
# line break.  It must be \(\)ed, such that it can be named in
# replacement patterns.
bol="\\(^\\|[\\n]\\)"

# Regular expression that matches the end of the pattern or a line
# break.  It must be \(\)ed, such that it can be named in replacement
# patterns.
eol="\\([\\n]\\|\$\\)"

# Regular expression that matches a C-style comment.
comment="\\([/][*][^*]*\\([*]\\+[^*/][^*]*\\)*[*]\\+[/]\\|[/][/][^\\n]*[\\n]\\)"

# Regular expression that matches comments typically used in assembly.
asmcomment="\\($comment\\|[;#][^\\n]*[\\n]\\)"

# Regular expression that matches a braced initializer containing at
# least one blob.
initblob="[^\\n=]*=\\([ 	\\n\\\\]\\|$comment\\)*[{]\\([^;/]\\|[/][^/*]\\|$comment\\)*$blobseq\\([^;/]\\|[/][^/*]\\|$comment\\)*[}]\\?\\([ 	\\n\\\\]*\\|$comment\\)[;]\\?"

# Regular expression that matches a C (possibly multi-line) #define
# that contains a blob.
defineblob='[ 	]*#[ 	]*define[ 	][^\n]*\([\\][\n][^\n]*\)*'"$blobseq"'\([^\n]*\\[\n]\)*'

# Regular expression that matches an assembly label followed by a blob
# without any intervening label.
asmblob="[a-zA-Z_.][^\\n:;#/ 	]*:\\([^:{}/]\\|[/][^/*]\\|$asmcomment\\)*$blobseq\\([^:]*\\|$asmcomment\\)*"

# Set up the sed script that will go through the (processed) input,
# looking for sequences of blobs and printing whatever was requested.
# It accepts 3 arguments.

# $1 is the action in case blobs were found in the input.

# $2 is the action in case no blobs were found, not even false positives.

# $3 is the action in case false positives were located.

# $4 is the action for every complete input pattern.

set_sed_main () {
  falsepos=`${SED-sed} -n 's,^[+]\^*,,p' < "$regex_name" |
    ${SED-sed} -n -e 's,[$]$,\\\\([\\\\n]\\\\|$\\\\),' \
	-e '1h; 1!H; ${g;s,[\n],\\\\|,g;s,^\(..*\)$,\\\\(\1\\\\),;p;}'`
  blobs=`${SED-sed} -n 's,^[-],,p' < "$regex_name" |
    ${SED-sed} -n -e 's,[$]$,\\\\([\\\\n]\\\\|$\\\\),' \
	-e '1h; 1!H; ${g;s,[\n],\\\\|,g;s,^\(..*\)$,\\\\(\1\\\\),;p;}'`

  # Regular expression that matches one or more blobs without
  # intervening line breaks.
  sblobctx="\\(\\([^\\n]\\|[/][*](DEBLOB-\\nBED)[*][/]\\)*$blobs\\)\\+"

  # Regular expression that matches the context for a long blob match.
  lblobctx="\\($initblob\\|$defineblob\\|$asmblob\\|$sblobctx\\)"

  if test "X$falsepos" != X; then
    check_false_positives="$v:???falsepos
/$bol$falsepos/!b blob
$v:+++falsepos
h
s/$bol$falsepos/\\1;\/**\/;/g
# See if, after removing all matches, we end up without any blobs.
$v:???blobs
/$blobs/!{
  g
  b falsepos
}
g
"
  else
    falsepos="$.^"
    check_false_positives=
  fi

  $echo "#! /bin/sed -nf

/^$/N
/^[\\n]\\?;[/][*]\\(end .*\\)\\?[*][/];$/{
  $4
  d
}
# /^;[/][*]begin /!{
#   : internal_error
#   $v:internal_error
#   s,.*,Internal error at\\n&[\\n]/*(DEBLOB-\\nERROR)*/,;
#   q 2
# }
$v:reading file in
h
n
: read_more
/^;[/][*]end [^\\n]*[*][/];$/! {
  H
  n
  b read_more
}
H
g
$4
$v:read all
s/^\\(;[/][*]begin [^\\n]*[\\n]\\)*//
s/\\($bol[\n]\?;[/][*]\\(end [^\\n]*\\)\\?[*][/];\\)*$//
$v:???!blobs
/$blobs/!b clean
$check_false_positives
# Fall through.
: blob
$v:blob
$1
d
: clean
$v:clean
$2
d
: falsepos
$v:falsepos
$3
d

: print_matches
$v:print_matches
/^$falsepos/! {
  $v:delete unmatching lines
  h
  s/[\\n]$falsepos.*//
  : print_matches_nomatch_loop
  /[\\n]/ {
    s/^[^\\n]*[\\n]//
    x
    s/^[^\\n]*[\\n]//
    x
    b print_matches_nomatch_loop
  }
  x
  b print_matches_delete_to_eol
}
h
s/^\\($falsepos[^\\n]*\\)\\([\\n].*\\)\\?$/\\1/
$v:narrowed to match
/$blobs/ {
  i\\
::: $file :::
  p
}
g
s/^\\($falsepos[^\\n]*\\)//
: print_matches_delete_to_eol
$v:delete to eol
s/^[^\\n]*//
/^$/d
s/^[\\n]//
b print_matches

: print_marked_matches
$v:print_marked_matches
/^$falsepos/! {
  h
  s/[\\n]$falsepos.*//
  : print_marked_matches_nomatch_loop
  /[\\n]/ {
    s/^[^\\n]*[\\n]//
    x
    s/^[^\\n]*[\\n]//
    x
    b print_marked_matches_nomatch_loop
  }
  x
  b print_marked_matches_delete_to_eol
}
h
s/^\\($falsepos[^\\n]*\\)\\([\\n].*\\)\\?$/\\1/
$v:narrowed to match
/$blobs/{
  i\\
::: $file :::
  # s/{\\($sepx\\)\\?$blobseq\\($sepx\\)\\?}[ 	]*;/{\/*(DEBLOBBED)*\/};/g
  s/$blobs/\/*(DEBLOBBED)*\//g
  p
}
g
s/^\\($falsepos[^\\n]*\\)//
: print_marked_matches_delete_to_eol
$v:delete to eol
s/^[^\\n]*//
/^$/d
s/^[\\n]//
b print_marked_matches

: print_blobs
$v:print_blobs
/^$falsepos/ {
  $v:delete false positive
  # This is tricky.  We don't want to print the false positive.
  /^$falsepos[^\\n]*$blobs/ {
    $v:delete false positive immediately followed by blob
    s/^\\($falsepos\\)/\\1\/*(DEBLOB-\\nBED)*\//
    h
    s/^\\($falsepos\\).*/\\1/
    $v:matched false positive
    : print_blobs_match_loop
    /[\\n]/ {
      s/^[^\\n]*[\\n]//
      x
      s/^[^\\n]*[\\n]//
      x
      b print_blobs_match_loop
    }
    G
    b print_blobs_delete_to_eol
  }
  /^$falsepos[/][*](DEBLOB-\\nBED)[*][/]/! {
    s/^$falsepos//
    b print_blobs_delete_to_eol
  }
}
/^\([^\\n]\|[/][*](DEBLOB-\\nBED)[*][/]\)*$blobs/! {
  $v:delete non-blob header
  h
  s/[\\n]\\($falsepos\\|[^\\n]*$blobs\\).*//
  $v:matched non-blob header
  : print_blobs_nomatch_loop
  /[\\n]/ {
    s/^[^\\n]*[\\n]//
    x
    s/^[^\\n]*[\\n]//
    x
    b print_blobs_nomatch_loop
  }
  x
  b print_blobs_delete_to_eol
}
i\\
::: $file :::
: print_blobs_output_false_positive
/[^\\n]*[/][*](DEBLOB-[\\n]BED)[*][/]/ {
  P
  s,^[^\\n]*[\\n],,
  b print_blobs_output_false_positive
}
h
s/\\($blobs\\([^\\n]*$blobs\\)*[^\\n]*\\)\\([\\n].*\\)\\?$/\\1/
$v:narrowed to blob
p
g
s/\\(\\($blobs[^\\n]*\\)\\+\\)//
: print_blobs_delete_to_eol
$v:delete to eol
s/^[^\\n]*//
/^$/d
s/^[\\n]//
b print_blobs

: print_marked_blobs
$v:print_marked_blobs
/^$falsepos/ {
  $v:delete false positive
  # This is tricky.  We don't want to print the false positive.
  /^$falsepos[^\\n]*$blobs/ {
    $v:delete false positive immediately followed by blob
    s/^\\($falsepos\\)/\\1\/*(DEBLOB-\\nBED)*\//
    h
    s/^\\($falsepos\\).*/\\1/
    $v:matched false positive
    : print_marked_blobs_match_loop
    /[\\n]/ {
      s/^[^\\n]*[\\n]//
      x
      s/^[^\\n]*[\\n]//
      x
      b print_marked_blobs_match_loop
    }
    G
    b print_marked_blobs_delete_to_eol
  }
  /^$falsepos[/][*](DEBLOB-\\nBED)[*][/]/! {
    s/^falsepos//
    b print_marked_blobs_delete_to_eol
  }
}
/^\([^\\n]\|[/][*](DEBLOB-\\nBED)[*][/]\)*$blobs/! {
  $v:delete non-blob header
  h
  s/[\\n]\\($falsepos\\|[^\\n]*$blobs\\).*//
  $v:matched non-blob header
  : print_marked_blobs_nomatch_loop
  /[\\n]/ {
    s/^[^\\n]*[\\n]//
    x
    s/^[^\\n]*[\\n]//
    x
    b print_marked_blobs_nomatch_loop
  }
  x
  b print_marked_blobs_delete_to_eol
}
i\\
::: $file :::
: print_marked_blobs_output_false_positive
/[^\\n]*[/][*](DEBLOB-[\\n]BED)[*][/]/ {
  P
  s,^[^\\n]*[\\n],,
  b print_marked_blobs_output_false_positive
}
h
s/\\($blobs\\([^\\n]*$blobs\\)*[^\\n]*\\)\\([\\n].*\\)\\?$/\\1/
$v:narrowed to blob
# s/{\\($sepx\\)\\?$blobseq\\($sepx\\)\\?}[ 	]*;/{\/*(DEBLOBBED)*\/};/g
s/$blobs/\/*(DEBLOBBED)*\//g
p
g
s/\\(\\($blobs[^\\n]*\\)\\+\\)//
: print_marked_blobs_delete_to_eol
$v:delete to eol
s/^[^\\n]*//
/^$/d
s/^[\\n]//
b print_marked_blobs

: print_cblobs
$v:print_cblobs
/^$falsepos/ {
  $v:delete false positive
  # This is tricky.  We don't want to print the false positive.
  /^$falsepos[^\\n]*$blobs/ {
    $v:delete false positive immediately followed by blob
    s/^\\($falsepos\\)/\\1\/*(DEBLOB-\\nBED)*\//
    h
    s/^\\($falsepos\\).*/\\1/
    $v:matched false positive
    : print_cblobs_match_loop
    /[\\n]/ {
      s/^[^\\n]*[\\n]//
      x
      s/^[^\\n]*[\\n]//
      x
      b print_cblobs_match_loop
    }
    G
    b print_cblobs_delete_to_eol
  }
  /^$falsepos[/][*](DEBLOB-\\nBED)[*][/]/! {
    s/^$falsepos//
    b print_cblobs_delete_to_eol
  }
}
/^$lblobctx/! {
  $v:delete non-blob header
  h
  s/[\\n]\\($falsepos\\|$lblobctx\\).*//
  $v:matched non-blob header
  : print_cblobs_nomatch_loop
  /[\\n]/ {
    s/^[^\\n]*[\\n]//
    x
    s/^[^\\n]*[\\n]//
    x
    b print_cblobs_nomatch_loop
  }
  x
  b print_cblobs_delete_to_eol
}
i\\
::: $file :::
: print_cblobs_output_false_positive
/[^\\n]*[/][*](DEBLOB-[\\n]BED)[*][/]/ {
  P
  s,^[^\\n]*[\\n],,
  b print_cblobs_output_false_positive
}
h
s/^\\($lblobctx\\([^\\n]*$blobs\\)*[^\\n]*\\)\\([\\n].*\\)\\?$/\\1/
$v:narrowed to blob
p
g
s/^\\($lblobctx[^\\n]*\\($blobs[^\\n]*\\)*\\)//
: print_cblobs_delete_to_eol
$v:delete to eol
s/^[^\\n]*//
/^$/d
s/^[\\n]//
b print_cblobs

: print_marked_cblobs
$v:print_marked_cblobs
/^$falsepos/ {
  $v:delete false positive
  # This is tricky.  We don't want to print the false positive.
  /^$falsepos[^\\n]*$blobs/ {
    $v:delete false positive immediately followed by blob
    s/^\\($falsepos\\)/\\1\/*(DEBLOB-\\nBED)*\//
    h
    s/^\\($falsepos\\).*/\\1/
    $v:matched false positive
    : print_marked_cblobs_match_loop
    /[\\n]/ {
      s/^[^\\n]*[\\n]//
      x
      s/^[^\\n]*[\\n]//
      x
      b print_marked_cblobs_match_loop
    }
    G
    b print_marked_cblobs_delete_to_eol
  }
  /^$falsepos[/][*](DEBLOB-\\nBED)[*][/]/! {
    s/^$falsepos//
    b print_marked_cblobs_delete_to_eol
  }
}
/^$lblobctx/! {
  $v:delete non-blob header
  h
  s/[\\n]\\($falsepos\\|$lblobctx\\).*//
  $v:matched non-blob header
  : print_marked_cblobs_nomatch_loop
  /[\\n]/ {
    s/^[^\\n]*[\\n]//
    x
    s/^[^\\n]*[\\n]//
    x
    b print_marked_cblobs_nomatch_loop
  }
  x
  b print_marked_cblobs_delete_to_eol
}
i\\
::: $file :::
: print_marked_cblobs_output_false_positive
/[^\\n]*[/][*](DEBLOB-[\\n]BED)[*][/]/ {
  P
  s,^[^\\n]*[\\n],,
  b print_marked_cblobs_output_false_positive
}
h
s/^\\($lblobctx\\([^\\n]*$blobs\\)*[^\\n]*\\)\\([\\n].*\\)\\?$/\\1/
$v:narrowed to blob
# s/{\\($sepx\\)\\?$blobseq\\($sepx\\)\\?}[ 	]*;/{\/*(DEBLOBBED)*\/};/g
s/$blobs/\/*(DEBLOBBED)*\//g
p
g
s/^\\($lblobctx[^\\n]*\\($blobs[^\\n]*\\)*\\)//
: print_marked_cblobs_delete_to_eol
$v:delete to eol
s/^[^\\n]*//
/^$/d
s/^[\\n]//
b print_marked_cblobs

: print_both
$v:print_both
/^\\($falsepos\\|[^\\n]*$blobs\\)/! {
  $v:delete non-blob header
  h
  s/[\\n]\\($falsepos\\|[^\\n]*$blobs\\).*//
  $v:matched non-blob header
  : print_both_nomatch_loop
  /[\\n]/ {
    s/^[^\\n]*[\\n]//
    x
    s/^[^\\n]*[\\n]//
    x
    b print_both_nomatch_loop
  }
  x
  b print_both_delete_to_eol
}
h
i\\
::: $file :::
s/^\\(\\($falsepos\\|[^\\n]*$blobs\\)\\([^\\n]*$blobs\\)*[^\\n]*\\)\\([\\n].*\\)\\?$/\\1/
$v:narrowed to blob
p
g
s/^\\(\\($falsepos[^\\n]*\\|[^\\n]*$blobs[^\\n]*\\)\\($blobs[^\\n]*\\)*\\)//
: print_both_delete_to_eol
$v:delete to eol
s/^[^\\n]*//
/^$/d
s/^[\\n]//
b print_both

: list_matches
$v:list_matches
/^$falsepos/! {
  $v:print unmatching lines
  h
  s/[\\n]$falsepos.*//
  p
  : list_matches_nomatch_loop
  /[\\n]/ {
    s/^[^\\n]*[\\n]//
    x
    s/^[^\\n]*[\\n]//
    x
    b list_matches_nomatch_loop
  }
  x
  b list_matches_delete_to_eol
}
h
s/^\\($falsepos[^\\n]*\\)\\([\\n].*\\)\\?$/\\1/
$v:narrowed to match
/$blobs/{
  # s/{\\($sepx\\)\\?$blobseq\\($sepx\\)\\?}[ 	]*;/{\/*(DEBLOBBED)*\/};/g
  s/$blobs/\/*(DEBLOBBED)*\//g
}
p
g
s/^\\($falsepos[^\\n]*\\)//
: list_matches_delete_to_eol
$v:delete to eol
s/^[^\\n]*//
/^$/d
s/^[\\n]//
b list_matches

: list_blobs
$v:list_blobs
/^$falsepos/ {
  $v:print false positive
  # This is tricky.  We don't want to deblob the false positive.
  /^$falsepos[^\\n]*$blobs/ {
    $v:print false positive immediately followed by blob
    s/^\\($falsepos\\)/\\1\/*(DEBLOB-\\nBED)*\//
    h
    s/^\\($falsepos\\).*/\\1\\n/
    : list_blobs_match_loop
    /[\\n]/ {
      s/^[^\\n]*[\\n]//
      x
      P
      s/^[^\\n]*[\\n]//
      x
      b list_blobs_match_loop
    }
    G
    b list_blobs_delete_to_eol
  }
  h
  s/^\\($falsepos[^\\n]*\\)[\\n].*/\\1/
  p
  g
  s/^\\($falsepos[^\\n]*\\)//
  b list_blobs_delete_to_eol
}
/^[^\\n]*$blobs/! {
  $v:print non-blob header
  h
  s/[\\n]\\($falsepos\\|[^\\n]*$blobs\\).*//
  p
  : list_blobs_nomatch_loop
  /[\\n]/ {
    s/^[^\\n]*[\\n]//
    x
    s/^[^\\n]*[\\n]//
    x
    b list_blobs_nomatch_loop
  }
  x
  b list_blobs_delete_to_eol
}
h
s/\\($blobs\\([^\\n]*$blobs\\)*[^\\n]*\\)\\([\\n].*\\)\\?$/\\1/
$v:narrowed to blob
# s/{\\($sepx\\)\\?$blobseq\\($sepx\\)\\?}[ 	]*;/{\/*(DEBLOBBED)*\/};/g
s/$blobs/\/*(DEBLOBBED)*\//g
p
g
s/\\(\\($blobs[^\\n]*\\)\\+\\)//
: list_blobs_delete_to_eol
$v:delete to eol
s/^[^\\n]*//
/^$/d
s/^[\\n]//
b list_blobs

: list_both
$v:list_both
/^\\($falsepos\\|[^\\n]*$blobs\\)/! {
  $v:print non-blob header
  h
  s/[\\n]\\($falsepos\\|[^\\n]*$blobs\\).*//
  p
  : list_both_nomatch_loop
  /[\\n]/ {
    s/^[^\\n]*[\\n]//
    x
    s/^[^\\n]*[\\n]//
    x
    b list_both_nomatch_loop
  }
  x
  b list_both_delete_to_eol
}
h
s/^\\(\\($falsepos\\|[^\\n]*$blobs\\)\\([^\\n]*$blobs\\)*[^\\n]*\\)\\([\\n].*\\)\\?$/\\1/
$v:narrowed to blob
# s/{\\($sepx\\)\\?$blobseq\\($sepx\\)\\?}[ 	]*;/{\/*(DEBLOBBED)*\/};/g
s/$blobs/\/*(DEBLOBBED)*\//g
p
g
s/^\\(\\($falsepos[^\\n]*\\|[^\\n]*$blobs[^\\n]*\\)\\($blobs[^\\n]*\\)*\\)//
: list_both_delete_to_eol
$v:delete to eol
s/^[^\\n]*//
/^$/d
s/^[\\n]//
b list_both

" > "$scriptname"

  scriptcmd='${SED-sed} -n -f "$scriptname"'

  case $vp in
  [01]) xv= ;;
  2) xv='# ';;
  esac

  sedunbreak='
: restart
/[/][*](DEBLOB-$/ {
  N
  /[/][*](DEBLOB-[\n]ERROR)[*][/]/{q 1;}'"
$xv"'s,[/][*](DEBLOB-[\n]BED)[*][/],,
  b restart
}
p
'
  scriptcmd2='${SED-sed} -n -e "$sedunbreak"'
}

set_flex_main () {
  adjust_rx='
s,\\\([{(|)}?+]\),\1,g
s,^\([-+]\)\(\^\?\)\(.*\)\(\$\?\)$,\2(?s:\3)\4\1,g
s,[+]$, { falsepos (); },
s,[-]$, { blob (); },
'

  echo '%%' > "$scriptname"
  ${SED-sed} "$adjust_rx" < "$regex_name" >> "$scriptname"
  echo '\n|. { unmatched (); }
%%
int falsepos () {}
int blob () {}
int unmatched () {}
' >> "$scriptname"

  scriptcmd=false
}

set_python_main () {
  adjust_rx='
s,\\(,\\(?:,g;
s,\\\([{(|)}?+]\),\1,g;
'

  cat >> "$scriptname" <<EOF
#! /usr/bin/python

import sys
import re

# Should we replace blobs and false positives with replacement?
replace_blob = 0
replace_falsepos = 0
replacement = '/*(DEBLOBBED)*/'

# Should we print lines containing blobs, false positives, and neither?
print_blob = 0
with_context = 0
print_falsepos = 0
print_nomatch = 0

# Should we print the input stack if we find blobs or false positives?
list_blob = 0
list_falsepos = 0

# Should we forget everything we know about false positives?
falsepos = None
no_falsepos = 0

verbose = $vp

# Which of the defaults above should we override?
$@ = 1

EOF

  if test "X$DEBLOB_CHECK_PYTHON_REGEX" = Xdebug; then
    ${SED-sed} -e 's,^[+-],,' -e "$adjust_rx" \
	-e "s,.*,re.compile (r'&'),g" \
	< "$regex_name" >> "$scriptname"
  fi

  ${SED-sed} -n 's,^[+],,p' < "$regex_name" |
    ${SED-sed} -n -e "$adjust_rx" -e 's,\^,,' \
	-e '1h; 1!H; $ { g; s,[\n],|,g; '"\
s,^\\(.*\\)\$,falsepos = r'(?P<falsepos>\\1)',;\
"' p;}' >> "$scriptname"

  ${SED-sed} -n 's,^[-],,p' < "$regex_name" |
    ${SED-sed} -n -e "$adjust_rx" \
	-e '1h; 1!H; $ { g; s,[\n],|,g; '"\
s,^\\(.*\\)\$,blob = r'(?P<blob>\\1)',;\
"' p;}' >> "$scriptname"

  $echo "\\($initblob\\|$defineblob\\|$asmblob\\)" |
    ${SED-sed} -e "$adjust_rx" \
        -e "s,^\\(.*\\)\$,cblob = r'(?P<cblob>\\1)'," >> "$scriptname"

  cat >> "$scriptname" <<\EOF

if no_falsepos or falsepos is None:
    falsepos = r'(?!)'

rx = '^%s|%s' % (falsepos, blob)

if with_context:
    rx += '|^' + cblob

rxc = re.compile('(?<=.)(?:%s)' % rx, re.M | re.S)

filenames = None

s = '\n'

for line in sys.stdin:
    # Read into s all lines between begin and end.  An empty line, without
    # even the '\n', flags the end of the input.
    if line[:3] == ';/*' and line[-4:] == '*/;\n':
        if line[3:9] == 'begin ':
            nextfilenames = (line[9:-4], filenames)
            if s == '\n':
                filenames = nextfilenames
                del nextfilenames
                continue
        elif line[3:7] == 'end ':
	    #if print_blob and not print_nomatch:
	    # from time import time
	    # sys.stderr.write('%i %i %s\n' % (time(), len(s), filenames[0]))
            assert line[7:-4] == filenames[0]
            nextfilenames = filenames[1]
        else:
            assert filenames != None
            s += line
            continue
    else:
        assert filenames != None
        s += line
        continue

    if verbose:
            print('looking for matches')
            sfilenames = filenames
            while filenames != None:
                if filenames[1] is None:
                    print(filenames[0])
                else:
                    print(filenames[0] + ' within')
                filenames = filenames[1]
            filenames = sfilenames

    if s[-1] == '\n':
        s = s[:-1]

    pp = 1
    p = pend = 0
    match = rxc.search (s, p)
    while match != None:
        firstmatch = match
        blobs = falses = 0
        while 1:
            if verbose:
                print('found match')
            what = match.lastgroup

            if what == 'cblob':
                if verbose: print('match is a blob context')
                pend = s.find ('\n', match.end()) + 1
                if pend == 0:
                    pend = len(s)
                p = match.start() + 1
                blob_p = 2
            else:
                blob_p = what == 'blob'
                assert blob_p or what == 'falsepos'

                if blob_p:
                    if verbose: print('match is a blob')
                    blobs += 1
                else:
                    if verbose: print('match is a false positive')
                    falses += 1

                if blob_p and replace_blob or not blob_p and replace_falsepos:
                    s = s[:match.start(what)] + replacement + s[match.end(what):]
                    p = match.start(what) + len(replacement)
                    if pend > match.start(what):
                        pend += p - match.end(what)
                else:
                    p = match.end(what)

                if p > pend:
                    pend = s.find ('\n', p) + 1
                    if (pend == 0):
                        pend = len(s)

            match = rxc.search (s, p)
            if match is None or match.start () >= pend or \
	       (blob_p and not print_blob and not falses) or \
	       (not blob_p and not print_falsepos and not blobs):
                break

        if print_nomatch:
            sys.stdout.write (s[pp:firstmatch.start() + 1])
            pp = firstmatch.start() + 1
        else:
            pp = s.rfind ('\n', 0, firstmatch.start () + 1) + 1

        if print_blob and blobs or print_falsepos and falses:
            if not print_nomatch:
                sfilenames = filenames
                while filenames != None:
                    print('::: ' + filenames[0] + ' :::')
                    filenames = filenames[1]
                filenames = sfilenames
            sys.stdout.write (s[pp:pend])
            pp = pend

        if list_blob and blobs or list_falsepos and falses:
            while filenames != None:
                if filenames[1] is None:
                    print(filenames[0])
                else:
                    print (filenames[0] + ' within')
                filenames = filenames[1]
            exit (1)

    if print_nomatch:
        sys.stdout.write(s[pp:])

    if verbose:
        print('no further matches')

    s = '\n'
    filenames = nextfilenames
    del nextfilenames

assert filenames is None

exit (0)
EOF

  scriptcmd="${PYTHON-python} "'"$scriptname"'
}

set_perl_main () {
  adjust_rx='
s,\\(,\\(?:,g;
s,\\\([{(|)}?+]\),\1,g;
'

  # Add $ before arguments
  set `echo "$@" | sed 's,\(^\|= *\),&$,g'`

  cat >> "$scriptname" <<\EOF
#! /usr/bin/perl

use strict;
use warnings;

# Should we replace blobs and false positives with replacement?
my $replace_blob = 0;
my $replace_falsepos = 0;
my $replacement = '/*(DEBLOBBED)*/';

# Should we print lines containing blobs, false positives, and neither?
my $print_blob = 0;
my $with_context = 0;
my $print_falsepos = 0;
my $print_nomatch = 0;

# Should we print the input stack and exit if we find blobs or false positives?
my $list_blob = 0;
my $list_falsepos = 0;

# Should we forget everything we know about false positives?
my $falsepos;
my $no_falsepos = 0;

EOF

  cat >> "$scriptname" <<EOF
my \$verbose = $vp;

# Which of the defaults above should we override?
$@ = 1;

EOF

  ${SED-sed} -n 's,^[+],,p' < "$regex_name" |
    ${SED-sed} -n -e "$adjust_rx" -e 's,\^,,' \
	-e '1h; 1!H; $ { g; s,[\n],|,g; '"\
s,^\\(.*\\)\$,\$falsepos = qr'(?<falsepos>\\1)'ms;,;\
"' p;}' >> "$scriptname"

  ${SED-sed} -n 's,^[-],,p' < "$regex_name" |
    ${SED-sed} -n -e "$adjust_rx" \
	-e '1h; 1!H; $ { g; s,[\n],|,g; '"\
s,^\\(.*\\)\$,my \$blob = qr'(?<blob>\\1)'ms;,;\
"' p;}' >> "$scriptname"

  $echo "\\($initblob\\|$defineblob\\|$asmblob\\)" |
    ${SED-sed} -e "$adjust_rx" \
        -e "s,^\\(.*\\)\$,my \$cblob = qr'(?<cblob>\\1)'ms if \$with_context;," >> "$scriptname"

  cat >> "$scriptname" <<\EOF

$falsepos = qr/(?<falsepos>(?!))/ if $no_falsepos || ! defined $falsepos;

my $rx = qr/^$falsepos|$blob/ms;

$rx = qr/$rx|^$cblob/ms if $with_context;

my @filenames;
my $nfilenames = 0;
my $nextnfilenames;

my $s = '';

while (<STDIN>) {
    # Read into s all lines between begin and end.  An empty line, without
    # even the '\n', flags the end of the input.
    if (m:^[;][/][*](begin|end) (.*)[*][/][;]$:) {
	if ($1 eq 'begin') {
	    print "entering $2\n" if $verbose;
	    $filenames[$nfilenames] = $2;
	    $nextnfilenames = $nfilenames + 1;
	    if ($s eq '') {
		$nfilenames = $nextnfilenames;
		next;
	    }
	} else {
	    $nextnfilenames = $nfilenames - 1;
	    print "processing $filenames[$nextnfilenames]\n" if $verbose;
	}
    } else {
	$s .= $_;
	next;
    }

    if ($verbose) {
	print "looking for matches in\n";
	for (my $i = $nfilenames; --$i > 0; ) {
	    print $filenames[$i], " within\n";
	}
	print $filenames[0], "\n";
    }

    $s =~ s/[\n]$//;

    my $pp = my $p = 0;

    my $matchfound = substr ($s, $p) =~ /$rx/o;
    while ($matchfound) {
	print "found first match\n" if $verbose;
	my $firstmatchstart = $-[0] + $p;
	my $blobs = my $falses = 0;
	my $matchstart = $-[0] + $p;
	my $pend = -1;
	my $blob_p;
	do {{
	    my $matchend = $+[0] + $p;
	    print "found match $matchstart..$matchend\n" if $verbose;
	    print "$&" if $verbose > 1;

	    if (defined $+{'cblob'}) {
		print "match is a blob context\n" if ($verbose);
		$pend = index ($s, "\n", $matchend) + 1;
		$pend = length $s if !$pend;
	    }

	    if (defined $+{'falsepos'}) {
		print "match is a false positive\n" if ($verbose);
		# $matchend -= $+[0] - $+[1];
		$blob_p = 0;
		$falses++;
	    } elsif (defined $+{'blob'}) {
		$blob_p = 1;
		$blobs++;
		print "match is a blob at $matchstart\n" if ($verbose);
	    } else {
		$blob_p = 2;
		$p = $matchstart;
		print "searching up to $pend\n" if $verbose;
		next;
	    }

	    if ($blob_p ? $replace_blob : $replace_falsepos) {
		substr ($s, $matchstart, $matchend - $matchstart,
			$replacement);
		$p = $matchstart + length $replacement;
		$pend += $p - $matchend if $pend >= $matchstart;
	    } else {
		$p = $matchend;
	    }

	    $pend = index ($s, "\n", $p) + 1 if $p >= $pend;
	    $pend = length $s if !$pend;
	    print "searching up to $pend\n" if $verbose;
	    $p--;
	}} while (($matchfound = (substr ($s, $p) =~ /(?<=.)$rx/mso))
		  && ($matchstart = $-[0] + $p) < $pend
		  && !($blob_p
		       ? (!$print_blob && !$falses)
		       : (!$print_falsepos && !$blobs)));

	print "last match before $pend\n" if $verbose;

	if ($print_nomatch) {
	    print substr ($s, $pp, $firstmatchstart - $pp);
	    $pp = $firstmatchstart;
	} elsif (($print_blob || $print_falsepos) && $firstmatchstart > 0) {
	    $pp = rindex ($s, "\n", $firstmatchstart - 1) + 1;
	}

	if (($print_blob && $blobs) || ($print_falsepos && $falses)) {
	    if (!$print_nomatch) {
		for (my $i = $nfilenames; $i-- > 0;) {
		    print "::: ", $filenames[$i], " :::\n";
		}
	    }

	    print substr ($s, $pp, $pend - $pp);
	    $pp = $pend;
	}

	if (($list_blob && $blobs) || ($list_falsepos && $falses)) {
	    for (my $i = $nfilenames; --$i > 0;) {
		print $filenames[$i], " within ";
	    }
	    print $filenames[0], "\n";
	    exit (1);
	}
    }

    print substr ($s, $pp) if $print_nomatch;

    print "no further matches\n" if $verbose;

    $s = '';
    $nfilenames = $nextnfilenames;
}

exit (0);
EOF

  scriptcmd="${PERL-perl} "'"$scriptname"'
}

set_awk_main () {
  adjust_rx='
s,[$]$,([\\n]|$),;
s,\[^\],[^\\],g;
s,\\\([{(|)}?+]\),\1,g;
'

  case " = $@ = " in
  *" = no_falsepos = "*) falsepos='$.^';;
  *) falsepos=`
    ${SED-sed} -n 's,^[+],,p' < "$regex_name" |
    ${SED-sed} -n -e "$adjust_rx" -e 's,\^,,' \
	-e '1h; 1!H; $ { g; s,[\n],|,g; p;}'
    `
     case $falsepos in "") falsepos='$.^';; esac;;
  esac

  blob=`
    ${SED-sed} -n 's,^[-],,p' < "$regex_name" |
    ${SED-sed} -n -e "$adjust_rx" \
	-e '1h; 1!H; $ { g; s,[\n],|,g; p;}'`

  case " = $@ = " in
  *" = with_context = "*) cblob=`
    $echo "\\($initblob\\|$defineblob\\|$asmblob\\)" |
    ${SED-sed} -e "$adjust_rx"
   `;;
  *) cblob='$.^';;
  esac

  xrs= nrs="# " eor="RT" eormatch='RT ~ ' eornl='[\n]' eornlsz=1
  # Uncomment the line below to disable the use of a regular
  # expression for the awk Record Separator, a GNU awk extension.
  # Using this extension appears to save a lot of memory for long
  # deblob-check runs.
  # xrs="# " nrs= eor='$0' eormatch='' eornl= eornlsz=0

  cat >> "$scriptname" <<EOF
#! /bin/gawk --re-interval -f

BEGIN {
    # Should we replace blobs and false positives with replacement?
    replace_blob = 0;
    replace_falsepos = 0;
    replacement = "/*(DEBLOBBED)*/";

    # Should we print lines containing blobs, false positives, and neither?
    print_blob = 0;
    with_context = 0;
    print_falsepos = 0;
    print_nomatch = 0;

    # Should we print the input stack and exit if we find blobs or
    # false positives?
    list_blob = 0;
    list_falsepos = 0;

    # Should we forget everything we know about false positives?
    no_falsepos = 0;

    verbose = $vp;

    nfilenames = 0;
    s = "\n";

    # Which of the defaults above should we override?
    $@ = 1;

    # requires GNU awk RS extension:
$xrs	RS = "[;][/][*](begin|end) [^\n]*[*][/][;][\n]";
}
# requires GNU awk RS extension:
$xrs { s = s \$0; }
# does not require GNU awk RS extension:
$nrs !/^[;][/][*].*[*][/][;]$/ {
$nrs	 s = s \$0 "\n";
$nrs	 next;
$nrs }
$eormatch /^[;][/][*]begin .*[*][/][;]$eornl$/ {
    filenames[nfilenames] = substr($eor, 10, length ($eor) - 12 - $eornlsz);
    if (verbose) print "entering " nfilenames ": " filenames[nfilenames];
    nextnfilenames = nfilenames + 1;
    if (s == "\n") {
	nfilenames = nextnfilenames;
	next;
    }
}
$eormatch /^[;][/][*]end .*[*][/][;]$eornl$/ {
    nextnfilenames = nfilenames - 1;
    if (verbose)
	print "got to the end of " nextnfilenames ": " filenames[nextnfilenames];
}
{
    if (verbose) {
	print "looking for matches";
	for (i = nfilenames; --i > 0;)
	    print filenames[i] " within";
	print filenames[0]
    }

    s = substr (s, 1, length (s) - 1)

    pp = 2;
    p = pend = 1;
    if (verbose > 1) print "searching starting at", substr (s, p, 10)
    matchfound = match (substr (s, p),
			/[\n]($falsepos)|[\n]($cblob)|.($blob)/);
    while (matchfound) {
	blobs = falses = 0;
	firstmatchstart = RSTART + p;
	for (;;) {
	    matchstart = RSTART + p - 1;
	    matchlen = RLENGTH;
	    if (verbose) {
		print "found match", matchstart, matchlen;
		if (verbose > 1)
		    print substr (s, matchstart + 1, matchlen - 1);
	    }

	    if (match (substr (s, matchstart, matchlen), /^[\n]($falsepos)/) == 1) {
		matchlen = RLENGTH;
		if (verbose) print "match is a false positive of length", matchlen;
		blob_p = 0;
		falses++;
	    } else if (match (substr (s, matchstart, matchlen), /^.($blob)/) == 1) {
		matchlen = RLENGTH;
		if (verbose) print "match is a blob of length", matchlen;
		blob_p = 1;
		blobs++;
	    } else if (match (substr (s, matchstart, matchlen), /^[\n]($cblob)$/) == 1) {
		if (verbose) print "match is a blob context";
		pend = index (substr (s, matchstart + matchlen), "\n");
		if (pend)
		    pend += matchstart + matchlen;
		else
		    pend = length (s);
		p = matchstart + 1;
		blob_p = 2;
		if (verbose > 1) print "range is:", substr (s, p, pend - p);
	    }

	    if (blob_p < 2) {
		if (blob_p ? replace_blob : replace_falsepos) {
		    s = substr (s, 1, matchstart)		\\
			replacement				\\
			substr (s, matchstart + matchlen);
		    p = matchstart + length (replacement) - 1;
		    pend += (p + 1 - matchstart - matchlen);
		} else
		    p = matchstart + matchlen - 1;

		if (p >= pend) {
		    i = index (substr (s, p + 1), "\n");
		    if (i)
			pend = p + 1 + i;
		    else
			pend = length (s)
		}
	    }

	    if (verbose) print "search until", pend;

	    if (!(matchfound = match (substr (s, p),
				      /[\n]($falsepos)|[\n]($cblob)|.($blob)/)) ||
		p + RSTART >= pend ||
		(blob_p ?
		 (!print_blob && !falses) :
		 (!print_falsepos && !blobs)))
		break;
	}

	if (print_nomatch)
	    printf "%s", substr (s, pp, firstmatchstart - pp);
	else if (print_blob || print_falsepos) {
	    lastline = substr (s, pp, firstmatchstart - pp);
	    sub (/.*[\n]/, "", lastline);
	    if (verbose) print "lastline: " lastline "\\\\n"
	    firstmatchstart -= length (lastline);
	}
	pp = firstmatchstart;

	if (verbose) print "match set range:", pp, pend

	if ((print_blob && blobs) || (print_falsepos && falses)) {
	    if (!print_nomatch)
		for (i = nfilenames; i-- > 0;)
		    print "::: " filenames[i] " :::";
	    printf "%s", substr (s, pp, pend - pp);
	    pp = pend;
	}

	if ((list_blob && blobs) || (list_falsepos && falses)) {
	    for (i = nfilenames; --i > 0;)
		print filenames[i] " within";
	    print filenames[0];
	    exit (1);
	}
    }

    if (print_nomatch)
	printf "%s", substr (s, pp)

    if (verbose)
	print "no further matches";

    s = "\n";
    nfilenames = nextnfilenames;
    next;
}
EOF

  scriptcmd="${AWK-gawk} --re-interval -f "'"$scriptname"'
}

set_flex_main () {
  adjust_rx='
s,\\\([{(|)}?+]\),\1,g
s,^\([-+]\)\(\^\?\)\(.*\)\(\$\?\)$,\2(?s:\3)\4\1,g
s,[+]$, { falsepos (); },
s,[-]$, { blob (); },
'

  echo '%%' > "$scriptname"
  ${SED-sed} "$adjust_rx" < "$regex_name" >> "$scriptname"
  echo '\n|. { unmatched (); }
%%
int falsepos () {}
int blob () {}
int unmatched () {}
' >> "$scriptname"

  scriptcmd=false
}

set_save_script_input_main () {
  savename=`mktemp -t deblob-check-input-XXXXXX`
  scriptcmd="{ echo saving input in $savename && cat > $savename && echo done; }"
}

# Process an input file named in $1 and run it through the blob
# recognizer.  Functions set_except and set_sed_cmd provide additional
# arguments on a per-file and per-action basis.

check () {
  case "$#" in 1) ;; *) echo ICE >&2; exit 1;; esac

  input=$1

  # Add $1 to falsepos.  Its usage makes it implicitly anchored to the
  # beginning of the line.  $2, if present, will some day narrow the
  # falsepos matches to files that match it.
  addx () {
    $echo "+^$1" >> $regex_name
  }

  # Add $1 to falseneg.  Unlike addx, it is NOT implicitly anchored to
  # the beginning of the line.  $2, if present, will some day narrow
  # the falseneg matches to files that match it.
  badx () {
    $echo "-$1" >> $regex_name
  }

  # Look for a multi-line definition starting with a line that matches
  # $1 (implicitly anchored to the beginning of the line), and ending
  # at the first ';'.  $2 may optionally name the files in which this
  # match is to be disregarded as a potential blob.
  initnc () {
    addx "$1[^;]*[;]\\?" $2
  }

  # Same as initnc, but require the terminating semicolon.
  defsnc () {
    addx "$1[^;]*[;]" $2
  }

  # Look for a multi-line definition starting with a line that matches
  # $1 (implicitly anchored to the beginning of the line), and ending
  # at the first ';' that's not within comments.
  initc () {
    addx "$1\\([^;/]\\+\\($comment\\|[/][^/*;]\\)\\+\\)*[^;/]*[;]\\?" $2
  }

  # Same as initc, but require the terminating semicolon.
  defsc () {
    addx "$1\\([^;/]\\+\\($comment\\|[/][^/*;]\\)\\+\\)*[^;/]*[;]" $2
  }

  # Accept as a non-blob an expression $1 that would have otherwise
  # triggered blob detection.  The expression must end in a way that
  # would trigger the blob detection machinery.
  accept () {
    addx "$1" $2
  }

  # Match up to the end a comment started in $1.
  ocomment () {
    addx "$1[/]*\\([*]*[^*/][/]*\\)*[*]\+[/]" $2
  }

  # Match $1 followed by backslash-terminated lines and a last
  # non-backslash-terminated line.
  oprepline () {
    addx "$1\\([^\\\\\\n]*[\\\\][\\n]\\)*[^\\\\\\n]*$" $2
  }

  # Match $1 in $2 as a blob.  Not anchored.
  blobna () {
    badx "$1" $2
  }

  # Match $1 as a blob anywhere.  $2 is just for documentation purposes.
  blobname () {
    badx "$1" $2
  }

  # Match $1 in $2 as a blob.  The expectation is a match in the
  # beginning of line, but we don't do anchoring of blob patterns ATM.
  blob () {
    badx "$1" $2
  }

  regex_name=`mktemp -t deblob-check-regex-XXXXXX`
  tempfiles="$regex_name"

  set_except "$input"

  # Check that all regular expressions match our requirements.
  ${SED-sed} -n '
s,^\(-\^\?\|[+]\^\),,
h
s,[$]$,,
s,\([^\\]\|^\)\(\(\\\\\)*\)\(\[^\?[]]\?[^]]\+\]\([*]\|\\[+?]\)\?\(\\\\\)*\)\+,\1\2,g
/\([^\\]\|^\)\(\\\\\)*\([{(|)}?+^$"'"'"'; 	]\)\|^$/{
  g
  i\
BAD regular expression:
  p
  q 1
}' $regex_name >&2 || exit 1

  scriptname=`mktemp -t deblob-check-script-XXXXXX`
  tempfiles="$tempfiles $scriptname"

  scriptcmd=false
  scriptcmd2=

  $set_cmd "$input"

  for f in $tempfiles; do
    case $f in "$scriptname") ;;
    *) rm -f "$f" ;;
    esac
  done
  tempfiles="$scriptname"

  # Choose the input source...
  case $input in
  -) in= ;;
  *) in='< "$input"' ;;
  esac

  set fnord # shifted out below

  # Decompress as needed...
  case $input in
  *.bz2) cmd='bunzip2' ;;
  *.xz) cmd='unxz' ;;
  *.lz) cmd='lzip -d' ;;
  *.gz | *.tgz) cmd='gunzip' ;;
  *) cmd= ;;
  esac
  if test -n "$cmd"; then
    set "$@" "$cmd"
  fi

  # Extract or otherwise munge...
  case /$input in
  *.tar*)
    tarwrap=`mktemp -t deblob-check-tarwrap-XXXXXX`
    tempfiles="$tempfiles $tarwrap"
    
    cat >> $tarwrap <<EOF
#! /bin/sh
echo='$echo' &&
if test "$DEBUG_VERBOSE_TARX_DEBLOB_CHECK" = yes; then \$echo "\$1" >&2; fi &&
\$echo ";/*begin \$1*/;" &&
cat &&
echo &&
\$echo ";/*end \$1*/;"
EOF
    chmod +x $tarwrap
    cmd="tar -xf - --to-command='$tarwrap \"\$TAR_FILENAME\"'"
    ;;
  *.patch | *.patch.*z* | */patch-* | *.diff | *.diff.*z*)
    if $reverse_patch; then
      s=- r=+
    else
      s=+ r=-
    fi
    sedpatch="
      /^[$r]/b testlastline;
      # /^[*!]/ {
      # 	s,^,context diffs are not properly supported\\n,;
      # 	W /dev/stderr
      # 	d;
      # }
      /^\\(@@ \\|$s$s$s \\|[^$s @]\\|$\\)/ {
	x;
	/^@@ /{
	  s,^,;/*end ,;
	  s,\\([\\n]\\|$\\),*/;&,;
	  i\\
;/**/;

	  P;
	  s,^[^\\n]*\\([\\n]\\|$\\),,;
	}
	x;
      }
      /^\\($s$s$s \\|[^$s @]\\|$\\)/ {
	x;
	/^$s$s$s /{
	  s,^$s$s$s,;/*end,;
	  s,\\([\\n]\\|$\\),*/;&,;
	  i\\

	  P;
	  s,^[^\\n]*\\([\\n]\\|$\\),,;
	}
	x;
      }
      /^$s$s$s / {
	H;
	x;
	s,^[\\n],,;
	s,^\\(.*\\)[\\n]\\([^\\n]*\\)$,\\2\\n\\1,;
	x;
	s,^$s$s$s \\(.*\\)$,;/*begin \\1*/;,;
	p;
	d;
      }
      /^@@ / {
        H;
	x;
	s,^[\\n],,;
	s,^\\(.*\\)[\\n]\\([^\\n]*\\)$,\\2\\n\\1,;
	x;
	# A number of patterns for patches depend on the ;/*@@ lines for
	# context.
	s,^.*$,;/*begin &*/;\\n;/*&*/;,;
	p;
	d;
      }
      s,^[ !$s],,
      p;
      :testlastline
      $ {
	x;
	/^@@ /{
	  s,^,;/*end ,;
	  s,\\([\\n]\\|$\\),*/;&,;
	  i\\
;/**/;

	  P;
	  s,^[^\\n]*\\([\\n]\\|$\\),,;
	}
	/^$s$s$s /{
	  s,^$s$s$s,;/*end,;
	  s,\\([\\n]\\|$\\),*/;&,;
	  i\\

	  P;
	  s,^[^\\n]*\\([\\n]\\|$\\),,;
	}
	x;
      }
      d;"
    cmd='${SED-sed} "$sedpatch"'
    ;;
  *)
    cmd='cat'
    ;;
  esac
  cmd="{ echo \";/*begin $input*/;\"; $cmd; echo; echo \";/*end $input*/;\"; }"
  set "$@" "$cmd"

  case $input in
  *.tar*)
    cmd="{ cat; cat > /dev/null; }"
    set "$@" "$cmd"
    ;;
  esac

  # Then run through the selected action.
  set "$@" "$scriptcmd"

  case $scriptcmd2 in "" | cat) ;;
  *) set "$@" "$scriptcmd2"
  esac

  # test $# = 1 || set "$@" "cat"

  shift # fnord goes out here

  pipe=
  for cmd
  do
    if test -z "$pipe"; then
      pipe="$cmd $in"
    else
      pipe="$pipe | $cmd"
    fi
  done

  eval "$pipe"
  status=$?

  $rm $tempfiles
  tempfiles=

  (exit $status)
}

# If no input given, use stdin.
case $# in
0)
  test -t 0 && echo reading from standard input >&2
  set fnord -
  shift
  ;;
esac

# The lines below commented out out #list: can be used to get a list
# of matching inputs.  ATM this is useless, so we just use a shell
# boolean.

#list: n=$#
pass=:

tempfiles=
trap "status=$?; test -z \"$tempfiles\" || rm -f $tempfiles; (exit $status); exit" 0 1 2 15

process_arg=

# Go through each of the input files in the command line.
for file
do
  case $process_arg in
  "") ;;
  --implied-prefix | --prefix | -i)
    prefix=$file
    case $prefix in
    /*/) ;;
    */) prefix=/$prefix ;;
    /*) prefix=$prefix/ ;;
    *) prefix=/$prefix/ ;;
    esac
    process_arg=
    continue
    ;;
  *)
    echo Internal error with process_arg=$process_arg >&2
    exit 1
    ;;
  esac

  case $sawdashdash$file in
  --implied-prefix | --prefix | -i)
    process_arg=$file
    continue
    ;;
  esac

  # If we print anything whatsoever (even a blank line) while
  # processing it, we've failed.
  if check "$file"; then
    :
  else
    pass=false
    #list: set fnord "$@" "$file"
    #list: shift
  fi
done

case $process_arg in
"") ;;
*)
  echo Missing argument to $process_arg >&2
  exit 1
  ;;
esac

#list: shift $n

#list: exec test $# = 0
$pass
exit
