diff --git a/README.md b/README.md
index aaa7caa..293545b 100644
--- a/README.md
+++ b/README.md
@@ -1,7 +1,3 @@
-[![pipeline status](https://salsa.debian.org/freedombox-team/freedom-maker/badges/master/pipeline.svg)](https://salsa.debian.org/freedombox-team/freedom-maker/commits/master)
-[![Debian Unstable](https://badges.debian.net/badges/debian/unstable/freedom-maker/version.svg)](https://packages.debian.org/unstable/freedom-maker)
-[![Debian Testing](https://badges.debian.net/badges/debian/testing/freedom-maker/version.svg)](https://packages.debian.org/testing/freedom-maker)
-
 # Freedom-Maker: The FreedomBox image builder
 
 These scripts build FreedomBox-images for various supported hardware
@@ -13,9 +9,9 @@ during releases and for advanced users who intend to build their own
 images. Regular users who wish to turn their devices into
 FreedomBoxes should instead download the pre-built images.
 
-Get a pre-built image via https://freedombox.org/download/.  There
+Get a pre-built image via https://cdimage.trisquel.info/trisquel-images/. There
 are images available for all supported target devices.  You also find
-the setup instructions on the [Wiki](https://wiki.debian.org/FreedomBox/).
+the setup instructions on the [Wiki](https://trisquel.info/en/wiki/FreedomBox/).
 
 If you wish to create your own FreedomBox image, perhaps with some
 tweaks, see the *Build Images* section below.
@@ -24,7 +20,7 @@ tweaks, see the *Build Images* section below.
 
 ## Supported Targets
 
-Freedom-maker supports building for the following targets:
+Trisquel Freedom-maker supports building for the following targets:
 
 | target                | description |
 |-----------------------|-------------|
@@ -42,25 +42,18 @@ Trisquel Freedom-maker supports building for the following targets:
 | *pine64-plus* | Pine64+ board's SD card |
 | *qemu-amd64* | 64-bit image for the Qemu virtualization tool |
 | *qemu-i386* | 32-bit image for the Qemu virtualization tool |
-| *raspberry2* | RasbperryPi 2's SD card |
-| *raspberry3* | RasbperryPi 3's SD card |
-| *raspberry3-b-plus* | RasbperryPi 3 Model B+'s SD card |
-| *raspberry64* | Single image for Raspberry Pi 3B, Raspberry Pi 3B+ and Raspberry Pi 4B |
-| *virtualbox-amd64* | 64-bit image for the VirtualBox virtualization tool |
-| *virtualbox-i386* | 32-bit image for the VirtualBox virtualization tool |
 
 ## Running Build
 
-1. Fetch the git source of freedom-maker:
+1. Fetch the 'freedom-maker' source code:
     ```
-    $ git clone https://salsa.debian.org/freedombox-team/freedom-maker.git
+    $ apt source freedom-maker
     ```
 
 2. Install the required dependencies:
     ```shell
     $ sudo apt install binfmt-support btrfs-progs debootstrap dmsetup dosfstools fdisk git kpartx parted psmisc qemu-user-static qemu-utils sshpass sudo u-boot-tools xz-utils
-    $ cd freedom-maker
-    $ sudo apt build-dep .
+    $ sudo apt build-dep freedom-maker
     ```
 
 3. Build images:
@@ -73,6 +62,7 @@ Freedom-maker supports building for the following targets:
     to run "parted".
 
     ```
+    $ cd $(find -type d -name 'freedom-maker-*')
     $ sudo python3 -m freedommaker <TARGET>
     ```
     where: &lt;TARGET&gt; is one of the 'Supported Targets' above.
diff --git a/doc/freedom-maker.xml b/doc/freedom-maker.xml
index 09c2f001..8c4abdd6 100644
--- a/doc/freedom-maker.xml
+++ b/doc/freedom-maker.xml
@@ -85,7 +85,7 @@
         <term> <option>--build-mirror</option></term>
          <listitem>
           <para>
-            Debian mirror to use for building
+            Trisquel mirror to use for building
           </para>
         </listitem>
       </varlistentry>
@@ -93,7 +93,7 @@
         <term> <option>--mirror</option></term>
          <listitem>
            <para>
-             Debian mirror to use in built image
+             Trisquel mirror to use in built image
           </para>
         </listitem>
       </varlistentry>
@@ -101,15 +101,7 @@
         <term> <option>--distribution</option></term>
          <listitem>
            <para>
-             Debian release to use in built image
-          </para>
-        </listitem>
-      </varlistentry>
-      <varlistentry>
-        <term> <option>--add-release-component</option></term>
-         <listitem>
-           <para>
-             Add an extra Debian release component (other than main)
+             Trisquel release to use in built image
           </para>
         </listitem>
       </varlistentry>
@@ -208,12 +200,10 @@
         <term> <option>targets</option></term>
         <listitem>
           <para>
-            Image targets to build. Choose one or more of a20-olinuxino-lime,
-            a20-olinuxino-lime2, a20-olinuxino-micro, amd64, arm64, armhf,
-            banana-pro, beaglebone, cubieboard2, cubietruck, i386, lamobo-r1,
-            orange-pi-zero, pcduino3, pine64-lts, pine64-plus, qemu-amd64,
-            qemu-i386, raspberry2, raspberry3, raspberry3-b-plus, raspberry64,
-            vagrant virtualbox-amd64, virtualbox-i386
+            Image targets to build. Choose one or more of freedommaker,
+            dreamplug, beaglebone, cubieboard2, cubietruck,
+            a20-olinuxino-lime,a20-olinuxino-lime2, a20-olinuxino-micro,
+            i386, amd64, qemu-i386, qemu-amd64, pcDuino3
           </para>
         </listitem>
       </varlistentry>
@@ -236,8 +226,7 @@
       <synopsis>$ freedommaker a20-olinuxino-lime a20-olinuxino-lime2
       a20-olinuxino-micro amd64 arm64 armhf banana-pro beaglebone cubieboard2
       cubietruck i386 lamobo-r1 orange-pi-zero pcduino3 pine64-lts pine64-plus
-      qemu-amd64 qemu-i386 raspberry2 raspberry3 raspberry3-b-plus raspberry64
-      vagrant virtualbox-amd64 virtualbox-i386</synopsis>
+      qemu-amd64 qemu-i386</synopsis>
       <para>
         Build all the available FreedomBox images using freedom-maker.
       </para>
